<?xml version="1.0" encoding="windows-1252"?><SEC xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="http://si.ksc.nasa.gov/sidownloads/xml/specsintactSEC.xsd"><MTA NAME="SUBFORMAT" CONTENT="NEW"/><MTA NAME="AUTONUMBER" CONTENT="TRUE"/><HDR><AST/><TAB BORDERS="0">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="4">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="366.00"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="365.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="14.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">USACE / NAVFAC / AFCEC</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">UFGS-01 35 26 (May 2024)</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="10.50">
         <CEL MERGEDOWN="1" STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Change 1 - 05/25</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="10.50">
         <CEL INDEX="2" STYLEID="s50">
<DTA TYPE="STRING"><HL3>------------------------------------</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="48.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Preparing Activity:  <PRA>NAVFAC</PRA></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Superseding<BRK/>UFGS-01 35 26 (November 2020)</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<HL4>UNIFIED FACILITIES GUIDE SPECIFICATIONS</HL4><BRK/>
<BRK/>
<HL4>References are in agreement with UMRL dated July 2025</HL4><BRK/>
<AST/><BRK/></HDR>
<BRK/>
<SCN>SECTION 01 35 26</SCN><BRK/>
<BRK/>
<STL>GOVERNMENTAL SAFETY REQUIREMENTS</STL><BRK/>
<DTE>05/24, CHG 1: 05/25</DTE><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This guide specification covers the requirements for <SCP>safety and occupational health requirements for the 
protection of Contractor and Government personnel, property, and resources</SCP>.</NPR><BRK/>
<BRK/>
<NPR>This guide specification is intended for use in Contracts that specify FAR 52.236-13 Accident Prevention, or its 
Alternate I, to include Contracts for construction, dismantling, renovation and demolition; dredging; environmental 
restoration (investigation, design, remediation); asbestos abatement or lead hazard control; projects in the continental 
U.S. and overseas.</NPR><BRK/>
<BRK/>
<NPR>The requirements of this guide specification are a supplement to the U.S. Army Corps of Engineers (USACE) Safety 
and Occupational Health Requirements, EM 385-1-1 and clarify safety concerns for high-risk construction activities.</NPR><BRK/>
<BRK/>
<NPR>Adhere to <URL HREF="https://www.wbdg.org/dod/ufc/ufc-1-300-02">UFS 1-300-02</URL> Unified Facilities Guide Specifications (UFGS) Format Standard when editing this guide 
specification or preparing new project specification sections.  Edit this guide specification for project specific 
requirements by adding, deleting, or revising text.  For bracketed items, choose applicable item(s) or insert 
appropriate information.</NPR><BRK/>
<BRK/>
<NPR>All additions to the specification by the designers, must be written in accordance with the Plain Writing Act 
of 2010.</NPR><BRK/>
<BRK/>
<NPR>Remove information and requirements not required in respective project, whether or not brackets are present.</NPR><BRK/>
<TAI OPT="NAVY"><BRK/>
<NPR>The Contractor Safety Self-Evaluation Checklist is available for download on the Whole Building Design Guide at: <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-01-35-26">
https://www.wbdg.org/dod/ufgs/ufgs-01-35-26</URL></NPR><BRK/></TAI>
<BRK/>
<NPR>Comments, suggestions and recommended changes for this guide specification are welcome and should be submitted 
as a <URL HREF="https://www.wbdg.org/dod/ufgs">Criteria Change Request (CCR)</URL>.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This guide specification includes tailoring for DESIGN-BUILD, DESIGN-BID-BUILD, ARMY, NAVY, NAVFAC MAR, 
NAVFAC HI, NAVFAC PAC, INDOOR AIR QUALITY, and DREDGING projects.  Where an Editor's Note states a paragraph is 
tailored for a Service or project type, the content of the paragraph, or a portion of the paragraph, is suited 
specifically to be included only for that Service or project type.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include other referenced sections in the Contract where work, such as environmental restoration, asbestos 
abatement, or lead hazard control, requires additional safety and health plans to be made part of and appended 
to the APP.  These sections include Section <SRF>01 35 29.13</SRF> HEALTH, SAFETY, AND EMERGENCY RESPONSE PROCEDURES FOR 
CONTAMINATED SITES for environmental restoration project; Section <SRF>02 82 00</SRF> ASBESTOS REMEDIATION, for asbestos 
abatement; Section <SRF>02 83 00</SRF> LEAD REMEDIATION for lead hazard control activities; and Section <SRF>02 85 00</SRF> MOLD REMEDIATION.  
For NAVY environmental restoration Contracts, an APP is required with the overall Contract and a site specific 
Health and Safety Plan is required for each task order (contact the FEAD Safety Manager for applicability).</NPR><BRK/>
<BRK/>
<NPR>Many states and municipalities have more stringent or additional requirements; modify this section as required 
to meet local requirements and regulations.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<PRT><TTL>PART 1   GENERAL</TTL><BRK/>
<BRK/>
<SPT><TTL>REFERENCES</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is used to list the publications cited in the text of the guide specification.  The publications 
are referred to in the text by basic designation only and listed in this paragraph by organization, designation, 
date, and title.</NPR><BRK/>
<BRK/>
<NPR>Use the Reference Wizard's Check Reference feature when you add a Reference Identifier (RID) outside of the Section's 
Reference Article to automatically place the reference in the Reference Article.  Also use the Reference Wizard's 
Check Reference feature to update the issue dates.</NPR><BRK/>
<BRK/>
<NPR>References not used in the text will automatically be deleted from this section of the project specification when 
you choose to reconcile references in the publish print process.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The publications listed below form a part of this specification to the extent referenced.  The publications are referred to within the text by 
the basic designation only.</TXT><BRK/>
<BRK/>
<REF><ORG>AMERICAN SOCIETY OF HEATING, REFRIGERATING AND AIR-CONDITIONING ENGINEERS (ASHRAE)</ORG><BRK/>
<BRK/>
<RID>ASHRAE 52.2</RID><RTL>(2017; Addenda B 2020; Errata 1 2020; Addenda C 2022; Errata 2 2024; Addenda D 
2025) Method of Testing General Ventilation Air-Cleaning Devices for Removal Efficiency 
by Particle Size</RTL><BRK/>
<BRK/></REF>
<REF><ORG>AMERICAN SOCIETY OF SAFETY PROFESSIONALS (ASSP)</ORG><BRK/>
<BRK/>
<RID>ANSI/ASSP A10.34</RID><RTL>(2021) Protection of the Public on or Adjacent to Construction Sites</RTL><BRK/>
<BRK/>
<RID>ANSI/ASSP A10.44</RID><RTL>(2020) Control of Energy Sources (Lockout/Tagout) for Construction and Demolition 
Operations</RTL><BRK/>
<BRK/>
<RID>ANSI/ASSP Z490.1</RID><RTL>(2016) Criteria for Accepted Practices in Safety, Health, and Environmental Training</RTL><BRK/>
<BRK/></REF>
<REF><ORG>ASTM INTERNATIONAL (ASTM)</ORG><BRK/>
<BRK/>
<RID>ASTM D6245</RID><RTL>(2012) Using Indoor Carbon Dioxide Concentrations to Evaluate Indoor Air Quality 
and Ventilation</RTL><BRK/>
<BRK/>
<RID>ASTM D6345</RID><RTL>(2010) Standard Guide for Selection of Methods for Active, Integrative Sampling 
of Volatile Organic Compounds in Air</RTL><BRK/>
<BRK/>
<RID>ASTM F855</RID><RTL>(2020) Standard Specifications for Temporary Protective Grounds to Be Used on 
De-energized Electric Power Lines and Equipment</RTL><BRK/>
<BRK/></REF>
<REF><ORG>INSTITUTE OF ELECTRICAL AND ELECTRONICS ENGINEERS (IEEE)</ORG><BRK/>
<BRK/>
<RID>IEEE 1048</RID><RTL>(2016) Guide for Protective Grounding of Power Lines</RTL><BRK/>
<BRK/>
<RID>IEEE C2</RID><RTL>(2023) National Electrical Safety Code</RTL><BRK/>
<BRK/></REF>
<REF><ORG>INTERNATIONAL SAFETY EQUIPMENT ASSOCIATION (ISEA)</ORG><BRK/>
<BRK/>
<RID>ANSI/ISEA Z89.1</RID><RTL>(2014; R 2019) American National Standard for Industrial Head Protection</RTL><BRK/>
<BRK/></REF>
<REF><ORG>NATIONAL ELECTRICAL MANUFACTURERS ASSOCIATION (NEMA)</ORG><BRK/>
<BRK/>
<RID>NEMA Z535.2</RID><RTL>(2011; R 2017)  Environmental and Facility Safety Signs</RTL><BRK/>
<BRK/></REF>
<REF><ORG>NATIONAL FIRE PROTECTION ASSOCIATION (NFPA)</ORG><BRK/>
<BRK/>
<RID>NFPA 51B</RID><RTL>(2024) Standard for Fire Prevention During Welding, Cutting, and Other Hot Work</RTL><BRK/>
<BRK/>
<RID>NFPA 70</RID><RTL>(2023; ERTA 1 2024; TIA 24-1; TIA 25-2) National Electrical Code</RTL><BRK/>
<BRK/>
<RID>NFPA 70E</RID><RTL>(2024) Standard for Electrical Safety in the Workplace</RTL><BRK/>
<BRK/>
<RID>NFPA 241</RID><RTL>(2022; ERTA 22-1) Standard for Safeguarding Construction, Alteration, and Demolition 
Operations</RTL><BRK/>
<BRK/>
<RID>NFPA 306</RID><RTL>(2024) Standard for the Control of Gas Hazards on Vessels</RTL><BRK/>
<BRK/></REF>
<REF><ORG>SHEET METAL AND AIR CONDITIONING CONTRACTORS' NATIONAL ASSOCIATION (SMACNA)</ORG><BRK/>
<BRK/>
<RID>ANSI/SMACNA 008</RID><RTL>(2007) IAQ Guidelines for Occupied Buildings Under Construction, 2nd Edition</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. ARMY CORPS OF ENGINEERS (USACE)</ORG><BRK/>
<BRK/>
<RID>EM 385-1-1</RID><RTL>(2024) Safety -- Safety and Occupational Health (SOH) Requirements</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. NATIONAL ARCHIVES AND RECORDS ADMINISTRATION (NARA)</ORG><BRK/>
<BRK/>
<RID>10 CFR 20</RID><RTL>Standards for Protection Against Radiation</RTL><BRK/>
<BRK/>
<RID>29 CFR 1910</RID><RTL>Occupational Safety and Health Standards</RTL><BRK/>
<BRK/>
<RID>29 CFR 1915</RID><RTL>Confined and Enclosed Spaces and Other Dangerous Atmospheres in Shipyard Employment</RTL><BRK/>
<BRK/>
<RID>29 CFR 1919</RID><RTL>Gear Certification</RTL><BRK/>
<BRK/>
<RID>29 CFR 1926</RID><RTL>Safety and Health Regulations for Construction</RTL><BRK/>
<BRK/>
<RID>49 CFR 173</RID><RTL>Shippers - General Requirements for Shipments and Packagings</RTL><BRK/>
<BRK/>
<RID>CPL 2.100</RID><RTL>(1995) Application of the Permit-Required Confined Spaces (PRCS) Standards, 29 
CFR 1910.146</RTL><BRK/>
<BRK/></REF>
</SPT><SPT><TTL>DEFINITIONS</TTL><BRK/>
<BRK/>
<TXT>The following definitions are for the convenience of the reader.  If there is a referenced document in the text of this specification section, 
that is the document that should define terms for that paragraph.  If further clarification is needed, contact the Contracting Officer.</TXT><BRK/>
<BRK/>
<SPT><TTL>Site Safety and Health Officer (SSHO)</TTL><BRK/>
<BRK/>
<TXT>A Contractor Employee that is responsible for overseeing and ensuring implementation of the prime Contractor's Safety and Occupational Health (SOH) 
program according to the Contract, <RID>EM 385-1-1</RID>, applicable federal, state, and local requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Level One SSHO</TTL><BRK/>
<BRK/>
<TXT>A designated employee with full-time SOH responsibility that meets and follows the requirements of <RID>EM 385-1-1</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Level Two SSHO</TTL><BRK/>
<BRK/>
<TXT>A designated employee with Level Two SSHO responsibility that meets and follows the requirements of <RID>EM 385-1-1</RID>.  Level Two SSHOs cannot be assigned 
to projects that have a residual Risk Assessment Code (RAC) of high or extremely high.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Level Three SSHO</TTL><BRK/>
<BRK/>
<TXT>A designated Qualified Person or Competent Person with SOH responsibility that meets and follows the requirements of <RID>EM 385-1-1</RID>.  Level 3 SSHOs 
cannot be assigned to projects that have a residual RAC of high or extremely high.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Alternate SSHO</TTL><BRK/>
<BRK/>
<TXT>An employee that meets the definition of the contract-required level SSHO, but is not the primary SSHO.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Competent Person (CP)</TTL> <BRK/>
<BRK/>
 <TXT>The CP is a person designated in writing, who, through training, knowledge and experience, is capable of identifying, evaluating, and addressing 
existing and predictable hazards in the working environment or working conditions that are unsanitary, hazardous, or dangerous to personnel, and 
who has authorization to take prompt corrective measures to eliminate them.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Qualified Person (QP)</TTL><BRK/>
<BRK/>
<TXT>The QP is a person designated in writing, who, by possession of a recognized degree, certificate, or professional standing, or extensive knowledge, 
training, and experience, has successfully demonstrated their ability to solve or resolve problems related to the subject matter, the work, or 
the project.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>SUBMITTALS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Review Submittal Description (SD) definitions in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES and edit the following 
list, and corresponding submittal items in the text, to reflect only the submittals required for the project.  
The Guide Specification technical editors have classified those items that require Government approval, due to 
their complexity or criticality, with a "G."  Generally, other submittal items can be reviewed by the Contractor's 
Quality Control System.  Only add a "G" to an item if the submittal is sufficiently important or complex in context 
of the project.</NPR><BRK/>
<BRK/>
<NPR><TAI OPT="ARMY">For Army projects, fill in the empty brackets following the "G" classification, with a code of up to three characters 
to indicate the approving authority.  Codes for Army projects using the Resident Management System (RMS) are:  
"AE" for Architect-Engineer; "DO" for District Office (Engineering Division or other organization in the District 
Office); "AO" for Area Office; "RO" for Resident Office; and "PO" for Project Office.  </TAI>Codes following the "G" 
typically are not used for Navy and Air Force projects.</NPR><BRK/>
<BRK/>
<NPR>The "S" classification indicates submittals required as proof of compliance for sustainability Guiding Principles 
Validation or Third Party Certification and as described in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Government Acceptance or Approval does not remove responsibility from the Contractors for their actions or liability.</TXT><BRK/>
<BRK/>
<TXT>Government approval is required for submittals with a "G" or "S" classification.<TAI OPT="AIR FORCE,NAVY">  Submittals not having a "G" or "S" classification are for Contractor 
Quality Control approval.</TAI><TAI OPT="ARMY">  Submittals not having a "G" or "S" classification are for information only.  When used, a code following the "G" classification 
identifies the office that will review the submittal for the Government.</TAI>  Submit the following in accordance with Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES:</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For NAVFAC PAC Area of Responsibility, select the "G" designation for Accident Prevention Plan (APP) and 
remove the "G" designation for Indoor Air Quality (IAQ) Management Plan, under the SD-01 Preconstruction Submittals.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<LST><SUB>SD-01 Preconstruction Submittals</SUB></LST><BRK/>
<BRK/>
<TAI OPT="DESIGN-BUILD"><ITM><SUB>Accident Prevention Plan (APP) Design</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/></TAI>
<ITM><SUB>Accident Prevention Plan (APP)<TAI OPT="DESIGN-BUILD"> Construction</TAI></SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Dive Operations Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<TAI OPT="INDOOR AIR QUALITY"><NTE><AST/><BRK/>
<NPR>NOTE:  The following two submittal items are tailored for INDOOR AIR QUALITY.  Include the following submittal 
when required by Section <SRF>01 33 29</SRF> SUSTAINABILITY REQUIREMENTS AND REPORTING, IAQ requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>Final IAQ Management Plan</SUB>; <SUB>S</SUB></ITM><BRK/>
<BRK/>
]<ITM><SUB>Indoor Air Quality (IAQ) Management Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/></TAI>
<LST><SUB>SD-06 Test Reports</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Accident Reports</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>LHE Inspection Reports</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Monthly Exposure Reports</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<LST><SUB>SD-07 Certificates</SUB></LST><BRK/>
<BRK/>
<TAI OPT="NAVFAC HI"><ITM><SUB>Crane Operators/Riggers</SUB></ITM><BRK/>
<BRK/></TAI>
<ITM><SUB>Activity Hazard Analysis (AHA)</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Certificate of Compliance</SUB></ITM><BRK/>
<BRK/>
<TAI OPT="NAVY"><ITM><SUB>Contractor Safety Self-Evaluation Checklist</SUB></ITM><BRK/>
<BRK/></TAI>
<ITM><SUB>Hot Work Permit</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>License Certificates</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Portable Gauge Operations Planning Worksheet</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Radiography Operation Planning Work Sheet</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Standard Lift Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Critical Lift Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<TAI OPT="NAVY"><ITM><SUB>Third Party Certification of Floating Cranes and Barge-Mounted Mobile Cranes</SUB></ITM><BRK/>
<BRK/></TAI>
</SPT><SPT><TTL>PUBLIC HEALTH EMERGENCIES</TTL><BRK/>
<BRK/>
<TXT>In the event of a declared public health emergency, follow safety precautions as required by the Occupational Safety and Health Administration 
(OSHA) <URL>www.osha.gov</URL>, the Centers for Disease Control and Prevention (CDC) <URL>www.cdc.gov</URL>, and as required by federal, state and local requirements.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>MONTHLY EXPOSURE REPORTS</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph contain ARMY tailoring.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide a Monthly Exposure Report by the fifth day of each month for the previous month.  This report is a compilation of employee-hours worked 
each month for all site workers, both Prime and subcontractor.  Failure to submit the report may result in retention of up to 10 percent of the 
progress payment.<TAI OPT="ARMY">  Submit the hours via the agency construction management system of record.</TAI></TXT><BRK/>
<BRK/></SPT>
<TAI OPT="NAVY"><SPT><TTL><SUB>CONTRACTOR SAFETY SELF-EVALUATION CHECKLIST</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph in NAVY projects only.  Do not use on ARMY projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Contracting Officer will provide a "Contractor Safety Self-Evaluation checklist" to the Contractor at the preconstruction conference.  Complete 
the checklist monthly and submit with each request for payment voucher.  This submission is required monthly even when a payment voucher is not 
requested.  An acceptable score of 90 or greater is required.  Failure to submit the completed safety self-evaluation checklist or achieve a score 
of at least 90 may result in retention of up to 10 percent of the voucher.  The Contractor Safety Self-Evaluation checklist can be found on the 
Whole Building Design Guide website at <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-01-35-26">www.wbdg.org/dod/ufgs/ufgs-01-35-26</URL></TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>REGULATORY REQUIREMENTS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Edit to include any additional requirements which apply to the work to be performed including Federal, state 
and local laws, regulations and statutes; Host Nation requirements; and NAVY, AIR FORCE and ARMY installation 
or US Army Corps of Engineers District requirements by authority and document number.  Consult with the supporting 
local Safety and Occupational Health Office (SOHO) for assistance in identifying local requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>In addition to the detailed requirements included in the provisions of this Contract, comply with the most recent edition of USACE <RID>EM 385-1-1</RID>, 
and the following[ federal, state, and local][ host nation] laws, ordinances, criteria, rules and regulations at the date of the Solicitation for 
this Contract.  Submit matters of interpretation of standards to the appropriate administrative agency for resolution before starting work.  Where 
the requirements of this specification, applicable laws, criteria, ordinances, regulations, and referenced documents vary, the most stringent requirements 
govern.</TXT><BRK/>
<BRK/>
<TAI OPT="NAVY"><SPT><TTL>Subcontractor Safety Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph and subsequent subparagraphs for NAVY projects in CONUS and Hawaii only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For this Contract, neither Contractor nor any subcontractor may enter into Contract with any subcontractor that fails to meet the following requirements.  
The term subcontractor in this and the following paragraphs means any entity holding a Contract with the Contractor or with a subcontractor at 
any tier.</TXT><BRK/>
<BRK/>
<SPT><TTL>Experience Modification Rate (EMR)</TTL><BRK/>
<BRK/>
<TXT>Subcontractors on this Contract must have an effective EMR less than or equal to 1.10, as computed by the National Council on Compensation Insurance 
(NCCI) or if not available, as computed by the state agency's rating bureau in the state where the subcontractor is registered, when entering into 
a subcontract agreement with the Prime Contractor or a subcontractor at any tier.  The Prime Contractor may submit a written request for additional 
consideration to the Contracting Officer where the specified acceptable EMR range cannot be achieved.  Relaxation of the EMR range will only be 
considered for approval on a case-by-case basis for special conditions and must not be anticipated as tacit approval.  Contractor's Site Safety 
and Health Officer (SSHO) must collect and maintain the certified EMR ratings for all subcontractors on the project and make them available to 
the Government at the Government's request.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>OSHA Days Away from Work, Restricted Duty, or Job Transfer (DART) Rate</TTL><BRK/>
<BRK/>
<TXT>Subcontractors on this Contract must have a DART rate, calculated from the most recent, complete calendar year, less than or equal to 3.4 when 
entering into a subcontract agreement with the Prime Contractor or a subcontractor at any tier.  The OSHA Dart Rate is calculated using the following 
formula:</TXT><BRK/>
<BRK/>
<LST>(N/EH) x 200,000</LST><BRK/>
<BRK/>
<LST>Where:</LST><BRK/>
<BRK/>
<LST>N = number of injuries and illnesses with days away, restricted work, or job transfer</LST><BRK/>
<BRK/>
<LST>EH = total hours worked by all employees during most recent, complete calendar year</LST><BRK/>
<BRK/>
<LST>200,000 = base for 100 full-time equivalent workers (working 40-hours per week, 50 weeks per year)</LST><BRK/>
<BRK/>
<TXT>The Prime Contractor may submit a written request for additional consideration to the Contracting Officer where the specified acceptable OSHA Dart 
rate range cannot be achieved for a particular subcontractor.  Relaxation of the OSHA DART rate range will only be considered for approval on a 
case-by-case basis for special conditions and must not be anticipated as tacit approval.  Contractor's Site Safety and Health Officer (SSHO) must 
collect and maintain self-certified OSHA DART rates for all subcontractors on the project and make them available to the Government at the Government's 
request.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI></SPT><SPT><TTL>SITE QUALIFICATIONS, DUTIES, AND MEETINGS</TTL><BRK/>
<BRK/>
<SPT><TTL>Site Safety and Health Officer (SSHO)</TTL><BRK/>
<BRK/>
<SPT><TTL>Qualifications of SSHO</TTL><BRK/>
<BRK/>
<TXT>All SSHOs will have met the training, experience requirements identified in the <RID>EM 385-1-1</RID> and this Contract.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Duties of SSHO</TTL><BRK/>
<BRK/>
<TXT>All SSHOs will carry out the roles and responsibilities as identified in this Contract and the <RID>EM 385-1-1</RID>.  All SSHOs will be designated on an 
ENG Form 6282, provided by the Contracting Officer.  Superintendent, QC Manager, and SSHO are subject to dismissal if their required duties are 
not being effectively carried out.  If either the Superintendent, QC Manager, or SSHO are dismissed, project work will be stopped and will not 
be allowed to resume until a suitable replacement is approved and the above duties are again being effectively carried out.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Safety Meetings</TTL><BRK/>
<BRK/>
<TXT>Conduct safety meetings to review past activities, plan for new or changed operations, review pertinent aspects of appropriate AHA (by trade), 
establish safe working procedures for anticipated hazards, and provide pertinent Safety and Occupational Health (SOH) training and motivation.  
Conduct meetings at least once a month for all supervisors at the project location.  The SSHO, supervisors, or foremen must conduct meetings at 
least once a week for the trade workers.  Document meeting minutes to include the date, persons in attendance, subjects discussed, and names of 
individual(s) who conducted the meeting.  Maintain documentation on-site and furnish copies to the Contracting Officer on request.  Notify the 
Contracting Officer of all scheduled meetings 7 calendar days in advance.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Roles and Responsibilities of Prime Contractor and SSHO</TTL><BRK/>
<BRK/>
<TXT>The Prime Contractor and SSHO must ensure that the requirements of all applicable OSHA and <RID>EM 385-1-1</RID> are met for the project.  The Prime Contractor 
must ensure an SSHO or an equally qualified Alternate SSHO(s) is at the worksite at all times to implement and administer the Contractor's safety 
program and Government accepted Accident Prevention Plan.  If the required SSHO has to temporarily (that is, up to 24 hours / 1 day) leave the 
site of work due to unforeseen or emergency situations, a Level One, Two, or Three SSHO may be used in the interim and must be on the site of work 
at all times when work is being performed.</TXT><BRK/>
<BRK/>
<TXT>If the SSHO must be off-site for a period longer than 24 hours / 1 day, a qualified alternate that meets the contract requirements must be onsite.</TXT><BRK/>
<OLG><BRK/>
<OLI>Prime contractor must ensure all SSHOs will:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Are designated on an ENG Form 6282.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Meet minimum training and experience requirements identified in <RID>EM 385-1-1</RID>.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Execute roles and responsibilities identified in <RID>EM 385-1-1</RID>.</OLI><BRK/></OLG>
<BRK/></SPT>
<TAI OPT="NAVY"><SPT><TTL>Additional Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVY.  Choose the bracketed items below when the project allows the SSHO 
to serve as the QC Manager or Superintendent or both.  Consult with the local NAVFAC, FEAD, or ROICC construction 
office to determine the potential for the SSHO to wear multiple hats on the specific project based on the hazards 
of the project, job complexity, size, and any other pertinent factors.  Coordinate with Section <SRF>01 45 00</SRF> QUALITY 
CONTROL.  A Level One must not serve any other roles.  A level Two or Three may serve in additional roles.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Level[ One][ Two][ Three] SSHO[ may also][ must not] serve as the Quality Control Manager.  The[ One][ Two][ Three] SSHO[ may also][ must not] 
serve as the Superintendent.</TXT><BRK/>
<TAI OPT="NAVFAC HI,NAVFAC MAR,NAVFAC PAC"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this subparagraph for NAVFAC Pacific (excluding Contingency Engineering), Hawaii, and Marianas projects 
only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The SSHO must have completed a 40-hour contract safety awareness course based on the content and principles of <RID>EM 385-1-1</RID>, and instructed in accordance 
with the guidelines of <RID>ANSI/ASSP Z490.1</RID>, by a trainer meeting the qualifications of paragraph QUALIFIED TRAINER REQUIREMENTS.  If the SSHO does 
not have a current certification, certification must be obtained within 60 days, maximum, of Contract award.</TXT><BRK/></TAI>
<BRK/></SPT>
</TAI>[<SPT><TTL>Contract Site Safety And Health Officer(s)(SSHOs) Minimum Requirements</TTL><BRK/>
<BRK/>
<TXT>Provide a minimum of one Level One SSHO that meets the requirements of <RID>EM 385-1-1</RID> for this project.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Contract Site Safety and Health Officer(s)(SSHOs) Minimum Requirements for Projects with[ Multiple Work Sites,][ Multiple Shifts,][ Limited Scope,][ 
or Maintenance, or Service Contracts].</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Insert this paragraph when a contract has:<BRK/>
<BRK/>
1)  More than one worksite or multiple shifts that require a separate full-time SSHO.<BRK/>
<BRK/>
2)  A limited Scope.<BRK/>
<BRK/>
3)  Maintenance and Service Contracts.</NPR><BRK/>
<BRK/>
<NPR>Fill in the worksite locations below and the required level of SSHO when a project has more than one worksite 
that requires a dedicated full-time SSHO.  Just because a project has more than one worksite does not automatically 
mean additional full-time SSHOs are required.  Only consider specifying additional full-time SSHOs when the contract 
includes separate projects and each project is uniquely different from one another usually having separate plans 
and specifications or large geographical distances.<TAI OPT="ARMY">  This is very rare and should only be specified after careful 
consideration and consultation with the KO, SOHO, and administering construction office.</TAI><TAI OPT="NAVY">  This is very rare and 
should only be specified after careful consideration and consultation with the FEAD/OICC/ROICC.</TAI>  Add or delete 
locations as needed.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide a separate full-time Level [One][Two][Three] SSHO at each of the following worksites:</TXT><BRK/>
<OLG><BRK/>
<OLI>[INDICATE WORKSITE LOCATION] Level [One][Two][Three] SSHO</OLI><BRK/>
<BRK/>
<OLI>[INDICATE WORKSITE LOCATION] Level [One][Two][Three] SSHO</OLI><BRK/>
<BRK/>
<OLI>[INDICATE WORKSITE LOCATION] Level [One][Two][Three] SSHO</OLI><BRK/></OLG>
<BRK/>
<TXT>The SSHOs for the worksites listed above must each have the required training, experience, and qualifications in accordance with <RID>EM 385-1-1</RID>.</TXT><BRK/>
<BRK/>
<TXT>Each SSHO is responsible for implementing and managing the Safety and Occupational Health (SOH) program at the worksite indicated, while ensuring 
that the <RID>29 CFR 1926</RID>, EM 385-1-1, Contracts, and all applicable federal, state, and Local requirements are met.</TXT><BRK/>
<BRK/></SPT>
]<TAI OPT="DREDGING"><SPT><TTL>Dredging Contract Site Safety and Health Officer(s)(SSHOs) Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>Note:  This paragraph and subsequent paragraphs are tailored for DREDGING.  Dredging Contracts may include several 
project sites.  Specification writers must coordinate with the local USACE District (KO and SOHO), NAVFAC, FEAD 
(Facilities, Engineering and Acquisition Division), or ROICC (Resident Officer in Charge of Construction) office 
to determine the project site and SSHO staffing requirements, considering size of Contract, organization of dredging 
operation requirements, dispersion of operations, and travel time to associated sites by SSHO.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Dredging SSHO Personnel Requirements</TTL><BRK/>
<OLG><BRK/>
<OLI>Provide a minimum of one primary Level One SSHO assigned for the primary shift.</OLI><BRK/>
<BRK/>
<LST>Note:  Hopper Dredges with U.S. Coast Guard, credentialed crews the prime contractor may designate a Level Two SSHO in lieu of having a 
Level one SSHO onboard.</LST><BRK/>
<BRK/>
<OLI>For a project involving multiple work shifts, provide a minimum of a Level[ One][ Two] SSHO for each additional shift.</OLI><BRK/>
<BRK/>
<OLI>For individual dredging projects the prime contractor will designate additional Level Three SSHOs at locations where the primary Level 
One SSHO is not located (example: on dredge, tug, material placement site).</OLI><BRK/>
<BRK/>
<LST>Examples of one dredging project site is reflected in each of the following:</LST><BRK/>
<BRK/>
<OLI LEVEL="2">a mechanical dredge, tug(s) and scow(s), scow route, and material placement site; or</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">a hydraulic pipeline dredge, attendant plant, and material placement site; or,</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">a hopper dredge (include land-based material placement site - if applicable.)</OLI><BRK/>
<BRK/>
<OLI>Designated SSHOs must be present at the project site, located so that they have full mobility and reasonable access to all major work operations 
and must be available during their shift for immediate verbal consultation and notification.</OLI><BRK/>
<BRK/>
<OLI>Designated Level One and Two SSHOs must have direct report authority to a senior project (or corporate) management official.</OLI>  <BRK/>
<BRK/>
<OLI>Designated Level Three SSHOs must report potential safety and occupational health hazards, incidents, and concerns to the Level One or 
Two SSHO on shift.</OLI><BRK/>
<BRK/>
<OLI>Level One and Level Two SSHOs for dredging must have a minimum of 3 years experience in one of the following areas:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Supervising/managing dredging activities.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Supervising/managing marine construction activities.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Supervising/managing land-based construction activities.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Work managing safety programs or processes.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Conducting hazard analyses and developing controls in activities or environments with similar hazards.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>Competent Person for Confined Space Entry</TTL><BRK/>
<BRK/>
<TXT>Provide a CP for Confined Space Entry who meets the requirements of <RID>EM 385-1-1</RID> and herein.  The CP for Confined Space Entry must supervise the 
entry into each confined space in accordance with <RID>EM 385-1-1</RID>.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph for operations involving combustible or hazardous materials.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Since this work involves operations that handle combustible or hazardous materials, this person must have the ability to understand and follow 
through on the air sampling, Personal Protective Equipment (PPE), and instructions of a Marine Chemist, Coast Guard authorized persons, or Certified 
Industrial Hygienist.  Confined space and enclosed space work must comply with <RID>NFPA 306</RID>, <RID>29 CFR 1915</RID>, "Confined and Enclosed Spaces and Other Dangerous 
Atmospheres in Shipyard Employment," or as applicable in <RID>29 CFR 1910</RID> for general industry, <RID>29 CFR 1926</RID> for construction.</TXT><BRK/>
<BRK/>
]</SPT><TAI OPT="NAVY"><SPT><TTL>Qualified Trainer Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Subparagraph Item "a" below with reference to NAVFAC is tailored for NAVFAC Marianas projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Individuals qualified to instruct the 40-hour contract safety awareness course, or portions thereof, must meet the definition of a Competent Person 
Trainer as defined in the <RID>EM 385-1-1</RID>, and, at a minimum, possess a working knowledge of the following subject areas:  <RID>EM 385-1-1</RID>, Electrical Standards, 
Lockout/Tagout, Fall Protection, Confined Space Entry for Construction; Excavation, Trenching and Soil Mechanics, and Scaffolds in accordance with <RID>
29 CFR 1926</RID>.</TXT><BRK/>
<BRK/>
<TXT>Instructors are required to:</TXT><BRK/>
<OLG><BRK/>
<OLI>Prepare class presentations that cover construction-related safety requirements<TAI OPT="NAVFAC MAR"> and includes topics covered in the NAVFAC Construction 
Safety Hazard Awareness Course for Contractors</TAI>.</OLI><BRK/>
<BRK/>
<OLI>Ensure that all attendees attend all sessions by using a class roster signed daily by each attendee.  Maintain copies of the roster for 
at least 5 years.  This is a certification class and must be attended 100 percent.  In cases of emergency where an attendee cannot make 
it to a session, the attendee can make it up in another class session for the same subject.</OLI><BRK/>
<BRK/>
<OLI>Update training course materials whenever an update of the <RID>EM 385-1-1</RID> becomes available.</OLI><BRK/>
<BRK/>
<OLI>Provide a written exam of at least 50 questions.  Students are required to answer 80 percent correctly to pass.</OLI><BRK/>
<BRK/>
<OLI>Request, review and incorporate student feedback into a continuous course improvement program.</OLI><BRK/></OLG>
<BRK/></SPT>
</TAI><TAI OPT="NAVFAC MAR"><SPT><TTL>Requirements for All Contractor Jobsite Personnel Holding H-1B or H-2B Visas</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for inclusion in NAVFAC MARIANAS projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>All Contractor jobsite workers holding an H-1B or H-2B visa must complete a minimum 16-hours of classroom training on the requirements of the latest 
version of <RID>EM 385-1-1</RID> prior to their first day on the jobsite to include but not limited to the following topics:  Sanitation; Medical and First 
Aid Requirements; Temporary Facilities; Personal Protective Equipment; Electrical; Hand and Power Tools; Material Handling and Storage; Motor Vehicles; 
Fall Protection; Work Platforms and Scaffoldings; Demolition; Safe Access, Ladders, Floor &amp; Wall Openings, Stairs and Railing Systems; Excavations 
and Trenching; and Confined Spaces, prior to reporting to the jobsite.</TXT><BRK/>
<BRK/>
<TXT>Submit a list of workers who have completed the training to the Contracting Officer prior to them reporting to the jobsite.  Update the list as 
additional workers are added.  Maintain the updated list at the jobsite for review by the Government's designated authority.  Include the name 
and qualifications of qualified trainer(s) that provided the training.  Personnel who have taken the 40-hour Construction Safety Hazard Awareness 
Training Course for Contractors or similar course that includes emphasis on <RID>EM 385-1-1</RID> compliance, are not required to take the 16-hours of classroom 
training on the requirements of the latest version of the <RID>EM 385-1-1</RID>.  The 16-hours classroom training may be provided by the Guam Contractors 
Association (GCA), Trades Academy, or other qualified trainers as outlined in paragraph QUALIFIED TRAINER REQUIREMENTS.</TXT><BRK/>
<BRK/></SPT>
</TAI><TAI OPT="NAVFAC HI"><SPT><TTL><SUB>Crane Operators/Riggers</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Add the following paragraph for projects in the State of Hawaii only.  Paragraph is tailored for NAVFAC 
HI.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Crane Operators must also meet the crane operator requirements of the State of Hawaii for Crane certification.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Preconstruction Conference</TTL><BRK/>
<OLG><BRK/>
<OLI>Contractor representatives who have a responsibility or significant role in accident prevention on the project must attend the preconstruction 
conference.  This includes the project superintendent, Site Safety and Occupational Health Officer, quality control manager, or any other 
assigned safety and health professionals who participated in the development of the APP (including the Activity Hazard Analyses (AHAs) 
and special plans, program and procedures associated with it).</OLI><BRK/>
<BRK/>
<OLI>Discuss the details of the submitted APP to include incorporated plans, programs, procedures and a listing of anticipated AHAs that will 
be developed and implemented during the performance of the Contract.  This list of proposed AHAs will be reviewed and an agreement will 
be reached between the Contractor and the Contracting Officer as to which phases will require an analysis.  In addition, establish a schedule 
for the preparation, submittal, and Government review of AHAs to preclude project delays.  The creation of the APP and Schedule will be 
created  after being given Notice to Proceed.</OLI><BRK/>
<BRK/>
<OLI>Deficiencies in the submitted APP, identified during the Contracting Officer's review, must be corrected, and the APP re-submitted for 
review prior to the start of construction.  Work is not permitted to begin until an APP is established that is acceptable to the Contracting 
Officer.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT><SPT><TTL>ACCIDENT PREVENTION PLAN (APP)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Contracts that include FAR 52.236-13 Accident Prevention require the Contractor to prepare and execute 
a written Accident Prevention Plan (APP) in accordance with EM 385-1-1 to include Activity Hazard Analyses (AHA).  
For Design-Build projects a Design Submittal of an APP is also required.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TAI OPT="DESIGN-BUILD"><SPT><TTL><SUB>Accident Prevention Plan (APP) Design</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD, use for DESIGN-BUILD projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide a site-specific Accident Prevention Plan (APP), including Activity Hazard Analyses (AHA), in accordance with <RID>EM 385-1-1</RID>, ENG Form 6293, 
for the design team to follow during site visits and investigations.  For subsequent visits, update the plan if there are changes in the personnel 
who will be attending, or the tasks to be performed.  Submit the APP for review and acceptance by the Government at least 15 calendar days prior 
to the start of the design field work after being given Notice to Proceed.  Field work must not begin until the design APP  is accepted by the 
Contracting Officer.  Prior to the start of construction incorporate the Design APP into the Construction APP so that one site specific APP exists 
for the project and submit to the Contracting Officer for acceptance.</TXT><BRK/>
<BRK/>
<TXT>If the design scope includes borings or other subsurface investigations, include in the APP the type of field investigation and verification techniques, 
such as visual, local utility locating service scanning and third party subcontractor scanning, potholing, or hand digging within two feet of a 
known utility that will be required.  Mark underground utilities before starting any ground-disturbing actions.  Notify the Contracting Officer 
15 days prior to the start of soil borings or sub-surface investigations.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL><SUB>Accident Prevention Plan (APP)<TAI OPT="DESIGN-BUILD"> Construction</TAI></SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Second paragraph includes tailoring for ARMY projects.  In second paragraph, choice of bracketed options 
are for ARMY projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Submit the Accident Prevention Plan (APP) for review and acceptance by the Government at least 15 calendar days prior to the start, after being 
given Notice to Proceed.  A competent person must prepare the written site-specific APP.  Prepare the APP in accordance with the format and requirements 
of <RID>EM 385-1-1</RID>, ENG Form 6293, and herein.  The APP must be job-specific and address any unusual or unique aspects of the project or activity for 
which it is written.  The APP must interface with the Contractor's overall safety and occupational health program referenced in the APP in the 
applicable APP element, and made site-specific.  Describe the methods to evaluate past safety performance of potential subcontractors in the selection 
process.  Also, describe innovative methods used to ensure and monitor safe work practices of subcontractors.  The Government considers the Prime 
Contractor to be the "controlling employer" for all worksite safety and health of the subcontractors.  Contractors are responsible for informing 
their subcontractors of the safety provisions under the terms of the Contract and the penalties for noncompliance, coordinating the work to prevent 
one craft from interfering with or creating hazardous working conditions for other crafts, and inspecting subcontractor operations to ensure that 
accident prevention responsibilities are being carried out.  The APP must be signed in accordance with the APP and ENG Form 6293 Accident Prevention 
Plan Worksheet.  The SSHO must provide and maintain the APP and a log of signatures by each subcontractor foreman, attesting that they have read 
and understand the APP, and make the APP and log available on-site to the Contracting Officer.  If English is not the foreman's primary language, 
the Prime Contractor must provide an interpreter.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects in the NAVFAC PAC Area of Responsibility, DESIGN-BUILD projects select the first set of brackets 
and edit the sentence by selecting "15" calendar days.  For DESIGN-BID-BUILD projects, select the second set of 
brackets.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[Submit the APP to the Contracting Officer <TAI OPT="ARMY">[</TAI>15<TAI OPT="ARMY">] [_____]</TAI> calendar days prior to the date of the preconstruction conference for acceptance.  ][Submit 
the APP to the Contracting Officer within 30 calendar days of Contract award and not less than 10 calendar days prior to the date of the preconstruction 
conference for acceptance.  ]Work cannot proceed without an accepted APP.  Once reviewed and accepted by the Contracting Officer, the APP and attachments 
will be enforced as part of the Contract.  Disregarding the provisions of this Contract or the accepted APP is cause for stopping of work, at the 
discretion of the Contracting Officer, until the matter has been rectified.  Continuously review and amend the APP, as necessary, throughout the 
life of the Contract.  Changes to the accepted APP must be made with the knowledge and concurrence of the Contracting Officer, project superintendent, 
SSHO and Quality Control Manager.  Incorporate unusual or high-hazard activities not identified in the original APP as they are discovered.  Should 
any severe hazard exposure (i.e., imminent danger) become evident, stop work in the area, secure the area, and develop a plan to remove the exposure 
and control the hazard.  Notify the Contracting Officer within 24 hours of discovery.  Eliminate and remove the hazard.  In the interim, take all 
necessary action to restore and maintain safe working conditions in order to safeguard onsite personnel, visitors, the public (as defined by <RID>ANSI/ASSP A10.34</RID>
), and the environment.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Names and Qualifications</TTL><BRK/>
<BRK/>
<TXT>Provide plans in accordance with the requirements outlined in <RID>EM 385-1-1</RID>, including the following:</TXT><BRK/>
<OLG><BRK/>
<OLI>Names and qualifications (resumes including education, training, experience and certifications) of site safety and health personnel designated 
to perform work on this project to include the designated Site Safety and Health Officer and other competent and qualified personnel to 
be used.  Specify the duties of each position.</OLI><BRK/>
<BRK/>
<OLI>As a minimum, designate and submit qualifications of Competent Persons (CP) for each of the following major areas: excavation; scaffolding; 
fall protection; hazardous energy; confined space; health hazard recognition, evaluation and control of chemical, physical and biological 
agents; and personal protective equipment and clothing to include selection, use and maintenance.  Designate and submit qualifications 
for additional CPs as applicable to the work performed under this Contract.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Plans</TTL><BRK/>
<BRK/>
<TXT>Provide plans in the APP in accordance with the requirements outlined in <RID>EM 385-1-1</RID>, including the following:</TXT><BRK/>
<BRK/>
[<SPT><TTL>Lead, Cadmium, and Chromium Compliance Plan</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this bracketed subparagraph and the following subparagraphs when project is expected to involve 
these hazardous materials or contaminated sites.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Identify the safety and health aspects of work involving lead, cadmium and chromium, and prepare in accordance with Section <SRF>02 83 00</SRF> LEAD REMEDIATION.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Asbestos Hazard Abatement Plan</TTL><BRK/>
<BRK/>
<TXT>Identify the safety and health aspects of asbestos work, and prepare in accordance with Section <SRF>02 82 00</SRF> ASBESTOS REMEDIATION.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Site Safety and Health Plan</TTL><BRK/>
<BRK/>
<TXT>Identify the safety and health aspects, and prepare in accordance with Section <SRF>01 35 29.13</SRF> HEALTH, SAFETY, AND EMERGENCY RESPONSE PROCEDURES FOR 
CONTAMINATED SITES</TXT>.<BRK/>
<BRK/></SPT>
][<SPT><TTL>Polychlorinated Biphenyls (PCB) Plan</TTL><BRK/>
<BRK/>
<TXT>Identify the safety and health aspects of Polychlorinated Biphenyls work, and prepare in accordance with Sections <SRF>02 84 33</SRF> REMOVAL AND DISPOSAL 
OF POLYCHLORINATED BIPHENYLS (PCBs) and <SRF>02 61 23</SRF> REMOVAL AND DISPOSAL OF PCB CONTAMINATED SOILS.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Site Demolition Plan</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this subparagraph when the project includes demolition or deconstruction activities.  This paragraph 
includes NAVY tailoring - include the last tailored sentence on NAVY projects only.  Refer to the other sections 
of the Contract for the types of surveys needed.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Identify the safety and health aspects, and prepare in accordance with Section <SRF>02 41 00</SRF> [DEMOLITION] [AND] [DECONSTRUCTION] and referenced sources.<TAI OPT="NAVY">
  Include engineering survey as applicable.</TAI></TXT><BRK/>
<BRK/></SPT>
]</SPT></SPT><SPT><TTL><SUB>ACTIVITY HAZARD ANALYSIS (AHA)</SUB></TTL><BRK/>
<BRK/>
<TXT>Before beginning each activity, task or Definable Feature of Work (DFOW) involving a type of work presenting hazards not experienced in previous 
project operations, or where a new work crew or subcontractor is to perform the work, the Contractor(s) performing that work activity must prepare 
an AHA.  AHAs must be developed by the Prime Contractor, subcontractor, or supplier performing the work, and provided for Prime Contractor review 
and approval before submitting to the Contracting Officer.  AHAs must be signed by the SSHO, Superintendent, QC Manager and the subcontractor Foreman 
performing the work.  Format the AHA in accordance with <RID>EM 385-1-1</RID> or as directed by the Contracting Officer.  Submit the AHA for review at least 
[15][_____] working days prior to the start of each activity task, or DFOW.  The Government reserves the right to require the Contractor to revise 
and resubmit the AHA if it fails to effectively identify the work sequences, specific anticipated hazards, site conditions, equipment, materials, 
personnel and the control measures to be implemented.</TXT><BRK/>
<BRK/>
<TXT>AHAs must identify competent persons required for phases involving high risk activities, including confined entry, crane and rigging, excavations, 
trenching, electrical work, fall protection, and scaffolding.</TXT><BRK/>
<BRK/>
<SPT><TTL>AHA Management</TTL><BRK/>
<BRK/>
<TXT>Review the AHA list periodically (at least monthly) at the Contractor supervisory safety meeting, and update as necessary when procedures, scheduling, 
or hazards change.  Use the AHA during daily inspections by the SSHO to ensure the implementation and effectiveness of the required safety and 
health controls for that work activity.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>AHA Signature Log</TTL><BRK/>
<BRK/>
<TXT>Each employee performing work as part of an activity, task or DFOW must review the AHA for that work and sign a signature log specifically maintained 
for that AHA prior to starting work on that activity.  The SSHO must maintain a signature log on site for every AHA.  Provide employees whose primary 
language is other than English, with an interpreter to ensure a clear understanding of the AHA and its contents.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>SITE SAFETY REFERENCE MATERIALS</TTL><BRK/>
<BRK/>
<TXT>Maintain safety-related references applicable to the project, including those listed in paragraph REFERENCES.  Maintain applicable equipment manufacturer's 
manuals.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>EMERGENCY MEDICAL TREATMENT</TTL><BRK/>
<BRK/>
<TXT>Contractors must arrange for their own emergency medical treatment in accordance with <RID>EM 385-1-1</RID>.  The Government has no responsibility to provide 
emergency medical treatment.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>NOTIFICATIONS AND REPORTS</TTL><BRK/>
<BRK/>
<SPT><TTL>Accident Notification</TTL><BRK/>
<BRK/>
<TXT>Notify the Contracting Officer in accordance with the <RID>EM 385-1-1</RID> Accident Reporting Timeline.</TXT><BRK/>
<TAB>
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="3" ROWCOUNT="4">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="225.00"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="225.00"/>
      <COL AUTOWIDTH="0" WIDTH="310.50"/>
      <ROW AUTOHEIGHT="0" HEIGHT="30.75">
         <CEL MERGEACROSS="2" STYLEID="s50">
<DTA TYPE="STRING"><HL3><HL4>Table<BRK/>Accident Reporting Required Timeline<BRK/></HL4></HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="45.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL4><HL3>Accident Type</HL3></HL4></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL4><HL3>Notify KO or COR</HL3></HL4></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL4><HL3>Complete Final Accident Report on ENG 3394 and provide to KO or COR</HL3></HL4></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="69.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Fatality, in-patient hospitalization, amputation, eye loss, or property damage over $600,000.</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Immediately, no later than (NLT) 8 Hours</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Within 7 Days</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="45.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">All other accidents and near misses</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Immediately, no later than (NLT) 24 Hours</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Within 7 Days</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<TXT>Within notification include Contractor name; Contract title; type of Contract; name of activity, installation or location where accident occurred; 
date and time of accident; names of personnel injured; extent of property damage, if any; extent of injury, if known, and brief description of 
accident (for example, type of construction equipment used and PPE used).  Preserve the conditions and evidence on the accident site until the 
Government investigation team arrives on-site and Government investigation is conducted.  Assist and cooperate fully with the Government's investigation(s) 
of any accident or near miss.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>Accident Reports</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following subparagraphs include tailoring for NAVY and ARMY projects.  The sentences referring to ESAMS 
are tailored for use on NAVY projects.  The sentences referring to ENG Form 3394 are tailored for use on ARMY 
projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TAI OPT="NAVY"><OLG><OLI>Conduct an accident investigation for recordable injuries and illnesses, property damage, and near misses as defined in <RID>EM 385-1-1</RID>, to 
establish the root cause(s) of the accident.  Complete the applicable NAVFAC Contractor Incident Reporting System (CIRS), and electronically 
submit via the NAVFAC Enterprise Safety Applications Management System (ESAMS).  Complete and submit an accident investigation report in 
ESAMS within 7 days for  accidents as defined by <RID>EM 385-1-1</RID>.  Complete the investigation report within 30 days.  Accidents must include 
a written report submitted as an attachment in ESAMS using the following outline:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Summary description to include:</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">process</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">findings</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">outcomes</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Root Cause</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Direct Factors</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Indirect and Contributing Factors</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Corrective Actions</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Recommendations</OLI><BRK/>
<BRK/>
<LST>All accidents are reportable, regardless of whether or not it is recordable.</LST><BRK/></OLG>
<BRK/></TAI>
<OLG><TAI OPT="ARMY"><OLI>Conduct an accident investigation for recordable injuries and illnesses, property damage, and near misses as defined in <RID>EM 385-1-1</RID>, to 
establish the root cause(s) of the accident.  All accidents are reportable, regardless of whether or not it is recordable.  Complete the 
applicable USACE Accident Report, ENG Form 3394, and provide the report to the Contracting Officer within 7 calendar days of the accident.  
The Contracting Officer will provide copies of any required or special forms.  All accidents are reportable, regardless of whether or not 
it is recordable.</OLI><BRK/></TAI>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following subparagraph includes tailoring for ARMY and NAVY projects.  The first set of sentences is 
tailored for use on NAVY projects only, and the second set is tailored for use on ARMY projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Near Misses: <TAI OPT="NAVY"> For Navy Projects, complete the applicable documentation in NAVFAC Contractor Incident Reporting System (CIRS), and electronically 
submit via the NAVFAC Enterprise Safety Applications Management System (ESAMS).</TAI><TAI OPT="ARMY"> For Army projects, report all "Near Misses" to the[ Contracting 
Officer][ COR][_____], using local accident reporting procedures, within 24 hours.  The[ Contracting Officer][ COR][_____] will provide 
the Contractor the required forms.</TAI>  Near miss reports are considered positive and proactive Contractor safety management actions.</OLI><BRK/>
<BRK/>
<TAI OPT="NAVY"><NTE><AST/><BRK/>
<NPR>NOTE:  Include the following subparagraph for all NAVY projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Conduct an accident investigation for any load handling equipment accident (including rigging accidents) to establish the root cause(s) 
of the accident.  Complete the Load Handling Equipment (LHE) Accident Report (Crane and Rigging Accident Report) form and provide the report 
to the Contracting Officer within 30 calendar days of the accident.  Do not proceed with crane operations until cause is determined and 
corrective actions have been implemented to the satisfaction of the Contracting Officer.  The Contracting Officer will provide a blank 
copy of the accident report form.</OLI><BRK/>
<BRK/></TAI>
</OLG></SPT><SPT><TTL><SUB>LHE Inspection Reports</SUB></TTL><BRK/>
<BRK/>
<TXT>Submit LHE inspection reports required in accordance with <RID>EM 385-1-1</RID> and as specified herein with Daily Reports of Inspections.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ARMY">[</TAI><SPT><TTL><SUB>Certificate of Compliance</SUB> and Pre-lift Plan/Checklist for LHE and Rigging</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following for all NAVY projects; the following is optional for ARMY projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Certificate of Compliance</TTL><BRK/>
<BRK/>
<TXT>Provide a Certificate of Compliance for LHE utilized to perform work under this Contract in accordance with Section 16-7 of the <RID>EM 385-1-1</RID>.  Post 
completed certificate on the crane.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Pre-Lift Plans</TTL><BRK/>
<BRK/>
<TXT>Develop either a <SUB>Standard Lift Plan</SUB> (SLP) or <SUB>Critical Lift Plan</SUB> (CLP) as required in accordance with <RID>EM 385-1-1</RID>.  Utilize the Standard Lift Plan 
ENG Form 6203 for routine crane lifts and use the Critical Lift Plan ENR Form 6213 for non-routine crane lifts requiring more detailed planning 
and additional safety precautions, as defined by Section 16-2j of the <RID>EM 385-1-1</RID>.  Submit lift plans to the Contracting Officer for approval within 
15 calendar days in advance of planned lift.</TXT><BRK/>
<BRK/></SPT>
</SPT><TAI OPT="ARMY">]</TAI><TAI OPT="NAVY">[<SPT><TTL><SUB>Third Party Certification of Floating Cranes and Barge-Mounted Mobile Cranes</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for NAVY projects.  Include this tailored paragraph for CONUS NAVY 
projects only.  Paragraph can be deleted on projects where no floating or barge-mounted mobile cranes would be 
used.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Floating cranes and barge-mounted mobile cranes used to perform work under the terms of this Contract must be certified in accordance with <RID>29 CFR 1919</RID>
 by an OSHA accredited person prior to submitting the required Lift Plan.  Include proof of certification with the initial Lift Plan submission.</TXT><BRK/>
<BRK/></SPT>
]</TAI></SPT><SPT><TTL><SUB>HOT WORK PERMIT</SUB></TTL><BRK/>
<BRK/>
<SPT><TTL>Permit and Personnel Requirements</TTL><BRK/>
<BRK/>
<TXT>Submit and obtain a written permit prior to performing "Hot Work" (i.e., welding or cutting) or operating other flame-producing/spark producing 
devices, from the [Fire Division][_____].  A permit is required from the Explosives Safety Office for work in and around where explosives are processed, 
stored, or handled.  Contractors are required to meet all criteria before a permit is issued.  Provide at least two<MET> 9 kg</MET><ENG> 20 pound</ENG> 4A:20 BC rated 
extinguishers for normal "Hot Work".  The extinguishers must be current inspection tagged, and contain an approved safety pin and tamper resistant 
seal.  It is also mandatory to have a designated FIRE WATCH for any "Hot Work" done at this activity.  The Fire Watch must be trained in accordance 
with <RID>NFPA 51B</RID> and remain on-site for a minimum of 1 hour after completion of the task or as specified on the hot work permit.</TXT><BRK/>
<BRK/>
<TXT>When starting work in the facility, require personnel to familiarize themselves with the location of the nearest fire alarm boxes and place in 
memory the emergency [Fire Division][_____] phone number.  Report any fire, no matter how small, to the responsible [Fire Division][_____] immediately.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Work Around Flammable Materials</TTL><BRK/>
<BRK/>
<TXT>Obtain permit approval from a NFPA Certified Marine Chemist, or Certified Industrial Hygienist for "Hot Work" within or around flammable materials 
(such as fuel systems or welding/cutting on fuel pipes) or confined spaces (such as sewer wet wells, manholes, or vaults) that have the potential 
for flammable or explosive atmospheres.</TXT><BRK/>
<BRK/>
<TXT>Whenever these materials, except beryllium and chromium (VI), are encountered in indoor operations, local mechanical exhaust ventilation systems 
that are sufficient to reduce and maintain personal exposures to within acceptable limits must be used and maintained in accordance with manufacturer's 
instruction and supplemented by exceptions noted in <RID>EM 385-1-1</RID>.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>RADIATION SAFETY REQUIREMENTS</TTL><BRK/>
<TAI OPT="NAVY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph includes tailoring for NAVY projects.  Include the tailored item for NAVY projects 
only.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Submit <SUB>License Certificates</SUB>, employee training records, and Leak Test Reports for radiation materials and equipment to the Contracting Officer 
and Radiation Safety Office (RSO)<TAI OPT="NAVY">, and Contracting Oversight Technician (COT)</TAI> for all specialized and licensed material and equipment proposed 
for use on the construction project (excludes portable machine sources of ionizing radiation including moisture density and X-Ray Fluorescence 
(XRF)).  Maintain on-site records whenever licensed radiological materials or ionizing equipment are on Government property.</TXT><BRK/>
<BRK/>
<TXT>Protect workers from radiation exposure in accordance with <RID>10 CFR 20</RID>, ensuring any personnel exposures are maintained As Low As Reasonably Achievable.</TXT><BRK/>
<BRK/>
<SPT><TTL>Radiography Operation Planning Work Sheet</TTL><BRK/>
<TAI OPT="NAVY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph includes tailoring for NAVY projects.  Include the tailored item for NAVY projects 
only.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Submit a Gamma and X-Ray <SUB>Radiography Operation Planning Work Sheet</SUB> to Contracting Officer 14 days prior to commencement of operations involving 
radioactive materials or radiation generating devices.  For portable machine sources of ionizing radiation, including moisture density and XRF, 
use and submit the <SUB>Portable Gauge Operations Planning Worksheet</SUB> instead.  The Contracting Officer<TAI OPT="NAVY"> and COT</TAI> will review the submitted worksheet and 
provide questions and comments.</TXT><BRK/>
<BRK/>
<TXT>Contractors must use primary dosimeters process by a National Voluntary Laboratory Accreditation Program (NVLAP) accredited laboratory.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Site Access and Security</TTL><BRK/>
<TAI OPT="NAVY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph includes tailoring for NAVY projects.  Include the tailored items for NAVY projects 
only.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Coordinate site access and security requirements with the Contracting Officer<TAI OPT="NAVY"> and COT</TAI> for all radiological materials and equipment containing ionizing 
radiation that are proposed for use on a government facility.  For gamma radiography materials and equipment, a Government escort is required for 
any travels on the Installation.  The <TAI OPT="NAVY">Navy COT or </TAI>Government authorized representative will meet the Contractor at a designated location outside 
the Installation, ensure safety of the materials being transported, and will escort the Contractor for gamma sources onto the Installation, to 
the job site, and off the Installation.  For portable machine sources of ionizing radiation, including moisture density and XRF, the <TAI OPT="NAVY">Navy COT or </TAI>
Government authorized representative will meet the Contractor at the job site.</TXT><BRK/>
<BRK/>
<TXT>Provide a copy of all calibration records, and utilization records<TAI OPT="NAVY"> to the COT</TAI> for radiological operations performed on the site.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Loss or Release and Unplanned Personnel Exposure</TTL><BRK/>
<BRK/>
<TXT>Loss or release of radioactive materials, and unplanned personnel exposures must be reported immediately to the Contracting Officer, RSO, and Base 
Security Department Emergency Number.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Site Demarcation and Barricade</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Add any applicable Instructions or local requirements to first sentence.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Properly demark and barricade an area surrounding radiological operations to preclude personnel entrance, in accordance with <RID>EM 385-1-1</RID>, Nuclear 
Regulatory Commission, and Applicable State regulations and license requirements, and in accordance with requirements established in the accepted 
Radiography Operation Planning Work Sheet.</TXT><BRK/>
<BRK/>
<TXT>Do not close or obstruct streets, walks, and other facilities occupied and used by the Government without written permission from the Contracting 
Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Security of Material and Equipment</TTL><BRK/>
<BRK/>
<TXT>Properly secure the radiological material and ionizing radiation equipment at all times, including keeping the devices in a properly marked and 
locked container, and secondarily locking the container to a secure point in the Contractor's vehicle or other approved storage location during 
transportation and while not in use.  While in use, maintain a continuous visual observation on the radiological material and ionizing radiation 
equipment.  In instances where radiography is scheduled near or adjacent to buildings or areas having limited access or one-way doors, make no 
assumptions as to building occupancy.  Where necessary, the Contracting Officer will direct the Contractor to conduct an actual building entry, 
search, and alert.  Where removal of personnel from such a building cannot be accomplished and it is otherwise safe to proceed with the radiography, 
position a fully instructed employee inside the building or area to prevent exiting while external radiographic operations are in process.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Transportation of Material</TTL><BRK/>
<BRK/>
<TXT>Comply with <RID>49 CFR 173</RID> for Transportation of Regulated Amounts of Radioactive Material.  Notify Local Fire authorities and the site Radiation Safety 
Officer (RSO) of any Radioactive Material use.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Schedule for Exposure or Unshielding</TTL><BRK/>
<BRK/>
<TXT>Actual exposure of the radiographic film or unshielding the source must not be initiated until after 5 p.m. on weekdays.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Transmitter Requirements</TTL><BRK/>
<BRK/>
<TXT>Adhere to the base policy concerning the use of transmitters, such as radios and cell phones.  Obey Emissions control (EMCON) restrictions.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>CONFINED SPACE ENTRY REQUIREMENTS</TTL><BRK/>
<TAI OPT="NAVY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph includes tailoring for NAVY projects.  Include the last bracketed sentence for 
NAVY projects only as applicable.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Confined space entry must comply with <RID>EM 385-1-1</RID>, <RID>29 CFR 1926</RID>, <RID>29 CFR 1910</RID>, and Directive <RID>CPL 2.100</RID>.  Any potential for a hazard in the confined 
space requires a permit system to be used.<TAI OPT="NAVY">[  Contractors entering and working in confined spaces while performing shipyard industry work are required 
to follow the requirements of <RID>29 CFR 1915</RID>.]</TAI></TXT><BRK/>
<BRK/>
<SPT><TTL>Rescue Procedures and Coordination with Local Emergency Responders</TTL><BRK/>
<BRK/>
<TXT>Develop and implement an on-site rescue and recovery plan and procedures.  The rescue plan must not rely on local emergency responders for rescue 
from a confined space.</TXT><BRK/>
<BRK/></SPT>
</SPT><TAI OPT="INDOOR AIR QUALITY"><SPT><TTL>CONSTRUCTION <SUB>INDOOR AIR QUALITY (IAQ) MANAGEMENT PLAN</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph and subsequent subparagraphs are tailored for INDOOR AIR QUALITY.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Preventing indoor air quality problems resulting from the construction process sustains the comfort and 
health of construction workers and building occupants. Include last bracketed sentence when required by Section 
<SRF>01 33 29</SRF> SUSTAINABILITY REQUIREMENTS AND REPORTING, IAQ requirements.</NPR><BRK/>
<BRK/>
<NPR>For projects in the NAVFAC PAC Area of Responsibility, select the second set of brackets, "not less than 10 calendar 
days before the preconstruction conference."</NPR><BRK/>
<BRK/>
<NPR>The following paragraph contains tailoring for DESIGN-BUILD and DESIGN-BID-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Submit an IAQ Management Plan [within [15][_____] calendar days after<TAI OPT="DESIGN-BUILD"> design</TAI><TAI OPT="DESIGN-BID-BUILD">[ Contract award][ notice to proceed]</TAI> and not less than 10 calendar 
days before the preconstruction conference.][not less than 10 calendar days before the preconstruction conference.]  Revise and resubmit Plan as 
required by the Contracting Officer.  Make copies of the final plan available to all workers on site.  Include provisions in the Plan to meet the 
requirements specified below and to ensure safe, healthy air for construction workers and building occupants.[  Submit <SUB>Final IAQ Management Plan</SUB>
 for inclusion in the Sustainability eNotebook, in accordance with Section <SRF>01 33 29</SRF> SUSTAINABILITY REQUIREMENTS AND REPORTING.]</TXT><BRK/>
<BRK/>
<SPT><TTL>Requirements During Construction</TTL><BRK/>
<BRK/>
<TXT>Provide for evaluation of indoor Carbon Dioxide concentrations in accordance with <RID>ASTM D6245</RID>.  Provide for evaluation of volatile organic compounds 
(VOCs) in indoor air in accordance with <RID>ASTM D6345</RID>.  Use filters with a Minimum Efficiency Reporting Value (MERV) of 8 in permanently installed 
air handlers during construction.</TXT><BRK/>
<BRK/>
<SPT><TTL>Control Measures</TTL><BRK/>
<BRK/>
<TXT>Meet or exceed the requirements of <RID>ANSI/SMACNA 008</RID> to help minimize contamination of the building from construction activities.  The five requirements 
of this manual which must be adhered to are described below:</TXT><BRK/>
<OLG><BRK/>
<OLI>HVAC protection:  Isolate return side of HVAC system from surrounding environment to prevent construction dust and debris from entering 
the duct work and spaces.</OLI><BRK/>
<BRK/>
<OLI>Source control:  Use low emitting paints and other finishes, sealants, adhesives, and other materials as specified. When available, cleaning 
products must have a low VOC content and be non-toxic to minimize building contamination.  Utilize cleaning techniques that minimize dust 
generation.  Cycle equipment off when not needed.  Prohibit idling motor vehicles where emissions could be drawn into building.  Designate 
receiving/storage areas for incoming material that minimize IAQ impacts.</OLI><BRK/>
<BRK/>
<OLI>Pathway interruption:  When pollutants are generated use strategies such as 100 percent outside air ventilation or erection of physical 
barriers between work and non-work areas to prevent contamination.</OLI><BRK/>
<BRK/>
<OLI>Housekeeping:  Clean frequently to remove construction dust and debris. Promptly clean up spills.  Remove accumulated water and keep work 
areas dry to discourage the growth of mold and bacteria.  Take extra measures when hazardous materials are involved.</OLI><BRK/>
<BRK/>
<OLI>Scheduling:  Control the sequence of construction to minimize the absorption of VOCs by other building materials.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Moisture Contamination</TTL><BRK/>
<OLG><BRK/>
<OLI>Remove accumulated water and keep work dry.</OLI><BRK/>
<BRK/>
<OLI>Use dehumidification to remove moist, humid air from a work area.</OLI><BRK/>
<BRK/>
<OLI>Do not use combustion heaters or generators inside the building.</OLI><BRK/>
<BRK/>
<OLI>Protect porous materials from exposure to moisture.</OLI><BRK/>
<BRK/>
<OLI>Remove and replace items which remain damp for more than a few hours.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT><SPT><TTL>Requirements After Construction</TTL><BRK/>
<BRK/>
<TXT>After construction ends and prior to occupancy, conduct a building flush-out or test the indoor air contaminant levels.  Flush-out must be a minimum 
2 weeks with MERV-13 filtration media as determined by <RID>ASHRAE 52.2</RID> at 100 percent outside air.  Air contamination testing must be consistent with 
EPA's current Compendium of Methods for the Determination of Air Pollutants in Indoor Air.  After building flush-out or testing and prior to occupancy, 
replace filtration media.  Filtration media must have a MERV of 13 as determined by <RID>ASHRAE 52.2</RID>.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>DIVE SAFETY REQUIREMENTS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  NAVFAC SE projects require 25 working days in the bracketed option.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Develop a <SUB>Dive Operations Plan</SUB>, AHA, emergency management plan, and personnel list that includes qualifications, for each separate diving operation.  
Submit these documents to the District Dive Coordinator (DDC) via the Contracting Officer, for review and approval at least [15][_____] working 
days prior to commencement of diving operations.  These documents must be at the diving location at all times.  Provide each of these documents 
as a part of the project file.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>[SEVERE STORM PLAN][SEVERE WEATHER PLAN FOR MARINE ACTIVITIES (SWPMA)]</TTL><BRK/>
<BRK/>
<TXT>In the event of a severe storm warning, the Contractor must comply with the applicable Storm Plan and:</TXT><BRK/>
<OLG><BRK/>
<OLI>Secure outside equipment and materials and place materials that could be damaged in protected areas.</OLI><BRK/>
<BRK/>
<OLI>Check surrounding area, including roof, for loose material, equipment, debris, and other objects that could be blown away or against existing 
facilities.</OLI><BRK/>
<BRK/>
<OLI>Ensure that temporary erosion controls are adequate.</OLI><BRK/></OLG>
<BRK/></SPT>
</PRT><PRT><TTL>PART 2   PRODUCTS</TTL><BRK/>
<TAI OPT="ARMY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this tailored paragraph for ARMY projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Not used.</TXT><BRK/></TAI>
<BRK/>
<TAI OPT="NAVY"><SPT><TTL>CONFINED SPACE SIGNAGE</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this tailored paragraph for NAVY projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide permanent signs integral to or securely attached to access covers for new permit-required confined spaces.  Signs for confined spaces must 
comply with <RID>NEMA Z535.2</RID>.  Provide signs with wording:  "DANGER--PERMIT-REQUIRED CONFINED SPACE, DO NOT ENTER" in bold letters a minimum of<MET> 25 mm</MET><ENG>
 one inch</ENG> in height and constructed to be clearly legible with all paint removed.  The signal word "DANGER" must be red and readable from<MET> 1520 
mm</MET><ENG> 5 feet</ENG>.</TXT><BRK/>
<BRK/></SPT>
</TAI></PRT><PRT><TTL>PART 3   EXECUTION</TTL><BRK/>
<BRK/>
<SPT><TTL>CONSTRUCTION AND OTHER WORK</TTL><BRK/>
<BRK/>
<TXT>Comply with <RID>EM 385-1-1</RID>, <RID>NFPA 70</RID>, <RID>NFPA 70E</RID>, <RID>NFPA 241</RID>, the APP, the AHA, Federal and State OSHA regulations, and other related submittals and activity 
fire and safety regulations.  The most stringent standard prevails.</TXT><BRK/>
<BRK/>
<TXT>PPE is governed in all areas by the nature of the work the employee is performing.  Use personal hearing protection at all times in designated 
noise hazardous areas or when performing noise hazardous tasks.  Safety glasses must be worn or carried/available on each person.  Mandatory PPE 
includes:</TXT><BRK/>
<OLG><BRK/>
<OLI>Head Protection that meets <RID>ANSI/ISEA Z89.1</RID></OLI><BRK/>
<BRK/>
<OLI>Long Pants</OLI><BRK/>
<BRK/>
<OLI>Appropriate Safety Footwear</OLI><BRK/>
<BRK/>
<OLI>Appropriate Class Reflective Vests</OLI><BRK/></OLG>
<BRK/>
<SPT><TTL>Worksite Communication</TTL><BRK/>
<BRK/>
<TXT>Employees working alone in a remote location or away from other workers must be provided an effective means of emergency communications (i.e., 
cellular phone, two-way radios, land-line telephones or other acceptable means).  The selected communication must be readily available (easily 
within the immediate reach) of the employee and must be tested prior to the start of work to verify that it effectively operates in the area/environment.  
Develop an employee check-in/check-out communication procedure to ensure employee safety.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="NAVY"><SPT><TTL>Hazardous Material Use</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVY.  Include this paragraph for NAVY projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Each hazardous material must receive approval from the Contracting Office or their designated representative prior to being brought onto the job 
site or prior to any other use in connection with this Contract.  Allow a minimum of 10 working days for processing of the request for use of a 
hazardous material.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Hazardous Material Exclusions</TTL><BRK/>
<BRK/>
<TXT>Notwithstanding any other hazardous material used in this Contract, radioactive materials or instruments capable of producing ionizing/non-ionizing 
radiation (with the exception of radioactive material and devices used in accordance with <RID>EM 385-1-1</RID> such as nuclear density meters for compaction 
testing and laboratory equipment with radioactive sources) as well as materials which contain asbestos, mercury or polychlorinated biphenyls, di-isocyanates, 
lead-based paint, and hexavalent chromium, are prohibited.  The Contracting Officer, upon written request by the Contractor, may consider exceptions 
to the use of any of the above excluded materials.  Low mercury lamps used within fluorescent lighting fixtures are allowed as an exception without 
further Contracting Officer approval.  Notify the Radiation Safety Officer (RSO) prior to excepted items of radioactive material and devices being 
brought on base.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Unforeseen Hazardous Material</TTL><BRK/>
<BRK/>
<TXT>Contract documents identify materials such as PCB, lead paint, and friable and non-friable asbestos and other OSHA regulated chemicals (i.e., 29 
CFR Part 1910.1000).  If material(s) that can be hazardous to human health upon disturbance are encountered during demolition, repair, renovation, 
or construction operations, stop portions of work that would disturb the material and notify the Contracting Officer immediately.  Within [14][_____] 
calendar days the Government will determine if the material is hazardous.  If material is not hazardous or poses no danger, the Government will 
direct the Contractor to proceed without change.  If material is hazardous and handling of the material is necessary to accomplish the work, the 
Government will issue a modification.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>UTILITY OUTAGE REQUIREMENTS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Consult with local Installation on notice required for utility outage.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Apply for utility outages[ at least [_____] days in advance][ in sufficient time as to not result in impacts or delays to the project schedule].  
At a minimum, the written request must include the location of the outage, utilities being affected, duration of outage, any necessary sketches, 
and a description of the means to fulfill energy isolation requirements in accordance with <RID>EM 385-1-1</RID>.  In accordance with <RID>EM 385-1-1</RID>, where outages 
involve Government or Utility personnel, coordinate with the Government on all activities involving the control of hazardous energy.</TXT><BRK/>
<BRK/>
<TXT>These activities include, but are not limited to, a review of Hazardous Energy Control Program (HECP) and HEC procedures, as well as applicable 
Activity Hazard Analyses (AHAs).  In accordance with <RID>EM 385-1-1</RID> and <RID>NFPA 70E</RID>, work on energized electrical circuits must not be performed without 
prior Government authorization.  Government permission is considered through the permit process and submission of a detailed AHA.  Energized work 
permits are considered only when de-energizing introduces additional or increased hazard or when de-energizing is infeasible.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>OUTAGE COORDINATION MEETING</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For bracketed items, choose representative required for the Installation.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>After the utility outage request is approved and prior to beginning work on the utility system requiring shut-down, conduct a pre-outage coordination 
meeting in accordance with <RID>EM 385-1-1</RID>.  This meeting must include the Prime Contractor, the Prime and subcontractors performing the work, the Contracting 
Officer, and the[ Installation representative][ Public Utilities representative].  All parties must fully coordinate HEC activities with one another.  
During the coordination meeting, all parties must discuss and coordinate on the scope of work, HEC procedures (specifically, the lock-out/tag-out 
procedures for worker and utility protection), the AHA, assurance of trade personnel qualifications, identification of competent persons, and compliance 
with HECP training in accordance with <RID>EM 385-1-1</RID>.  Clarify when personal protective equipment is required during switching operations, inspection, 
and verification.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>CONTROL OF HAZARDOUS ENERGY (LOCKOUT/TAGOUT)</TTL><BRK/>
<BRK/>
<TXT>Provide and operate a Hazardous Energy Control Program (HECP) in accordance with <RID>EM 385-1-1</RID>, <RID>29 CFR 1910</RID>, <RID>29 CFR 1915</RID>, <RID>ANSI/ASSP A10.44</RID>, <RID>NFPA 70E</RID>
.</TXT><BRK/>
<BRK/>
<SPT><TTL>Safety Preparatory Inspection Coordination Meeting with the Government or Utility</TTL><BRK/>
<BRK/>
<TXT>For electrical distribution equipment that is to be operated by Government or Utility personnel, the Prime Contractor and the subcontractor performing 
the work must attend the safety preparatory inspection coordination meeting, which will also be attended by the Contracting Officer's Representative, 
and required by <RID>EM 385-1-1</RID>.  The meeting will occur immediately preceding the start of work and following the completion of the outage coordination 
meeting.  Both the safety preparatory inspection coordination meeting and the outage coordination meeting must occur prior to conducting the outage 
and commencing with lockout/tagout procedures.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Lockout/Tagout Isolation</TTL><BRK/>
<BRK/>
<TXT>Where the Government or Utility performs equipment isolation and lockout/tagout, the Contractor must place their own locks and tags on each energy-isolating 
device and proceed in accordance with the HECP.  Before any work begins, both the Contractor and the Government or Utility must perform energy 
isolation verification testing while wearing required PPE detailed in the Contractor's AHA and required by <RID>EM 385-1-1</RID>.  Install personal protective 
grounds, with tags, to eliminate the potential for induced voltage in accordance with <RID>EM 385-1-1</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Lockout/Tagout Removal</TTL><BRK/>
<BRK/>
<TXT>Upon completion of work, conduct lockout/tagout removal procedure in accordance with the HECP.  In accordance with <RID>EM 385-1-1</RID>, each lock and tag 
must be removed from each energy isolating device by the authorized individual or systems operator who applied the device.  Provide formal notification 
to the Government (by completing the Government form if provided by Contracting Officer's Representative), confirming that steps of de-energization 
and lockout/tagout removal procedure have been conducted and certified through inspection and verification.  Government or Utility locks and tags 
used to support the Contractor's work will not be removed until the authorized Government employee receives the formal notification.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>FALL PROTECTION PROGRAM</TTL><BRK/>
<BRK/>
<TXT>Establish a fall protection program, for the protection of all employees exposed to fall hazards.  Within the program include company policy, identify 
roles and responsibilities, education and training requirements, fall hazard identification, prevention and control measures, inspection, storage, 
care and maintenance of fall protection equipment and rescue and evacuation procedures in accordance with <RID>EM 385-1-1</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Fall Protection Equipment and Systems</TTL><BRK/>
<BRK/>
<TXT>Enforce use of personal fall protection equipment and systems designated (to include fall arrest, restraint, and positioning) for each specific 
work activity in the Site Specific Fall Protection and Prevention Plan and AHA at all times when an employee is exposed to a fall hazard.  Protect 
employees from fall hazards as specified in <RID>EM 385-1-1</RID>.</TXT><BRK/>
<BRK/>
<TXT>Provide personal fall protection equipment, systems, subsystems, and components that comply with <RID>EM 385-1-1</RID> and <RID>29 CFR 1926</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Additional Personal Fall Protection Measures</TTL><BRK/>
<BRK/>
<TXT>In addition to the required fall protection systems, other protective measures such as safety skiffs, personal floatation devices, and life rings, 
are required when working above or next to water in accordance with <RID>EM 385-1-1</RID>.  Personal fall protection systems and equipment are required when 
working from an articulating or extendible boom, swing stages, or suspended platform.  In addition, personal fall protection systems are required 
when operating other equipment such as scissor lifts.  The need for tying-off in such equipment is to prevent ejection of the employee from the 
equipment during raising, lowering, travel, or while performing work.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Personal Fall Protection Equipment</TTL><BRK/>
<BRK/>
<TXT>Only a full-body harness with a shock-absorbing lanyard or self-retracting lanyard is an acceptable personal fall arrest body support device.  
The use of body belts is not acceptable.  Harnesses must have a fall arrest attachment affixed to the body support (usually a Dorsal D-ring) and 
specifically designated for attachment to the rest of the system.  Snap hooks and carabineers must be self-closing and self-locking, capable of 
being opened only by at least two consecutive deliberate actions and have a minimum gate strength of<MET> 1633 kg</MET><ENG> 3,600 lbs</ENG> in all directions.  Use 
webbing, straps, and ropes made of synthetic fiber.  The maximum free fall distance when using fall arrest equipment must not exceed<MET> 1.8 m</MET><ENG> 6 feet</ENG>
, unless the proper energy absorbing lanyard is used.  Always take into consideration the total fall distance and any swinging of the worker (pendulum-like 
motion), that can occur during a fall, when attaching a person to a fall arrest system.  Equip all full body harnesses with Suspension Trauma Preventers 
such as stirrups, relief steps, or similar in order to provide short-term relief from the effects of orthostatic intolerance in accordance with <RID>
EM 385-1-1</RID>.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT><TAI OPT="NAVY">[<SPT><TTL>SHIPYARD REQUIREMENTS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVY.  Include this paragraph for Navy projects located within a shipyard 
only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>All personnel who enter the Controlled Industrial Area (CIA) must wear mandatory personal protective equipment (PPE) at all times and comply with 
PPE postings of shops both inside and outside the CIA.</TXT><BRK/>
<BRK/></SPT>
]</TAI><SPT><TTL>USE OF EXPLOSIVES</TTL><BRK/>
<BRK/>
<TXT>Explosives must not be used or brought to the project site without prior written approval from the Contracting Officer.  Such approval does not 
relieve the Contractor of responsibility for injury to persons or for damage to property due to blasting operations.</TXT><BRK/>
<BRK/>
<TXT>Storage of explosives, when permitted on Government property, must be only where directed and in approved storage facilities.  These facilities 
must be kept locked at all times except for inspection, delivery, and withdrawal of explosives.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>ELECTRICAL </TTL><BRK/>
<BRK/>
<TXT>Perform electrical work in accordance with <RID>EM 385-1-1</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Electrical Work</TTL><BRK/>
<BRK/>
<TXT>As described in <RID>EM 385-1-1</RID>, electrical work is to be conducted in a de-energized state unless there is no alternative method for accomplishing 
the work.  In those cases obtain an energized work permit from the[ Contracting Officer][ Commanding Officer].  The energized work permit application 
must be accompanied by the AHA and a summary of why the equipment/circuit needs to be worked energized.  Underground electrical spaces must be 
certified safe for entry before entering to conduct work.  Cables that will be cut must be positively identified and de-energized prior to performing 
each cut.  Attach temporary grounds in accordance with <RID>ASTM F855</RID> and <RID>IEEE 1048</RID>.  Perform all high voltage cable cutting remotely using hydraulic 
cutting tool.  When racking in or live switching of circuit breakers, no additional person other than the switch operator is allowed in the space 
during the actual operation.  Plan so that work near energized parts is minimized to the fullest extent possible.  Use of electrical outages clear 
of any energized electrical sources is the preferred method.</TXT><BRK/>
<BRK/>
<TXT>When working in energized substations, only qualified electrical workers are permitted to enter.  When work requires work near energized circuits 
as defined by <RID>NFPA 70</RID>, high voltage personnel must use personal protective equipment that includes, as a minimum, electrical hard hat, safety footwear, 
insulating gloves and electrical arc flash protection for personnel as required by <RID>NFPA 70E</RID>.  Insulating blankets, hearing protection, and switching 
suits may also be required, depending on the specific job and as delineated in the Contractor's AHA.  Ensure that each employee is familiar with 
and complies with these procedures and <RID>29 CFR 1910</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Qualifications</TTL><BRK/>
<BRK/>
<TXT>Electrical work must be performed by QP with verifiable credentials who are familiar with applicable code requirements.  Verifiable credentials 
consist of State, National and Local Certifications or Licenses that a Master or Journeyman Electrician may hold, depending on work being performed, 
and must be identified in the appropriate AHA.  Journeyman/Apprentice ratio must be in accordance with State, Local[ and Host Nation] requirements 
applicable to where work is being performed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Arc Flash</TTL><BRK/>
<BRK/>
<TXT>Conduct a hazard analysis/arc flash hazard analysis whenever work on or near energized parts greater than 50 volts is necessary, in accordance 
with <RID>NFPA 70E</RID>.</TXT><BRK/>
<BRK/>
<TXT>All personnel entering the identified arc flash protection boundary must be QPs and properly trained in <RID>NFPA 70E</RID> requirements and procedures.  
Unless permitted by <RID>NFPA 70E</RID>, no Unqualified Person is permitted to approach nearer than the Limited Approach Boundary of energized conductors 
and circuit parts.  Training must be administered by an electrically qualified source and documented.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Grounding</TTL><BRK/>
<BRK/>
<TXT>Ground electrical circuits, equipment and enclosures in accordance with [<RID>NFPA 70</RID>][ and ][<RID>IEEE C2</RID>] to provide a permanent, continuous and effective 
path to ground unless otherwise noted by <RID>EM 385-1-1</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Testing</TTL><BRK/>
<BRK/>
<TXT>Temporary electrical distribution systems and devices must be inspected, tested and found acceptable for Ground-Fault Circuit Interrupter (GFCI) 
protection, polarity, ground continuity, and ground resistance before <NED/>initial use, before use after modification and at least monthly.  Monthly 
inspections and tests must be maintained for each temporary electrical distribution system, and signed by the electrical CP or QP.</TXT><BRK/>
<BRK/></SPT>
</SPT></PRT>    <END/><BRK/></SEC>
