<?xml version="1.0" encoding="windows-1252"?><SEC xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="http://si.ksc.nasa.gov/sidownloads/xml/specsintactSEC.xsd"><MTA NAME="SUBFORMAT" CONTENT="NEW"/><MTA NAME="AUTONUMBER" CONTENT="TRUE"/><HDR><AST/><TAB BORDERS="0">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="4">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="366.00"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="365.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="12.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">USACE / NAVFAC / AFCEC</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">UFGS-01 57 19 (August 2022)</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="8.25">
         <CEL MERGEDOWN="1" STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Change 2 - 08/25</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="8.25">
         <CEL INDEX="2" STYLEID="s50">
<DTA TYPE="STRING"><HL3>------------------------------------</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="66.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Preparing Activity:  <PRA>NAVFAC</PRA></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Superseding<BRK/>UFGS-01 57 19 (November 2015)<BRK/>UFGS-01 57 19.01 20 (November 2015)</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<HL4>UNIFIED FACILITIES GUIDE SPECIFICATIONS</HL4><BRK/>
<BRK/>
<HL4>References are in agreement with UMRL dated July 2025</HL4><BRK/>
<AST/><BRK/></HDR>
<BRK/>
<SCN>SECTION 01 57 19</SCN><BRK/>
<BRK/>
<STL>TEMPORARY ENVIRONMENTAL CONTROLS</STL><BRK/>
<DTE>08/22, CHG 2: 08/25</DTE><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This guide specification covers the requirements for <SCP>environmental protection and other environmental temporary 
controls</SCP>.</NPR><BRK/>
<BRK/>
<NPR>Use this specification for design and construction projects located CONUS and OCONUS.  Edit this specification 
to the extent that is allowed and does not conflict with the applicable Status of Forces Agreements (SOFA), Host 
Nation-Funded Construction Agreements (HNFA), and in some instances, Bilateral Infrastructure Agreements (BIA), 
and country-specific Final Governing Standards (FGS) or the DoD Overseas Environmental Baseline Guidance Document 
(OEBGD), DoD 4715.05.  The OEBGD applies when there are no FGS in place.</NPR><BRK/>
<BRK/>
<NPR>Only edit the parts of this specification section that have bracketed choices.</NPR><BRK/>
<BRK/>
<NPR>Many States and Municipalities have more stringent or additional requirements:</NPR><BRK/>
<BRK/>
<NPR>For Navy projects, use this section and those portions of this section which contain State and Local requirements.  
Add any further local requirements into this section.  Use these sections for both Design-Bid-Build and Design-Build 
projects.</NPR><BRK/>
<BRK/>
<NPR>For Army projects.  Edit this section to include weblinks to the State or Local requirement.  Add the State and 
Local source to the Reference list and cite within the body of this section.  Clearly state in this section deviations 
from the State and Local requirements.</NPR><BRK/>
<BRK/>
<NPR>Adhere to <URL HREF="https://www.wbdg.org/dod/ufc/ufc-1-300-02">UFS 1-300-02</URL> Unified Facilities Guide Specifications (UFGS) Format Standard when editing this guide 
specification or preparing new project specification sections.  Edit this guide specification for project specific 
requirements by adding, deleting, or revising text.  For bracketed items, choose applicable item(s) or insert 
appropriate information.</NPR><BRK/>
<BRK/>
<NPR>Remove information and requirements not required in respective project, whether or not brackets are present.</NPR><BRK/>
<BRK/>
<NPR>NOTE:  To download UFGS Forms, Graphics, and Tables, go to: <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables</URL></NPR><BRK/>
<BRK/>
<NPR>Comments, suggestions and recommended changes for this guide specification are welcome and should be submitted 
as a <URL HREF="https://www.wbdg.org/dod/ufgs">Criteria Change Request (CCR)</URL>.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<PRT><TTL>PART 1   GENERAL</TTL><BRK/>
<BRK/>
<SPT><TTL>REFERENCES</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is used to list the publications cited in the text of the guide specification.  The publications 
are referred to in the text by basic designation only and listed in this paragraph by organization, designation, 
date, and title.</NPR><BRK/>
<BRK/>
<NPR>Use the Reference Wizard's Check Reference feature when you add a Reference Identifier (RID) outside of the Section's 
Reference Article to automatically place the reference in the Reference Article.  Also use the Reference Wizard's 
Check Reference feature to update the issue dates.</NPR><BRK/>
<BRK/>
<NPR>References not used in the text will automatically be deleted from this section of the project specification when 
you choose to reconcile references in the publish print process.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The publications listed below form a part of this specification to the extent referenced.  The publications are referred to within the text by 
the basic designation only.</TXT><BRK/>
<BRK/>
<REF><ORG>ASSOCIATION OF ILLINOIS SOIL AND WATER CONSERVATION DISTRICTS (AISWCD)</ORG><BRK/>
<BRK/>
<RID>IUM</RID><RTL>(2020) Illinois Urban Manual</RTL><BRK/>
<BRK/></REF>
<REF><ORG>ASTM INTERNATIONAL (ASTM)</ORG><BRK/>
<BRK/>
<RID>ASTM E2356</RID><RTL>(2018) Standard Practice for Comprehensive Building Asbestos Surveys</RTL><BRK/>
<BRK/></REF>
<REF><ORG>ILLINOIS ENVIRONMENTAL PROTECTION AGENCY (IEPA)</ORG><BRK/>
<BRK/>
<RID>35 IAC 900-901</RID><RTL>Title 35 of Illinois Administrative Code, Subtitle H: Noise, Chapter I: Pollution 
Control Board</RTL><BRK/>
<BRK/></REF>
<REF><ORG>INDIANA DEPARTMENT OF ENVIRONMENTAL MANAGEMENT (IDEM)</ORG><BRK/>
<BRK/>
<RID>327 IAC 2-6.1</RID><RTL>Indiana Administrative Code, Volume 6, Title 327, Article 2, Rule 6.1. Spills; 
Reporting, Containment, and Response</RTL><BRK/>
<BRK/>
<RID>327 IAC 15-5</RID><RTL>Indiana Administrative Code, Volume 6, Title 327, Article 15, Section 5. Storm 
Water Run-off Associated with Construction Activity</RTL><BRK/>
<BRK/>
<RID>327 IAC 15-5-6</RID><RTL>Indiana Administrative Code, Volume 6, Title 327, Article 15, Section 5-6. Submittal 
of an NOI Letter and Construction Plans</RTL><BRK/>
<BRK/>
<RID>327 IAC 15-5-6.5</RID><RTL>Indiana Administrative Code, Volume 6, Title 327, Article 15, Section 5-6.5. Requirements 
for Construction Plans</RTL><BRK/>
<BRK/>
<RID>327 IAC 15-5-7</RID><RTL>Indiana Administrative Code, Volume 6, Title 327, Article 15, Section 5-7. General 
Requirements for Storm Water Quality Control</RTL><BRK/>
<BRK/></REF>
<REF><ORG>INSTRUCTIONS AND STANDARDS FOR NAVBASE GUANTANAMO BAY CUBA (COMNAVBASEGTMOINST)</ORG><BRK/>
<BRK/>
<RID>1710.10</RID><RTL>Outdoor Recreational and Wildlife Instruction</RTL><BRK/>
<BRK/>
<RID>4400.2A</RID><RTL>Consolidated Hazardous Material Reutilization and Inventory Management Program</RTL><BRK/>
<BRK/>
<RID>5090.1</RID><RTL>Hazardous Waste Management Plan</RTL><BRK/>
<BRK/>
<RID>5090.4</RID><RTL>Standard Operating Procedures for Landfill</RTL><BRK/>
<BRK/>
<RID>5090.7</RID><RTL>Pollution Control Procedures for Oil and Hazardous Substances</RTL><BRK/>
<BRK/>
<RID>5090.8</RID><RTL>Asbestos Program Management</RTL><BRK/>
<BRK/>
<RID>5100.13</RID><RTL>Hazardous Material/Excess Hazardous Material Control and Safety Program</RTL><BRK/>
<BRK/>
<RID>FGS</RID><RTL>(1994) Final Governing Standards for Environmental Protection by U.S. Forces in 
Cuba</RTL><BRK/>
<BRK/></REF>
<REF><ORG>NORTHWEST REGION CLEAN AIR AGENCY (NWCAA)</ORG><BRK/>
<BRK/>
<RID>NWCAA Regulation</RID><RTL>(2019) Regulation of the Northwest Clean Air Agency</RTL><BRK/>
<BRK/></REF>
<REF><ORG>OLYMPIC REGION CLEAN AIR AGENCY (ORCAA)</ORG><BRK/>
<BRK/>
<RID>ORCAA Regulations</RID><RTL>(2024) Regulations of the Olympic Region Clean Air Agency</RTL><BRK/>
<BRK/></REF>
<REF><ORG>PUGET SOUND CLEAN AIR AGENCY (PSCAA)</ORG><BRK/>
<BRK/>
<RID>PSCAA Regulation</RID><RTL>Regulation I, II, and III</RTL><BRK/>
<BRK/></REF>
<REF><ORG>STATE OF VIRGINIA ADMINISTRATIVE CODE (VAC)</ORG><BRK/>
<BRK/>
<RID>9 VAC 25-840</RID><RTL>Title 9, Agency 25, Chapter 840: Erosion And Sediment Control Regulations</RTL><BRK/>
<BRK/>
<RID>9 VAC 25-850</RID><RTL>Title 9, Agency 25, Chapter 850: Erosion And Sediment Control And Stormwater Management 
Certification Regulations</RTL><BRK/>
<BRK/>
<RID>9 VAC 25-870</RID><RTL>Title 9, Agency 25, Chapter 870: Virginia Stormwater Management Program (VSMP) 
Regulation</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. ARMY CORPS OF ENGINEERS (USACE)</ORG><BRK/>
<BRK/>
<RID>EM 385-1-1</RID><RTL>(2024) Safety -- Safety and Occupational Health (SOH) Requirements</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. ENVIRONMENTAL PROTECTION AGENCY (EPA)</ORG><BRK/>
<BRK/>
<RID>EPA SW-846</RID><RTL>(Third Edition; Update VII) Test Methods for Evaluating Solid Waste: Physical/Chemical 
Methods</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. NATIONAL ARCHIVES AND RECORDS ADMINISTRATION (NARA)</ORG><BRK/>
<BRK/>
<RID>29 CFR 1910.1053</RID><RTL>Respirable Crystalline Silica</RTL><BRK/>
<BRK/>
<RID>29 CFR 1910.1200</RID><RTL>Hazard Communication</RTL><BRK/>
<BRK/>
<RID>29 CFR 1926.1153</RID><RTL>Respirable Crystalline Silica</RTL><BRK/>
<BRK/>
<RID>40 CFR 50</RID><RTL>National Primary and Secondary Ambient Air Quality Standards</RTL><BRK/>
<BRK/>
<RID>40 CFR 60</RID><RTL>Standards of Performance for New Stationary Sources</RTL><BRK/>
<BRK/>
<RID>40 CFR 61.145</RID><RTL>Standard for Demolition and Renovation</RTL><BRK/>
<BRK/>
<RID>40 CFR 63</RID><RTL>National Emission Standards for Hazardous Air Pollutants for Source Categories</RTL><BRK/>
<BRK/>
<RID>40 CFR 64</RID><RTL>Compliance Assurance Monitoring</RTL><BRK/>
<BRK/>
<RID>40 CFR 68</RID><RTL>Chemical Accident Prevention Provisions</RTL><BRK/>
<BRK/>
<RID>40 CFR 82</RID><RTL>Protection of Stratospheric Ozone</RTL><BRK/>
<BRK/>
<RID>40 CFR 112</RID><RTL>Oil Pollution Prevention</RTL><BRK/>
<BRK/>
<RID>40 CFR 122.26</RID><RTL>Storm Water Discharges (Applicable to State NPDES Programs, see section 123.25)</RTL><BRK/>
<BRK/>
<RID>40 CFR 152</RID><RTL>Pesticide Registration and Classification Procedures</RTL><BRK/>
<BRK/>
<RID>40 CFR 152 - 186</RID><RTL>Pesticide Programs</RTL><BRK/>
<BRK/>
<RID>40 CFR 241</RID><RTL>Guidelines for Disposal of Solid Waste</RTL><BRK/>
<BRK/>
<RID>40 CFR 243</RID><RTL>Guidelines for the Storage and Collection of Residential, Commercial, and Institutional 
Solid Waste</RTL><BRK/>
<BRK/>
<RID>40 CFR 258</RID><RTL>Subtitle D Landfill Requirements</RTL><BRK/>
<BRK/>
<RID>40 CFR 260</RID><RTL>Hazardous Waste Management System:  General</RTL><BRK/>
<BRK/>
<RID>40 CFR 261</RID><RTL>Identification and Listing of Hazardous Waste</RTL><BRK/>
<BRK/>
<RID>40 CFR 261.7</RID><RTL>Residues of Hazardous Waste in Empty Containers</RTL><BRK/>
<BRK/>
<RID>40 CFR 262</RID><RTL>Standards Applicable to Generators of Hazardous Waste</RTL><BRK/>
<BRK/>
<RID>40 CFR 262.11</RID><RTL>Hazardous Waste Determination and Recordkeeping</RTL><BRK/>
<BRK/>
<RID>40 CFR 262.34</RID><RTL>Standards Applicable to Generators of Hazardous Waste-Accumulation Time</RTL><BRK/>
<BRK/>
<RID>40 CFR 263</RID><RTL>Standards Applicable to Transporters of Hazardous Waste</RTL><BRK/>
<BRK/>
<RID>40 CFR 264</RID><RTL>Standards for Owners and Operators of Hazardous Waste Treatment, Storage, and 
Disposal Facilities</RTL><BRK/>
<BRK/>
<RID>40 CFR 265</RID><RTL>Interim Status Standards for Owners and Operators of Hazardous Waste Treatment, 
Storage, and Disposal Facilities</RTL><BRK/>
<BRK/>
<RID>40 CFR 266</RID><RTL>Standards for the Management of Specific Hazardous Wastes and Specific Types of 
Hazardous Waste Management Facilities</RTL><BRK/>
<BRK/>
<RID>40 CFR 268</RID><RTL>Land Disposal Restrictions</RTL><BRK/>
<BRK/>
<RID>40 CFR 273</RID><RTL>Standards for Universal Waste Management</RTL><BRK/>
<BRK/>
<RID>40 CFR 273.2</RID><RTL>Standards for Universal Waste Management - Batteries</RTL><BRK/>
<BRK/>
<RID>40 CFR 273.3</RID><RTL>Standards for Universal Waste Management - Pesticides</RTL><BRK/>
<BRK/>
<RID>40 CFR 273.4</RID><RTL>Standards for Universal Waste Management - Mercury Containing Equipment</RTL><BRK/>
<BRK/>
<RID>40 CFR 273.5</RID><RTL>Standards for Universal Waste Management - Lamps</RTL><BRK/>
<BRK/>
<RID>40 CFR 273.6</RID><RTL>Applicability - Aerosol Cans</RTL><BRK/>
<BRK/>
<RID>40 CFR 279</RID><RTL>Standards for the Management of Used Oil</RTL><BRK/>
<BRK/>
<RID>40 CFR 300</RID><RTL>National Oil and Hazardous Substances Pollution Contingency Plan</RTL><BRK/>
<BRK/>
<RID>40 CFR 300.125</RID><RTL>National Oil and Hazardous Substances Pollution Contingency Plan - Notification 
and Communications</RTL><BRK/>
<BRK/>
<RID>40 CFR 302</RID><RTL>Designation, Reportable Quantities, and Notification</RTL><BRK/>
<BRK/>
<RID>40 CFR 355</RID><RTL>Emergency Planning and Notification</RTL><BRK/>
<BRK/>
<RID>40 CFR 372</RID><RTL>Toxic Chemical Release Reporting</RTL><BRK/>
<BRK/>
<RID>40 CFR 403</RID><RTL>General Pretreatment Regulations for Existing and New Sources of Pollution</RTL><BRK/>
<BRK/>
<RID>40 CFR 745</RID><RTL>Lead-Based Paint Poisoning Prevention in Certain Residential Structures</RTL><BRK/>
<BRK/>
<RID>40 CFR 761</RID><RTL>Polychlorinated Biphenyls (PCBs) Manufacturing, Processing, Distribution in Commerce, 
and Use Prohibitions</RTL><BRK/>
<BRK/>
<RID>49 CFR 171</RID><RTL>General Information, Regulations, and Definitions</RTL><BRK/>
<BRK/>
<RID>49 CFR 172</RID><RTL>Hazardous Materials Table, Special Provisions, Hazardous Materials Communications, 
Emergency Response Information, and Training Requirements</RTL><BRK/>
<BRK/>
<RID>49 CFR 172.101</RID><RTL>Hazardous Material Regulation-Purpose and Use of Hazardous Material Table</RTL><BRK/>
<BRK/>
<RID>49 CFR 173</RID><RTL>Shippers - General Requirements for Shipments and Packagings</RTL><BRK/>
<BRK/>
<RID>49 CFR 178</RID><RTL>Specifications for Packagings</RTL><BRK/>
<BRK/>
<RID>84 FR 24503</RID><RTL>Final Modification to National Pollutant Discharge Elimination System (NPDES) 
General Permit for Stormwater Discharges from Construction Activities\</RTL><BRK/>
<BRK/></REF>
<REF><ORG>WASHINGTON STATE ADMINISTRATIVE CODE (WAC)</ORG><BRK/>
<BRK/>
<RID>WAC-173-60</RID><RTL>Maximum Environmental Noise Levels</RTL><BRK/>
<BRK/>
<RID>WAC-173-160</RID><RTL>Minimum Standards for Construction and Maintenance of Wells</RTL><BRK/>
<BRK/>
<RID>WAC-173-303</RID><RTL>Washington Dangerous Waste Regulations</RTL><BRK/>
<BRK/>
<RID>WAC-173-303-330</RID><RTL>Personnel Training</RTL><BRK/>
<BRK/>
<RID>WAC-173-303-573</RID><RTL>Standards for Universal Waste Management</RTL><BRK/>
<BRK/>
<RID>WAC-173-303-573(2)</RID><RTL>Standards for Universal Waste Management - Batteries</RTL><BRK/>
<BRK/>
<RID>WAC-173-303-573(3)</RID><RTL>Standards for Universal Waste Management - Mercury-containing Equipment</RTL><BRK/>
<BRK/>
<RID>WAC-173-303-573(5)</RID><RTL>Standards for Universal Waste Management - Lamps</RTL><BRK/>
<BRK/>
<RID>WAC-173-350</RID><RTL>Solid Waste Handling Standards</RTL><BRK/>
<BRK/>
<RID>WAC-173-443</RID><RTL>Hydrofluorocarbons (HFCs) and Other Fluorinated Greenhouse Gases</RTL><BRK/>
<BRK/>
<RID>WAC-222-30</RID><RTL>Timber Harvesting</RTL><BRK/>
<BRK/>
<RID>WAC-246-290</RID><RTL>Department of Health Drinking Water Regulation</RTL><BRK/>
<BRK/></REF>
<REF><ORG>WASHINGTON STATE DEPARTMENT OF ECOLOGY (WSDE)</ORG><BRK/>
<BRK/>
<RID>WSDE SWMMWW</RID><RTL>(2019) Stormwater Management Manual for Western Washington</RTL><BRK/>
<BRK/></REF>
<REF><ORG>WISCONSIN DEPARTMENT OF NATURAL RESOURCES (WDNR)</ORG><BRK/>
<BRK/>
<RID>s. NR 415, Wis. Adm. Code</RID><RTL>Control of Particulate Emissions</RTL><BRK/>
<BRK/></REF>
</SPT><SPT><TTL>DEFINITIONS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Delete definitions not used within the section edited for a project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Class I and II Ozone Depleting Substance (ODS)</TTL><BRK/>
<BRK/>
<TXT>Class I ODS is defined in Section 602(a) of The Clean Air Act.  A list of Class I ODS can be found on the EPA website at the following weblink. <URL>
https://www.epa.gov/ozone-layer-protection/ozone-depleting-substances</URL>.</TXT><BRK/>
<BRK/>
<TXT>Class II ODS is defined in Section 602(s) of The Clean Air Act.  A list of Class II ODS can be found on the EPA website at the following weblink. <URL>
https://www.epa.gov/ozone-layer-protection/ozone-depleting-substances</URL>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Contractor Generated Hazardous Waste</TTL><BRK/>
<BRK/>
<TXT>Contractor generated hazardous waste is materials that, if abandoned or disposed of, may meet the definition of a hazardous waste.  These waste 
streams would typically consist of material brought on site by the Contractor to execute work, but are not fully consumed during the course of 
construction.  Examples include, but are not limited to, excess paint thinners (i.e., methyl ethyl ketone, toluene), waste thinners, excess paints, 
excess solvents, waste solvents, excess pesticides, and contaminated pesticide equipment rinse water.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Electronics Waste</TTL><BRK/>
<BRK/>
<TXT>Electronics waste is discarded electronic devices intended for salvage, recycling, or disposal.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Environmental Pollution and Damage</TTL><BRK/>
<BRK/>
<TXT>Environmental pollution and damage is the presence of chemical, physical, or biological elements or agents which adversely affect human health 
or welfare; unfavorably alter ecological balances of importance to human life; affect other species of importance to humankind; or degrade the 
environment aesthetically, culturally or historically.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Environmental Protection</TTL><BRK/>
<BRK/>
<TXT>Environmental protection is the prevention/control of pollution and habitat disruption that may occur to the environment during construction.  
The control of environmental pollution and damage requires consideration of land, water, and air; biological and cultural resources; and includes 
management of visual aesthetics; noise; solid, chemical, gaseous, and liquid waste; radiant energy and radioactive material as well as other pollutants.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Hazardous Debris</TTL><BRK/>
<BRK/>
<TXT>As defined in paragraph SOLID WASTE, debris that contains listed hazardous waste (either on the debris surface, or in its interstices, such as 
pore structure) in accordance with <RID>40 CFR 261</RID>.  Hazardous debris also includes debris that exhibits a characteristic of hazardous waste in accordance 
with <RID>40 CFR 261</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Hazardous Materials</TTL><BRK/>
<BRK/>
<TXT>Hazardous material is any material that:  Is defined in <RID>49 CFR 171</RID>, listed in <RID>49 CFR 172</RID>, regulated as a hazardous material in accordance with <RID>
49 CFR 173</RID>; or requires a Safety Data Sheet (SDS) in accordance with <RID>29 CFR 1910.1200</RID>; or during end use, treatment, handling, packaging, storage, 
transportation, or disposal meets or has components that meet or have potential to meet the definition of a hazardous waste as defined by <RID>40 CFR 261</RID>
 Subparts A, B, C, or D.  Designation of a material by this definition, when separately regulated or controlled by other sections or directives, 
does not eliminate the need for adherence to that hazard-specific guidance which takes precedence over this section for "control" purposes.  Such 
material includes ammunition, weapons, explosive actuated devices, propellants, pyrotechnics, chemical and biological warfare materials, medical 
and pharmaceutical supplies, medical waste and infectious materials, bulk fuels, radioactive materials, and other materials such as asbestos, mercury, 
and polychlorinated biphenyls (PCBs).</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Hazardous Waste</TTL><BRK/>
<BRK/>
<TXT>Hazardous Waste is any material that meets the definition of a solid waste and exhibits a hazardous characteristic (ignitability, corrosivity, 
reactivity, or toxicity) as specified in <RID>40 CFR 261</RID>, Subpart C, or contains a listed hazardous waste as identified in <RID>40 CFR 261</RID>, Subpart D, or 
meets a state, local, or host nation definition of a hazardous waste.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ARMY"><SPT><TTL>Installation Pest Management Coordinator</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ARMY.  Use this paragraph for Army projects only.  Do not use for 
Navy or Air Force projects.  Delete as appropriate if project is not on an installation.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Installation Pest Management Coordinator (IPMC) is the individual officially designated by the Installation Commander to oversee the Installation 
Pest Management Program and the Installation Pest Management Plan.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Land Application</TTL><BRK/>
<BRK/>
<TXT>Land Application means spreading or spraying discharge water at a rate that allows the water to percolate into the soil.  No sheeting action, soil 
erosion, discharge into storm sewers, discharge into defined drainage areas, or discharge into the "waters of the United States" must occur.  Comply 
with federal, state, and local laws and regulations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Municipal Separate Storm Sewer System (MS4) Permit</TTL><BRK/>
<BRK/>
<TXT>MS4 permits are those held by municipalities or installations to obtain NPDES permit coverage for their stormwater discharges.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>National Pollutant Discharge Elimination System (NPDES)</TTL><BRK/>
<BRK/>
<TXT>The NPDES permit program controls water pollution by regulating point sources that discharge pollutants into waters of the United States.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Oily Waste</TTL><BRK/>
<BRK/>
<TXT>Oily waste are those materials that are, or were, mixed with Petroleum, Oils, and Lubricants (POLs) and have become separated from that POLs.  
Oily wastes also means materials, including wastewaters, centrifuge solids, filter residues or sludges, bottom sediments, tank bottoms, and sorbents 
which have come into contact with and have been contaminated by, POLs and may be appropriately tested and discarded in a manner which is in compliance 
with other state and local requirements.</TXT><BRK/>
<BRK/>
<TXT>This definition includes materials such as oily rags, "kitty litter" sorbent clay and organic sorbent material.  These materials may be land filled 
provided that:  It is not prohibited in other state regulations or local ordinances; the amount generated is "de minimus" (a small amount); it 
is the result of minor leaks or spills resulting from normal process operations; and free-flowing oil has been removed to the practicable extent 
possible.  Large quantities of this material, generated as a result of a major spill or in lieu of proper maintenance of the processing equipment, 
are a solid waste.  As a solid waste, perform a hazardous waste determination prior to disposal.  As this can be an expensive process, it is recommended 
that this type of waste be minimized through good housekeeping practices and employee education.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ARMY"><SPT><TTL>Pesticide</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ARMY use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Pesticide is any substance or mixture of substances intended for preventing, destroying, repelling, or mitigating any pest, or intended for use 
as a plant regulator, defoliant or desiccant.</TXT><BRK/>
<BRK/></SPT>
</TAI><TAI OPT="ARMY"><SPT><TTL>Pesticide Treatment Plan</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ARMY use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>A plan for the prevention, monitoring, and control to eliminate pest infestation.</TXT><BRK/>
<BRK/></SPT>
</TAI><TAI OPT="ARMY"><SPT><TTL>Pests</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ARMY use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Pests are arthropods, birds, rodents, nematodes, fungi, bacteria, viruses, algae, snails, marine borers, snakes, weeds and other organisms (except 
for human or animal disease-causing organisms) that adversely affect readiness, military operations, or the well-being of personnel and animals; 
attack or damage real property, supplies, equipment, or vegetation; or are otherwise undesirable.</TXT><BRK/>
<BRK/></SPT>
</TAI><TAI OPT="ARMY"><SPT><TTL>Project Pesticide Coordinator</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ARMY use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Project Pesticide Coordinator (PPC) is an individual who resides at a Civil Works Project office and who is responsible overseeing of pesticide 
application on project grounds.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Regulated Waste</TTL><BRK/>
<BRK/>
<TXT>Regulated waste are solid wastes that have specific additional federal, state, or local controls for handling, storage, or disposal.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Sediment</TTL><BRK/>
<BRK/>
<TXT>Sediment is soil and other debris that have eroded and have been transported by runoff water or wind.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Solid Waste</TTL><BRK/>
<BRK/>
<TXT>Solid waste is a solid, liquid, semi-solid or contained gaseous waste.  A solid waste can be a hazardous waste, non-hazardous waste, or non-Resource 
Conservation and Recovery Act (RCRA) regulated waste.  Types of solid waste typically generated at construction sites may include:</TXT><BRK/>
<BRK/>
<SPT><TTL>Debris</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  State and local requirements regarding the acceptability of reinforcement in inert debris vary.  Check 
with the Solid Waste Authority at the state or local level and edit the second sentence accordingly.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Debris is non-hazardous solid material generated during the construction, demolition, or renovation of a structure that exceeds<MET> 60 mm</MET><ENG> 2.5-inch</ENG> 
particle size that is: a manufactured object; plant or animal matter; or natural geologic material (for example, cobbles and boulders), broken 
or removed concrete, masonry, and rock asphalt paving; ceramics; roofing paper and shingles.  Inert materials [may][may not] be reinforced with 
or contain ferrous wire, rods, accessories and weldments.  A mixture of debris and other material such as soil or sludge is also subject to regulation 
as debris if the mixture is comprised primarily of debris by volume, based on visual inspection.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ILLINOIS"><SPT><TTL>Clean Construction and Demolition Debris (CCDD)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ILLINOIS and is for State of Illinois use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>As defined by the Illinois Environmental Protection Agency, CCDD is uncontaminated broken concrete without protruding metal bars, bricks, rock, 
stone, or reclaimed asphalt pavement generated from construction or demolition activities.  When uncontaminated soil is mixed with any of these 
materials, the uncontaminated soil is considered CCDD.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Green Waste</TTL><BRK/>
<BRK/>
<TXT>Green waste is the vegetative matter from landscaping, land clearing and grubbing, including, but not limited to, grass, bushes, scrubs, small 
trees and saplings, tree stumps and plant roots.  Marketable trees, grasses and plants that are indicated to remain, be re-located, or be re-used 
are not included.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Material Not Regulated As Solid Waste</TTL><BRK/>
<BRK/>
<TXT>Material not regulated as solid waste is nuclear source or byproduct materials regulated under the Federal Atomic Energy Act of 1954 as amended; 
suspended or dissolved materials in domestic sewage effluent or irrigation return flows, or other regulated point source discharges; regulated 
air emissions; and fluids or wastes associated with natural gas or crude oil exploration or production.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Non-Hazardous Waste</TTL><BRK/>
<BRK/>
<TXT>Non-hazardous waste is waste that is excluded from, or does not meet, hazardous waste criteria in accordance with <RID>40 CFR 261</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Recyclables</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  State and local requirements regarding the inclusion within recyclables of paint cans and lead contaminated 
or lead based paint contaminated metal or wiring sold to scrap metal companies vary.  Check with the Solid Waste 
Authority at the state or local level and edit accordingly.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Recyclables are materials, equipment and assemblies such as doors, windows, door and window frames, plumbing fixtures, glazing and mirrors that 
are recovered and sold as recyclable,[ wiring,][ insulated/non-insulated copper wire cable,][ wire rope,] and structural components.  It also includes 
commercial-grade refrigeration equipment with Freon removed, household appliances where the basic material content is metal, clean polyethylene 
terephthalate bottles, cooking oil, used fuel oil, textiles, high-grade paper products and corrugated cardboard, stackable pallets in good condition, 
clean crating material, and clean rubber/vehicle tires.  Metal meeting the definition of "lead contaminated" or "lead based paint contaminated" 
may be included as recyclable only if the metal is handled and transported in accordance with regulations, and the facility receiving the material 
is permitted and authorized to accept and process lead contaminated materials.  Paint cans that meet the definition of empty containers in accordance 
with <RID>40 CFR 261.7</RID> may be included as recyclable if sold to a scrap metal company.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Surplus Soil</TTL><BRK/>
<BRK/>
<TXT>Surplus soil is existing soil that is in excess of what is required for this work, including aggregates intended, but not used, for on-site mixing 
of concrete, mortars, and paving.  Contaminated soil meeting the definition of hazardous material or hazardous waste is not included and must be 
managed in accordance with paragraph HAZARDOUS MATERIAL MANAGEMENT.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Scrap Metal</TTL><BRK/>
<BRK/>
<TXT>This includes scrap and excess ferrous and non-ferrous metals such as reinforcing steel, structural shapes, pipe, and wire that are recovered or 
collected and disposed of as scrap.  Scrap metal meeting the definition of hazardous material or hazardous waste is not included.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Wood</TTL><BRK/>
<BRK/>
<TXT>Wood is dimension and non-dimension lumber, plywood, chipboard, hardboard.  Treated or painted wood that meets the definition of lead contaminated 
or lead based contaminated paint is not included.  Treated wood includes, but is not limited to, lumber, utility poles, crossties, and other wood 
products with chemical treatment.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Surface Discharge</TTL><BRK/>
<BRK/>
<TXT>Surface discharge means discharge of water into drainage ditches, storm sewers, or creeks meeting the definition of "waters of the United States".  
Surface discharges from construction sites are discrete, identifiable sources and require a permit from the governing agency.  Comply with federal, 
state, and local laws and regulations.</TXT><BRK/>
<BRK/>
<TAI OPT="ILLINOIS"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ILLINOIS and is for State of Illinois use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The term "Surface Discharge" implies that the water is discharged with possible sheeting action and subsequent soil erosion may occur.  Waters 
that are surface discharged may terminate in drainage ditches, storm sewers, creeks, or "waters of the United States" and would require a permit 
to discharge water from the governing agency.  All projects with land disturbances greater than or equal to one acre in total area must have a 
National Pollution Discharge Elimination System (NPDES) Construction Site Activity Storm Water Permit to discharge surface water from a construction 
site, issued by the Illinois Environmental Protection Agency.  All projects with discharge of dredged or fill material to waters of the United 
States must have a Section 401 Water Quality Permit issued by the Illinois Environmental Protection Agency.</TXT><BRK/>
<BRK/></TAI>
<TAI OPT="INDIANA"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for INDIANA and is for State of Indiana use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The term "Surface Discharge" implies that the water is discharged with possible sheeting action and subsequent soil erosion may occur.  Waters 
that are surface discharged may terminate in drainage ditches, storm sewers, creeks, or "waters of the United States".  All projects with land 
disturbances greater than or equal to one acre in total area must have a National Pollution Discharge Elimination System (NPDES) Construction Site 
Activity Storm Water Permit, issued by the Indiana Department of Environmental Management.  All projects with discharge of dredged or fill material 
to waters of the United States must have a Section 401 Water Quality Permit issued by the Indiana Department of Environmental Management.</TXT><BRK/>
<BRK/></TAI>
<TAI OPT="WISCONSIN"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for WISCONSIN and is for State of Wisconsin use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The term "Surface Discharge" implies that the water is discharged with possible sheeting action and subsequent soil erosion may occur. Waters that 
are surface discharged may terminate in drainage ditches, storm sewers, creeks, or "waters of the United States". All projects with land disturbances 
greater than or equal to one acre in total area must have a National Pollution Discharge Elimination System (NPDES) Construction Site Activity 
Storm Water Permit, issued by the Wisconsin Department of Natural Resources (WDNR).  All projects with discharge of dredged or fill material to 
waters of the United States must comply with Sections 404 and 401 of the Clean Water Act, including obtaining all required permits and approvals.</TXT><BRK/>
<BRK/></TAI>
</SPT><SPT><TTL>Wastewater</TTL><BRK/>
<BRK/>
<TXT>Wastewater is the aqueous liquid waste generated by a project, to include both domestic wastewater (sewage) and industrial wastewater.</TXT><BRK/>
<BRK/>
<SPT><TTL>Stormwater</TTL><BRK/>
<BRK/>
<TXT>Stormwater is any precipitation in an urban or suburban area that does not evaporate or soak into the ground, but instead collects and flows into 
storm drains, rivers, and streams.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Waters of the United States</TTL><BRK/>
<BRK/>
<TXT>Waters of the United States means Federally jurisdictional waters, including wetlands, that are subject to regulation under Section 404 of the 
Clean Water Act or navigable waters, as defined under the Rivers and Harbors Act.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Wetlands</TTL><BRK/>
<BRK/>
<TXT>Wetlands are those areas that are inundated or saturated by surface or groundwater at a frequency and duration sufficient to support, and that 
under normal circumstances do support, a prevalence of vegetation typically adapted for life in saturated soil conditions.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Universal Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>Note:  States' universal waste regulations may differ from the federal requirements below. Verify all constituents 
listed below are categorized as universal waste by the State where the project is located and edit accordingly.  
Some states may include additional materials.  Include those here.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The universal waste regulations streamline collection requirements for certain hazardous wastes in the following categories: batteries, pesticides, 
mercury-containing equipment (for example, thermostats), and lamps (for example, fluorescent bulbs).  The rule is designed to reduce hazardous 
waste in the municipal solid waste (MSW) stream by making it easier for universal waste handlers to collect these items and send them for recycling 
or proper disposal.  These regulations can be found at <RID>40 CFR 273</RID>.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="WASHINGTON"><SPT><TTL>Location Specific Universal Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for WASHINGTON and is for State of Washington use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Any of the following dangerous waste that are subject to the universal waste requirements of <RID>WAC-173-303-573</RID>: Batteries as described in <RID>WAC-173-303-573(2)</RID>
); Lamps as described in <RID>WAC-173-303-573(5)</RID>; Mercury-containing equipment as described in <RID>WAC-173-303-573(3)</RID>.</TXT><BRK/>
<BRK/></SPT>
</TAI><TAI OPT="NAVFAC NW"><SPT><TTL>Dangerous Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Waste defined as dangerous waste in accordance with <RID>WAC-173-303</RID>.  This includes, but is not limited to, hazardous waste, extremely hazardous waste 
and state-only dangerous waste.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Encountered Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Material that is of Government origin that becomes a waste during construction at or on Government property.  This term includes both foreseen 
and unforeseen Government waste discovered at the worksite.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Firewood</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Raw, woody material cut into short lengths and burned to produce energy.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Fugitive Dust</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Particulate matter or any visible air contaminant (smoke, dust, or fume) other than uncombined water that is not collected by a capture system 
and emitted from a stack, but is released to the atmosphere at the point of generation.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Ozone Depleting Substance (ODS) Substitute</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Any chemical or product, whether existing or new, that is used by any person as an EPA-approved replacement for a Class I or Class II ODS in a 
given refrigeration or air-conditioning end-use.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Prohibited Substances</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Prohibited substitutes perform a function previously performed by a class I substance or class II substance and any substitute subsequently adopted 
to perform that function including, but not limited to, hydrofluorocarbons that are listed as prohibited in <RID>WAC-173-443</RID>-040.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Refrigerant</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Any substance consisting in part or whole of a Class I or Class II ODS, or an ODS substitute that is used for heat transfer purposes and provides 
a cooling effect.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Refuse</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Includes, but is not limited to garbage, rubbish, trash, some soils, and non-painted demolition and construction debris.  The Government will designate 
refuse.  When designated as "refuse," the Government has determined the waste is not "Dangerous Waste."</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Sewage</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Liquid waste designated by the Government as "domestic sanitary sewage" and normally discharged through domestic sanitary sewage systems. Liquids 
designated as "sewage" include human body waste, and wastewater from sinks, showers, laundries, dishwashers, and garbage disposals when these liquids 
use only chemicals approved by the Government for discharge into the sanitary sewer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Spill Event</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph and subparagraphs are tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>A spill is any release of oil or hazardous substances to the water or ground that is not controlled or permitted.  This includes any spilling, 
leaking, pumping, emitting, discharging, injecting, escaping, leaching, disposing, or dumping of liquid or solid material that is not authorized 
in writing by the Contracting Officer.</TXT><BRK/>
<BRK/>
<SPT><TTL>Reportable Release</TTL><BRK/>
<BRK/>
<TXT>A reportable release means any spilling, leaking, pumping, pouring, emitting, emptying, discharging, injecting, escaping, leaching, dumping, or 
disposing into the environment of a known or unknown material or hazardous substance that poses an immediate threat to human health or the environment 
to the air, soil, or water.  Reportable releases are: a sheen of oil on the water; a violation of the Installation's or project's water permit 
(NPDES permit); a sewage spill that threatens human health or the environment or that reaches the stormwater system or any waterbody; a Comprehensive 
Environmental Response, Compensation, and Liability Act reportable quantity for hazardous/toxic substances (<RID>40 CFR 302</RID>); an air or hazardous substance 
release that is a threat to human health or the environment, or released outside the facility boundaries; any discharge from an underground storage 
tank regulated under WAC 173-360; or oil spilled to the ground or to permeable secondary containment of<MET> 160 liters</MET><ENG> 42 gallons</ENG> and greater.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Non-emergency Spill Event</TTL><BRK/>
<BRK/>
<TXT>A non-emergency spill event is a discharge of a known material or any hazardous substance that does not pose an immediate threat to human health 
or the environment, can be cleaned up as part of normal housekeeping by the personnel who discovered the spill, and is not released on the soil 
or into any waterway inlet (for example, storm drain) or outside Navy property boundaries.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Timber, Merchantable</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Any raw material yielded by a forest that is of a size, quality and condition suitable for marketing under given economic conditions, even if it 
is situated such that it is not immediately accessible for logging.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Nonroad Engine</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Nonroad engines are any internal combustion engine that, by itself or in or on a piece of equipment, is portable or transportable, meaning designed 
to be and capable of being carried or moved from one location to another.  Indicia of transportability include, but are not limited to, wheels, 
skids, carrying handles, dolly, trailer, or platform.  This definition is based on the principle of mobility and portability, and includes engines 
installed on (1) self-propelled equipment, (2) equipment that is propelled while performing its function, or (3) equipment that is portable or 
transportable, as indicated by the presence of wheels, skids, carrying handles, dolly, trailer, or platform.  Examples of regulated applications 
include farm tractors, excavators, bulldozers, wheel loaders, backhoe loaders, road graders, diesel lawn tractors, logging equipment, portable 
generators, skid steer loaders, or forklifts.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Critical Root Zone (CRZ)</TTL><BRK/>
<BRK/>
<TXT>The critical root zone is the area around and under a tree where the majority of its roots are located.  The CRZ is usually measured as a circle 
with a radius of<MET> 457 mm</MET><ENG> 1.5 foot</ENG> for every<MET> 25 mm</MET><ENG> inch</ENG> of the tree's diameter at breast height (DBH), and a depth of<MET> 610 mm</MET><ENG> 24 inches</ENG>.</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Landfill-Controlled Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC NW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Waste containing harmful substances but not designated as dangerous in accordance with <RID>WAC-173-303</RID> that are screened by a receiving facility to 
ensure that it meets the requirements of their operating permit.  Examples include petroleum-contaminated soil, abrasive blast grit, street or 
dry-dock sweepings, treated wood, oily debris, and waste containing free liquids as determined by the Paint Filter Liquids Test method 9095.</TXT><BRK/>
<BRK/></SPT>
]</TAI></SPT><SPT><TTL>SUBMITTALS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Review Submittal Description (SD) definitions in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES and edit the following 
list, and corresponding submittal items in the text, to reflect only the submittals required for the project.  
The Guide Specification technical editors have classified those items that require Government approval, due to 
their complexity or criticality, with a "G."  Generally, other submittal items can be reviewed by the Contractor's 
Quality Control System.  Only add a "G" to an item if the submittal is sufficiently important or complex in context 
of the project.</NPR><BRK/>
<BRK/>
<NPR><TAI OPT="ARMY">For Army projects, fill in the empty brackets following the "G" classification, with a code of up to three characters 
to indicate the approving authority.  Codes for Army projects using the Resident Management System (RMS) are:  
"AE" for Architect-Engineer; "DO" for District Office (Engineering Division or other organization in the District 
Office); "AO" for Area Office; "RO" for Resident Office; and "PO" for Project Office.  </TAI>Codes following the "G" 
typically are not used for Navy and Air Force projects.</NPR><BRK/>
<BRK/>
<NPR>The "S" classification indicates submittals required as proof of compliance for sustainability Guiding Principles 
Validation or Third Party Certification and as described in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
<TAI OPT="NAVY DESIGN-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Navy Design-Build projects, delete <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES, and replace with UFGS 01 33 00.05 
20 CONSTRUCTION SUBMITTAL PROCEDURES and UFGS 01 33 10.05 20 DESIGN SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Government approval is required for submittals with a "G" or "S" classification.<TAI OPT="AIR FORCE,NAVY">  Submittals not having a "G" or "S" classification are for Contractor 
Quality Control approval.</TAI><TAI OPT="ARMY">  Submittals not having a "G" or "S" classification are for information only.  When used, a code following the "G" classification 
identifies the office that will review the submittal for the Government.</TAI>  Submit the following in accordance with Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES:</TXT><BRK/>
<BRK/>
<LST><SUB>SD-01 Preconstruction Submittals</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Contractor Hazardous Material Inventory Log</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<TAI OPT="NAVFAC NW"><NTE><AST/><BRK/>
<NPR>NOTE:  Include the following submittal for NBK Bangor and NBK Keyport.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Waste Originator Training Certification</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<NTE><AST/><BRK/>
<NPR>NOTE:  Include the following submittal for NBK Bangor, NBK Keyport, NBK Bremerton, NAVSTA Everett.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>PSCAA Nonroad Engine Notification Form</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Include the following submittal for construction of a new air pollution source.  At NBK Bangor, NBK Keyport, 
NBK Bremerton, and Everett choose PSCAA.  At Indian Island, choose ORCAA.  At Whidbey, choose NWCAA.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Notice of Construction</SUB>, [PSCAA][ORCAA][NWCAA]; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC SE"><NTE><AST/><BRK/>
<NPR>NOTE:  Include the following three submittals for NAVFAC SE projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>Dewatering Permit</SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Florida Environmental Resource Permit</SUB></ITM><BRK/>
<BRK/>
]<ITM><SUB>Excavation Permits</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC PAC,ARMY"><NTE><AST/><BRK/>
<NPR>NOTE:  Include the following submittal item for Army projects and NAVFAC PAC projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Storage Material Inventory</SUB></ITM><BRK/>
<BRK/></TAI>
<ITM><SUB>Preconstruction Survey</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Regulatory Notifications</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Environmental Manager Qualifications</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Employee Training Records</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Environmental Protection Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Dirt and Dust Control Plan</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Solid Waste Management Permit</SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Stormwater Pollution Prevention Plan</SUB> (SWPPP); <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Stormwater Notice of Intent</SUB> (for NPDES coverage under the general permit for construction activities)</ITM><BRK/>
<BRK/>
]<ITM><SUB>Spill Prevention Control And Countermeasure (SPCC) Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<TAI OPT="NAVFAC NW"><NTE><AST/><BRK/>
<NPR>NOTE:  The following two submittal items are tailored for NAVFAC NW.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>Project Report</SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Contractor's Operation and Maintenance (O &amp; M) Plan</SUB></ITM><BRK/>
<BRK/>
]</TAI><LST><SUB>SD-06 Test Reports</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Monthly Solid Waste Disposal Report</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Inspection Reports</SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Laboratory Analysis</SUB></ITM><BRK/>
<BRK/>
]<LST><SUB>SD-07 Certificates</SUB></LST><BRK/>
<BRK/>
<TAI OPT="NAVY"><NTE><AST/><BRK/>
<NPR>NOTE:  The following submittal item is tailored for NAVY.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>ECATTS Certificate Of Completion</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/></TAI>
<ITM><SUB>Employee Training Records</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Erosion and Sediment Control Inspector</SUB> Qualifications</ITM><BRK/>
<BRK/>
]<TAI OPT="ARMY"><NTE><AST/><BRK/>
<NPR>NOTE:  The following submittal item is tailored for ARMY.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Certificate of Competency</SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC NW"><NTE><AST/><BRK/>
<NPR>NOTE:  Include the following for NBK Bremerton and NAVSTA Everett.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Storm Drain and Sanitary Sewer Discharge Approval</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Monthly Project Waste Summary Report</SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Landfill Disposal Form</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Dangerous Waste Profile</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Dangerous Waste Manifests</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Contractor Request for 45/90-Day Hazardous Waste Accumulation Certification/Recertification</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Contractor Request for Hazardous Waste Accumulation Area (SAA) Registration</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]<ITM><SUB>Accumulation Area Inspection Record</SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Hazardous Waste Accumulation Area Registration Form</SUB></ITM><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Include the following submittal for Whidbey and NAVSTA Everett.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Certificate Of Final Disposal</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/></TAI>
<LST><SUB>SD-11 Closeout Submittals</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Contractor Hazardous Material Inventory Log</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<TAI OPT="NAVFAC NW"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following submittal for NBK Keyport, NBK Bangor, NAVSTA Everett, and Indian Island.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Refrigerant Work Checklist</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Refuse and Recycle Quantity Form</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Project Completion Report</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Operation and Maintenance Records</SUB> (Air Pollution Sources)</ITM><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Select ORCAA for Indian Island, NWCAA for Whidbey, or PSCAA for Everett, NBK Bangor, NBK Bremerton, and 
NBK Keyport.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Notice of Completion</SUB>, [PSCAA][NWCAA][ORCAA]</ITM><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following submittal item for NBK Bremerton and Whidbey.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>Solid Waste Tracking Sheet</SUB></ITM><BRK/>
<BRK/></TAI>
<ITM><SUB>Regulatory Notifications</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Assembled Employee Training Records</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Solid Waste Management Permit</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Stormwater Pollution Prevention Plan Compliance Notebook</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Stormwater Notice of Termination</SUB> (for NPDES coverage under the general permit for construction activities); <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>As-Built Topographic Survey</SUB></ITM><BRK/>
<BRK/>
]<ITM><SUB>Waste Determination Documentation</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Project Solid Waste Disposal Documentation Report</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Sales Documentation</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Contractor Certification</SUB></ITM><BRK/>
<BRK/>
]<ITM><SUB>Hazardous Waste/Debris Management</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Disposal Documentation for Hazardous and Regulated Waste</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<TAI OPT="NAVFAC SE"><NTE><AST/><BRK/>
<NPR>NOTE:  Include the following submittal for NAVFAC SE projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>Hazardous Waste Inspection Logs</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]</TAI></SPT><SPT><TTL>ENVIRONMENTAL PROTECTION REQUIREMENTS</TTL><BRK/>
<BRK/>
<TXT>Provide and maintain, during the life of the contract, environmental protection as defined.  Plan for and provide environmental protective measures 
to control pollution that develops during construction practice.  Plan for and provide environmental protective measures required to correct conditions 
that develop during the construction of permanent or temporary environmental features associated with the project.  Protect the environmental resources 
within the project boundaries and those affected outside the limits of permanent work during the entire duration of this Contract.  Comply with 
federal, state, and local regulations pertaining to the environment, including water, air, solid waste, hazardous waste and substances, oily substances, 
and noise pollution.</TXT><BRK/>
<BRK/>
<TXT>Tests and procedures assessing whether construction operations comply with Applicable Environmental Laws may be required.  Analytical work must 
be performed by qualified laboratories; and where required by law, the laboratories must be certified.</TXT><BRK/>
<BRK/>
<TAI OPT="NAVY"><SPT><TTL>Training in Environmental Compliance Assessment Training and Tracking System (ECATTS)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following is tailored for NAVY.  Use this paragraph and subparagraphs for Navy projects only.  Delete 
for other projects.</NPR><BRK/>
<BRK/>
<NPR>Coordinate with the Installation Environmental Office to add additional staff that require training.  Coordinate 
with paragraph ENVIRONMENTAL MANAGER.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Personnel Requirements</TTL><BRK/>
<BRK/>
<TXT>The Environmental Manager is responsible for environmental compliance on projects.  The Environmental Manager[ and other staff], must complete 
applicable ECATTS training modules (installation specific or general) prior to starting respective portions of on-site work under this Contract.  
If personnel changes occur for any of these positions after starting work, replacement personnel must complete applicable ECATTS training within 
14 days of assignment to the project.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Certification</TTL><BRK/>
<BRK/>
<TXT>Submit an <SUB>ECATTS certificate of completion</SUB> for personnel who have completed the required ECATTS training.  This training is web-based and can be 
accessed from any computer with Internet access using the following instructions.</TXT><BRK/>
<BRK/>
<TXT>Register for NAVFAC Environmental Compliance Assessment, Training, and Tracking System, by logging on to <URL>https://environmentaltraining.ecatts.com/</URL>
.  Obtain the password for registration from the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Refresher Training</TTL><BRK/>
<BRK/>
<TXT>This training has been structured to allow contractor personnel to receive credit under this contract and to carry forward credit to future contracts.  
Ensure the Environmental Manager review their training plans for new modules or updated training requirements prior to beginning work.  Some training 
modules are tailored for specific state regulatory requirements; therefore, Contractors working in multiple states will be required to retake modules 
tailored to the state where the contract work is being performed.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>Conformance with the Environmental Management System</TTL><BRK/>
<BRK/>
<TXT>Perform work under this contract consistent with the policy and objectives identified in the installation's Environmental Management System (EMS).  
Perform work in a manner that conforms to objectives and targets of the environmental programs and operational controls identified by the EMS.  
Support Government personnel when environmental compliance and EMS audits are conducted by escorting auditors at the Project site, answering questions, 
and providing proof of records being maintained.  Provide monitoring and measurement information as necessary to address environmental performance 
relative to environmental, energy, and transportation management goals.  In the event an EMS nonconformance or environmental noncompliance associated 
with the contracted services, tasks, or actions occurs, take corrective and preventative actions.  In addition, employees must be aware of their 
roles and responsibilities under the installation EMS and of how these EMS roles and responsibilities affect work performed under the contract.</TXT><BRK/>
<BRK/>
<TXT>Coordinate with the installation's EMS coordinator to identify training needs associated with environmental aspects and the EMS, and arrange training 
or take other action to meet these needs.  Provide training documentation to the Contracting Officer.  The Installation Environmental Office will 
retain associated environmental compliance records.  Make EMS Awareness training completion certificates available to Government auditors during 
EMS audits and include the certificates in the Employee Training Records.  See paragraph EMPLOYEE TRAINING RECORDS.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>SPECIAL ENVIRONMENTAL REQUIREMENTS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The special environmental requirements with which the Contractor must comply must be developed during the 
design process, included in the bidding documents, and made a part of the contract.  The special environmental 
requirements must be developed by the Designer from such documents as the National Environmental Policy Act (NEPA) 
compliance measures specified in the Categorical Exclusion documentation, Environmental Assessment (EA), or the 
Environmental Impact Statement (EIS), the Installation Master Plan, or the Installation Storm Water Management 
Plan.  For Civil Works projects, the Environmental commitments made during planning are usually tracked by Project 
Management.  Coordination with the Project Manager is essential in developing the special requirements.</NPR><BRK/>
<BRK/>
<NPR>List attachments referenced below in paragraph LICENSES AND PERMITS, which require Contractor's actions, in the 
blank provided and attach to the end of this Section.  Remove this paragraph if not required in the project after 
coordination with paragraph LICENSES AND PERMITS.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the special environmental requirements listed here [_____] and attached at the end of this section.</TXT><BRK/>
<BRK/>
<TAI OPT="NAVFAC ML"><SPT><TTL>Mid-Atlantic</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph and subparagraphs are tailored for NAVFAC ML use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Applicable environmental requirements such as; erosion/sediment control, storm water, hazardous waste, 
and solid waste may have unique state regulations.  Edit this section to include these unique state requirements 
for each state listed below.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For each project, provide the following:<BRK/>
1. Unique local requirements and state regulations.<BRK/>
2. Environmental Point of Contact information for design review and base specific requirements.<BRK/>
3. For every installation in area of responsibility, the FEC must identify the facility Hazardous Waste Generator 
status as specified in paragraph FACILITY HAZARDOUS WASTE GENERATOR STATUS.<BRK/>
4. For each installation listed below, provide specific requirements of the installation's Environmental Management 
System (EMS) that relate to construction operations.  Identify those site specific EMS actions that the Contractor 
must perform under this contract.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the following state, regional, and local requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Virginia</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraphs apply to Hampton Roads Installations (Norfolk Naval Station, NAS Oceana, Dam Neck 
Annex, JEB Little Creek/Fort Story, Norfolk Naval Shipyard, NWS Yorktown, NSA Hampton Roads)  Modify and add requirements 
if used for other Installations in Virginia according to their practices.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Definition and Disposal Requirements of Empty Paint Cans</TTL><BRK/>
<BRK/>
<TXT>Paint Cans:  Paint cans that are empty (free of liquids and as defined in <RID>40 CFR 261.7</RID>) of paints, solvents, thinners and adhesives may be disposed 
of in dumpsters.</TXT><BRK/>
<BRK/>
<TXT>Metal paint cans that meet the empty standard can be placed in dumpsters marked "metal only"; plastic cans may be placed in solid waste dumpsters.  
Manage paint cans with liquid or more than<MET> 2.54 cm</MET><ENG> one inch</ENG> of solidified oil-based paint as a hazardous waste and label properly.  Manage paint 
cans with excess water-based paint as non-hazardous waste provided that they do not contain free liquids or contain any substance with a hazardous 
characteristic as defined in <RID>40 CFR 261</RID>.  Contact NAVFAC MIDLANT Environmental Services for management requirements.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Erosion and Sediment Control Measures and Stormwater Management</TTL><BRK/>
<BRK/>
<SPT><TTL>Erosion and Sediment Control</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph where land disturbance is<MET> 929 square meters</MET><ENG> 10,000 square feet</ENG> or greater.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Submit an erosion and sediment control plan, and comply with the requirements specified in the Virginia Erosion and Sediment Control Law and Regulations. 
(Virginia Code: <RID>9 VAC 25-840</RID>).  Obtain a Certificate of Competency in accordance with <RID>9 VAC 25-850</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Construction Dewatering</TTL><BRK/>
<BRK/>
<TXT>Construction site stormwater runoff must be treated using proper erosion control measures or stormwater management practices prior to release from 
the construction site.  Pollutants, including but not limited to chemicals, fuels, lubricants, sewage, paints, sedimentation, and other harmful 
materials must not be discharged into or alongside any river, stream, or impoundment, or into any channels leading to them.  Implement appropriate 
erosion and sediment control measures to all disturbed areas or bare soils to prevent unauthorized offsite sedimentation.  Apply stabilization 
measures to denuded portions of a project that are at final grade or where work has temporarily ceased within 7 days.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Virginia Stormwater Management</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph where land disturbance is<MET> 4047 square meters</MET><ENG> one acre</ENG> or greater.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Where land disturbance is equal to or exceeds<MET> 4046 square meters</MET><ENG> one acre</ENG>, prepare and submit a Stormwater Pollution Prevention Plan (SWPPP) and 
comply with the requirements specified in the Virginia Stormwater Management Law and Regulations (Virginia Code: <RID>9 VAC 25-870</RID>).  Obtain Certificate 
of Competency in accordance with <RID>9 VAC 25-850</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Stormwater General Permit for Construction Activities Registration Statement</TTL><BRK/>
<BRK/>
<TXT>In accordance with <RID>9 VAC 25-870</RID>, submit a Registration Statement to the State to obtain Virginia Stormwater Management Program General Permit coverage, 
and as required under the General Permit, develop a SWPPP for the project.  The SWPPP must meet the requirements of the State General Permit for 
storm water discharges from construction activities.  Submit the Registration Statement and appropriate permit fees to the appropriate state agency 
for approval a minimum of 15 calendar days prior to the start of any land disturbing activities.  Maintain an approved copy of the SWPPP at the 
onsite construction office, and continually update as regulations require, reflecting current site conditions.</TXT><BRK/>
<BRK/>
<TXT>Coverage under this permit requires the Contractor to prepare a SWPPP, prepare and submit a Registration Statement and provide the permit fee to 
the responsible state agency before any land disturbing activities begin.  File for permit coverage on behalf of both the Contractor and the Construction 
Officer, and file a Notice of Termination once construction is complete and the site is stabilized with a final sustainable cover.  Install, inspect, 
maintain best management practices (BMPs), and submit stormwater BMP inspection reports and SWPPP inspection reports as required under the terms 
and conditions of the permit.  Ensure construction operations and management comply with the terms and conditions of the general permit for stormwater 
discharges from construction activities.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Stormwater General Permit Inspection Reports</TTL><BRK/>
<BRK/>
<TXT>Complete and document, in the SWPPP Notebook, the Stormwater Inspection Reports as required by the State VSMP General Permit.  The Stormwater inspections 
reports must include items required by the General Permit and must be completed at the inspection frequency detailed in <RID>9 VAC 25-870</RID>.  Obtain certificate 
of competency in accordance with <RID>9 VAC 25-850</RID>.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Asbestos Abatement and Notification Procedures</TTL><BRK/>
<BRK/>
<TXT>Structures must be surveyed for the presence of asbestos prior to demolition or renovation in accordance with <RID>40 CFR 61.145</RID>.  A structure is defined 
as including any load-bearing portion of a structure.  The survey must be performed by a licensed, certified, accredited asbestos inspector in 
accordance with <RID>ASTM E2356</RID>.</TXT><BRK/>
<BRK/>
<TXT>Notify EPA and Virginia Department of Labor and Industry (VADOLI) at least 20 calendar days before start of asbestos abatement if asbestos is expected 
to total at least<MET> 79 linear meters</MET><ENG> 260 linear feet</ENG>,<MET> 14.9 square meters</MET><ENG> 160 square feet</ENG>, or<MET> one cubic meter</MET><ENG> 35 cubic feet</ENG>.  Provide copies of notifications 
to the environmental office (Air Manager) through the Contracting Officer prior to beginning work.  Make notifications for any project that includes 
asbestos abatement (and for all demolition projects, regardless of whether asbestos containing materials are present in the structure or facility) 
in accordance with paragraph DEMOLITION.  Notification is not required if asbestos is nonfriable asbestos containing roofing, flooring, or siding 
materials that when installed, encapsulated, or removed do not become friable.  If the material is damaged, the matrix binding the asbestos fibers 
has deteriorated, or mechanical removal results in more-than-incidental breakage, then notification is required.  Activities such as grinding, 
mechanical chipping, sawing or drilling can make the asbestos containing material friable and would require notification.</TXT><BRK/>
<BRK/>
<SPT><TTL>Best Management Practices</TTL><BRK/>
<BRK/>
<TXT>Use BMPs to ensure EPA and VADOLI requirements are met, including: preventing airborne emissions via wetting asbestos prior to removal; using glove 
bags or containment; using HEPA-filtered vacuum or ventilation systems; restricting access to asbestos-control areas until thoroughly cleaned and 
inspected, and acceptable air-samples have been received.  Consideration should be given to other environmental program requirements such as Clean 
Water Act (CWA) requirements when making decisions regarding BMPs.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Asbestos Waste Disposal</TTL><BRK/>
<BRK/>
<TXT>For asbestos waste disposal, phone the NAVFAC MIDLANT Environmental (EV) Service Desk to arrange pick up in your area.  A manifest must be signed 
by this office prior to waste being removed from the installation.  Provide copies of manifests and notifications to NAVFAC Mid-Atlantic EV Hazardous 
Waste (HW) Program Manager.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Hazardous Waste Requirements for Virginia Installations</TTL><BRK/>
<BRK/>
<SPT><TTL>Demolition</TTL><BRK/>
<BRK/>
<TXT>Remove the following items from the site prior to demolition: polychlorinated biphenyls (PCBs), fluorescent bulbs, mercury and metal components 
(such as furnaces, ducts, and piping), and any hazardous materials.  Manage lead, fluorescent bulbs, mercury-containing equipment, and any other 
waste as "hazardous or universal waste" as appropriate (see paragraph HAZARDOUS AND UNIVERSAL WASTE GENERATION).  If the demolition activity encompasses 
the whole building (the building must be demolished to the ground), the resulting construction debris (including lead paint) requires Toxicity 
Characteristic Leaching Procedure (TCLP) analysis to make a waste determination and ensure proper management and disposal before it can be disposed 
as solid waste.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Hazardous and Universal Waste Generation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Activity Hazardous Material Reutilization, Hazardous Waste Minimization and Disposal Guide is available 
for download at <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables</URL></NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Hazardous and Universal Waste includes fluorescent bulbs, PCB ballast, lead paint, and mercury-containing equipment.  Contact the EV HW Program 
Manager to set up an appropriate accumulation area.  Manage waste in a satellite accumulation area (SAA), hazardous waste accumulation area (HWAA), 
or universal waste accumulation area (UWAA) as directed by the EV HW Program Manager through the Contracting Officer.  Keep containers securely 
closed unless adding or removing material and waste.  Ensure custodians managing the accumulation area(s) have appropriate training that has been 
taken within the year prior to the area being established.  Training is an annual requirement that can be taken on the <URL HREF="https://environmentaltraining.ecatts.com">https://environmentaltraining.ecatts.com/</URL>
 site.  Keep copies of training records and certificates on site.</TXT><BRK/>
<BRK/>
<TXT>Hazardous Waste Accumulation Areas (less than 90-day sites) require Virginia Department of Environmental Quality (VDEQ) notification.  Notify the 
HA Media Manager (HW MM) 14 days prior to the start of waste accumulation.  The EV HW Program Manager is authorized to notify VDEQ when Hazardous 
Waste Accumulation Areas are established.  A copy of the Activity Hazardous Material Reutilization, Hazardous Waste Minimization and Disposal Guide 
will be provided by the Contracting Officer.  For waste disposal, phone the NAVFAC MIDLANT EV Service Desk to arrange pick up in your area.  Fax 
a completed DD 1348-1A to the Service Desk for all waste turn-ins.  Notify the Service Desk if any containers are leaking or are in poor condition.  
A representative from NAVFAC MIDLANT EV Services is the authorized entity approved to sign manifests for off-site waste disposal.</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Waste Management - Disposal by the Contractor</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate with the installation EV to determine whether paragraph WASTE MANAGEMENT - DISPOSAL BY THE CONTRACTOR 
or paragraph WASTE MANAGEMENT - DISPOSAL BY THE NAVY is applicable for the project's location.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Manage and dispose of all Hazardous Waste generated or discovered during the project.  Dispose of all waste in accordance with all federal and 
state environmental regulations.  Sign and submit all paperwork (lab analyses, profiles, manifests) and records to the Navy.  Allow inspection 
by the Regional Environmental Core for compliance with federal, state and Navy requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Contractor Site Custodian</TTL><BRK/>
<OLG><BRK/>
<OLI>Designate a Site Custodian and an Alternate for waste management.  Provide 24-hour phone numbers where Site Custodian and alternate can 
be contacted in the event of an emergency.</OLI><BRK/>
<BRK/>
<OLI>Personnel must be trained in hazardous waste management procedures to comply with the requirements of <RID>40 CFR 262.34</RID> and <RID>40 CFR 265</RID>.16.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Waste Accumulation</TTL><BRK/>
<OLG><BRK/>
<OLI>Establish a SAA, UWAA or a temporary 90-Day HWAA for waste accumulation. Obtain the HW Media Manager approval.  Do not use accumulation 
areas as lay-down areas.</OLI><BRK/>
<BRK/>
<OLI>EV Core HW MM will notify VDEQ.  Notify the HW MM 14 days prior to the start of waste accumulation.  All agency notifications will originate 
from the Regional Environmental Core.</OLI><BRK/>
<BRK/>
<OLI>The Site Custodian and Alternate must attend the HW MM training session for the management of the SAA, UWAA or HWAA.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Waste Disposal</TTL><BRK/>
<OLG><BRK/>
<OLI>The Navy will be considered the "generator" for all wastes that are generated on Navy property, regardless if the waste was generated as 
result of Contractor activity.</OLI><BRK/>
<BRK/>
<OLI>Pack, mark, label and transport all waste in accordance with Department of Transportation 49 CFR Regulations.</OLI><BRK/>
<BRK/>
<OLI>Obtain the EPA Hazardous Waste Identification Number (EPA ID#) for the installation or off-site Contractor location, from the EV Core HW 
MM.  Use the generator's EPA ID# on the Hazardous Waste Manifest.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Provide the name and EPA ID Number for the Hazardous Waste Transporter and the disposal facility to the HW MM.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Submit all waste profiles and documentation supporting the waste disposal to the HW MM for review.</OLI><BRK/>
<BRK/>
<OLI>Obtain the Hazardous Waste Manifest signature from designated representative of the Regional Environmental Services Group (EV Services).  
Contact the Environmental Services Department Dispatcher to schedule this service.  Obtain signature on the day the waste is scheduled 
to be picked up.</OLI><BRK/>
<BRK/>
<OLI>The Contractor is to ensure that the Certificates of Disposal and Manifests are mailed to EV Services, in accordance with the all Federal 
and State regulations.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT>][<SPT><TTL>Waste Management - Disposal by the Navy</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate with the installation EV to determine whether paragraph WASTE MANAGEMENT - DISPOSAL BY THE CONTRACTOR 
or paragraph WASTE MANAGEMENT - DISPOSAL BY THE NAVY is applicable for the project's location.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Coordinate waste management actions with the HW MM responsible for the installation.  Manage all hazardous waste in accordance with federal, state 
and Navy Environmental Regulations.  Sign and submit all paperwork (lab analyses, profiles, manifests) and records to the Navy.  Allow inspection 
by the Regional Environmental Core for compliance with federal, state and Navy requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Contractor Site Custodian</TTL><BRK/>
<BRK/>
<TXT>a.  Designate a Site Custodian and an alternate for waste management.  Provide 24-hour phone numbers where Site Custodian or Site Manager and alternate 
can be contacted in the event of an emergency.</TXT><BRK/>
<BRK/>
<TXT>b.  Personnel must be trained in hazardous waste management procedures to comply with the requirements of <RID>40 CFR 262.34</RID> and <RID>40 CFR 265</RID>.16.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Waste Accumulation</TTL><BRK/>
<OLG><BRK/>
<OLI>Establish a Satellite Accumulation Area (SAA), Universal Waste Accumulation Area (UWAA) or a temporary 90-Day Hazardous Waste Accumulation 
Area (HWAA) for waste accumulation.  Do not use accumulation areas as Contractor lay-down areas.</OLI><BRK/>
<BRK/>
<OLI>EV Core HW MM will notify VDEQ.  Notify the HW MM 14 days prior to the start of waste accumulation.  All agency notifications will originate 
from the Regional Environmental Core.</OLI><BRK/>
<BRK/>
<OLI>The Site Custodian and alternate must attend the HW MM training session for the management of the SAA, UWAA or HWAA.</OLI><BRK/>
<BRK/>
<OLI>Manage waste containers in accordance with all applicable Federal, State, and Navy regulations.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Waste Disposal</TTL><BRK/>
<OLG><BRK/>
<OLI>The Navy will be considered the "generator" (EPA definition) for all wastes that are generated on Navy property, regardless if the waste 
was generated as result of Contractor activity.</OLI><BRK/>
<BRK/>
<OLI>Obtain a Job Order Number from the NAVFAC MIDLANT Financial Management Business Line, Accounts Receivable Department.</OLI><BRK/>
<BRK/>
<OLI>Submit all waste profiles and documentation supporting the waste disposal to the HW MM for review.</OLI><BRK/>
<BRK/>
<OLI>Coordinate with the HW MM for waste pickup by EV Services.  EV Services will pick up the waste and coordinate transport to an off-site 
permitted Treatment Storage or Disposal facility.</OLI><BRK/>
<BRK/>
<OLI>Obtain the Hazardous Waste Manifest signature from designated representative of the Regional EV Services.  Contact the Environmental Services 
Department Dispatcher to schedule this service. Obtain signature on the day the waste is scheduled to be picked up.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT>]<SPT><TTL>Excavation</TTL><BRK/>
<BRK/>
<TXT>If soil is to be reused onsite, sampling is not required unless otherwise directed.  Excavated soil may be reused within the construction site 
with no testing necessary.  Soil may be stockpiled until the end of the project, then reused as much as possible prior to sampling and analysis 
for residual soil to be disposed.  Store in a manner that prevents rain from infiltrating the soil matrix and preventing runoff into the surrounding 
soil or pavement (for example, store the soil on top of plastic sheets and covered with plastic sheets or store in lined, covered dumpsters).  
If the soil is going to be relocated or disposed outside the construction site, sampling and analysis is required. Contact the installation HW 
Program Manager prior to disposal to determine the appropriate sampling and test parameter.  Soil disposal requirements will depend on test results.  
If soil is to be shipped to a destination outside the fire ant quarantine area (outside of James City County, York County, Chesapeake, Hampton, 
Newport News, Norfolk, Poquoson, Portsmouth, Suffolk, Virginia Beach, or Williamsburg) it MUST have a valid inspection certificate issued by an 
Officer of the Plant Protection and Quarantine Program (PPQ) of the U.S. Department of Agriculture.  Contact the EV Pest Management Coordinator 
for additional information.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Painting and Paint Removal</TTL><BRK/>
<BRK/>
<TXT>Air-drying cans for disposal are allowed only if liquid residue is less than<MET> 2.54 cm</MET><ENG> one inch</ENG>; keep all paint or solvent containers closed and 
secured when not adding or removing material or waste.  Waste paint chips and debris must be collected and sampled to determine the proper disposal 
method.  Contact the NAVFAC MIDLANT EV HW Program Manager for sampling requirements.  If waste paint is determined to be hazardous, waste must 
be managed as hazardous and an appropriate accumulation area must be established.  Contact the NAVFAC MIDLANT EV HW Program Manager for site setup.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Dumpsters</TTL><BRK/>
<BRK/>
<TXT>Label trash containers to appropriately describe the contents.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Air Requirements</TTL><BRK/>
<BRK/>
<SPT><TTL>Concrete Crushing</TTL><BRK/>
<BRK/>
<TXT>Secure an air permit for the crusher from the regulatory agency where the equipment is home-based (in Virginia contact VADEQ).  Provide a copy 
of the permit to the EV Office (Air Program Manager) through the Contracting Officer at least 30 days prior to bringing crusher onsite.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Spill Response and Reporting</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Attach Table 1 - Spill Reporting Contact Numbers, which is available for download at <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables</URL></NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Report spills at Hampton Roads Navy installations to the appropriate installation Emergency Call Center (ECC) immediately upon discovery.</TXT><BRK/>
<BRK/>
<TXT>After notifying the installation ECC, notify the Navy point of contact.  Refer to the Installation Hazardous Material Reutilization, Hazardous 
Waste Minimization and Disposal Guide Appendix 3 for spill contact procedures.  Refer to <ATT>Table 1 - Spill Reporting Contact Number</ATT> for the appropriate 
point of contact.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Maryland</TTL><BRK/>
<OLG><BRK/>
<OLI>Patuxent River</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>West Virginia</TTL><BRK/>
<OLG><BRK/>
<OLI>Sugar Grove</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Pennsylvania</TTL><BRK/>
<BRK/></SPT>
<SPT><TTL>New Jersey</TTL><BRK/>
<BRK/></SPT>
<SPT><TTL>North Carolina</TTL><BRK/>
<BRK/>
<SPT><TTL>Camp Lejeune</TTL><BRK/>
<BRK/>
<SPT><TTL>Removal of Waste from Camp Lejeune</TTL><BRK/>
<BRK/>
<TXT>Remove and dispose of rubbish and debris from Government property.  Provide 24-hour advance written notice to the Contracting Office of Contractor's 
intention to dispose rubbish and debris off base.  Disposal at sites or landfills not holding a valid state of North Carolina permit is specifically 
prohibited.  The prohibition also applies to sites where a permit my have been applied for but not yet obtained.  If construction debris has been 
disposed off-base outside the parameter of this paragraph at a site without state permits or not in accordance with regulatory requirements, remove, 
transport, and relocate the debris to a state-approved site at Contractor expense.  Pay any required fines, penalties, or fees related to the illegal 
disposal of construction debris.  Metal will not be accepted at the Base Sanitary Landfill.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Surplus Soils Disposal for Camp Lejeune &amp; MCAS New River</TTL><BRK/>
<BRK/>
<TXT>Transport all surplus soil to one of the designated locations on government property.  No surplus material will leave government property without 
approval of installation Environmental Program Manager and the Contracting Officer.  Deliver and properly manage surplus soil that cannot be reused 
on its originating site to one of the following locations:</TXT><BRK/>
<OLG><BRK/>
<OLI>Area managed by G-3/5 for reuse on training areas for various maintenance activities:</OLI><BRK/>
<BRK/>
<OLI>3.5 acre storage, within TLZ Condor off Verona Loop Road, approximate coordinates 34d 38'07.3"N 77d 26' 41.7"W.</OLI><BRK/>
<BRK/>
<OLI>Coordinate with G-3/5 Project Development Specialist, MCIEAST-MCB CAMLEJ at (910) 451-5772 to determine capacity available at the storage 
location, prior to delivery.</OLI><BRK/>
<BRK/>
<OLI>This site operates Monday through Thursday between 0730 and 1500.</OLI><BRK/>
<BRK/>
<OLI>Area managed by PWD for use as daily cover:</OLI><BRK/>
<BRK/>
<OLI>Base landfill, located on Piney Green Road, approximate coordinates 34d 41' 26.9"N 77d 19' 27.4"W.</OLI><BRK/>
<BRK/>
<OLI>Contractor must provide temporary silt fencing around designated stockpile areas as needed.</OLI><BRK/>
<BRK/>
<OLI>Coordinate with Landfill Manager at (910) 451-8666.  Landfill use letters will be provided so that deliveries can be tracked.</OLI><BRK/>
<BRK/>
<OLI>This site operates Monday through Thursday between 0730 and 1500 and on Friday between 0700 and 1400.</OLI><BRK/>
<BRK/>
<TXT>Contact POCs listed above 7 to 10 days in advance to coordinate delivery of material at the storage locations.</TXT><BRK/>
<BRK/>
<TXT>Prior to transportation to one of the designated locations, screen all surplus soil to remove all objects greater than<MET> 75 mm</MET><ENG> 3 inches</ENG> and deleterious 
material.  Deleterious material consists of organic debris such as roots, stumps, timber, and construction debris.  Construction debris may include, 
but is not limited to wood, plastic, glass, concrete, brick, and metal.  Dispose of deleterious material and objects larger than<MET> 75 mm</MET><ENG> 3 inches</ENG>
 as specified.</TXT><BRK/>
<BRK/>
<TXT>Provide all plant, material, and labor for placement and management of the surplus material at the designated locations.  Grade surplus material 
to a flat condition and slope to provide positive drainage daily.  Submit the following verification documents to the Contracting Officer for review 
and approval:</TXT><BRK/>
<BRK/>
<OLI LEVEL="2">Photographic documentation that surplus soil has been properly placed.  Photograph will include time and date of image.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Certification statement indicating volume, in cubic yards (CY), of material delivered and confirming material is free of contaminants.</OLI><BRK/></OLG>
<BRK/>
<TXT>NOTE: Soil contaminated with debris or chemicals cannot be disposed at the stockpile locations.  If contaminated soils are suspected or confirmed 
through presence of UXO, odors, or visual staining, affected soils must be properly tested, manifested, and disposed of in accordance with RCRA 
regulations.  Contact Base EMD, ER Program Manager, for more information.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>MCAS Cherry Point</TTL><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>New York</TTL><BRK/>
<BRK/></SPT>
<SPT><TTL>Maine</TTL><BRK/>
<BRK/></SPT>
<SPT><TTL>District of Columbia</TTL><BRK/>
<BRK/></SPT>
</SPT></TAI><TAI OPT="NAVFAC NW"><SPT><TTL>Northwest (Washington and Oregon)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph and subparagraphs are tailored for NAVFAC NW use only.</NPR><BRK/>
<BRK/>
<NPR>Forms referenced for attachment are available for download at: <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables</URL></NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the following state, regional, and local requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Contractor Employee Training Records</TTL><BRK/>
<BRK/>
<TXT>Train employees in accordance with <RID>WAC-173-303-330</RID>.  Training must be completed and documented prior to the generation of waste.</TXT><BRK/>
<BRK/>
<SPT><TTL>Waste Originator Training for NBK Bangor</TTL><BRK/>
<BRK/>
<TXT>NBK Environmental Division <SUB>Waste Originator Training Certification</SUB> is obtained either by in person training offered every third Thursday of the 
month or by completing the electronic "Waste Originator Training: NB Kitsap" training module available via ECATTS (https://environmentaltraining.ecatts.com/) 
and passing the test at the end of the training module.  For in person, please contact the NBK Environmental Office at (360) 315-1021.  Training 
must be completed and documented prior to the generation of waste.  Refresher training must be completed annually.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Waste Originator Training for NBK Keyport</TTL><BRK/>
<BRK/>
<TXT>NBK Keyport <SUB>Waste Originator Training Certification</SUB> is obtained by taking the electronic "Hazardous Waste Site Manager/Alternate (Waste Generator)" 
training module (contact the Contracting Officer for an electronic copy) and passing the test at the end of the training module.  Training must 
be completed and documented prior to the generation of waste.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Waste Originator Training for NBK Bremerton</TTL><BRK/>
<BRK/>
<TXT>Employees must be familiar (read and understand) the approved Environmental Protection Plan and the "Contractor's Guide to Environmental Compliance."  
Complete the ECATTS course titled "Site Specific Hazardous Waste Management Training for the Bremerton Naval Complex" in order to satisfy the Contractor 
Employee Training Records submittal requirement.  Taken annually, this course will satisfy the refresher-training requirement of <RID>WAC-173-303</RID> for 
work at NBK Bremerton and is not required on a per project basis.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Waste Originator Training for NBK Everett</TTL><BRK/>
<BRK/>
<TXT>Contractor personnel generating hazardous waste must obtain Site-Specific Hazardous Waste Training.  Allow one hour for training.  Coordinate with 
the NAVFAC NW PWC Environmental Division, 425-304-3470.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Refrigerant Work Checklist</TTL><BRK/>
<BRK/>
<TXT>Submit a completed <ATT><SUB>Refrigerant Work Checklist</SUB></ATT> form to document that work was performed in compliance with <RID>40 CFR 82</RID> requirements.  Complete one 
form for each piece of equipment containing refrigerant that must be installed, removed, or serviced as part of this Contract.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Environmental Protection Plan (EPP)</TTL><BRK/>
<BRK/>
<TXT>The following clarifications and requirements supplement paragraph ENVIRONMENTAL PROTECTION PLAN.</TXT><BRK/>
<BRK/>
<SPT><TTL>Solid Waste Management</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For NBK Bangor, choose the second bracketed sentence and delete the first.  For other locations, choose 
the first bracketed sentence and delete the second.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[Include the Solid Waste Management Plan as part of the EPP.  Identify each solid-waste disposal facility, including:  the type of facility, name, 
physical address, phone numbers, issuing authority and approval signature, permitted entity and period of issuance for waste.  Submit a copy of 
the county hauling permit (for nonexempt franchised haulers).] [Include the Solid Waste Management Plan as part of the EPP.  Specify name and address 
of permitted refuse disposal facilities (clearly state how asbestos waste will be handled).  Specify procedures for providing the Contracting Officer 
with dump tickets that include waste quantities and dates of disposal.  Specify procedures for providing refuse waste quantities, dates and certifications 
of disposal on the <SUB>Refuse and Recycle Quantity Form</SUB>.]</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose PSNS&amp;IMFINST 5090.30 and 5090.5 for projects at NBK Bremerton, choose BKCHD 2010-1 for projects 
in Kitsap County, or choose JCC Chapter 8.10 projects at Indian Island.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Perform waste management practices in accordance with[ PSNS&amp;IMFINST 5090.30, Water Pollution Prevention and Control Plan; PSNS&amp;IMFINST 
5090.5, Waste Management Plan][ Bremerton-Kitsap County Health District Ordinance 2010-1, Solid Waste Regulations;][ Jefferson County Code, Chapter 
8.10, Solid Waste Regulations;] <RID>WAC-173-303</RID>, <RID>WAC-173-350</RID>, <RID>40 CFR 262</RID>, <RID>40 CFR 263</RID>, <RID>40 CFR 264</RID>, <RID>49 CFR 172</RID>, and <RID>49 CFR 178</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Control and Management of Hazardous Waste</TTL><BRK/>
<BRK/>
[<SPT><TTL>Dangerous Waste Turn-in</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Select "turn-in" for NBK Bangor, NBK Keyport, Indian Island, and most projects at NBK Bremerton.</NPR><BRK/>
<BRK/>
<NPR>Delete paragraphs for Installations other than where the work is to be performed.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Specify procedures to handle, process and dispose of dangerous waste.  Project-generated dangerous waste must be turned into the Government for 
disposal.  Collect dangerous waste in Department of Transportation (DOT)-approved containers in accordance with <RID>49 CFR 171</RID>, <RID>49 CFR 172</RID>, and <RID>49 CFR 178</RID>
 properly labeled to identify the type of waste, hazard to personnel, and the start date.  Containers and labels will be supplied by the Government.</TXT><BRK/>
<BRK/>
<TXT>Notify the Contracting Officer 14 calendar days in advance for request of bulk containers.  Request is accomplished by submission of a Waste Information 
Specification including an estimated quantity of dangerous waste and the number of containers.  Identify dangerous waste generated within the confines 
of the station by the use of the station's EPA generator identification (ID) number.  Accumulate in an approved satellite or 90-day accumulation 
area that meets the requirements set forth in <RID>WAC-173-303</RID>.  Contact the Contracting Officer no more than 45 calendar days from the start date for 
90-day accumulation areas to arrange for transport.  Accumulate bulk dangerous waste in a 90-day area.  Turn in non-bulk dangerous waste from a 
90-day area within 45 days of the start date.  Turn in dangerous waste from satellite accumulation areas to the Government prior to exceeding time 
and quantity limits.  Onsite treatment of waste is prohibited.</TXT><BRK/>
<BRK/>
<SPT><TTL>Naval Base Kitsap (NBK) Bangor</TTL><BRK/>
<BRK/>
<TXT>Complete Waste Information Specification in accordance with paragraph WASTE DETERMINATION DOCUMENTATION, for each waste stream.  Contractor personnel 
submitting Waste Information Specification forms must have already received Bangor Waste Originator Training and Certification.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Naval Base Kitsap (NBK) Keyport</TTL><BRK/>
<BRK/>
<TXT>NBK Keyport will not provide a copy of the Hazardous Waste Management Plan.  Information required for the control and disposal of Hazardous Waste 
at NBK Keyport is included in the "Hazardous Waste Site Manager/Alternate (Waste Generator)" training module and the NAVSEA Keyport Contractor's 
Guide to Environmental Compliance.</TXT><BRK/>
<BRK/>
<TXT>Explain how waste designated by the Government will be disposed of in accordance with Waste Generation Record (WGR) instructions.  Complete WGR 
in accordance with paragraph WASTE DETERMINATION DOCUMENTATION, for each waste stream.  Contractor personnel submitting WGR forms must have already 
received Keyport Waste Originator Training and Certification.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Indian Island</TTL><BRK/>
<BRK/>
<TXT>Complete Waste Generation Record in accordance with paragraph WASTE DETERMINATION DOCUMENTATION for each waste stream.  Contractor personnel submitting 
WGR forms must have already received Bangor Waste Originator Training and Certification.</TXT><BRK/>
<BRK/></SPT>
</SPT>][<SPT><TTL>Dangerous Waste Disposal</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Select "disposal" for projects at Whidbey Island, Everett, and Reserve Centers.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Specify procedures to handle, process, and dispose of dangerous waste.  For disposal at a TSDF, provide the following if the TSDF is not on the 
approved list of the Defense Reutilization and Marketing Service (DRMS) <URL HREF="https://www.dla.mil/DispositionServices/Offers/Disposal/HazardousWaste/QualifiedFacilitiesList">https://www.dla.mil/DispositionServices/Offers/Disposal/HazardousWaste/<BRK/>
QualifiedFacilitiesList/</URL>:  facility name, physical address, telephone number, description of the facility, EPA waste numbers that the facility 
accepts, and date of most recent Resource Conservation and Recovery Act(RCRA) inspection.  If the TDSF is on the DRMS list, then provide the name 
and physical address.</TXT><BRK/>
<BRK/>
<TXT>For transporters to be used to transport dangerous waste, furnish the following:  name, address, EPA ID number, and phone numbers of the transport 
firm and the principal Contractor.  Onsite treatment of waste is prohibited.</TXT><BRK/>
<BRK/></SPT>
]</SPT><SPT><TTL>Stormwater Management and Control</TTL><BRK/>
<BRK/>
<TXT>Submit a construction SWPPP with the EPP in accordance with requirements in paragraph STORMWATER POLLUTION PREVENTION PLAN or paragraph MUNICIPAL 
SEPARATE STORM SEWER SYSTEM (MS4) PERMIT MANAGEMENT, as applicable.</TXT><BRK/></SPT>
[<SPT><TTL>Clean Air Act Compliance for [NBK Bangor][NBK Keyport][NBK Bremerton][Everett]</TTL><BRK/>
<BRK/>
<TXT>Identify any air pollution generating equipment or processes that may require a Notice of Construction pursuant to[ PSCAA] Regulation.</TXT><BRK/>
<BRK/>
<TXT>Identify portable and stationary internal combustion engines (ICEs) that will must be supplied, used, or serviced.  Address compliance with <RID>40 CFR 60</RID>
 Subpart IIII, <RID>40 CFR 63</RID> Subpart ZZZZ, and[ PSCAA] Regulations as applicable.  Include <SUB>PSCAA Nonroad Engine Notification Form</SUB>.</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Clean Air Act Compliance for Whidbey Island and Indian Island</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use ORCAA for Indian Island.  Use NWCAA for Whidbey Island.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Identify any air pollution generating equipment or processes that may require a Notice of Construction pursuant to [<RID>ORCAA Regulations</RID>][<RID>NWCAA Regulation</RID>
].</TXT><BRK/>
<BRK/>
<TXT>Identify portable and stationary internal combustion engines (ICEs) that must be supplied, used, or serviced.  Address compliance with <RID>40 CFR 60</RID>
 Subpart IIII, <RID>40 CFR 63</RID> Subpart ZZZZ, and [<RID>ORCAA Regulations</RID>][<RID>NWCAA Regulation</RID>] as applicable.</TXT><BRK/>
<BRK/>
<TXT>As a minimum, include the following:</TXT><BRK/>
<OLG><BRK/>
<OLI>Identify engine certification status.</OLI><BRK/>
<BRK/>
<OLI>Identify non-resettable hour meter status.</OLI><BRK/>
<BRK/>
<OLI>For portable (skid- or trailer-mounted) ICEs, identify the make, model, manufacture date, size, and brake horsepower.</OLI><BRK/>
<BRK/>
<OLI>Identify methods of recording run time and reason for operation.</OLI><BRK/>
<BRK/>
<OLI>Do NOT include motor vehicles.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL><SUB>Notice of Construction</SUB> (NOC) and <SUB>Notice of Completion</SUB> Licenses and Permits</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Identify all local permit requirements, as found in the Permits Record of Decision (PROD).</NPR><BRK/>
<BRK/>
<NPR>Identify, and include copies of, all project permits obtained by the Government (prior to award).</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include if NOC is required.  Delete this subparagraph if NOC is not required.  Permit requirements are 
found in the Permits Record of Decision (PROD).  NOC permits may require up to 120 days to receive approval from 
outside regulatory agencies.  Examples of taskings that may require an NOC include, but are not limited to, the following:<BRK/>
- Installation of certain Boilers or other stationary combustion sources such as electrical generators<BRK/>
- Certain portable combustion sources (not including motor vehicles)<BRK/>
- Blasting or paint spray booths<BRK/>
- Fuel storage tanks, dispensers, and loading racks<BRK/>
- Modification of existing equipment that has a NOC<BRK/>
- Industrial ventilation and dust control systems to control dust and fumes from activities such as grinding, 
sanding, or solvent cleaning.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects in the NAVFAC PAC Area of Operation, edit this paragraph by removing "approval" and selecting 
"review" to this paragraph.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Allow up to 120 days to receive approval from outside regulatory agencies for NOC permits.  Prepare and forward the permit application package 
to the Contracting Officer for [approval] [review] and submittal to the applicable regulatory agency.  Pay for associated fees.  Permit approval 
must be obtained prior to the start of work covered by the permit.  Upon completion of work, notify the Contracting Officer, who will submit the 
Notification of Completion to the applicable regulatory agency.</TXT><BRK/>
<BRK/>
<TXT>Equipment and work provided as part of this Contract must comply with the terms and conditions of the permit, and other applicable federal, state, 
and local air pollution-control regulations.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT></TAI><TAI OPT="NAVFAC SE"><SPT><TTL>Southeast</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph and subparagraphs are tailored for NAVFAC SE use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Applicable environmental requirements such as; erosion/sediment control, storm water, hazardous waste, 
and solid waste may have unique state regulations.  Edit this section to include these unique state requirements 
for each state listed below.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For each project, provide the following:<BRK/>
1. Unique local requirements.<BRK/>
2. Environmental Point of Contact information for design review and location specific requirements. <BRK/>
3. For every installation in area of responsibility, the FEC must identify the facility Hazardous Waste Generator 
status as specified in paragraph FACILITY HAZARDOUS WASTE GENERATOR STATUS.<BRK/>
4. For each installation listed below, provide specific requirements of the installation's Environmental Management 
System (EMS) that relate to construction operations.  Identify those site specific EMS actions that the Contractor 
must perform under this contract.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the following state, regional, and local requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Florida</TTL><BRK/>
<BRK/>
[<TXT><SUB>Dewatering Permit</SUB></TXT><BRK/>
<BRK/>
][<TXT><SUB>Florida Environmental Resource Permit</SUB></TXT><BRK/>
<BRK/>
]<SPT><TTL>Naval Air Station (NAS) Jacksonville</TTL><BRK/>
<BRK/>
<SPT><TTL>Definition: Petroleum-Contaminated Waste</TTL><BRK/>
<BRK/>
<TXT>Surface water, groundwater, soil, or sediment that has the presence of petroleum or petroleum products or their chemical constituents (except hazardous 
waste as defined in the paragraph HAZARDOUS WASTE in quantities that exceed the applicable cleanup target levels as stated in FL 62-780.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Environmental Protection Requirements</TTL><BRK/>
<BRK/>
<TXT>NAS Jacksonville is governed by the Federal Facilities Agreement (FFA) signed by the Government, the EPA, and the Florida Department of Environmental 
Protection.  The FFA is incorporated by reference into this Contract and subcontracts.  Specific restoration sites have been identified in the 
FFA, and other Contractors or Government personnel may undertake sampling, investigative work, or remediation actions related to other projects 
simultaneously with the efforts related to this project.  Information concerning this agreement or specific site information may be obtained from 
the Facilities Department at NAS Jacksonville.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Employee Training Records</TTL><BRK/>
<BRK/>
<TXT>Maintain a copy of the training certificate at the job site showing that the required module(s) were completed in accordance with requirements 
in paragraph TRAINING IN ENVIRONMENTAL COMPLIANCE ASSESSMENT TRAINING AND TRACKING SYSTEM (ECATTS).  Complete this training prior to starting work 
on this project, but not later than 30 days after award of the Contract.  Contractor employees must carry a wallet-size card demonstrating that 
the required module(s) have been completed.  The card must be presented to the Contracting Officer or the Contracting Officer's Representative 
upon request.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Control and Management of Hazardous Waste</TTL><BRK/>
<BRK/>
<TXT>Dispose of hazardous waste generated during construction through PWC Jacksonville; do not take hazardous waste off station.  Pay disposal costs 
in accordance with PWC Jacksonville's published rates.  Air-drying any containers to render them empty is prohibited.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Battery Disposal</TTL><BRK/>
<BRK/>
<TXT>Comply with hazardous waste requirements when disposing of waste lead-acid batteries and electrolyte.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Mercury Containing Devices Management and Disposal</TTL><BRK/>
<BRK/>
<TXT>Manage mercury-containing devices in compliance with hazardous waste or universal waste management and disposal, as applicable.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Naval Air Station (NAS) Pensacola</TTL><BRK/>
<BRK/>
<SPT><TTL><SUB>Excavation Permits</SUB></TTL><BRK/>
<BRK/>
<TXT>Before any excavation is started, obtain an approved NAS Pensacola Permit through the Contracting Officer (excavation is defined as digging or 
opening of an existing surface to a depth exceeding<MET> 20 cm</MET><ENG> 8 inches</ENG> below the existing grade, as well as driving of piles or auger borings).  The 
permit form is self-explanatory.  Fill in the applicable items on the permit and give it to the Contracting Officer in sufficient time for Station 
personnel to process the permit, but not less than 5 working days prior to the planned excavation.</TXT><BRK/>
<BRK/>
<TXT>Ensure each employee and subcontractor employee performing construction or service work on this project completes a course entitled "NAS Pensacola 
Environmental Compliance Training" using the website developed by the Government and Florida Department of Environmental Protection <URL HREF="http://www.navfac.navy.mil">http://www.navfac.navy.mil</URL>
. Log on: contract (lower case), Password: navfac (lower case).</TXT><BRK/>
<BRK/>
<TXT>After gaining entry to the website, establish a unique password.  Each Contractor and subcontractor employee doing (or managing) construction or 
service work on this project must complete the course and have a certificate on file at the job site.  Employees (except those involved in any 
painting, caulking, asbestos work, or well pointing) will complete training within 30 days of mobilization on this project.  Employees performing 
painting, caulking, asbestos work, or well pointing must complete training before starting work on this project.  Within 30 days of mobilization, 
submit a letter to the Contracting Officer certifying that employees have obtained training and provide copies of certificates.  The letter must 
certify that future employees will obtain training in accordance with this specification requirement.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT><SPT><TTL>Georgia</TTL><BRK/>
<OLG><BRK/>
<OLI>Naval Submarine Base (NSB) Kings Bay</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Mississippi</TTL><BRK/>
<BRK/>
<SPT><TTL>Naval Construction Battalion Command (NCBC) Gulfport</TTL><BRK/>
<BRK/>
<SPT><TTL><SUB>Excavation Permits</SUB></TTL><BRK/>
<BRK/>
<TXT>Before any excavation is started, obtain an approved NCBC Gulfport permit through the Public Works Management Engineering Division via the Contracting 
Officer (excavation is defined as digging or opening of an existing surface to a depth exceeding<MET> 20 cm</MET><ENG> 8 inches</ENG> below the existing grade, as well 
as driving of piles or auger borings).  The permit form is self-explanatory.  Fill in the applicable items on the permit and give it to the Contracting 
Officer in sufficient time for Station personnel to process the permit, but not less than 5 working days prior to planned excavation</TXT>.<BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Naval Air Station (NAS) Meridian</TTL><BRK/>
<BRK/>
<SPT><TTL>Contractor Hazardous Material Inventory Log</TTL><BRK/>
<BRK/>
<TXT>Submit a "Contractor Hazardous Material Inventory Log" to the Contracting Officer on the 10th day of each month.  Copies of the Station-specific 
forms can be obtained from the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT><SPT><TTL>South Carolina</TTL><BRK/>
<OLG><BRK/>
<OLI>Naval Weapons Station (NWS) Charleston</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Texas</TTL><BRK/>
<OLG><BRK/>
<OLI>Naval Air Station (NAS) Corpus Christi</OLI><BRK/>
<BRK/>
<OLI>Naval Air Station (NAS) Dallas</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Cuba</TTL><BRK/>
<BRK/>
<SPT><TTL>Naval Station, Guantanamo Bay (GTMO)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This guide specification is for use in construction projects at U.S. Naval Station Guantanamo Bay, Cuba 
where environmental protection and other environmental temporary controls are required.  All paragraph have been 
revised in accordance with U.S. Naval Station Guantanamo Bay, Cuba rules and regulations.</NPR><BRK/>
<BRK/>
<NPR>Remove information and requirements not required in respective project, whether or not brackets are present.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Contractor Liabilities for Environmental Protection</TTL><BRK/>
<BRK/>
<TXT>Obtain copies of the following GTMO instructions prior to the start of work:  <RID>4400.2A</RID>, <RID>5090.1</RID>, <RID>5090.4</RID>, <RID>5090.7</RID>, <RID>5090.8</RID>, <RID>5100.13</RID> and <RID>1710.10</RID>.  The 
station is subject to Commander Fleet Forces Command or Naval Facilities Engineering Systems Command - Southeast inspections to review compliance 
with environmental protection laws.  A Multi-media inspection by CFFC or NAVFAC SE may include questioning of Contractor personnel who are working 
with or have contact with Hazardous Materials and waste.</TXT><BRK/>
<BRK/>
<TXT>Complete and provide documentation for environmental training required by the <RID>FGS</RID>/OEGBD and station instructions.  Ensure employees, even during 
employee off-duty hours, are aware and comply with Station regulations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Licenses and Permits</TTL><BRK/>
<BRK/>
<TXT>A landfill pass is required for asbestos-containing materials and is available at the Hazardous Waste Storage Area (Bldg. 850) after a load inspection 
is performed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Environmental Protection Plan (EPP)</TTL><BRK/>
<BRK/>
<TXT>Meet with the Contracting Officer to discuss the proposed EPP 10 days after the award of Contract.  Submit the EPP for further discussion, review, 
and approval 14 days after the meeting.  The EPP should include the following, in addition to what is listed in paragraph ENVIRONMENTAL PROTECTION 
PLAN:</TXT><BRK/>
<OLG><BRK/>
<OLI>A listing of any hazardous materials planned for use on the station, in accordance with <RID>4400.2A</RID>.  The total amount of hazardous material 
stored onsite is to be less than<MET>416 liters</MET><ENG> 110 gallons</ENG> unless preapproved by the Government.  This information is included in the Station's 
Hazardous Material Tracking Program.  To assist this effort, submit a list (including quantities) of hazardous materials to be brought 
to the safety station and copies of the corresponding Safety Data Sheets (SDSs).  Submit this list to the Contracting Officer.  Develop 
an Authorized User List (AUL) request form for each hazardous material item and update this list as additional materials are required.  
Barcode hazardous material items as specified in the MOU and Station Instruction.  Include a plan addressing excess hazardous materials 
will be managed at the conclusion of each task order or at the end of the project.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Storage of POLs in containers<MET> 208</MET><ENG> 55 gallons</ENG> or greater on the jobsite is prohibited, as well as bulk fuel storage on base.</OLI><BRK/>
<BRK/>
<OLI>In accordance with Station regulations, substitute materials as necessary to reduce the generation of hazardous material and include a 
statement to that effect in the EPP.</OLI><BRK/>
<BRK/>
<OLI>For major activities covering large acreage or steep slopes, submit a separate Land-Disturbing Activity Plan, as required, addressing erosion 
and sedimentation control in major land- clearing and grading operations.</OLI><BRK/>
<BRK/>
<OLI>Provide a point-of-contact to address Cuban rock iguanas, Cuban boas, and other protected species that may be onsite during each phases 
of work associated with this Contract.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></SPT></SPT></TAI><TAI OPT="NAVFAC SW"><SPT><TTL>Southwest</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph and subparagraphs are tailored for NAVFAC SW use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Applicable environmental requirements such as; erosion/sediment control, storm water, hazardous waste, 
and solid waste may have unique state regulations.  Edit this section to include these unique state requirements 
for each state listed below.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For each project, provide the following:<BRK/>
1. Unique local requirements and state regulations.<BRK/>
2. Environmental Point of Contact information for design review and base specific requirements.<BRK/>
3. For every installation in area of responsibility, the FEC must identify the facility Hazardous Waste Generator 
status as specified in paragraph FACILITY HAZARDOUS WASTE GENERATOR STATUS.<BRK/>
4. For each installation listed below, provide specific requirements of the installation's Environmental Management 
System (EMS) that relate to construction operations.  Identify those site specific EMS actions that the Contractor 
must perform under this contract.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the following state, regional, and local requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Arizona</TTL><BRK/>
<BRK/>
<SPT><TTL>Regulatory Requirements for the Notice of Intent (NOI)</TTL><BRK/>
<BRK/>
<TXT>Submit a vicinity map and a NOI to the Arizona Department of Environmental Quality (ADEQ).  ADEQ does not require a filing fee).  If the construction 
project is scheduled to exceed one year, submit NAVFAC SW Legal Fee Letter to ADEQ - attach it to the NOI.  Resident Officer in Charge of Construction 
(ROICC) or Facilities Engineering and Acquisition Division (FEAD) Contracting Officer reviews and signs NOI and NOT.  If discharges to a unique 
or impaired water body are proposed, submit the SWPPP along with the NOI.  See the General Permit for instructions.  Submit NOT to ADEQ within 
30 days after permit conditions have been met.</TXT><BRK/>
<BRK/>
<TXT>Arizona Pollutant Discharge Elimination System General Permit for Dischargers from Construction Activities to Water of the United States 2008, 
Permit No. AZG2013-001 expires June 3, 2025.</TXT><BRK/>
<BRK/>
<TXT><URL HREF="https://static.azdeq.gov/permits/azpdes/cgp_permit.pdf">https://static.azdeq.gov/permits/azpdes/cgp_permit.pdf</URL></TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>California</TTL><BRK/>
<BRK/>
<SPT><TTL>Regulatory Requirements for the Notice of Intent</TTL><BRK/>
<BRK/>
<TXT>Submit a site map of the vicinity, NOI, and applicable filing fee (not to exceed $700.00) to the State Water Resources Control Board (SERCB).  
If the construction project is scheduled to exceed one year, submit NAVFAC SW Legal Fee Letter to SWRCB as an attachment the NOI.  State of California 
requires the NOI to be submitted 30 days prior to start of construction.  The ROICC or FEAD Contracting Officer reviews and signs NOI.</TXT><BRK/>
<BRK/>
<TXT>Complete and submit the NOT to the local Regional Water Quality Control Board (RWQCB).</TXT><BRK/>
<BRK/>
<TXT><URL HREF="https://www.waterboards.ca.gov/water_issues/programs/stormwater/construction.html">https://www.waterboards.ca.gov/water_issues/programs/stormwater/construction.html</URL></TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Stormwater Notice of Termination</TTL><BRK/>
<BRK/>
<TXT>Submittal of the NOT constitutes notice that the Government (and their Contractor) of the site identified on this form is no longer authorized 
to discharge storm water associated with construction activity by NPDES General Permit No. CAS000002.  Submit the NOT to the appropriate Executive 
Officer of the RWQCB responsible for the area in which the facility is located.  The ROICC or FEAD Contracting Officer reviews and signs the NOT.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Sampling and Analysis of Hazardous Waste</TTL><BRK/>
<BRK/>
<TXT>The analysis must be performed by a California certified laboratory.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Nevada</TTL><BRK/>
<BRK/>
<SPT><TTL>Regulatory Requirements for the Notice of Intent</TTL><BRK/>
<BRK/>
<TXT>Submit a vicinity map and NOI to the Nevada Division of Environmental Protection (NDEP).  If the construction project is scheduled to exceed one 
year, submit NAVFAC SW Legal Fee Letter to NDEP - attach it to the NOI.  ROICC or FEAD Contracting Officer reviews and signs the NOI.</TXT><BRK/>
<BRK/>
<TXT>Prepare and submit a complete NOT to the NDEP within 30 days after permit conditions have been met.</TXT><BRK/>
<BRK/>
<TXT>2002 Stormwater Nevada General Permit No. NRV10000-General Permit.</TXT><BRK/>
<BRK/>
<TXT><URL HREF="https://ndep.nv.gov/water/water-pollution-control/permitting/stormwater-discharge-permits">https://ndep.nv.gov/water/water-pollution-control/permitting/stormwater-discharge-<BRK/>
permits</URL></TXT><BRK/>
<BRK/>
<TXT>NDEP Best Management Practices Handbook: <URL HREF="https://ndep.nv.gov/uploads/water-nonpoint-docs/NVBMPHandbook1994.pdf">https://ndep.nv.gov/uploads/water-nonpoint-docs/NVBMPHandbook1994.pdf</URL></TXT><BRK/>
<BRK/></SPT>
</SPT></SPT></TAI><TAI OPT="NAVFAC PAC"><SPT><TTL>Pacific</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph and subparagraphs are tailored for NAVFAC PAC use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Applicable environmental requirements such as; erosion/sediment control, storm water, hazardous waste, 
and solid waste may have unique state regulations.  Edit this section to include these unique state requirements 
for each state listed below.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For each project provide the following:<BRK/>
1. Unique local requirements and state regulations.<BRK/>
2. Environmental Point of Contact information for design review and base specific requirements.<BRK/>
3. For every installation in area of responsibility, the FEC must identify the facility Hazardous Waste Generator 
status as specified in paragraph FACILITY HAZARDOUS WASTE GENERATOR STATUS.<BRK/>
4. For each installation listed below, provide specific requirements of the installation's Environmental Management 
System (EMS) that relate to construction operations.  Identify those site specific EMS actions that the Contractor 
must perform under this contract.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the following state, regional and local requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Control and Disposal of [Ionization Smoke Detectors][Tritium Exit Signs]</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For NAVFAC PAC projects requiring control and disposal of ionization smoke detectors (which contain low-level 
radioactive material) and tritium exit signs by Radiological Affairs Support Office (RASO).</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Material Bagging</TTL><BRK/>
<BRK/>
<TXT>Remove existing [ionization smoke detectors][ and tritium exit signs,] and place like types, together (that is same manufacturer and model number) 
in a plastic bag.  Label the bag with the following data:</TXT><BRK/>
<BRK/>
<ITM>Manufacturer:                  Activity:</ITM><BRK/>
<ITM>MODEL No.:                     Contract No.:</ITM><BRK/>
<ITM>Isotope and Quantity (if known):</ITM><BRK/>
<BRK/></SPT>
<SPT><TTL>Material Storage</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Insert applicable activity in the blank space.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Store plastic bags in<MET> 208 liter</MET><ENG> 55 gallon</ENG> covered drum(s).  Do not seal the drum(s).  Provide a label with a description of the contents and note 
on the label "TO BE DISPOSED OF BY RASO".  Apply the label to the exterior surface of the cover and site of the drum(s).  Provide a record copy 
of the label for each drum <SUB>storage material inventory</SUB> to the Contracting Officer[, the RASO at COMNAVREG Pearl Harbor,] and [_____].</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Storage Site and Disposal</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For NAVFAC PAC projects where government is responsible for storage and disposal.  Insert location of storage 
site in the blank space.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Deliver drums to [_____] [MCBH Bunker 709, Sumner Road] [PWC Pearl Harbor Bldg. [_____]] for storage and disposal of [ionization smoke detectors][ 
and ][tritium exit signs][ as directed by the Contracting Officer].</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Storage and Disposal by Contractor</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For NAVFAC PAC projects where the Contractor is responsible for storage and disposal.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Store of[ ionization smoke detectors][ and tritium exit signs] in accordance with federal, state, and local laws and regulations.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Hawaii</TTL><BRK/>
<BRK/></SPT>
<SPT><TTL>Guam</TTL><BRK/>
<BRK/></SPT>
<SPT><TTL>Japan</TTL><BRK/>
<BRK/></SPT>
</SPT></TAI><TAI OPT="NAVFAC EURAFCENT"><SPT><TTL>Europe</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph and subparagraphs are tailored for NAVFAC EURAFCENT use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Applicable environmental requirements such as; erosion/sediment control, storm water, hazardous waste, 
and solid waste may have unique local regulations.  Edit this section to include these unique state requirements 
for each location listed below.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For each project, provide the following:<BRK/>
1. Unique local requirements and state regulations.<BRK/>
2. Environmental Point of Contact information for design review and base specific requirements. <BRK/>
3. For every installation in area of responsibility, the FEC must identify the facility Hazardous Waste Generator 
status as specified in paragraph FACILITY HAZARDOUS WASTE GENERATOR STATUS.<BRK/>
4. For each installation listed below, provide specific requirements of the installation's Environmental Management 
System (EMS) that relate to construction operations.  Identify those site specific EMS actions that the Contractor 
must perform under this contract.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the following regional and local requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Italy</TTL><BRK/>
<OLG><BRK/>
<OLI>Naval Air Station (NAS) Naples</OLI><BRK/>
<BRK/>
<OLI>Naval Air Station (NAS) Sigonella</OLI><BRK/>
<BRK/>
<OLI>Aviano (NAVFAC EURAFCENT)</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Spain</TTL><BRK/>
<OLG><BRK/>
<OLI>Naval Station (NS) Rota</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Greece</TTL><BRK/>
<OLG><BRK/>
<OLI>Naval Support Activity (NSA) Souda Bay</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>Material Storage</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for ARMY projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Store plastic bags in<MET> 208 liter</MET><ENG> 55 gallon</ENG> covered drum(s).  Do not seal the drum(s).  Provide a label with a description of the contents and note 
on the label "TO BE DISPOSED OF BY RASO".  Apply the label to the exterior surface of the cover and site of the drum(s).  Provide a record copy 
of the label for each drum <SUB>storage material inventory</SUB> to the Contracting Officer and [_____].</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>QUALITY ASSURANCE</TTL><BRK/>
<BRK/>
<SPT><TTL>Preconstruction Survey and Protection of Features</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph as applicable.  For example, it may not be necessary for an interior renovation project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>This paragraph supplements the Contract Clause PROTECTION OF EXISTING VEGETATION, STRUCTURES, EQUIPMENT, UTILITIES, AND IMPROVEMENTS.  Prior to 
start of any onsite construction activities, perform a <SUB>Preconstruction Survey</SUB> of the project site with the Contracting Officer, and take photographs 
showing existing environmental conditions in and adjacent to the site.  Submit a report for the record.  Include in the report a plan describing 
the features requiring protection under the provisions of the Contract Clauses, which are not specifically identified on the drawings as environmental 
features requiring protection along with the condition of trees, shrubs and grassed areas immediately adjacent to the site of work and adjacent 
to the Contractor's assigned storage area and access route(s), as applicable.  The Contractor and the Contracting Officer will sign this survey 
report upon mutual agreement regarding its accuracy and completeness.  Protect those environmental features included in the survey report and any 
indicated on the drawings, regardless of interference that their preservation may cause to the work under the Contract.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>Regulatory Notifications</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate with the Installation Environmental Office as applicable to fill in the number of days that 
notification is required prior to work starting.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide regulatory notification requirements in accordance with federal, state and local regulations.  In cases where the Government will also 
provide public notification (such as stormwater permitting), coordinate with the Contracting Officer.  Submit copies of regulatory notifications 
to the Contracting Officer at least [_____] days prior to commencement of work activities.  Typically, regulatory notifications must be provided 
for the following (this listing is not all-inclusive): demolition, renovation, NPDES defined site work, construction, removal or use of a permitted 
air emissions source, and remediation of controlled substances (asbestos, hazardous waste, lead paint).</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Environmental Brief</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate incorporation of this requirement with the Installation Environmental Office as applicable.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Attend an environmental brief to be included in the preconstruction meeting.  Provide the following information: types, quantities, and use of 
hazardous materials that will be brought onto the installation; and types and quantities of wastes/wastewater that may be generated during the 
Contract. Discuss the results of the Preconstruction Survey at this time.</TXT><BRK/>
<BRK/>
<TXT>Prior to initiating any work on site, meet with the Contracting Officer and installation Environmental Office to discuss the proposed Environmental 
Protection Plan (EPP) or equipment local requirement.  Develop a mutual understanding relative to the details of environmental protection, including 
measures for protecting natural and cultural resources, required reports, required permits, permit requirements (such as mitigation measures), 
and other measures to be taken.</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Environmental Manager</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate incorporation of this requirement with the Installation Environmental Office as applicable.  
Consider project environmental risks versus project size or dollar value.  A small project, such as demolishing 
a plating shop could be low cost, but high risk and a large project, such as replacing a roof on a hangar, could 
be high cost, but low risk.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Appoint in writing an Environmental Manager for the project site.  The Environmental Manager is directly responsible for coordinating contractor 
compliance with federal, state, local, and installation requirements.  The Environmental Manager must ensure compliance with Hazardous Waste Program 
requirements (including hazardous waste handling, storage, manifesting, and disposal); implement the EPP; ensure environmental permits are obtained, 
maintained, and closed out; ensure compliance with Stormwater Program requirements; ensure compliance with Hazardous Materials (storage, handling, 
and reporting) requirements; and coordinate any remediation of regulated substances (lead, asbestos, PCB transformers).  This can be a collateral 
position; however, the person in this position must be trained to adequately accomplish the following duties: ensure waste segregation and storage 
compatibility requirements are met; inspect and manage Satellite Accumulation areas; ensure only authorized personnel add wastes to containers; 
ensure Contractor personnel are trained in 40 CFR requirements in accordance with their position requirements; coordinate removal of waste containers; 
and maintain the Environmental Records binder and required documentation, including environmental permits compliance and close-out.  Submit <SUB>Environmental 
Manager Qualifications</SUB> to the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Employee Training Records</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Insert the bracketed text for projects on a Large Quantity Generator Facility.  See paragraph FACILITY 
HAZARDOUS WASTE GENERATOR STATUS for determination of generator status.</NPR><BRK/>
<BRK/>
<NPR>Erosion and Sediment Control Inspector Qualifications are determined by the state; not all states require the 
inspector be certified by the state.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Prepare and maintain <SUB>Employee Training Records</SUB> throughout the term of the contract meeting applicable 40 CFR requirements.  Provide Employee Training 
Records in the Environmental Records Binder.[  Ensure every employee completes a program of classroom instruction or on-the-job training that teaches 
them to perform their duties in a way that ensures compliance with federal, state and local regulatory requirements for RCRA Large Quantity Generator.  
Provide a Position Description for each employee, by subcontractor, based on the Davis-Bacon Wage Rate designation or other equivalent method, 
evaluating the employee's association with hazardous and regulated wastes.  This Position Description will include training requirements as defined 
in <RID>40 CFR 265</RID> for a Large Quantity Generator facility.]  Submit these <SUB>Assembled Employee Training Records</SUB> to the Contracting Officer at the conclusion 
of the project, unless otherwise directed.</TXT><BRK/>
<BRK/>
<TXT>Train personnel to meet [EPA][state] requirements.  Conduct environmental protection/pollution control meetings for personnel prior to commencing 
construction activities.  Conduct additional meetings for new personnel and when site conditions change.  Include in the training and meeting agenda: 
methods of detecting and avoiding pollution; familiarization with statutory and contractual pollution standards; installation and care of devices, 
vegetative covers, and instruments required for monitoring purposes to ensure adequate and continuous environmental protection/pollution control; 
anticipated hazardous or toxic chemicals or wastes, and other regulated contaminants; recognition and protection of archaeological sites, artifacts, 
waters of the United States, and endangered species and their habitat that are known to be in the area.[  Provide copy of the <SUB>Erosion and Sediment 
Control Inspector</SUB>[ Qualifications as defined by EPA][ Certification as required by[ state]].]</TXT><BRK/>
<BRK/>
<TAI OPT="ARMY"><SPT><TTL>Pest Control Training</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ARMY.  Use this paragraph for Army projects only.  Delete for other 
projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Trained personnel in pest control.  Conduct a pest control meeting for personnel prior to commencing construction activities.  Conduct additional 
meetings for new personnel and when site conditions change.  Include in the training and meeting agenda:  methods of detecting and pest infestation; 
familiarization with statutory and contractual pest control standards; installation and care of devices, and instruments, if required, for monitoring 
purposes to ensure adequate and continuous pest control; anticipated hazardous or toxic chemicals or wastes, and other regulated contaminants; 
recognition and protection of waters of the United States, and endangered species and their habitat that are known to be in the area. Provide a <SUB>
Certificate of Competency</SUB> for the personnel who will be conducting the pesticide application and management of pest control.</TXT><BRK/>
<BRK/></SPT>
</TAI></SPT><SPT><TTL>Non-Compliance Notifications</TTL><BRK/>
<BRK/>
<TXT>The Contracting Officer will notify the Contractor in writing of any observed noncompliance with federal, state or local environmental laws or 
regulations, permits, and other elements of the Contractor's EPP.  After receipt of such notice, inform the Contracting Officer of the proposed 
corrective action and take such action when approved by the Contracting Officer.  The Contracting Officer may issue an order stopping all or part 
of the work until satisfactory corrective action has been taken.  FAR 52.242-14 Suspension of Work provides that a suspension, delay, or interruption 
of work due to the fault or negligence of the Contractor allows for no adjustments to the contract for time extensions or equitable adjustments.  
In addition to a suspension of work, the Contracting Officer may use additional authorities under the contract or law.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL><SUB>ENVIRONMENTAL PROTECTION PLAN</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Edit this paragraph to include any environmental concerns or plans that may be required for the construction 
Contractor to protect the environment during construction of the project.  Coordinate the requirements with the 
Installation Environmental Office as applicable in addition to the Federal, State, Regional, and Local agencies.</NPR><BRK/>
<BRK/>
<NPR>Some permits required under the Environmental Protection Plan require up to 90 days advance regulator notice before 
site work may begin.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For DBB projects in the NAVFAC PAC Area of Operation, remove the second bracketed sentence and select the 
first bracketed sentence and edit this paragraph sentence to include "EPP within 30 calendar days after Contract 
award..."  and "...not less than 10 calendar days before the preconstruction meeting."  For DB projects remove 
the first bracketed sentence and select the second bracketed sentence.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The purpose of the EPP is to present an overview of known or potential environmental issues that must be considered and addressed during construction.  
Incorporate construction related objectives and targets from the installation's EMS into the EPP.  Include in the EPP measures for protecting natural 
and cultural resources, required reports, and other measures to be taken.  Meet with the Contracting Officer or Contracting Officer Representative 
to discuss the EPP and develop a mutual understanding relative to the details for environmental protection including measures for protecting natural 
resources, required reports, and other measures to be taken.[  Submit the EPP within [15][_____] days after [Contractor award][notice to proceed] 
and not less than [_____][10] days before the[ preconstruction] meeting.][  Submit the EPP not less than 60 calendar days before scheduled final 
site or building design approval.]  Revise the EPP throughout the project to include any reporting requirements, changes in site conditions, or 
contract modifications that change the project scope of work in a way that could have an environmental impact.  No requirement in this section 
will relieve the Contractor of any applicable federal, state, and local environmental protection laws and regulations.  During Construction, identify, 
implement, and submit for approval any additional requirements to be included in the EPP.  Maintain the current version onsite.</TXT><BRK/>
<BRK/>
<TXT>The EPP includes, but is not limited to, the following elements:</TXT><BRK/>
<BRK/>
<SPT><TTL>General Overview and Purpose</TTL><BRK/>
<BRK/>
<SPT><TTL>Descriptions</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Edit paragraph below to include those plans required for the project.  The bracketed list of plans is for 
example only and not meant to be all inclusive.</NPR><BRK/>
<BRK/>
<NPR>Use bracketed option for Pesticide Treatment Plan for Army projects only; this option is tailored for ARMY use.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>A brief description of each specific plan required by environmental permit or elsewhere in this Contract such as[ stormwater pollution prevention  
plan,][ spill control plan,][ solid waste management plan,][ wastewater management plan,][ air pollution control plan,][ contaminant prevention 
plan,]<TAI OPT="ARMY">[ pesticide treatment plan,]</TAI>[ a historical, archaeological, cultural resources, biological resources and wetlands plan,][ traffic control 
plan][ Hazardous, Toxic and Radioactive Waste (HTRW) Plan][ Non-Hazardous Solid Waste Disposal Plan][ borrowing material plan][_____].</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Duties</TTL><BRK/>
<BRK/>
<TXT>The duties and level of authority assigned to the person(s) on the job site who oversee environmental compliance, such as who is responsible for 
adherence to the EPP, who is responsible for spill cleanup and training personnel on spill response procedures, who is responsible for manifesting 
hazardous waste to be removed from the site (if applicable), and who is responsible for training the Contractor's environmental protection personnel.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Procedures</TTL><BRK/>
<BRK/>
<TXT>A copy of any standard or project-specific operating procedures that will be used to effectively manage and protect the environment on the project 
site.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Communications</TTL><BRK/>
<BRK/>
<TXT>Communication and training procedures that will be used to convey environmental management requirements to Contractor employees and subcontractors.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Contact Information</TTL><BRK/>
<BRK/>
<TXT>Emergency contact information contact information (office phone number, cell phone number, and e-mail address).</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>General Site Information</TTL><BRK/>
<BRK/>
<SPT><TTL>Drawings</TTL><BRK/>
<BRK/>
<TXT>Drawings showing locations of proposed temporary excavations or embankments for haul roads, stream crossings, jurisdictional wetlands, material 
storage areas, structures, sanitary facilities, storm drains and conveyances, and stockpiles of excess soil.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Work Area</TTL><BRK/>
<BRK/>
<TXT>Work area plan showing the proposed activity in each portion of the area and identify the areas of limited use or nonuse.  Include measures for 
marking the limits of use areas, including methods for protection of features to be preserved within authorized work areas and methods to control 
runoff and to contain materials on site, and a traffic control plan.</TXT><BRK/>
<BRK/>
<TXT>Show where any fuels, hazardous substances, solvents, or lubricants will be stored.  Provide a spill plan to address any releases of those materials.</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate documentation with paragraph ENVIRONMENTAL MANAGER requirements to ensure appropriate environmental 
manager oversight for this project.  Consider project environmental risks versus project size or dollar value.  
A small project, such as demolishing a plating shop could be low cost, but high risk and a large project, such 
as replacing a roof on a hangar, could be high cost, but low risk.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>A letter signed by an officer of the firm appointing the Environmental Manager and stating that person is responsible for managing and implementing 
the Environmental Program as described in this contract.  Include in this letter the Environmental Manager's authority to direct the removal and 
replacement of non-conforming work.</TXT><BRK/>
<BRK/></SPT>
]</SPT><SPT><TTL>Management of Natural Resources</TTL><BRK/>
<OLG><BRK/>
<OLI>Land resources</OLI><BRK/>
<BRK/>
<OLI>Tree protection</OLI><BRK/>
<BRK/>
<OLI>Replacement of damaged landscape features</OLI><BRK/>
<BRK/>
<OLI>Temporary construction</OLI><BRK/>
<BRK/>
<OLI>Stream crossings</OLI><BRK/>
<BRK/>
<OLI>Fish and wildlife resources</OLI><BRK/>
<BRK/>
<OLI>Wetland areas</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Protection of Historical and Archaeological Resources</TTL><BRK/>
<OLG><BRK/>
<OLI>Objectives</OLI><BRK/>
<BRK/>
<OLI>Methods</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Stormwater Management and Control</TTL><BRK/>
<OLG><BRK/>
<OLI>Ground cover</OLI><BRK/>
<BRK/>
<OLI>Erodible soils</OLI><BRK/>
<BRK/>
<OLI>Temporary measures</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Structural Practices</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Temporary and permanent stabilization</OLI><BRK/>
<BRK/>
<OLI>Effective selection, implementation and maintenance of Best Management Practices (BMPs).</OLI><BRK/>
<BRK/>
<OLI>Stormwater Pollution Prevention Plan (SWPPP).</OLI><BRK/>
<BRK/>
<TAI OPT="INDIANA"><NTE><AST/><BRK/>
<NPR>NOTE:  The following listed items are tailored for INDIANA and are for State of Indiana use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>f.  Construction Plan and Storm Water Pollution Prevention Plan.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">All projects must comply with the State of Indiana's NPDES General Permit for storm water run-off associated with construction 
activity, as described in <RID>327 IAC 15-5</RID>.  The Construction Plan must meet all requirements listed in <RID>327 IAC 15-5-6.5</RID>, including, 
but not limited to: project narrative and supporting documents; vicinity map depicting the project site location; existing project 
site layout map that indicates structures, waterways, soil maps, vegetation, adjacent land-use, and topography; final project 
site layout map; a grading plan indicating locations of proposed temporary excavations or embankments for haul roads, stream 
crossings, material storage areas, structures, sanitary facilities, and stockpiles of excess or spoil material; a drainage plan; 
and a Storm Water Pollution Prevention Plan.  The Storm Water Pollution Prevention Plan must include all items listed in <RID>327 IAC 15-5-7</RID>
 including, but not limited to, the following: description of temporary and permanent storm water quality measures; temporary 
stabilization plans; permanent stabilization plans; construction sequencing describing the relationship between implementation 
of storm water quality measures and stages of construction, including a schedule of these activities; self-monitoring program; 
description of potential pollutant sources associated with construction activities; and material handling and storage.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">If land disturbing activities are greater than or equal to one acre, it is the responsibility of the Contractor to have the Construction 
Plan, which includes the Storm Water Pollution Prevention Plan, reviewed and approved by the applicable reviewing agency. The 
State of Indiana designates different reviewing agencies for different counties in the state.  Commonly, the reviewing agency 
is the local Soil and Water Conservation District (SWCD) or Department of Natural Resources Division of Soil Conservation.  Information 
on approving agencies can be obtained from the Indiana Department of Environmental Management.  The reviewing agency has up to 
28 calendar days from the date of submittal to review the Construction Plan.  The Environmental Protection Plan must include 
documentation of the reviewing agency's approval of the Construction Plan, or the Contractor may submit, in the instance that 
the reviewing agency has exceeded the 28 calendar day review period, documentation that the reviewing agency has exceeded the 
review period.  If notice of a deficient plan is received, the plans must be revised to satisfy the deficiencies in accordance 
with <RID>327 IAC 15-5-6</RID> and resubmitted to the reviewing agency, at which time the 28 calendar-day review period starts over.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Government will review the Environmental Protection Plan, including the Construction and Storm Water Pollution Prevention 
Plans and then will submit the Notice of Intent (NOI), along with the proof of public notice and permit fee, to the Indiana Department 
of Environmental Management and the appropriate reviewing agency after the plan has been approved.  The Contractor will be notified 
of the submission date for the NOI.  No land disturbing activity may take place until 48 hours after submission of the NOI.  
Approval of the Contractor's plan will not relieve the Contractor of his responsibility for adequate and continuing control of 
pollutants and other environmental protection measures.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Government will provide copies of the NOI, and all other Government correspondence with IDEM, to the Contractor.  The Contractor 
must post the information required in <RID>327 IAC 15-5-7</RID>(b)(6) in a publicly accessible location near the main entrance of the project 
site.  The location will be jointly agreed to by the Contractor and the Government during the Pre-Construction Conference. The 
Contractor must take all actions necessary to keep the NOI and correspondence protected from the weather so that it remains legible.  
If, in the judgment of the Contracting Officer's Representative, the documents degrade to the point of being illegible, the Contractor 
must replace the documents with fresh copies and remedy the problems that caused the degradation.</OLI><BRK/>
<BRK/>
<OLI>Spill Control Plan must include the procedures, instructions, and reports to be used in the event of an unforeseen spill of a substance 
regulated by <RID>40 CFR 68</RID>, <RID>40 CFR 302</RID>, <RID>40 CFR 355</RID>, or regulated under State or Local laws and regulations.  The Spill Control Plan supplements 
the requirements of <RID>EM 385-1-1</RID>.  The plan must meet the requirements of <RID>327 IAC 2-6.1</RID>.  This plan must include as a minimum:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The name of the individual who will report any spills or hazardous substance releases and who will follow up with complete documentation.  
This individual must immediately notify the Contracting Officer and the local fire department or emergency response agency in 
addition to the legally required Federal, State, and local reporting channels (including the National Response Center 1-800-424-8802) 
if a reportable quantity is released to the environment.  The plan must contain a list of the required reporting channels and 
telephone numbers.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The name and qualifications of the individual who will be responsible for implementing and supervising the containment and cleanup.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Training requirements for Contractor's personnel and any subcontractors, and methods of accomplishing the training.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A list of materials and equipment to be immediately available at the job site, tailored to cleanup work of the potential hazard(s) 
identified.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The names and locations of suppliers of containment materials and locations of additional fuel oil recovery, cleanup, restoration, 
and material-placement equipment available in case of an unforeseen spill emergency.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The methods and procedures to be used for expeditious contaminant cleanup.</OLI><BRK/>
<BRK/></TAI>
</OLG><TAI OPT="ILLINOIS"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph and list are tailored for ILLINOIS and are for State of Illinois use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The EPP must include a Stormwater Pollution Prevention Plan (SWPPP).  The Government will review the EPP, including the Stormwater Pollution Prevention 
Plan, and then will submit the Notice of Intent (NOI) to the Illinois Environmental Protection Agency after the plan has been approved.  No construction 
will take place before the submission of the NOI; approval of the NPDES permit requires 30 calendar days after the submission of the NOI.  The 
Contractor may NOT begin earthmoving activities until 30 calendar days after the submission of the NOI.  Approval of the Contractor's plan by the 
Government will not relieve the Contractor of his responsibility for control of pollutants and other environmental protection measures.  Address 
all comments to the SWPPP generated by the Illinois Environmental Protection Agency within seven calendar days of receipt of comments.  Certify, 
in writing, that all recommended changes have been made to the SWPPP, and must submit certification to the Contracting Officer's Representative 
(COR).  Post, in a visible location accessible for public viewing, the IEPA response letter, to be provided by the Government, and ILR10 at the 
project site.</TXT><BRK/>
<OLG><BRK/>
<OLI>A Stormwater Pollution Prevention Plan which identifies the type and location of the erosion and sediment controls to be provided.  The 
plan must meet the requirements of the Illinois NPDES Permit No. ILR10 (included at the end of this section).  The management practices, 
controls, and other provisions contained in the plan must be as protective as the requirements in the Illinois Urban Manual, <RID>IUM</RID>.  The 
contents of the plan must address all items listed in Part IV of the permit, including but not limited to:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Site description, controls, maintenance, inspections, and non-stormwater discharges.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A map of the final site conditions.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A site construction plan that includes the locations and dimensions of land disturbing activities, locations of soil stockpiles, 
locations and dimensions of erosion control measures, and a schedule with the start and finish dates of each land disturbing 
activity, including the installation of erosion control measures.  Provisions and a schedule for maintenance of the erosion control 
measures during construction must also be included in the plan.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Name and qualifications of the person(s) responsible for inspecting the site in accordance with the requirements given in ILR10.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A copy of the blank inspection checklist that will be used during ILR10 site inspections.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The plan must contain the certification statement contained in Part IV(F) of the NPDES Permit No. ILR10.</OLI><BRK/></OLG>
<BRK/></TAI>
</SPT><SPT><TTL>Protection of the Environment from Waste Derived from Contractor Operations</TTL><BRK/>
<BRK/>
<TXT>This item consists of the management procedures for hazardous waste to be generated.  The elements of those procedures will coincide with the Installation 
Hazardous Waste Management Plan when within an installation.  The Contracting Officer will provide a copy of the Installation Hazardous Waste Management 
Plan as applicable.</TXT><BRK/>
<BRK/>
<TXT>As a minimum, include the following:</TXT><BRK/>
<OLG><BRK/>
<OLI>List of the types of hazardous wastes expected to be generated</OLI><BRK/>
<BRK/>
<OLI>Procedures to ensure a written waste determination is made for appropriate wastes that are to be generated</OLI><BRK/>
<BRK/>
<OLI>Sampling/analysis plan, including laboratory method(s) that will be used for waste determinations and copies of relevant laboratory certifications</OLI><BRK/>
<BRK/>
<OLI>Methods and proposed locations for hazardous waste accumulation/storage (that is, in tanks or containers)</OLI><BRK/>
<BRK/>
<OLI>Management procedures for storage, labeling, transportation, and disposal of waste (treatment of waste is not allowed unless specifically 
noted)</OLI><BRK/>
<BRK/>
<OLI>Management procedures and regulatory documentation ensuring disposal of hazardous waste complies with Land Disposal Restrictions (<RID>40 CFR 268</RID>
)</OLI><BRK/>
<BRK/>
<OLI>Management procedures for recyclable hazardous materials such as lead-acid batteries, used oil, and similar</OLI><BRK/>
<BRK/>
<OLI>Used oil management procedures in accordance with <RID>40 CFR 279</RID>; Hazardous waste minimization procedures</OLI><BRK/>
<BRK/>
<OLI>Plans for the disposal of hazardous waste by permitted facilities; and Procedures to be employed to ensure required employee training records 
are maintained.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Prevention of Releases to the Environment</TTL><BRK/>
<BRK/>
<TXT>Procedures to prevent releases to the environment</TXT><BRK/>
<BRK/>
<TXT>Notifications in the event of a release to the environment</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Regulatory Notification and Permits</TTL><BRK/>
<BRK/>
<TXT>List what notifications and permit applications must be made.  Some permits require up to 180 days to obtain.  Demonstrate that those permits have 
been obtained or applied for by including copies of applicable environmental permits.  The EPP will not be approved until the permits have been 
obtained.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Clean Air Act Compliance</TTL><BRK/>
<BRK/>
<TAI OPT="WISCONSIN"><SPT><TTL>Environmental Protection Plan</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for WISCONSIN and is for State of Wisconsin use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>An Air Pollution Control Plan detailing provisions to assure that dust, debris, materials, trash, do not become airborne and travel off the project 
site.  The air pollution control plan must include a dust control plan.  Air pollution control must comply with <RID>s. NR 415, Wis. Adm. Code</RID>.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Haul Route</TTL><BRK/>
<BRK/>
<TXT>Submit truck and material haul routes along with a <SUB>Dirt and Dust Control Plan</SUB> for controlling dirt, debris, and dust on Installation roadways.  
As a minimum, identify in the plan the subcontractor and equipment for cleaning along the haul route and measures to reduce dirt, dust, and debris 
from roadways.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Pollution Generating Equipment</TTL><BRK/>
<BRK/>
<TXT>Identify air pollution generating equipment or processes that may require federal, state, or local permits under the Clean Air Act.  Determine 
requirements based on any current installation permits and the impacts of the project. Provide a list of all fixed or mobile equipment, machinery 
or operations that could generate air emissions during the project to the Installation Environmental Office (Air Program Manager).  Ensure required 
permits are obtained prior to installing and operating applicable equipment/processes.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Stationary Internal Combustion Engines</TTL><BRK/>
<BRK/>
<TXT>Identify portable and stationary internal combustion engines that will be supplied, used or serviced.  Comply with <RID>40 CFR 60</RID> Subpart IIII, <RID>40 CFR 60</RID>
 Subpart JJJJ, <RID>40 CFR 63</RID> Subpart ZZZZ, and local regulations as applicable.  At minimum, include the make, model, serial number, manufacture date, 
size (engine brake horsepower), and EPA emission certification status of each engine.  Maintain applicable records and log hours of operation and 
fuel use.  Logs must include reasons for operation and delineate between maintenance/testing, emergency, and non-emergency operation.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Refrigerants</TTL><BRK/>
<BRK/>
<TXT>Identify management practices to ensure that heating, ventilation, and air conditioning (HVAC) work involving refrigerants complies with <RID>40 CFR 82</RID>
 requirements.  Technicians must be certified, maintain copies of certification on site, use certified equipment and log work that requires the 
addition or removal of refrigerant. Any refrigerant reclaimed is the property of the Government, coordinate with the Installation Environmental 
Office to determine the appropriate turn in location.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Air Pollution-engineering Processes</TTL><BRK/>
<BRK/>
<TXT>Identify planned air pollution-generating processes and management control measures (including, but not limited to, spray painting, abrasive blasting, 
demolition, material handling, fugitive dust, and fugitive emissions).  Log hours of operations and track quantities of materials used.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ARMY"><SPT><TTL>Monitoring</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ARMY projects only.  This paragraph pertains to Hazardous, Toxic 
and Radioactive Waste (HTRW) construction when the Designer has determined that the need to protect Air Quality 
during HTRW remedial action is necessary and appropriate.  The paragraph applies to contaminant emissions to the 
air from HTRW remedial action construction area sources.</NPR><BRK/>
<BRK/>
<NPR>An air pathway analysis needs to be conducted prior to specifying the items below.  The Designer is referred to 
EP 1110-1-21 Air Pathway Analysis (APA) for the Design of HTRW Remedial Action Project.  Design perimeter air 
monitoring requirements (action levels for the contaminants of concern, monitoring/sampling frequency) based on 
APA results.  Specify airborne contaminants of concern, action levels, monitoring/sampling locations below.  See 
40 CFR 300.430(e)(9) of the National Contingency Plan.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For the protection of public health, monitor and control contaminant emissions to the air from Hazardous, Toxic, and Radioactive Waste remedial 
action area sources to minimize short-term risks that might be posed to the community during implementation of the remedial alternative in accordance 
with the following.</TXT><BRK/>
<OLG><BRK/>
<OLI>Perimeter Air Contaminant of Concern [_____].</OLI><BRK/>
<BRK/>
<OLI>Time Averaged Perimeter Action Levels [_____].</OLI><BRK/>
<TAB>
<WBK>
   <STS/>
   <TDA COLUMNCOUNT="2" ROWCOUNT="2">
      <COL AUTOWIDTH="0" WIDTH="351.00"/>
      <COL AUTOWIDTH="0" WIDTH="351.00"/>
      <ROW AUTOHEIGHT="0" HEIGHT="30.00">
         <CEL>
<DTA TYPE="STRING">Concentration</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="29.25">
         <CEL>
<DTA TYPE="STRING">Time</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<OLI>Perimeter Sampling/Monitoring Location[s] [_____].</OLI><BRK/>
<BRK/>
<OLI>Monitoring Instruments/Sampling and Analysis Methods [_____].</OLI><BRK/>
<BRK/>
<OLI>Staffing [_____].</OLI><BRK/></OLG>
<BRK/></SPT>
</TAI><SPT><TTL>Compliant Materials</TTL><BRK/>
<BRK/>
<TXT>Provide the Government a list of SDSs for all hazardous materials proposed for use on site.  Materials must be compliant with all Clean Air Act 
regulations for emissions including solvent and volatile organic compound contents, and applicable National Emission Standards for Hazardous Air 
Pollutants requirements.  The Government may alter or limit use of specific materials as needed to meet installation permit requirements for emissions.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT><SPT><TTL>LICENSES AND PERMITS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The terms and conditions contained in any permits obtained by the Government must be made a part of the 
contract.  The design must be in accordance with these permits.  The title and requirements of this paragraph 
may be changed to include environmental reviews and approvals, if pertinent.  Coordinate this paragraph with paragraph 
SPECIAL ENVIRONMENTAL REQUIREMENTS.</NPR><BRK/>
<BRK/>
<NPR>For Design-Bid-Build (DBB) projects, establish a list of permits, prepare the permits for review and signature 
and obtain approval of all permits prior to bid. In rare occasions it may be permissible to note the anticipated 
permit approval date in the contract.  If this is the case, the contract documents need to clearly define which 
portion of the work is not to be disturbed by the Contractor and for what time period.</NPR><BRK/>
<BRK/>
<NPR>For Design-Build (DB) projects (Request for Proposals) edit the paragraphs below for permits to be obtained.</NPR><BRK/>
<AST/><BRK/></NTE>
<TAI OPT="NAVY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Navy DB and DBB projects:  Complete the Permit Record of Decision (PROD) in consultation with the cognizant 
Navy civil and environmental engineers and in accordance with FC 1-300-09N, NAVY AND MARINE CORPS DESIGN PROCEDURES.  
Edit the paragraph below to coordinate with the identified requirements.  Refer to the applicable section for 
guidance on locally required permits and licenses.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Obtain licenses and permits required for the construction of the project and in accordance with FAR 52.236-7 Permits and Responsibilities.  Notify 
the Government of all equipment that may require permits or special approvals that the Contractor plans to use on site.  This paragraph supplements 
the Contractor's responsibility under FAR 52.236-7 Permits and Responsibilities.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Edit the applicable bracketed paragraphs below as required for the particular project.</NPR><BRK/>
<BRK/>
<NPR>Use this paragraph for permits obtained by the Government.  Identify which permits have been obtained by the Government.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
[<OLI>The following permits have been obtained by the Government:</OLI><BRK/>
<BRK/>
[<OLI LEVEL="2">[_____]</OLI><BRK/>
<BRK/>
][<OLI LEVEL="2">[_____]</OLI><BRK/>
<BRK/>
][<OLI LEVEL="2">[_____]</OLI><BRK/>
]]<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Identify which permits will be obtained by the Government.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>The following permits will be obtained by the Government:</OLI><BRK/>
<BRK/>
[<OLI LEVEL="2">[_____]</OLI><BRK/>
<BRK/>
][<OLI LEVEL="2">[_____]</OLI><BRK/>
<BRK/>
][<OLI LEVEL="2">[_____]</OLI><BRK/></OLG>
<BRK/>
]]</SPT><SPT><TTL>ENVIRONMENTAL RECORDS BINDER</TTL><BRK/>
<BRK/>
<TXT>Maintain on-site a separate three-ring Environmental Records Binder and submit at the completion of the project.  Make separate parts within the 
binder that correspond to each submittal listed under paragraph CLOSEOUT SUBMITTALS in this section.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ARMY"><SPT><TTL>PESTICIDE DELIVERY, STORAGE, AND HANDLING</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This Article is tailored for ARMY.  Use this paragraph and subsequent subparagraphs for Army projects only.  
Do not use for Navy or Air Force projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Delivery and Storage</TTL><BRK/>
<BRK/>
<TXT>Deliver pesticides to the site in the original, unopened containers bearing legible labels indicating the EPA registration number and the manufacturer's 
registered uses.  Store pesticides according to manufacturer's instructions and under lock and key when unattended.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Handling Requirements</TTL><BRK/>
<BRK/>
<TXT>Formulate, treat with, and dispose of pesticides and associated containers in accordance with label directions and use the clothing and personal 
protective equipment specified on the labeling for use during each phases of the application.  Furnish SDSs for pesticide products.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><SPT><TTL><SUB>SOLID WASTE MANAGEMENT PERMIT</SUB></TTL><BRK/>
<BRK/>
<TXT>Provide the Contracting Officer with written notification of the quantity of anticipated solid waste or debris that is anticipated or estimated 
to be generated by construction.  Include in the report the locations where various types of waste will be disposed or recycled.  Include letters 
of acceptance from the receiving location or as applicable; submit one copy of the receiving location state and local Solid Waste Management Permit 
or license showing such agency's approval of the disposal plan before transporting wastes off Government property.</TXT><BRK/>
<BRK/>
<SPT><TTL><SUB>Monthly Solid Waste Disposal Report</SUB></TTL><BRK/>
<BRK/>
<TXT>Monthly, submit a solid waste disposal report to the Contracting Officer.  For each waste, the report will state the classification (using the 
definitions provided in this section), amount, location, and name of the business receiving the solid waste.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>FACILITY HAZARDOUS WASTE GENERATOR STATUS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Insert the name of the installation as applicable in the blank space.  Contact the installation Environmental 
Office prior to start of design to determine the generator status of the activity, and edit to select the appropriate 
status.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[_____] is designated as a[ Large Quantity Generator][ Small Quantity Generator][ Conditionally Exempt-Small Quantity Generator].  Meet the regulatory 
requirements of this generator designation for any work conducted within the boundaries of this Installation.  Comply with provisions of federal, 
state, and local regulatory requirements applicable to this generator status regarding training and storage, handling, and disposal of construction 
derived wastes.</TXT><BRK/>
<BRK/></SPT>
</PRT><PRT><TTL>PART 2   PRODUCTS</TTL><BRK/>
<BRK/>
<TXT>Not Used</TXT><BRK/>
<BRK/></PRT>
<PRT><TTL>PART 3   EXECUTION</TTL><BRK/>
<BRK/>
<SPT><TTL>PROTECTION OF NATURAL RESOURCES</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Specify any special protection requirements and specifically describe how the Contractor is to protect 
the resources.  This paragraph should be used when the Government knows of resources which should be protected 
and there are no requirements under Federal, State or local laws or regulations which would ensure that the Contractor 
would provide protection.  If there are known Endangered or Threatened Species onsite or in the area including 
their habitat, this paragraph must identify the species and their habitat and must include any requirements or 
methods for protection.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Minimize interference with, disturbance to, and damage to fish, wildlife, and plants, including their habitats.  Prior to the commencement of activities, 
consult with the Installation Environmental Office as applicable, regarding rare species or sensitive habitats that need to be protected.  The 
protection of rare, threatened, and endangered animal and plant species identified, including their habitats, is the Contractor's responsibility.[  
The following species are known and could be affected within the construction area: [_____].]</TXT><BRK/>
<BRK/>
<TXT>Preserve the natural resources within the project boundaries and outside the limits of permanent work.  Restore to an equivalent or improved condition 
upon completion of work that is consistent with the requirements of the Installation Environmental Office or as otherwise specified.  Confine construction 
activities to within the limits of the work indicated or specified.</TXT><BRK/>
<BRK/>
<SPT><TTL>Flow Ways</TTL><BRK/>
<BRK/>
<TXT>Do not alter water flows or otherwise significantly disturb the native habitat adjacent to the project and critical to the survival of fish and 
wildlife, except as specified and permitted.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Vegetation</TTL><BRK/>
<BRK/>
<TXT>Except in areas to be cleared, do not remove, cut, deface, injure, or destroy trees or shrubs without the Contracting Officer's permission.  Do 
not fasten or attach ropes, cables, or guys to existing nearby trees for anchorages unless authorized by the Contracting Officer.  Where such use 
of attached ropes, cables, or guys is authorized, the Contractor is responsible for any resultant damage.</TXT><BRK/>
<BRK/>
<TXT>Protect existing trees and critical root zones (CRZ) that are to remain to ensure they are not injured, bruised, defaced, or otherwise damaged 
by construction operations.  Remove displaced rocks from uncleared areas.  Coordinate with the Contracting Officer and Installation Environmental 
Office to determine appropriate action for trees and other landscape features scarred or damaged by equipment operations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Streams</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Review federal, state, and local requirements and obtain all necessary permits that are required for stream 
crossings.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Stream crossings must allow movement of materials or equipment without violating water pollution control standards of the federal, state, and local 
governments.  Construction of stream crossing structures must be in compliance with all required permits including, but not limited to, Clean Water 
Act Section 404, and Section 401 Water Quality.</TXT><BRK/>
<BRK/>
<TXT>The Contracting Officer's approval and appropriate permits are required before any equipment will be permitted to ford live streams.  In areas 
where frequent crossings are required, install temporary culverts or bridges.  Obtain Contracting Officer's approval prior to installation.  Remove 
temporary culverts or bridges upon completion of work, and repair the area to its original condition unless otherwise required by the Contracting 
Officer.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>STORMWATER</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Check with Installation Environmental Office as applicable to make sure that you are including all relevant 
state and local agency requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Do not discharge stormwater from construction sites to the sanitary sewer.  If the water is noted or suspected of being contaminated, it may only 
be released to the storm drain system if the discharge is specifically permitted.  Obtain authorization in advance from the Installation Environmental 
Office for any release of contaminated water.</TXT><BRK/>
<BRK/>
[<SPT><TTL>Construction General Permit</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph and subparagraphs when one or more acres (0.4 or more hectares) of total land area 
are to be disturbed or disturbs less than one acre but is part of a larger common plan of development or sale 
that will disturb one or more acres.  Coordinate with Installation Environmental Office as applicable to determine 
if project is part of larger common plan of development.  Most states are approved to implement the General Permits 
Program.  EPA remains the permitting authority in a few states, territories, and on most land in Indian Country.  
Refer to <URL HREF="https://www.epa.gov/npdes/authorization-status-epas-construction-and-industrial-stormwater-programs">https://www.epa.gov/npdes/authorization-status-epas-<BRK/>
construction-and-industrial-stormwater-programs</URL> for the approved list.  Edit the bracketed item accordingly.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide a Construction General Permit as required by <RID>40 CFR 122.26</RID> or [EPA][the State of [_____]] General Permit.  Under the terms and conditions 
of the permit, install, inspect, maintain BMPs, prepare stormwater erosion and sediment control inspection reports, and submit SWPPP inspection 
reports.  Maintain construction operations and management in compliance with the terms and conditions of the general permit for stormwater discharges 
from construction activities.</TXT><BRK/>
<BRK/>
<SPT><TTL>Stormwater Pollution Prevention Plan</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects in the NAVFAC PAC Area of Operation, edit this paragraph to include bracketed portion "within 
30 calendar days of Contract award and..."</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Submit a project-specific <SUB>Stormwater Pollution Prevention Plan</SUB> (SWPPP) to the Contracting Officer for approval, [within 30 days of Contract Award 
and ]prior to the commencement of work.  The SWPPP must meet the requirements of <RID>40 CFR 122.26</RID> and [the EPA General Permit][the [_____] State General 
Permit] for stormwater discharges from construction sites.</TXT><BRK/>
<TAI OPT="NAVY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate with the Installation Environmental Management Office to edit the bracketed items.  Use the 
last bracketed item "d" for NAVY only projects when local environmental controls are provided.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Include the following:</TXT><BRK/>
<BRK/>
<LST INDENT="-0.33">a.  Comply with terms of the [EPA][state] general permit for stormwater discharges from construction activities.  Prepare SWPPP in accordance 
with [state][EPA] requirements. Use [state][EPA guide Developing your Stormwater Pollution Prevention Plan located at <URL HREF="https://www.epa.gov/npdes/developing-stormwater-pollution-prevention-plan-swppp">https://www.epa.gov/npdes/developing-stormwater-pollution-prevention-<BRK/>
plan-swppp</URL> to prepare the SWPPP.]</LST> <BRK/>
<BRK/>
<LST INDENT="-0.33">b.  Select applicable BMPs from EPA Fact Sheets located at <URL HREF="https://www.epa.gov/npdes/national-menu-best-management-practices-bmps-stormwater#constr">https://www.epa.gov/npdes/national-menu-best-management-practices-<BRK/>
bmps-stormwater#constr</URL> or in accordance with applicable state or local requirements.</LST><BRK/>
<BRK/>
<LST INDENT="-0.33">c.  Include a completed copy of the Notice of Intent, BMP Inspection Report Template, and Stormwater Notice of Termination, except for 
the effective date.</LST><BRK/>
<BRK/>
<TAI OPT="NAVY"><NTE><AST/><BRK/>
<NPR>NOTE:  The following item is tailored for NAVY use only.</NPR><BRK/>
<AST/><BRK/></NTE>
[<LST INDENT="-0.33">d.  Comply with local additional requirements.</LST><BRK/>
<BRK/>
]</TAI></SPT><SPT><TTL><SUB>Stormwater Notice of Intent</SUB> for Construction Activities</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Refer to the Construction General Permit for Construction Activities permit application form to determine 
if co-permittee status, with the Contractor and Installation covered under one permit, is required by the permitting 
authority.  Choose first bracketed sentence when co-permittee status is not required.  Choose second bracketed 
sentence when co-permittee status is required.<BRK/>
<TAI OPT="NAVY"><BRK/>
Use the last, NAVY tailored paragraph for Navy projects only.</TAI></NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects in the NAVFAC PAC Area of Operation, add the first and last bracketed paragraphs to this paragraph.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Prepare and submit the Notice of Intent for NPDES coverage under the general permit for construction activities to the Contracting Officer for 
review.</TXT><BRK/>
<BRK/>
][<TXT>Prepare and submit the Notice of Intent for NPDES coverage under the general permit for construction activities to the Contracting Officer for 
review and approval.</TXT><BRK/>
<BRK/>
][<TXT>Prepare and submit a Notice of Intent as a co-permittee to the Contracting Officer, for review and approval.</TXT><BRK/>
<BRK/>
]<TXT>Submit the approved NOI and appropriate permit fees onto the appropriate federal or state agency for approval.  No land disturbing activities may 
commence without permit coverage.  Maintain an approved copy of the SWPPP at the onsite construction office, and continually update as regulations 
require, reflecting current site conditions.</TXT><BRK/>
<BRK/>
<TAI OPT="NAVY"><TXT>Comply with additional state and local requirements.</TXT><BRK/>
<BRK/></TAI>
</SPT><SPT><TTL><SUB>Inspection Reports</SUB></TTL><BRK/>
<TAI OPT="NAVY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the last NAVY tailored, bracketed sentence for Navy projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Submit "Inspection Reports" to the Contracting Officer in accordance with [EPA][the State of [_____]]Construction General Permit.<TAI OPT="NAVY">[  Provide Inspection 
Reports in accordance with local requirements.]</TAI></TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>Stormwater Pollution Prevention Plan Compliance Notebook</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the bracketed option to identify the permit issuing agency.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Create and maintain a three ring binder of documents that demonstrate compliance with the Construction General Permit.  Include a copy of the permit 
Notice of Intent, proof of permit fee payment, SWPPP and SWPPP update amendments, inspection reports and related corrective action records, copies 
of correspondence with the [EPA][the [_____]State Permitting Agency], and a copy of the permit Notice of Termination in the binder.  At project 
completion, the notebook becomes property of the Government.  Provide the compliance notebook to the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>Stormwater Notice of Termination</SUB> for Construction Activities</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use bracketed item if as-built topographic survey information is required by the permitting agency for 
certification of the stormwater management system.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Submit a Notice of Termination to the Contracting Officer for approval once construction is complete and final stabilization has been achieved 
on all portions of the site for which the permittee is responsible.  Once approved, submit the Notice of Termination to the appropriate state or 
federal agency.[  Prepare <SUB>as-built topographic survey</SUB> information required by the permitting agency for certification of the stormwater management 
system, and provide to the Contracting Officer.]</TXT><BRK/>
<BRK/></SPT>
</SPT>]<SPT><TTL>Erosion and Sediment Control Measures</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects that have a State permit, delete subparagraphs EROSION CONTROL and SEDIMENT CONTROL PRACTICES.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide erosion and sediment control measures in accordance with state and local laws and regulations.  Preserve vegetation to the maximum extent 
practicable.</TXT><BRK/>
<BRK/>
<TAI OPT="ILLINOIS"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ILLINOIS and is for State of Illinois use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Contractor's best management practices must also be in accordance with the State of Illinois National Pollutant Discharge Elimination System 
(NPDES) Storm Water Pollution Prevention requirements.  Any temporary measures must be removed after the area has been stabilized.</TXT><BRK/>
<BRK/></TAI>
<TAI OPT="INDIANA"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for INDIANA and is for State of Indiana use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Contractor will be responsible for providing erosion and sediment control measures in accordance with Federal, State, and local laws and regulations.  
The erosion and sediment controls selected and maintained by the Contractor must be such that water quality standards are not violated as a result 
of the Contractor's construction activities.  The area of bare soil exposed at any one time by construction operations should be kept to a minimum.  
The Contractor must construct or install temporary and permanent erosion and sediment control best management practices (BMPs).  BMPs may include, 
but not be limited to, vegetation cover, stream bank stabilization, slope stabilization, silt fences, construction of terraces, interceptor channels, 
sediment traps, inlet and outfall protection, diversion channels, and sedimentation basins.  The Contractor's best management practices must also 
be in accordance with the State of Indiana National Pollutant Discharge Elimination System (NPDES) Storm Water Pollution Prevention requirements.  
Any temporary measures must be removed after the area has been stabilized.</TXT><BRK/>
<BRK/></TAI>
<TAI OPT="WISCONSIN"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for WISCONSIN and is for State of Wisconsin use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Contractor will be responsible for providing erosion and sediment control measures in accordance with Federal, State, and local laws and regulations.  
The erosion and sediment controls selected and maintained by the Contractor must be such that water quality standards are not violated as a result 
of the Contractor's construction activities.  The area of bare soil exposed at any one time by construction operations should be kept to a minimum.  
The Contractor must construct or install temporary and permanent erosion and sediment control best management practices (BMPs).  BMPs may include, 
but not be limited to, vegetation cover, stream bank stabilization, slope stabilization, silt fences, construction of terraces, interceptor channels, 
sediment traps, inlet and outfall protection, diversion channels, and sedimentation basins.  The Contractor's best management practices must also 
be in accordance with the State of Wisconsin National Pollutant Discharge Elimination System (NPDES) Storm Water Pollution Prevention requirements.  
Any temporary measures must be removed after the area has been stabilized.</TXT><BRK/>
<BRK/></TAI>
<TXT>Erosion control inspection reports may be compiled as part of a stormwater pollution prevention plan inspection reports.</TXT><BRK/>
<BRK/>
[<SPT><TTL>Erosion Control</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use last bracketed sentence if Section <SRF>32 92 19</SRF> SEEDING is included in the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Prevent erosion by[ mulching,][ Compost Blankets,][ Geotextiles,][ temporary slope drains,][_____].  Stabilize slopes by[ chemical stabilization,][ 
sodding,][ seeding,][_____] or such combination of these methods necessary for effective erosion control.  Use of hay bales is prohibited.</TXT><BRK/>
<BRK/>
[<TXT>Provide seeding in accordance with Section <SRF>32 92 19</SRF> SEEDING.</TXT><BRK/>
<BRK/>
]</SPT>][<SPT><TTL>Sediment Control Practices</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Select the sediment control practices appropriate for the project.  See <URL HREF="https://www.epa.gov/npdes/national-menu-best-management-practices-bmps-stormwater#constr">https://www.epa.gov/npdes/national-menu-best-<BRK/>
management-practices-bmps-stormwater#constr</URL>.  Use last bracketed sentence when sediment control practices are 
indicated on the drawings. Include details.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Implement sediment control practices to divert flows from exposed soils, temporarily store flows, or otherwise limit runoff and the discharge of 
pollutants from exposed areas of the site.  Implement sediment control practices prior to soil disturbance and prior to creating areas with concentrated 
flow, during the construction process to minimize erosion and sediment laden runoff.  Include the following devices:[ silt fence,][ temporary diversion 
dikes,][ storm drain inlet protection,][_____,][ Location and details of installation and construction are indicated on the drawings].</TXT><BRK/>
<BRK/></SPT>
]</SPT><SPT><TTL>Work Area Limits</TTL><BRK/>
<BRK/>
<TXT>Mark the areas that need not be disturbed under this Contract prior to commencing construction activities.  Mark or fence isolated areas within 
the general work area that are not to be disturbed.  Protect monuments and markers before construction operations commence.  Where construction 
operations are to be conducted during darkness, all markers must be visible in the dark.  Personnel must be knowledgeable of the purpose for marking 
and protecting particular objects.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Contractor Facilities and Work Areas</TTL><BRK/>
<BRK/>
<TXT>Place field offices, staging areas, stockpile storage, and temporary buildings in areas designated on the drawings or as directed by the Contracting 
Officer.  Move or relocate the Contractor facilities only when approved by the Government.  Provide erosion and sediment controls for onsite borrow 
and spoil areas to prevent sediment from entering nearby waters.  Control temporary excavation and embankments for plant or work areas to protect 
adjacent areas.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Municipal Separate Storm Sewer System (MS4) Management</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph if the Installation holds a MS4 permit.  Coordinate with the Installation Environmental 
Office.<TAI OPT="NAVY">  Use tailored, bracketed sentence for Navy only projects.</TAI></NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the Installation's MS4 permit requirements.<TAI OPT="NAVY">[  Comply with local requirements.]</TAI></TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>SURFACE AND GROUNDWATER</TTL><BRK/>
<BRK/>
<SPT><TTL>Cofferdams, Diversions, and Dewatering</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Edit the first sentence by removing items not included in the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Construction operations for dewatering, removal of cofferdams, tailrace excavation, and tunnel closure must be constantly controlled to maintain 
compliance with existing state water quality standards and designated uses of the surface water body.  Comply with[ the State of [_____] water 
quality standards and anti-degradation provisions] [and][ the Clean Water Act Section 404, Nation Wide Permit No. [_____]].  Do not discharge excavation 
ground water to the sanitary sewer, storm drains, or to surface waters without prior specific authorization in writing from the Installation Environmental 
Office or Contracting Officer.  Discharge of hazardous substances will not be permitted under any circumstances.  Use sediment control BMPs to 
prevent construction site runoff from directly entering any storm drain or surface waters.</TXT><BRK/>
<BRK/>
<TAI OPT="ILLINOIS"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ILLINOIS and is for State of Illinois use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Contractors diversions and dewatering operations must comply with the state of Illinois water quality standards and anti-degradation provisions, 
Section 404 of the Clean Water Act, and the Section 401 Water Quality Certification for this project.</TXT><BRK/>
<BRK/></TAI>
<TXT>If the construction dewatering is noted or suspected of being contaminated, it may only be released to the storm drain system if the discharge 
is specifically permitted.  Obtain authorization for any contaminated groundwater release in advance from the Installation Environmental Officer 
and the federal or state authority, as applicable.  Discharge of hazardous substances will not be permitted under any circumstances.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Waters of the United States</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  All wetlands on the site or adjacent to the site must be identified on the drawings and this paragraph 
edited accordingly.  If the wetlands on site must be disturbed, coordination with the regulatory agencies during 
design for identification of Section 401 and 404 of the Clean Water Act permits whether the permit is an Individual, 
Nationwide, Regional, State, or Local 404 or similar permit.  Include permit requirements in the LICENSES AND 
PERMITS paragraph and attach to this specification.  In addition, coordinate any mitigation requirements for the 
project.</NPR><BRK/>
<BRK/>
<NPR>Government Natural Resources staff will approve all Section 404 permit mitigations; the Contractor is not authorized 
to agree to mitigations on behalf of the Government.</NPR><BRK/>
<BRK/>
<NPR>If no wetlands are onsite or adjacent to the site, delete this paragraph in its entirety.  The first sentence 
should normally remain intact with the first bracketed item.  This will require the Contractor to be cognizant 
of the responsibility to protect wetlands regardless of whether they are identified on drawings or in the event 
site conditions have changed since design.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Do not enter, disturb, destroy, or allow discharge of contaminants into waters of the United States[.][ except as authorized herein.  The protection 
of waters of the United States shown on the drawings in accordance with paragraph LICENSES AND PERMITS is the Contractor's responsibility.  Authorization 
to enter specific waters of the United States identified does not relieve the Contractor from any obligation to protect other waters of the United 
States within, adjacent to, or in the vicinity of the construction site and associated boundaries.]</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ILLINOIS"><SPT><TTL>Stream Crossings</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for ILLINOIS and is for State of Illinois use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Comply with the State of Illinois water quality standards and anti-degradation provisions, Section 404 of the Clean Water Act, and the Section 
401 Water Quality Certification for construction of stream crossing for this project.</TXT><BRK/>
<BRK/></SPT>
</TAI></SPT><SPT><TTL>PROTECTION OF CULTURAL RESOURCES</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Obtain the National Historic Preservation Act Section 106 documentation from the Government and include 
requirements agreed to during the consultation process with the State Historic Preservation Officer.  If Section 
106 has not been completed delete the following paragraphs.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Archaeological Resources</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  If there are known archaeological resources on the project site, include the bracketed sentence and show 
the required protection area and other protection measures on the drawings.  The exact location of known archaeological 
resources is sensitive information that will not be distributed unless necessary for protection.  The Contracting 
Officer will review and approve what is shown on the drawings.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[Existing archaeological resources within the work area are shown on the drawings.  Protect these resources and be responsible for their preservation 
during the life of the Contract.  ]If, during excavation or other construction activities, any previously unidentified or unanticipated historical, 
archaeological, and cultural resources are discovered or found, activities that may damage or alter such resources will be suspended.  Resources 
covered by this paragraph include, but are not limited to: any human skeletal remains or burials; artifacts; shell, midden, bone, charcoal, or 
other deposits; rock or coral alignments, pavings, wall, or other constructed features; and any indication of agricultural or other human activities.  
Upon such discovery or find, immediately notify the Contracting Officer so that the appropriate authorities may be notified and a determination 
made as to their significance and what, if any, special disposition of the finds should be made.  Cease all activities that may result in impact 
to or the destruction of these resources.  Secure the area and prevent employees or other persons from trespassing on, removing, or otherwise disturbing 
such resources.  The Government retains ownership and control over archaeological resources.</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Historical Resources</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  If there are known historical or other cultural resources on the project site, include this paragraph and 
show the required protection area and other protection measures on the drawings. Show the exact location of known 
historical resources on the drawings.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Existing historical resources within the work area are shown on the drawings.  Protect these resources and be responsible for their preservation 
during the life of the Contract.</TXT><BRK/>
<BRK/></SPT>
]</SPT><SPT><TTL>AIR RESOURCES</TTL><BRK/>
<BRK/>
<TXT>Equipment operation, activities, or processes will be in accordance with <RID>40 CFR 64</RID> and state air emission and performance laws and standards.</TXT><BRK/>
<BRK/>
<SPT><TTL>Preconstruction Air Permits</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate with local Installation Environmental Office as applicable to determine if Government will obtain 
these permits, or if Contractor will be required to obtain them.</NPR><BRK/>
<BRK/>
<NPR>Include permit application fees; coordinate with the Installation Environmental Office for the estimated fee based 
on project specifics.  Fee amount will depend on location of work and type of work.  Typical fees range from $250 
to $3500.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Notify the Air Program Manager, through the Contracting Officer, at least 6 months prior to bringing equipment, assembled or unassembled, onto 
the Installation, so that air permits can be secured.  Necessary permitting time must be considered in regard to construction activities.  Clean 
Air Act (CAA) permits must be obtained prior to bringing equipment, assembled or unassembled, onto the Installation.</TXT><BRK/>
<BRK/>
<TXT>[Permits will be provided by the Government.] [Confirm that these permits have been obtained.]</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Oil or Dual-fuel Boilers and Furnaces</TTL><BRK/>
<BRK/>
<TXT>Provide product data and details for new, replacement, or relocated fuel fired boilers, heaters, or furnaces to the Installation Environmental 
Office (Air Program Manager) through the Contracting Officer.  Data to be reported include: equipment purpose (water heater, building heat, process), 
manufacturer, model number, serial number, fuel type (oil type, gas type) size (MMBTU heat input).  Provide in accordance with paragraph PRECONSTRUCTION 
AIR PERMITS.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Burning</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Edit the paragraph after coordinating with the governing agencies.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[Burning is prohibited on the Government premises.] [Burning is allowed on Government premises[; confine fires to a closed vessel that is guarded 
and under constant surveillance until contents have burned out or have been extinguished].[  Burning must completely reduce the materials to ashes.]]</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Class I [and II ]ODS Prohibition</TTL><BRK/>
<BRK/>
<TXT>Class I [and II ]ODS are Government property and must be returned to the Government for appropriate management.  Coordinate with the Installation 
Environmental Office to determine the appropriate location for turn in of all reclaimed refrigerant.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Venting of Refrigerant</TTL><BRK/>
<BRK/>
<TXT>Accidental venting of a refrigerant is a release and must be reported immediately to the Contracting Officer.  Intentional venting of refrigerants 
(including most Non-ODS substitute refrigerants) is prohibited per <RID>40 CFR 82</RID>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>EPA Certification Requirements</TTL><BRK/>
<BRK/>
<TXT>Heating and air conditioning technicians must be certified through an EPA-approved program.  Maintain copies of certifications at the employees' 
places of business; technicians must carry certification wallet cards, as provided by environmental law.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Dust Control</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Only use the bracketed sentence if dust suppressants are allowed at the Installation and with permission 
of the Installation's Environmental office.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Keep dust down at all times, including during nonworking periods.[  Sprinkle or treat, with dust suppressants, the soil at the site, haul roads, 
and other areas disturbed by operations.]  Dry power brooming will not be permitted.  Instead, use vacuuming, wet mopping, wet sweeping, or wet 
power brooming.  Air blowing will be permitted only for cleaning nonparticulate debris such as steel reinforcing bars.  Only wet cutting will be 
permitted for cutting concrete blocks, concrete, and bituminous concrete.  Do not unnecessarily shake bags of cement, concrete mortar, or plaster.  
Since these products contain Crystalline Silica, comply with the applicable OSHA standard, <RID>29 CFR 1910.1053</RID> or <RID>29 CFR 1926.1153</RID> for controlling 
exposure to Crystalline Silica Dust.</TXT><BRK/>
<BRK/>
<SPT><TTL>Particulates</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This is a general performance type requirement for particulate control.  For projects where special construction 
activities, such as concrete batch plants, or extensive earthwork are involved, the Designer should consider the 
need for a more descriptive specification giving methods, frequency of application, and monitoring methods for 
controlling particulates.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Dust particles, aerosols and gaseous by-products from construction activities, and processing and preparation of materials (such as from asphaltic 
batch plants) must be controlled at all times, including weekends, holidays, and hours when work is not in progress.  Maintain excavations, stockpiles, 
haul roads, permanent and temporary access roads, plant sites, spoil areas, borrow areas, and other work areas within or outside the project boundaries 
free from particulates that would exceed <RID>40 CFR 50</RID>, state, and local air pollution standards or that would cause a hazard or a nuisance.  Sprinkling, 
chemical treatment of an approved type, baghouse, scrubbers, electrostatic precipitators, or other methods will be permitted to control particulates 
in the work area.  Sprinkling, to be efficient, must be repeated to keep the disturbed area damp.  Provide sufficient, competent equipment available 
to accomplish these tasks.  Perform particulate control as the work proceeds and whenever a particulate nuisance or hazard occurs.  Comply with 
state and local visibility regulations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Abrasive Blasting</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Determine whether the paint to be removed contains any hazardous components.  Test a representative sample 
of the paint in accordance with 40 CFR 261.  Include the bracketed sentence on hazardous material if it is determined 
the paint is toxic.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Blasting operations cannot be performed without prior approval of the Installation Air Program Manager.  The use of silica sand is prohibited in 
sandblasting.</TXT><BRK/>
<BRK/>
<TXT>Provide tarpaulin drop cloths and windscreens to enclose abrasive blasting operations to confine and collect dust, abrasive agent, paint chips, 
and other debris.[  Perform work involving removal of hazardous material in accordance with 29 CFR 1910.]</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Odors</TTL><BRK/>
<BRK/>
<TXT>Control odors from construction activities.  The odors must be in compliance with state regulations and local ordinances and may not constitute 
a health hazard.</TXT><BRK/>
<BRK/>
<TAI OPT="INDIANA"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for INDIANA and is for State of Indiana use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Odors must be controlled at all times.  The odors must not cause a health hazard and must be in compliance with State of Indiana regulations and 
ordinances.</TXT><BRK/>
<BRK/></TAI>
<TAI OPT="WISCONSIN"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for WISCONSIN and is for State of Wisconsin use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Odors must be controlled at all times.  The odors must not cause a health hazard and must be in compliance with State of Wisconsin regulations 
and local ordinances.</TXT><BRK/>
<BRK/></TAI>
</SPT></SPT><SPT><TTL>WASTE MINIMIZATION</TTL><BRK/>
<BRK/>
<TXT>Minimize the use of hazardous materials and the generation of waste.  Include procedures for pollution prevention/ hazardous waste minimization 
in the Hazardous Waste Management Section of the EPP.  Obtain a copy of the installation's Pollution Prevention/Hazardous Waste Minimization Plan 
for reference material when preparing this part of the EPP.  If no written plan exists, obtain information by contacting the Contracting Officer.  
Describe the anticipated types of the hazardous materials to be used in the construction when requesting information.</TXT><BRK/>
<BRK/>
<SPT><TTL>Salvage, Reuse and Recycle</TTL><BRK/>
<BRK/>
<TXT>Identify anticipated materials and waste for salvage, reuse, and recycling.  Describe actions to promote material reuse, resale or recycling.  
To the extent practicable, all scrap metal must be sent for reuse or recycling and will not be disposed of in a landfill.</TXT><BRK/>
<BRK/>
<TXT>Include the name, physical address, and telephone number of the hauler, if transported by a franchised solid waste hauler.  Include the destination 
and, unless exempted, provide a copy of the state or local permit (cover) or license for recycling.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Nonhazardous Solid Waste Diversion Report</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Edit the Nonhazardous Solid Waste Diversion Report to reflect the Using Service's requirements.</NPR><BRK/>
<BRK/>
<NPR>Coordinate the requirements in this paragraph with Section <SRF>02 41 00</SRF> [DEMOLITION][ AND ][DECONSTRUCTION].</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Maintain an inventory of nonhazardous solid waste diversion and disposal of construction and demolition debris.  Submit a report to [_____ through] 
the Contracting Officer on the first working day after each fiscal year quarter, starting the first quarter that nonhazardous solid waste has been 
generated.  Include the following in the report:</TXT><BRK/>
<TAB>
<WBK>
   <STS/>
   <TDA COLUMNCOUNT="2" ROWCOUNT="5">
      <COL AUTOWIDTH="0" WIDTH="380.25"/>
      <COL AUTOWIDTH="0" WIDTH="380.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="30.75">
         <CEL>
<DTA TYPE="STRING">Construction and Demolition (C&amp;D) Debris Disposed</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____] [cubic yards][tons],[cubic meters] as appropriate</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="27.75">
         <CEL>
<DTA TYPE="STRING">C&amp;D Debris Recycled</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____] [cubic yards][tons],[cubic meters] as appropriate</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="22.50">
         <CEL>
<DTA TYPE="STRING">C&amp;D Debris Composted</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____] [cubic yards][tons],[cubic meters] as appropriate</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="30.75">
         <CEL>
<DTA TYPE="STRING">Total C&amp;D Debris Generated</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____] [cubic yards][tons],[cubic meters] as appropriate</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="67.50">
         <CEL>
<DTA TYPE="STRING">Waste Sent to Waste-To-Energy Incineration Plant (This amount should not be included in the recycled amount)</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____] [cubic yards][tons],[cubic meters] as appropriate</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/></SPT>
</SPT><SPT><TTL>WASTE MANAGEMENT AND DISPOSAL</TTL><BRK/>
<BRK/>
<SPT><TTL><SUB>Waste Determination Documentation</SUB></TTL><BRK/>
<BRK/>
<TXT>Complete a Waste Determination form (provided at the pre-construction conference) for Contractor-derived wastes to be generated.  All potentially 
hazardous solid waste streams that are not subject to a specific exclusion or exemption from the hazardous waste regulations (e.g., scrap metal, 
domestic sewage) or subject to special rules, (lead-acid batteries and precious metals) must be characterized in accordance with the requirements 
of <RID>40 CFR 262.11</RID> or corresponding applicable state or local regulations.  Base waste determination on user knowledge of the processes and materials 
used, and analytical data when necessary.  Consult with the Installation environmental staff for guidance on specific requirements.  Attach support 
documentation to the Waste Determination form.  As a minimum, provide a Waste Determination form for the following waste (this listing is not exhaustive): 
oil- and latex -based painting and caulking products, solvents, adhesives, aerosols, petroleum products, and containers of the original materials.</TXT><BRK/>
<BRK/>
[<SPT><TTL>Sampling and Analysis of Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph when the project generates HW that are not identified in 40 CFR 261, Hazardous Waste 
Listing.</NPR><BRK/>
<BRK/>
<NPR>Coordinate with the Installation Environmental Office as applicable to determine if the installation provides 
sampling and analysis for Contractor Waste.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Waste Sampling</TTL><BRK/>
<BRK/>
<TXT>Sample waste in accordance with <RID>EPA SW-846</RID>.  Clearly mark each sampled drum or container with the Contractor's identification number, and cross 
reference to the chemical analysis performed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>Laboratory Analysis</SUB></TTL><BRK/>
<BRK/>
<TXT>Follow the analytical procedure and methods in accordance with the <RID>40 CFR 261</RID>.  Provide analytical results and reports performed to the Contracting 
Officer.  Coordinate all activities with Installation Hazardous Waste Manager.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Analysis Type</TTL><BRK/>
<BRK/>
<TXT>Identify hazardous waste by analyzing for the following characteristics:[ ignitability,][ corrosivity,][ reactivity,][ toxicity based on TCLP results,] 
[_____].</TXT><BRK/>
<BRK/></SPT>
</SPT>]</SPT><SPT><TTL>Solid Waste Management</TTL><BRK/>
<BRK/>
<SPT><TTL><SUB>Project Solid Waste Disposal Documentation Report</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Select bracketed item when sales documentation is not available.  Revise close out submittal to include 
Contractor Certification instead of the sales documentation.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide copies of the waste handling facilities' weight tickets, receipts, bills of sale, and other <SUB>sales documentation</SUB>.  In lieu of sales documentation, 
a statement indicating the disposal location for the solid waste that is signed by an employee authorized to legally obligate or bind the firm 
may be submitted.  The sales documentation[ <SUB>Contractor certification</SUB>] must include the receiver's tax identification number and business, EPA or 
state registration number, along with the receiver's delivery and business addresses and telephone numbers.  For each solid waste retained for 
the Contractor's own use, submit the information previously described in this paragraph on the solid waste disposal report.  Prices paid or received 
do not have to be reported to the Contracting Officer unless required by other provisions or specifications of this Contract or public law.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Control and Management of Solid Wastes</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Select appropriate disposal alternative.  In some states certain quantities of clearing debris may be classified 
as solid waste.  Include appropriate language to comply with State requirements.  Remove non-applicable bracketed 
options.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Pick up solid wastes, and place in covered containers that are regularly emptied.  Do not prepare or cook food on the project site.  Prevent contamination 
of the site or other areas when handling and disposing of wastes.  At project completion, leave the areas clean.  Employ segregation measures so 
that no hazardous or toxic waste will become co-mingled with non-hazardous solid waste.[  Transport solid waste off Government property and dispose 
of it in compliance with <RID>40 CFR 260</RID>, state, and local requirements for solid waste disposal.  A Subtitle D RCRA permitted landfill is the minimum 
acceptable offsite solid waste disposal option.  Verify that the selected transporters and disposal facilities have the necessary permits and licenses 
to operate.][  Haul waste materials to the Government landfill site[ shown on the drawings][ designated by the Contracting Officer].][  Comply 
with site procedures.][  Segregate and separate treated wood components disposed at a lined landfill approved to accept this waste in accordance 
with local and state regulations]  Solid waste disposal offsite must comply with most stringent local, state, and federal requirements, including <RID>
40 CFR 241</RID>, <RID>40 CFR 243</RID>, and <RID>40 CFR 258</RID>.</TXT><BRK/>
<BRK/>
<TXT>Manage hazardous material used in construction, including but not limited to, aerosol cans, waste paint, cleaning solvents, contaminated brushes, 
and used rags, in accordance with <RID>49 CFR 173</RID>.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Control and Management of Hazardous Waste</TTL><BRK/>
<BRK/>
<TXT>Do not dispose of hazardous waste on Government property.  Do not discharge any waste to a sanitary sewer, storm drain, or to surface waters or 
conduct waste treatment or disposal on Government property without written approval of the Contracting Officer and Installation Hazardous Waste 
Manager.</TXT><BRK/>
<BRK/>
<SPT><TTL><SUB>Hazardous Waste/Debris Management</SUB></TTL><BRK/>
<BRK/>
<TXT>Identify construction activities that will generate hazardous waste or debris.  Provide a documented waste determination for resultant waste streams.  
Identify, label, handle, store, and dispose of hazardous waste or debris in accordance with federal, state, and local regulations, including <RID>40 CFR 261</RID>
, <RID>40 CFR 262</RID>, <RID>40 CFR 263</RID>, <RID>40 CFR 264</RID>, <RID>40 CFR 265</RID>, <RID>40 CFR 266</RID>, and <RID>40 CFR 268</RID>.</TXT><BRK/>
<BRK/>
<TXT>Manage hazardous waste in accordance with the approved Hazardous Waste Management Section of the EPP.  Store hazardous wastes in approved containers 
in accordance with <RID>49 CFR 173</RID> and <RID>49 CFR 178</RID>.  Hazardous waste generated within the confines of Government facilities is identified as being generated 
by the Government.  Prior to removal of any hazardous waste from Government property, hazardous waste manifests must be signed by personnel from 
the Installation Environmental Office.  Do not bring hazardous waste onto Government property.  Provide the Contracting Officer with a copy of 
waste determination documentation for any solid waste streams that have any potential to be hazardous waste or contain any chemical constituents 
listed in <RID>40 CFR 372</RID>-SUBPART D.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Waste Storage/Satellite Accumulation/90 Day Storage Areas</TTL><BRK/>
<BRK/>
<TXT>Accumulate hazardous waste at satellite accumulation points and in compliance with <RID>40 CFR 262</RID> and applicable state or local regulations.  Individual 
waste streams will be limited to<MET> 208 liter</MET><ENG> 55 gallons</ENG> of accumulation (or<MET> 0.95 liter</MET><ENG> one quart</ENG> for acutely hazardous wastes).  If the Contractor 
expects to generate hazardous waste at a rate and quantity that makes satellite accumulation impractical, the Contractor may request a temporary 
90-day or 180-day, as appropriate, accumulation point be established.  Submit a request in writing to the Contracting Officer and provide the following 
information (Attach Site Plan to the Request):</TXT><BRK/>
<TAB>
<WBK>
   <STS/>
   <TDA COLUMNCOUNT="2" ROWCOUNT="9">
      <COL AUTOWIDTH="0" WIDTH="380.25"/>
      <COL AUTOWIDTH="0" WIDTH="380.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="16.50">
         <CEL>
<DTA TYPE="STRING">Contract Number</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="16.50">
         <CEL>
<DTA TYPE="STRING">Contractor</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="16.50">
         <CEL>
<DTA TYPE="STRING">Haz/Waste or Regulated Waste POC</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="16.50">
         <CEL>
<DTA TYPE="STRING">Phone Number</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="16.50">
         <CEL>
<DTA TYPE="STRING">Type of Waste</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="16.50">
         <CEL>
<DTA TYPE="STRING">Source of Waste</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="16.50">
         <CEL>
<DTA TYPE="STRING">Emergency POC</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="16.50">
         <CEL>
<DTA TYPE="STRING">Phone Number</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="47.25">
         <CEL>
<DTA TYPE="STRING">Location of the Site</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">[_____]</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<TXT>Attach a Waste Determination form for the expected waste streams.  Allow 10 working days for processing this request.  Additional compliance requirements 
(e.g., training and contingency planning) that may be required are the responsibility of the Contractor.  Barricade the designated area where waste 
is being stored and post a sign identifying as follows:</TXT><BRK/>
<BRK/>
<LST>"DANGER - UNAUTHORIZED PERSONNEL KEEP OUT"</LST><BRK/>
<BRK/></SPT>
<SPT><TTL>Hazardous Waste Disposal</TTL><BRK/>
<BRK/>
[<SPT><TTL>Responsibilities for Contractor's Disposal</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose this paragraph for Contractor Disposal of the Hazardous Waste.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide hazardous waste manifest to the Installations Environmental Office for review, approval, and signature prior to shipping waste off Government 
property.</TXT><BRK/>
<BRK/>
<SPT><TTL>Services</TTL><BRK/>
<BRK/>
<TXT>Provide service necessary for the final treatment or disposal of the hazardous material or waste in accordance with <RID>40 CFR 260</RID> - <RID>40 CFR 279</RID>, local, 
and state, laws and regulations, and the terms and conditions of the Contract within 60 days after the materials have been generated.  These services 
include necessary personnel, labor, transportation, packaging, detailed analysis (if required for disposal or transportation, include manifesting 
or complete waste profile sheets, equipment, and compile documentation).</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Samples</TTL><BRK/>
<BRK/>
<TXT>Obtain a representative sample of the material generated for each job done to provide waste stream determination.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Analysis</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph when the project generates HW that are not identified in 40 CFR 261, Hazardous Waste 
Listing.</NPR><BRK/>
<BRK/>
<NPR>Coordinate with the Installation Environmental Office as applicable to determine if the installation provides 
sampling and analysis for Contractor Waste.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Analyze each sample taken and provide analytical results to the Contracting Officer.  See paragraph WASTE DETERMINATION DOCUMENTATION.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Labeling</TTL><BRK/>
<BRK/>
<TXT>During waste accumulation label all containers in accordance with <RID>40 CFR 262</RID>.  Prior to offering a waste for off-site transport, determine the 
Department of Transportation's (DOT's) proper shipping names for waste in accordance with <RID>49 CFR 172</RID> (each container requiring disposal) and demonstrate 
to the Contracting Officer how this determination is developed and supported by the sampling and analysis requirements contained herein.  Label 
all containers of hazardous waste with the words "Hazardous Waste" or other words to describe the contents of the container in accordance with <RID>
40 CFR 262</RID> and applicable state or local regulations.</TXT><BRK/>
<BRK/></SPT>
</SPT>][<SPT><TTL>Contractor Disposal Turn-In Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose this paragraph if Contractor will turn-in waste into an Installation's waste accumulation facilities.  
Coordinate with the Installations Environmental Office to further edit this paragraph to meet Installation requirements.  
Contractor will not prepare manifest documentation when this option of disposal is selected.  Coordinate language 
in other paragraphs to clarify manifesting requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Hazardous waste generated must be disposed of in accordance with the following conditions to meet installation requirements:</TXT><BRK/>
<OLG><BRK/>
<OLI>Drums must be compatible with waste contents and drums must meet DOT requirements for <RID>49 CFR 173</RID> for transportation of materials.</OLI><BRK/>
<BRK/>
<OLI>Band drums to wooden pallets.</OLI><BRK/>
<BRK/>
<OLI>No more than three<MET> 208 liter</MET><ENG> 55 gallon</ENG> drums or two<MET> 321 liter</MET><ENG> 85 gallon</ENG> over packs are to be banded to a pallet.</OLI><BRK/>
<BRK/>
<OLI>Band using<MET> 32 millimeters</MET><ENG> 1-1/4 inch</ENG> minimum band on upper third of drum.</OLI><BRK/>
<BRK/>
<OLI>Provide label in accordance with <RID>49 CFR 172.101</RID>.</OLI><BRK/>
<BRK/>
<OLI>Leave<MET> 7 to 12 centimeters</MET><ENG> 3 to 5 inches</ENG> of empty space above volume of material.</OLI><BRK/></OLG>
<BRK/></SPT>
]</SPT><SPT><TTL>Universal Waste Management</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following list contains tailoring for ARMY and NAVY</NPR><BRK/>
<BRK/>
<NPR>State requirements may differ from federal regulation.  Use last ARMY tailored item for Army projects only.  For 
Navy projects, use NAVY tailored item for additional requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Manage the following categories of universal waste in accordance with federal, state, and local requirements and installation instructions:</TXT><BRK/>
<BRK/>
<LST INDENT="-0.33">a.  Batteries as described in <RID>40 CFR 273.2</RID></LST><BRK/>
<BRK/>
<LST INDENT="-0.33">b.  Lamps as described in <RID>40 CFR 273.5</RID></LST><BRK/>
<BRK/>
<LST INDENT="-0.33">c.  Mercury-containing equipment as described in <RID>40 CFR 273.4</RID></LST><BRK/>
<BRK/>
<LST INDENT="-0.33">d.  Aerosol cans as described in <RID>40 CFR 273.6</RID></LST><BRK/>
<BRK/>
<TAI OPT="ARMY"><LST INDENT="-0.33">e.  Pesticides as described in <RID>40 CFR 273.3</RID></LST><BRK/>
<BRK/></TAI>
<TAI OPT="NAVY"><LST INDENT="-0.33">e.  Installation specific</LST><BRK/>
<BRK/></TAI>
<TXT>Mercury is prohibited in the construction of this facility, unless specified otherwise, and with the exception of mercury vapor lamps and fluorescent 
lamps.  Dumping of mercury-containing materials and devices such as mercury vapor lamps, fluorescent lamps, and mercury switches, in rubbish containers 
is prohibited.  Remove without breaking, pack to prevent breakage, and transport out of the activity in an unbroken condition for disposal as directed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Electronics End-of-Life Management</TTL><BRK/>
<BRK/>
<TXT>Recycle or dispose of electronics waste, including, but not limited to, used electronic devices such computers, monitors, hard-copy devices, televisions, 
mobile devices, in accordance with <RID>40 CFR 260</RID>-262, state, and local requirements, and installation instructions.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>Disposal Documentation for Hazardous and Regulated Waste</SUB></TTL><BRK/>
<BRK/>
<TXT>Contact the Contracting Officer [or designated representative ]for the facility RCRA identification number that is to be used on each manifest.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following bracketed item for Navy projects only.  Coordinate with installation special requirements.  
A Base Environmental point of contact will be identified for Base specific requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Submit a copy of the applicable EPA and or state permit(s), manifest(s), or license(s) for transportation, treatment, storage, and disposal of 
hazardous and regulated waste by permitted facilities.  Hazardous or toxic waste manifests must be reviewed, signed, and approved by the Contracting 
Officer before the Contractor may ship waste.  To obtain specific disposal instructions, coordinate with the Installation Environmental Office.  
Refer to location special requirements for the Installation Point of Contact information.</TXT><BRK/>
<BRK/>
]</SPT></SPT><SPT><TTL>Releases/Spills of Oil and Hazardous Substances</TTL><BRK/>
<BRK/>
<SPT><TTL>Response and Notifications</TTL><BRK/>
<BRK/>
<TXT>Exercise due diligence to prevent, contain, and respond to spills of hazardous material, hazardous substances, hazardous waste, sewage, regulated 
gas, petroleum, lubrication oil, and other substances regulated in accordance with <RID>40 CFR 300</RID>.  Maintain spill cleanup equipment and materials 
at the work site.  In the event of a spill, take prompt, effective action to stop, contain, curtail, or otherwise limit the amount, duration, and 
severity of the spill/release.  In the event of any releases of oil and hazardous substances, chemicals, or gases; immediately (within 15 minutes) 
notify the Installation Fire Department, the Installation Command Duty Officer, the Installation Environmental Office, the Contracting Officer[ 
and the state or local authority].</TXT><BRK/>
<BRK/>
<TXT>Submit verbal and written notifications as required by the federal (<RID>40 CFR 300.125</RID> and <RID>40 CFR 355</RID>), state, local regulations and instructions.  
Provide copies of the written notification and documentation that a verbal notification was made within 20 days.  Spill response must be in accordance 
with <RID>40 CFR 300</RID> and applicable state and local regulations.  Contain and clean up these spills without cost to the Government.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Clean Up</TTL><BRK/>
<BRK/>
<TXT>Clean up hazardous and non-hazardous waste spills.  Reimburse the Government for costs incurred including sample analysis materials, clothing, 
equipment, and labor if the Government will initiate its own spill cleanup procedures, for Contractor- responsible spills, when: Spill cleanup 
procedures have not begun within one hour of spill discovery/occurrence; or, in the Government's judgment, spill cleanup is inadequate and the 
spill remains a threat to human health or the environment.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Mercury Materials</TTL><BRK/>
<BRK/>
<TXT>Immediately report to the Environmental Office and the Contracting Officer instances of breakage or mercury spillage.  Clean mercury spill area 
to the satisfaction of the Contracting Officer.</TXT><BRK/>
<BRK/>
<TXT>Do not recycle a mercury spill cleanup; manage it as a hazardous waste for disposal.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Wastewater</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate with the Installation Environmental Office as applicable.  Identify and obtain permits required 
by governing agencies.  Insert or delete the brackets with the name of process producing the wastewater.  If there 
is an area on the project site for a retention pond, a choice may be given for disposal in a retention pond.  
If there is a possibility that the water is contaminated, then identify and specify the appropriate analytical 
testing be performed.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Disposal of Wastewater</TTL><BRK/>
<BRK/>
<TXT>Disposal of wastewater must be as specified below.</TXT><BRK/>
<BRK/>
<SPT><TTL>Treatment</TTL><BRK/>
<BRK/>
<TXT>Do not allow wastewater from construction activities, such as onsite material processing, concrete curing, foundation and concrete clean-up, water 
used in concrete trucks, and forms to enter water ways or to be discharged into the stormwater system or sanitary sewer system..  Dispose of the 
construction- related waste water[ off-Government property in accordance with <RID>40 CFR 403</RID>, state, regional, and local laws and Prior to disposal, 
submit a WIS to the Installation Environmental Office and have the results reviewed and approved by the Contracting Officer prior to being discharged 
or disposed of off- Government property].</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Surface Discharge</TTL><BRK/>
<BRK/>
<TXT>For discharge of ground water,[ obtain a state or federal permit specific for pumping and discharging ground water prior to surface discharging.][  
Surface discharge in accordance with federal, state, and local laws and regulations.][  Surface discharge in accordance with the requirements of 
the NPDES or state STORMWATER DISCHARGES FROM CONSTRUCTION SITES permit.]</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Land Application</TTL><BRK/>
<BRK/>
<TXT>Water generated from the flushing of lines after[ disinfection or disinfection in conjunction with hydrostatic testing][ hydrostatic testing] must 
be[ land- applied in accordance with federal, state, and local laws and regulations for land application][ discharged into the sanitary sewer with 
prior approval and notification to the Wastewater Treatment Plant's Operator].</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT></SPT><SPT><TTL>HAZARDOUS MATERIAL MANAGEMENT</TTL><BRK/>
<BRK/>
<TXT>Include hazardous material control procedures in the Accident Prevention Plan (APP), in accordance with Section <SRF>01 35 26</SRF> GOVERNMENTAL SAFETY REQUIREMENTS.  
Address procedures and proper handling of hazardous materials, including the appropriate transportation requirements.  Do not bring hazardous material 
onto Government property that does not directly relate to requirements for the performance of this contract.  Submit an SDS and estimated quantities 
to be used for each hazardous material to the Contracting Officer prior to bringing the material on the installation.  Typical materials requiring 
SDS and quantity reporting include, but are not limited to, oil and latex based painting and caulking products, solvents, adhesives, aerosol, and 
petroleum products.  Use hazardous materials in a manner that minimizes the amount of hazardous waste generated.  Containers of hazardous materials 
must have National Fire Protection Association labels or their equivalent.  Certify that hazardous materials removed from the site are hazardous 
materials and do not meet the definition of hazardous waste, in accordance with <RID>40 CFR 261</RID> and state[ and installation] requirements.</TXT><BRK/>
<BRK/>
<TAI OPT="NAVY"><SPT><TTL><SUB>Contractor Hazardous Material Inventory Log</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for NAVY.  Use this paragraph for Navy projects only.  Delete for other 
projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Submit the "Contractor Hazardous Material Inventory Log"(found at: <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs<BRK/>
/forms-graphics-tables</URL>), which provides information required by (EPCRA Sections 312 and 313) along with corresponding SDS, to the Contracting Officer 
at the start and at the end of construction (30 days from final acceptance), and update no later than January 31 of each calendar year during the 
life of the contract.  Keep copies of the SDSs for hazardous materials onsite. At the end of the project, provide the Contracting Officer with 
copies of the SDSs, and the maximum quantity of each material that was present at the site at any one time, the dates the material was present, 
the amount of each material that was used during the project, and how the material was used.</TXT><BRK/>
<BRK/>
<TXT>The Contracting Officer may request documentation for any spills or releases, environmental reports, or off-site transfers.</TXT><BRK/>
<BRK/></SPT>
</TAI></SPT><SPT><TTL>PREVIOUSLY USED EQUIPMENT</TTL><BRK/>
<BRK/>
<TXT>Clean previously used construction equipment prior to bringing it onto the project site.  Equipment must be free from soil residuals, egg deposits 
from plant pests, noxious weeds, and plant seeds.  Consult with the U.S. Department of Agriculture jurisdictional office for additional cleaning 
requirements.</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>CONTROL AND MANAGEMENT OF ASBESTOS-CONTAINING MATERIAL (ACM)</TTL><BRK/>
<BRK/>
<TXT>Manage and dispose of asbestos- containing waste in accordance with all applicable federal, state, and local (or Host Nation) requirements.  Refer 
to Section <SRF>02 82 00</SRF> ASBESTOS REMEDIATION.  Manifest asbestos-containing waste and provide the manifest to the Contracting Officer.  Notifications 
to the regulatory authorities and Installation Air Program Manager are required before starting any asbestos work.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>CONTROL AND MANAGEMENT OF LEAD-BASED PAINT (LBP)</TTL><BRK/>
<BRK/>
<TXT>Manage and dispose of lead-contaminated waste in accordance with <RID>40 CFR 745</RID> and Section <SRF>02 83 00</SRF> LEAD REMEDIATION.  Manifest any lead-contaminated 
waste and provide the manifest to the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>CONTROL AND MANAGEMENT OF POLYCHLORINATED BIPHENYLS (PCBs)</TTL><BRK/>
<BRK/>
<TXT>Manage and dispose of PCB-contaminated waste in accordance with <RID>40 CFR 761</RID> and Section <SRF>02 84 33</SRF> REMOVAL AND DISPOSAL OF POLYCHLORINATED BIPHENYLS 
(PCBs).</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>CONTROL AND MANAGEMENT OF LIGHTING BALLAST AND LAMPS CONTAINING PCBs</TTL><BRK/>
<BRK/>
<TXT>Manage and dispose of contaminated waste in accordance with <RID>40 CFR 761</RID>.[  Refer to Section <SRF>02 84 16</SRF> HANDLING OF LIGHTING BALLASTS AND LAMPS CONTAINING 
PCBs AND MERCURY.]</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>MILITARY MUNITIONS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Delete this paragraph if not needed in the project</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>In the event military munitions, as defined in <RID>40 CFR 260</RID>, are discovered or uncovered, immediately stop work in that area and immediately inform 
the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>PETROLEUM, OIL, LUBRICANT (POL) STORAGE AND FUELING</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose one of the last bracketed sentences after coordination with the Installation Environmental Office.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>POL products include flammable or combustible liquids, such as gasoline, diesel, lubricating oil, used engine oil, hydraulic oil, mineral oil, 
and cooking oil.  Store POL products and fuel equipment and motor vehicles in a manner that affords the maximum protection against spills into 
the environment.  Manage and store POL products in accordance with EPA <RID>40 CFR 112</RID>, and other federal, state, regional, and local laws and regulations.  
Use secondary containments, dikes, curbs, and other barriers, to prevent POL products from spilling and entering the ground, storm or sewer drains, 
stormwater ditches or canals, or navigable waters of the United States.  Describe in the EPP (see paragraph ENVIRONMENTAL PROTECTION PLAN) how 
POL tanks and containers must be stored, managed, and inspected and what protections must be provided.[  Storage of oil, including fuel, on the 
project site is not allowed.  Fuel must be brought to the project site each day that work is performed.][  Storage of fuel on the project site 
must be in accordance with EPA, state, and local laws and regulations and paragraph OIL STORAGE INCLUDING FUEL TANKS.] </TXT><BRK/>
<BRK/>
<SPT><TTL>Used Oil Management</TTL><BRK/>
<BRK/>
<TXT>Manage used oil generated on site in accordance with <RID>40 CFR 279</RID>.  Determine if any used oil generated while onsite exhibits a characteristic of 
hazardous waste.  Used oil containing 1,000 parts per million of solvents is considered a hazardous waste and disposed of at the Contractor's expense.  
Used oil mixed with a hazardous waste is also considered a hazardous waste.  Dispose in accordance with paragraph HAZARDOUS WASTE DISPOSAL.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Oil Storage Including Fuel Tanks</TTL><BRK/>
<BRK/>
<TXT>Provide secondary containment and overfill protection for oil storage tanks.  A berm used to provide secondary containment must be of sufficient 
size and strength to contain the contents of the tanks plus<MET> 12 centimeters</MET><ENG> 5 inches</ENG> freeboard for precipitation.  Construct the berm to be impervious 
to oil for 72 hours that no discharge will permeate, drain, infiltrate, or otherwise escape before cleanup occurs.  Use drip pans during oil transfer 
operations; adequate absorbent material must be onsite to clean up any spills and prevent releases to the environment.  Cover tanks and drip pans 
during inclement weather.  Provide procedures and equipment to prevent overfilling of tanks.  If tanks and containers with an aggregate aboveground 
capacity greater than<MET> 5000 liter</MET><ENG> 1320 gallons</ENG> will be used onsite (only containers with a capacity of<MET> 208 liter</MET><ENG> 55 gallons</ENG> or greater are counted), 
provide and implement a <SUB>Spill Prevention Control and Countermeasure (SPCC) plan</SUB> meeting the requirements of <RID>40 CFR 112</RID>.  Do not bring underground 
storage tanks to the installation for Contractor use during a project.  Submit the SPCC plan to the Contracting Officer for approval.</TXT><BRK/>
<BRK/>
<TXT>Monitor and remove any rainwater that accumulates in open containment dikes or berms.  Inspect the accumulated rainwater prior to draining from 
a containment dike to the environment, to determine there is no oil sheen present.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>INADVERTENT DISCOVERY OF PETROLEUM-CONTAMINATED SOIL OR HAZARDOUS WASTES</TTL><BRK/>
<BRK/>
<TXT>If petroleum-contaminated soil, or suspected hazardous waste is found during construction that was not identified in the Contract documents, immediately 
notify the Contracting Officer.  Do not disturb this material until authorized by the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ARMY"><SPT><TTL>PEST MANAGEMENT</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following Article is tailored for ARMY.  Use the following paragraphs for Army projects only.  Do not 
use for Navy or Air Force projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  DoD Installations are required under DoDI 4150.7 to develop an integrated pest management plan (IPMP).  
This does not apply to USACE Civil Works Projects.  The Facility IPMP has been developed by the installation to 
identify potential pest-related risks of damage to installation properties as well as approaches to be used to 
limit these risks.  The Designer should coordinate with the Installation Pest Management Coordinator early in 
the design process to address structural, landscaping and other pest damage reduction alternatives to pesticide 
applications when cost effective.  This effort may be multidisciplinary in scope (e.g., planner/landscape architect 
and natural resource manager).  The pest management plans and strategies developed during design and construction 
should be reviewed and approved by DoD pest management professionals and coordinated with IPMC as required by 
DA AR 200-1 and DoDI 4150.7.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is to be used when the application of pest management chemicals is OR is NOT anticipated.  
These requirements must be included as a plan within the Environmental Protection Plan.  When a pest is known 
to be in the soil, identify the pest and the area to be treated.  This paragraph should be left intact to cover 
pesticides applications not anticipated by the Designer.  When termiticide is required, include the bracketed 
sentence and Section <SRF>33 40 00</SRF> STORMWATER UTILITIES in the contract specifications.  Delete last sentence when 
not applicable.  The "installation pest management coordinator" is a term used in DA AR 200-1.  DA AR 200-1 is 
not applicable to USACE Civil Works activities.  Appropriate USACE personnel should be referenced when this specification 
is used for civil works.  See CECW-ON EP 1130-2-540 ENVIRONMENTAL STEWARDSHIP OPERATIONS AND MAINTENANCE GUIDANCE 
AND PROCEDURES, Chapter 3 - Pest Control Program for Civil Works Projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>In order to minimize impacts to existing fauna and flora, coordinate with the Installation Pest Management Coordinator (IPMC) or Project Pesticide 
Coordinator (PPC), through the Contracting Officer, at the earliest possible time prior to pesticide application.  Discuss integrated pest management 
strategies including prevention of invasive species as applicable with the [IPMC][PPC] and receive concurrence from the [IPMC][PPC] through the 
Contracting Officer prior to the application of any pesticide associated with these specifications.  Provide Installation Project Office Pest Management 
personnel the opportunity to be present at meetings concerning treatment measures for pest or disease control and during application of the pesticide.[  
For termiticide requirements, see[ Section <SRF>31 31 16.13</SRF> CHEMICAL TERMITE CONTROL][ Section <SRF>31 31 16.19</SRF> TERMITE CONTROL BARRIERS]]  The use and management 
of pesticides are regulated under <RID>40 CFR 152 - 186</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Application</TTL><BRK/>
<BRK/>
<TXT>Apply pesticides using a state-certified pesticide applicator in accordance with EPA label restrictions and recommendation.  The certified applicator 
must wear clothing and personal protective equipment as specified on the pesticide label.  The Contracting Officer will designate locations for 
water used in formulating.  Do not allow the equipment to overflow.  Inspect equipment for leaks, clogging, wear, or damage and repair prior to 
application of pesticide.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Pesticide Treatment Plan</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The pesticide treatment plan serves two purposes:  It provides a mechanism for early coordination with 
the appropriate installation personnel through the Contracting Officer and provides a mechanism for reporting 
pesticide use information to the Installation as required by the Federal Insecticide Fungicide and Rodenticide 
Act (FIFRA).  For military construction, this information must be provided to the Installation under DoDI 4150.7 
DoD Pest Management Instruction, under DA AR 200-1, Chapter 5--Pest Management.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Include and update a pesticide treatment plan, as information becomes available.  Include in the plan the sequence of treatment, dates, times, 
locations, pesticide trade name, EPA registration numbers, authorized uses, chemical composition, formulation, original and applied concentration, 
application rates of active ingredient (that is, pounds of active ingredient applied), equipment used for application and calibration of equipment.  
Comply with <RID>40 CFR 152</RID>-189, state, regional, and local pest management record-keeping and reporting requirements as well as any additional Installation 
Project Office specific requirements in conformance with [DA AR 200-1 Chapter 5, Pest Management, Section 5-4 "Program requirements"] for data 
required to be reported to the Installation.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>CHLORDANE</TTL><BRK/>
<BRK/>
<TXT>Evaluate excess soils and concrete foundation debris generated during the demolition of housing units or other wooden structures for the presence 
of chlordane or other pesticides prior to reuse or final disposal.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>SOUND INTRUSION</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Insert State's name or remove last sentence when State rules are not applicable.  Include any facility 
specific requirements such as operational hours around base housing.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Make the maximum use of low-noise emission products, as certified by the EPA.  Blasting or use of explosives are not permitted without written 
permission from the Contracting Officer, and then only during the designated times.  Confine pile-driving operations to the period between [_____] 
[8 a.m.] and [_____] [4 p.m.], [_____] [Monday through Friday], exclusive of holidays, unless otherwise specified.</TXT><BRK/>
<BRK/>
<TXT>Keep construction activities under surveillance and control to minimize environment damage by noise.  Comply with the provisions of the State of 
[_____] rules.</TXT><BRK/>
<TAI OPT="ILLINOIS"><BRK/>
<NTE><AST/><BRK/>
<NPR>NOTE:  Use the following tailored paragraph for the State of Illinois.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Keep construction activities under surveillance and control to minimize environment damage by noise. Comply with the provisions of the State of 
Illinois rules given in <RID>35 IAC 900-901</RID>.</TXT><BRK/></TAI>
<BRK/></SPT>
<SPT><TTL>POST CONSTRUCTION CLEANUP</TTL><BRK/>
<BRK/>
<TXT>Clean up areas used for construction in accordance with Contract Clause: "Cleaning Up".  Unless otherwise instructed in writing by the Contracting 
Officer, remove traces of temporary construction facilities such as haul roads, work area, structures, foundations of temporary structures, stockpiles 
of excess or waste materials, and other vestiges of construction prior to final acceptance of the work.  Grade parking area and similar temporarily 
used areas to conform with surrounding contours.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="NAVFAC NW"><SPT><TTL>NORTHWEST (Washington and Oregon)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This Article is tailored for NAVFAC NW.  Use this paragraphs and subparagraphs for NAVFAC NW projects only.  
Delete for other projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Protection of Natural Resources</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following paragraphs as applicable for the work.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Only native species for the local area are permitted for use.</TXT><BRK/>
<BRK/>
]<TXT>[Implement landscaping and construction operations in a manner that prevents the spread of invasive species (for example, scotch broom, knotweed, 
butterfly bush).] [Damaged trees must be appraised.  Reimburse the Government for the lost tree value based on current rates at the time the damages 
occurred.]</TXT><BRK/>
<BRK/>
<SPT><TTL>Water Resources</TTL><BRK/>
<BRK/>
[<TXT>For Project work near streams, lakes, wetlands, or other waterways, maintain buffers as follows according to the Washington State Wetland Rating 
System established in <RID>WAC-222-30</RID>-021:</TXT><BRK/>
<BRK/>
<TXT>Wetland Buffer Width</TXT><BRK/>
<TAB WIDTH="90">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="5">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="378.00"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="306.00"/>
      <ROW AUTOHEIGHT="0" HEIGHT="19.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Category of Wetland</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Buffer Width</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="19.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Category I</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><MET>60 meter</MET><ENG> 200 feet</ENG></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="19.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Category II</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><MET>30 meter</MET><ENG> 100 feet</ENG></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="19.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Category III</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><MET>15 meter</MET><ENG> 50 feet</ENG></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="29.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Category IV</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><MET>9 meter</MET><ENG> 30 feet</ENG></DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<TXT>Riparian Zone Buffer Widths</TXT><BRK/>
<TAB WIDTH="90">
<WBK>
   <STS/>
   <TDA COLUMNCOUNT="2" ROWCOUNT="3">
      <COL AUTOWIDTH="0" WIDTH="381.00"/>
      <COL AUTOWIDTH="0" WIDTH="303.00"/>
      <ROW AUTOHEIGHT="0" HEIGHT="18.75">
         <CEL>
<DTA TYPE="STRING">Category of Water Body</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Buffer Width</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="32.25">
         <CEL>
<DTA TYPE="STRING">Contains habitat for salmonids, game fish, and other anadromous fish</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><MET>45 meter</MET><ENG> 150 feet</ENG></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="32.25">
         <CEL>
<DTA TYPE="STRING">Does not contain fish habitat</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><MET>15 meter</MET><ENG> 50 feet</ENG></DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
]</SPT><SPT><TTL>Groundwater</TTL><BRK/>
<BRK/>
<TXT>Construct, maintain, and decommission any wells and wellheads associated with, or impacted by, the project in accordance with Washington State 
Standards for Construction and Maintenance of Wells (<RID>WAC-173-160</RID>).</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Merchantable Timber</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph if trees or other forest products are present in areas to be cleared or disturbed, 
either temporarily or permanently (e.g,. geotechnical analysis, construction trailer placement, lay-down areas, 
stormwater ponds, road construction/reconstruction, utility placement, project implementation.)</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Contact the Contracting Officer prior to site disturbance to request a timber appraisal by a Navy Forester.  Delineate the limits of clearing on 
the ground in a manner that the boundary can be easily identified during timber appraisal.  Once delineation is complete, notify the Contracting 
Officer and allow [30][_____] days for timber appraisal.</TXT><BRK/>
<BRK/>
<TXT>Merchantable forest products such as timber and firewood must be appraised and payment received by the Government prior to disturbance or removal, 
in accordance with COMNAVREGNWINST 11015.1, Forest Product Sales and Permit Program.  Purchase, through the Navy Forestry program, merchantable 
forest products at a neutrally determined rate.  Timber value and related expenses are not reimbursable under any circumstance.  Federal timber 
may not be exported and timber excise tax is the responsibility of the purchaser.</TXT><BRK/>
<BRK/></SPT>
]</SPT>[<SPT><TTL>Historical and Archaeological Resources</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For NBK Bremerton and PSNS &amp; IMF, use archaeological probability map.  Include this paragraph as necessary 
for the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Excavation is in an area of [high][moderate] archaeological potential.</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Stormwater</TTL><BRK/>
<BRK/>
<SPT><TTL>EPA Construction General Permit (CGP)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph and subparagraphs when one or more acres (0.4 or more hectares) of total land area 
are to be disturbed or disturbs less than one acre but is part of a larger common plan of development or sale 
that will disturb one or more acres.  Coordinate with Installation Environmental Office to determine if project 
is part of larger common plan of development.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The contractor must comply with all the EPA CGP sampling, reporting, and recordkeeping provisions, and with the corrective action requirements.</TXT><BRK/>
<BRK/>
<TXT>The contractor must comply with any State, Tribal, or territory-specific requirements in the EPA CGP.</TXT><BRK/>
<BRK/>
<SPT><TTL>Stormwater Pollution Prevention Plan</TTL><BRK/>
<BRK/>
<TXT>A Construction Stormwater Pollution Prevention Plan (SWPPP) is required[ including mandatory Bremerton Naval Complex BMPs and Washington State 
Department of Ecology (WSDE) Stormwater Management Manual for Western Washington BMPs].  Use the EPA SWPPP template available at <URL HREF="https://www.epa.gov/npdes/construction-general-permit-resources-tools-and-templates">https://www.epa.gov/npdes/construction-general-permit-resources-tools-and-templates</URL>
 to prepare the Construction SWPPP in accordance with the requirements in <RID>84 FR 24503</RID>, the EPA CGP and any applicable MS4 permit requirements (see 
paragraph MUNICIPAL SEPARATE STORM SEWER SYSTEM (MS4) PERMIT MANAGEMENT).  The Construction SWPPP must be completed and approved prior to submitting 
the Notice of Intent.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Stormwater Notice of Intent (NOI) for Construction Activities</TTL><BRK/>
<BRK/>
<TXT>Upon Government approval of the SWPPP, submit a draft NOI for the EPA CGP to the Government for approval 4 weeks before commencement of construction 
activities.  The NOI must be approved prior to EPA submittal.  The NOI must be approved by EPA prior to commencing construction activities.  Note 
that EPA imposes a mandatory 14-day wait after receiving the NOI before construction activities that could lead to the generation of pollutants 
may begin.  Only electronic submittals to EPA via NPDES eReporting tool (NeT) are acceptable.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Inspection Reports</TTL><BRK/>
<BRK/>
<TXT>Site inspections must be conducted by a qualified person to verify permit compliance in accordance with the EPA CGP.  By the initiation of construction, 
the Construction SWPPP must identify the inspector, who must be present on site or on-call at all times, in accordance with the <RID>WSDE SWMMWW</RID>.  The 
Construction SWPPP must also designate inspection frequency in compliance with EPA CGP inspection requirements.</TXT><BRK/>
<BRK/>
<TXT>Complete inspections and reports as required by the EPA CGP and MS4 permit.  Submit completed inspection reports to the Installation Environmental 
Office within two working days of the inspection.  Report any condition triggering corrective action per the EPA CGP to the contracting officer 
and Installation Environmental Office immediately.  Photographs must be taken prior to site stabilization to support Notice of Termination documentation 
requirements.  Take photographs prior to meeting final stabilization criteria in support of Notice of Termination requirements.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Stormwater Pollution Prevention Plan Compliance Notebook</TTL><BRK/>
<BRK/>
<TXT>Keep the SWPPP updated and maintain it on the construction site.  Keep a copy of all inspection reports at the site or at an easily accessible 
location, so that they can be made immediately available at the time of an on-site inspection or upon request.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Stormwater Notice of Termination (NOT) for Construction Activities</TTL><BRK/>
<BRK/>
<TXT>Upon completion of construction, submit the NOT to the Government for approval prior to submitting to the NOT of coverage under the CGP to the 
EPA.  Refer to electronic NOI webpage for electronic submission of the NOT.  Include site stabilization photographs as required by the EPA CGP.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Public Notice</TTL><BRK/>
<BRK/>
<TXT>Post a notice near the main entrance of the construction site with a copy of the NOI, Contractor name, name and phone number of a local contact 
person (Construction Manager's office), brief description of the project, and the location of the SWPPP.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Erosion and Sediment Control Measures</TTL><BRK/>
<BRK/>
<TXT>Erosion control BMPs must be selected for the site to meet the requirements 
of the <RID>WSDE SWMMWW</RID>.</TXT><BRK/>
<BRK/>
<TXT>The contractor must implement erosion and sediment controls and pollution prevention practices throughout the entire construction project.  The 
contractor must conduct routine maintenance and take corrective action to fix problems with controls or discharges.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following text for work at NBK Bremerton and NAVSTA Everett.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[ <TXT>Use of straw or hay bales is prohibited.</TXT><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Include the following text for work at NBK Bangor.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>If straw is used as an erosion control BMP, it must be certified weed free.</TXT><BRK/>
<BRK/>
]</SPT><SPT><TTL>Municipal Separate Storm Sewer System (MS4) Permit Management</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for work at NBK (excepting NBK Bremerton and Manchester), NASWI (except Outlying 
Airfield Coupeville), and NS Everett (except Jim Creek).</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>A Construction SWPPP is required for construction sites exceeding thresholds in the <RID>WSDE SWMMWW</RID>, in accordance with the installation MS4 Permit.  
If the project is less than one acre, the Contracting Officer will provide a Construction SWPPP template to the Contractor at the pre-construction 
meeting to prepare the construction SWPPP in accordance with the <RID>WSDE SWMMWW</RID>.  The SWPPP must also meet EPA CGP requirements, if applicable.  Sites 
below <RID>WSDE SWMMWW</RID> thresholds are not required to prepare a Construction SWPPP, but must consider all of the Construction SWPPP Elements and develop 
controls for all Construction SWPPP Elements that pertain to the project site.</TXT><BRK/>
<BRK/>
<TXT>Maintain stormwater BMPs and manage construction sites in accordance with MS4 permit requirements, this Section, and minimum requirements listed 
in the <RID>WSDE SWMMWW</RID>.  In Airport Operation Areas (AOA), prepare stormwater site plans consistent with the Aviation Stormwater Design Manual (2008).  
For road projects, prepare the design requirements and best management practices consistent with the Highway Runoff Manual (WSDOT 2019).  To avoid 
washing pollutants into the MS4, the amount of street wash and dust control water used must be minimized.  At active construction sites, street 
sweeping must be performed prior to washing the street.  Discharges to the storm sewer that are not entirely composed of storm water are prohibited 
unless coordinated in advance with the Installation Environmental Office.  In particular, discharges from potable water sources, including but 
not limited to water line flushing, hyper-chlorinated water line flushing, fire hydrant system flushing, and pipeline hydrostatic test water, must 
be dechlorinated to a total residual chlorine concentration of 0.1 parts per million (ppm) or less, pH-adjusted, if necessary, and volumetrically 
and velocity controlled to prevent resuspension of sediments in the MS4.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Surface and Groundwater</TTL><BRK/>
<BRK/>
<SPT><TTL>Cofferdams, Diversions, and Dewatering</TTL><BRK/>
<BRK/>
<TXT>The contractor must comply with turbidity monitoring requirements for dewatering discharges to sensitive waters of the United States.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following subparagraph for work<BRK/>
at NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Perform dewatering of excavation sites as specified in the Groundwater/Stormwater Flow Chart.  Coordinate requirements with Section <SRF>31 00 00</SRF> EARTHWORK.</TXT><BRK/>
<BRK/>
<TXT>Submit a <ATT><SUB>Storm Drain and Sanitary Sewer Discharge Approval</SUB></ATT> form to obtain approval before discharging uncontaminated water into storm drain.</TXT><BRK/>
<BRK/>
]</SPT></SPT>[<SPT><TTL>Concrete Operations</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this subparagraph as applicable for the work.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Sawcutting and rinse water must be collected and managed as waste.  Sawcutting and rinse water is not allowed to be infiltrated nor discharged 
to the stormwater system.  Dispose of collected waste as directed by the Installation Environmental Office.</TXT><BRK/>
<BRK/>
][<SPT><TTL>Washing of Concrete Truck</TTL><BRK/>
<BRK/>
<TXT>Concrete trucks are prohibited from being washed on station without approval from the Installation Environmental Office.  Approved washout station 
must be on a project site that is going to be a future pour site (for example, a foundation) or have an impermeable barrier to prevent infiltration 
of the concrete wash water.  The approved washout location must not be subject to surface water runoff and is more than<MET> 15 meter</MET><ENG> 50 feet</ENG> away from 
a storm drain, open ditch, or receiving water.</TXT><BRK/>
<BRK/></SPT>
]</SPT>][<SPT><TTL>Control and Management of Solid Waste at Whidbey Island</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for work at Whidbey Island.  Attach Solid Waste tracking sheet located at: <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables</URL></NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Do not dispose of solid waste on Island County nor use the solid waste transfer facilities on Island County.  Do not contact County officials.  
Complete the <SUB>Solid Waste Tracking Sheet</SUB> (SWTS).  Complete the SWTS in accordance with the instructions on the back of the form.  Submit a SWTS 
for each load of solid waste.  The SWTS requires the weight of solid waste.  If scales are not available, calculate the weight based on the formula 
provided in <SUB>Monthly Project Waste Summary Report</SUB> (for example, for refuse, 3 cubic yards multiplied by 250 = 750 pounds).</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Control and Management of Solid Waste at NBK Bremerton</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for work at NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Complete a serialized Solid Waste Tracking Sheet (SWTS) for each off site shipment of solid waste (except sanitary sewage), recyclable materials, 
and non-dangerous recyclable waste.  Do not use SWTS for asbestos, PCBs, or dangerous waste.  Ensure the transporter has the SWTS before leaving 
the base. Hand-off exchange is preferred.  When a face-to-face hand-off is not possible, the following procedure is required:</TXT><BRK/>
<OLG><BRK/>
<OLI>Firmly affix a clear (no color), waterproof envelope to the front left corner of the accumulation container (a zipper sealed baggie duct-taped 
to the box is acceptable).  At the end of the shift prior to pick-up time, inspect the box, complete the applicable portion of the SWTS, 
and place it in a waterproof envelope.</OLI><BRK/>
<BRK/>
<OLI>The transporter removes the SWTS from the envelope, signs on the appropriate line, and provides it to the receiver for signature at the 
disposal site.  The receiver completes their portion of the SWTS and returns it to the Contractor.</OLI><BRK/>
<BRK/>
<OLI>When no SWTS is in the envelope, the waste must not be transported for disposal.</OLI><BRK/></OLG>
<BRK/></SPT>
][<SPT><TTL>Wastewater Discharge</TTL><BRK/>
<BRK/>
<TXT>Submit Waste Determination Documentation for each unique type of wastewater.</TXT><BRK/>
<BRK/>
[<SPT><TTL>Discharge at NBK Bangor</TTL><BRK/>
<BRK/>
<TXT>Submit Waste Determination Documentation for each unique type of Wastewater and notify the Contracting Officer to request wastewater discharges 
to the sanitary sewer.  All discharges to the sanitary sewer must be approved by NBK Environmental.<BRK/></TXT>
<BRK/>
<BRK/></SPT>
][<SPT><TTL>Discharge at NBK Bremerton</TTL><BRK/>
<BRK/>
<TXT>Notify the Contracting Officer for wastewater discharges to the sanitary sewer in quantities greater than<MET> 3785 liter</MET><ENG> 1,000 gallons</ENG> per day or<MET> 3,785 
liter</MET><ENG> 1,000 gallons</ENG> for the entire project, and allow 10 working days to obtain discharge approval from the City of Bremerton via the Contracting 
Officer.  If discharge is less than<MET> 3785 liter</MET><ENG> 1,000 gallons</ENG> per day or per project, then complete the Waste Determination Documentation specifying 
disposition to sanitary sewer completes the approval process.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Discharge at Everett</TTL><BRK/>
<BRK/>
<TXT>Conduct work in compliance with processed waste water permit, City of Everett Permit No. 7722-14.  Provide sampling and analysis of waste water 
effluent prior to discharge to sanitary system.  Effluents must meet and not exceed permit limits for metals, fats, oils, and grease, as well as 
pH, biological oxygen demand and total suspended solids.  Contact the Waste Water Operations Project Manager, via the Contracting Officer, for 
specific analytical requirements prior to discharge.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Hydrotest Water Discharge at NBK Bremerton</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Reconcile NBK Bremerton requirements with Section <SRF>33 11 00</SRF> WATER UTILITY DISTRIBUTION PIPING.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Waste Determination Documentation is not required to discharge water from new, clean piping system to the sanitary system at a flow rate less than<MET>
 [385] [_____] liter</MET><ENG> [100] [_____] gallons</ENG> per minute and<MET> [11356] [_____] liter</MET><ENG> [3000] [_____] gallons</ENG> per day.  Notify the Contracting Officer 
10 working days prior to discharge to the sanitary system to obtain approval for greater flowrates.  Clean, uncontaminated, hydrotest water may 
also be discharged to the storm drain.  Submit a Storm Drain/Sanitary Sewer Discharge Approval form to obtain approval before discharging.</TXT><BRK/>
<BRK/></SPT>
]</SPT>]<SPT><TTL>Control and Disposal of Landfill-Controlled Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include these subparagraphs for work at Everett, Indian Island, Whidbey Island, or NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Store landfill controlled waste under cover in a manner that minimizes contact with process water or storm water.  Keep covered and secured except 
when adding waste or taking samples.  Store in containers or in the following manner:</TXT><BRK/>
<OLG><BRK/>
<OLI>Underlay the waste with a continuous impervious sheet of plastic with a thickness sufficient to contain the waste with a minimum thickness 
of 10 mils.  Thicker or reinforced plastic, or other measures, to protect the integrity of the plastic underlayment may be required if 
there is danger that the plastic will be punctured or torn during accumulation. Weld, heat seal, or continuously tape (on both sides) seams.  
Protect the plastic from perforation during loading and handling operations.</OLI><BRK/>
<BRK/>
<OLI>Install a berm around the pile so that the landfill-controlled waste remains in the designated area.  Straw or hay bales are prohibited.  
The edges of the underlayment must be laid over the top of the berm and secured to prevent water from running under<BRK/>
the pile.</OLI><BRK/>
<BRK/>
<OLI>Install an impervious continuous sheet of plastic, 10 mils minimum thickness, over the pile and over the outside of the berm so that rainwater 
is directed away from the landfill controlled waste inside the berm.  Weld, heat seal, or continuously tape (on both sides) seams. </OLI><BRK/>
<BRK/>
<OLI>Secure the top cover to ensure that wind will not balloon the<BRK/>
cover or blow it aside leaving the pile exposed to weather.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following bracketed text for work at NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>Place a label on stockpiled soil containers or top cover that identifies the waste or soil as "Soil, Non-hazardous Pending Sampling."</OLI><BRK/>
<BRK/>
][<OLI>Disposal of Landfill Controlled Waste:</OLI><BRK/>
<BRK/>
<OLI>Submit a <SUB>Landfill Disposal Form</SUB> as required by the receiving landfill prior to removal of solid waste off Government property.  The Landfill 
Disposal Form may have different titles, depending upon the landfill (for example, Waste Disposal Application, Contaminated Soil Waste 
Information Sheet, and Industrial Waste Information Sheet).  The Government will co-sign forms.</OLI><BRK/></OLG>
<BRK/>
]</SPT><SPT><TTL><SUB>Waste Determination Documentation</SUB> Northwest</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Identify waste to be generated by the work and complete the Encountered Waste Summary (a.k.a Estimated 
Waste Table).  At NBK Bremerton and PSNS &amp; IMF, submit a Sampling and Analysis Plan for approval prior to 
TCLP sample collection and analysis.  At NBK Bangor, perform site visit with Base Environmental Office prior to 
survey.</NPR><BRK/>
<BRK/>
<NPR>The Designer must provide survey data only for NBK Bremerton and PSNS &amp; IMF projects.  The Encountered Waste 
Summary will be prepared by the Government.  Elsewhere, provide survey data and provide, with draft specifications, 
a waste designation table for review and approval by base environmental office.</NPR><BRK/>
<BRK/>
<NPR>Local Waste Tables are available for download at: <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables</URL></NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the following bracketed item for Design-Build Projects only and delete the next bracketed item.  
This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TAI OPT="DESIGN-BUILD">[<TXT>Comply with the requirements of FC 3-810-10N, including building survey and analytical services required to identify existing materials that may 
represent health risks, and to properly demolish, designate, and dispose of materials during site improvements.</TXT><BRK/>
]</TAI><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the following bracketed sentences and attach the completed/approved table in the RFP for Design-Bid-Build 
Projects.</NPR><BRK/>
<BRK/>
<NPR>For bracketed items, choose "Estimated Waste Table" for work at NBK Bangor, NBK Keyport, or Indian Island; choose 
"Encountered Waste Summary" for all other locations.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>The [<ATT>Estimated Waste Table</ATT>] [<ATT>Encountered Waste Summary</ATT>], attached, provides a summary table of anticipated encountered waste along with the corresponding 
probable waste designation.  This table may not be inclusive of waste that could be encountered.  This table does not require such waste to be 
disposed rather than recycled or reused.  This table is intended to provide a bid basis.  These estimated designations are subject to change upon 
receipt of the completed Waste Determination Documentation.  Any segregation, addition, or mixing of identified waste invalidates these estimated 
designations.  Where such action increases the quantity of dangerous waste, such waste must be disposed at the Contractor's expense.</TXT><BRK/>
<BRK/>
]<TXT>Waste Determination Documentation must consist of the base-specific waste form and related documentation prepared by the Contractor and submitted 
to the Government for the purpose of Government designation of waste.  Examples of related documentation include SDS, sampling and analysis plans, 
analytical information, and description of waste or process that generate waste.  No waste must be transported off site without completed Waste 
Determination Documentation.  Follow instructions provided on completed Waste Determination Documentation forms.</TXT><BRK/>
<BRK/>
[<SPT><TTL>Waste Information Specification Form for NBK Bangor</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for work at NBK Bangor.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For waste produced during the project, provide a completed "Side One" of Naval Base Kitsap at Bangor form, via the Contracting Officer.  Return 
the Waste Information Specification form to the Naval Base Kitsap Environmental Division, via the Contracting Officer.  Follow the Originator Disposal 
instructions provided on "Side Two" of the Waste Information Specification form.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Waste Information Sheet Form for Everett</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following paragraph for work at Everett.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Not less than 15 working days before removal of waste to locations off Government property, submit a Waste Information Sheet for each unique process 
that potentially generates recyclable material, solid waste (except garbage), dangerous waste, sewage, sediment, asbestos, PCB, stormwater, and 
wastewater generated onsite.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Waste Information Sheet Form for NBK Bremerton</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for work at NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Within one working day after waste stream has been produced, submit a Waste Information Sheet for each waste (except sanitary waste) generated 
on site for designation by the Government.  Submit a[ Waste Information Specification][ Waste Information Sheet] for each waste stream anticipated 
to be produced to the maximum extent possible for pre-designation of waste.  The Government will complete Section II and Section III of the Waste 
Information Sheet.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Waste Generation Record for[ Indian Island][ NBK Keyport][ Whidbey Island]</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for work at Indian Island, NBK Keyport, or Whidbey Island.</NPR><BRK/>
<BRK/>
<NPR>For NBK Keyport, choose "20" in brackets.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Not less than [15][20][_____] working days before removal of waste to locations off Government property, submit a <ATT>Waste Generation Record (WGR)</ATT>
 for each unique process that potentially generates recyclable material, solid waste (except garbage), dangerous waste, sewage, sediment, asbestos, 
PCB, stormwater, and wastewater generated on site.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for work at Indian Island or NBK Keyport.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>The Government will complete the portion entitled "ENVIRONMENTAL USE ONLY BELOW THIS LINE."</TXT><BRK/>
<BRK/>
]</SPT>][<SPT><TTL>Control of Waste Without Documented Waste Determination</TTL><BRK/>
<BRK/>
<TXT>Collect waste for which the Waste Determination Documentation has not been completed; label "waste awaiting designation" or "WAD" to indicate that 
analysis is pending.  Accumulate and manage in an area that meets the minimum criteria for satellite accumulation in accordance with <RID>WAC-173-303</RID>
 and the Contract specifications[, except for the time and quantity limitations].</TXT><BRK/>
<BRK/>
<TXT>Submit Waste Determination Documentation for each undesignated waste type within one day of generation.  Do not transport waste offsite prior to 
designation by the Government.</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Laboratory Analysis</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Select the waste analysis responsibilities.</NPR><BRK/>
<BRK/>
<NPR>For work at NBK Bremerton:  Select the first paragraph by default and delete the second.  For NBK Bremerton projects 
generating large quantities of waste, such as whole building demolition, delete the first paragraph.</NPR><BRK/>
<BRK/>
<NPR>For work at all other locations, select the second paragraph and delete the first.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[When analytical information is necessary to designate waste, the Government will sample and test waste in accordance with <RID>WAC-173-303</RID> and <RID>EPA SW-846</RID>
.] [When, at the sole discretion of the Government, laboratory analytical information is necessary to designate waste, provide sampling and analysis 
services in accordance with <RID>WAC-173-303</RID> and <RID>EPA SW-846</RID>.]</TXT><BRK/>
<BRK/>
<TXT>Submit analytical results and reports to the Contracting Officer as part of the Waste Determination Documentation.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Contractor Hazardous Material Inventory Log</TTL><BRK/>
<BRK/>
<TXT>In addition to the materials (for example, paints, lacquers, thinners, adhesives, sealants, cleaners) required in the Contractor Hazardous Material 
Inventory Log, include the following materials:</TXT><BRK/>
<OLG><BRK/>
<OLI>If performing abrasive blasting operations, denote blast grit usage, blast nozzle throughput in tons, and blasting unit efficiency. </OLI><BRK/>
<BRK/>
<OLI>If performing welding, denote welding rod usage and welding rod type (for example, aluminum, carbon steel).</OLI><BRK/></OLG>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this sentence for work at NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Use local form, <ATT>PSNS 5090/132 CHMI</ATT> for this purpose.</TXT><BRK/>
<BRK/>
]</SPT>[<SPT><TTL>Hazardous Materials Prohibition</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Include this paragraph for work at Indian Island, NBK Bangor, or NBK Keyport.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Products prohibited by the Government, which will not be approved for use, include but are not limited to: leads, chromiums, mercury, phenols, 
trichloroethylene, chlorofluorocarbons, halons, PCBs, asbestos, silica sand (for use as blasting agent), Class I ODS as defined and identified 
herein, radioactive materials or instruments capable of producing ionizing radiation, and chemicals listed in <RID>40 CFR 355</RID>.50, Appendix A.  This 
prohibition prevails over any other provision, specification, drawings, or referenced documents.  The Contracting Officer may consider exceptions 
to the use of any of the above excluded materials upon written request by the Contractor, and with Base Environmental Office approval.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Solid Waste Management Report</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For bracketed items, choose "not required" for work at Everett.  Choose "Monthly Project Waste Summary 
Report" for work at NBK Bremerton or Whidbey Island or "Refuse and Recycle Quantity Form" for work at Indian Island, 
NBK Bangor, or NBK Keyport.</NPR><BRK/>
<BRK/>
<NPR>Attach report or form as appropriate, located at: <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables</URL> and 
choose "and attached" in brackets.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Solid Waste Management Report is[ not required][ known locally as the Contractor's Monthly Project Waste Summary Report][ known locally as 
the Refuse and Recycle Quantity Form][ and attached].</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Fuel Tanks</TTL><BRK/>
<BRK/>
<TXT>Provide and implement a SPCC plan if tanks and containers of oil will have an aggregate aboveground capacity greater than<MET> 5,000 liters</MET><ENG> 1,320 gallons</ENG>
 (only containers with a capacity of<MET> 208 liters</MET><ENG> 55 gallons</ENG> or greater are counted).  Do not bring underground storage tanks to this installation 
for Contractor use during a project.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Releases and Spills of Oil and Hazardous Substances</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose applicable location.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>In the event of an reportable release immediately notify the[ PSNS &amp; IMF and NBK Bremerton Regional Dispatch Center, station phone 911, or 
(360) 476-3333 on outside lines or cellular phones][ NAS Whidbey Fire Department at (360) 257-3333][ NBK Regional Dispatch Center, station phone 
911, or (360) 396-4444][ Regional Dispatch Center, station phone 911, or (360) 396-4444][ Everett Central Monitoring Dispatch Center at (425) 304-3333, 
NAVSTA Everett phone 911][ Hospital Communication Center at phone 4444 within the Hospital or (360) 475-4444][ FISC Puget Sound, Fuel Department 
Operator In Charge (OIC) at (360) 476-2135, ext. 232 for oil spills][ Port Hadlock Detachment Central Monitoring Dispatch Center at (360) 396-5333], 
then notify the Contracting Officer.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this item for work at Indian Island, NBK Bangor, or NBK Keyport.  Include phone numbers for Indian 
Island.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Notify the Base Environmental Office[ at: (360) 396-5353, (360) 396-5394, or (360)396-5221].</TXT><BRK/>
]<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this item for work at NBK Bangor.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>The Government will respond to emergency spills.  Follow incident commander verbal instructions.  Notify the Base Environmental Office of spills, 
and reportable and non-reportable releases.</TXT><BRK/>
<BRK/>
]</SPT><SPT><TTL>Control and Management of Hazardous Waste</TTL><BRK/>
<BRK/>
<TXT>The following clarifications and requirements supplement paragraph CONTROL AND MANAGEMENT OF HAZARDOUS WASTE.</TXT><BRK/>
<BRK/>
<SPT><TTL>Facility Hazardous Waste Generator Status</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose appropriate location.  Coordinate with paragraph FACILITY HAZARDOUS WASTE GENERATOR STATUS.  Include 
this paragraph in this section with name and status.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>[Naval Base Kitsap, Bremerton ][PSNS &amp; IMF ][Naval Base Kitsap, Bangor ][Naval Station (NAVSTA), Everett ][Naval Magazine, Indian Island, WA 
(NAVMAGII) ][Naval Undersea Warfare Center (NUWC), Keyport ][Naval Hospital (NAVHOSP), Bremerton ][Naval Air Station, Whidbey Island (NASWI) ]is 
a fully regulated Large Quantity Generator.</TXT><BRK/>
<BRK/>
][<TXT>FISC Puget Sound, Manchester Fuel Department is a fully regulated medium quantity generator.</TXT><BRK/>
<BRK/>
]</SPT><SPT><TTL>Hazardous Waste Management</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose one of the paragraphs below and delete the other.  Choose the first paragraph for NBK Keyport.  
Also choose for NBK Bremerton projects, that do not generate large quantities of dangerous waste.  Coordinate 
the requirement with NBK Bremerton.</NPR><BRK/>
<BRK/>
<NPR>Choose the second paragraph for projects at Everett and Whidbey Island, and large projects generating large quantities 
of dangerous waste at NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Containers and labels will be supplied by the Government.  Notify the Contracting Officer 14 calendar days in advance for request of bulk containers.  
Submit Waste Determination Documentation including an estimated quantity of dangerous waste and the number of containers.  Accumulate in an approved 
satellite or 90-day accumulation area meeting the requirements set forth in <RID>WAC-173-303</RID>[ and the Keyport "Hazardous Waste Site Manager/Alternate 
(Waste Generator)" training module].  Contact the Contracting Officer no more than 45 calendar days from the start date for 90-day accumulation 
areas to arrange for transport.  Accumulate bulk dangerous waste in a 90-day area.  Turn in non-bulk dangerous waste from a 90-day area within 
45 days of the start date.</TXT><BRK/>
<BRK/>
][<TXT>Collect and dispose of dangerous waste in accordance with <RID>WAC-173-303</RID>.  Identify dangerous waste generated within the confines of the station by 
the use of the station's EPA generator ID number.  Submit a <SUB>Dangerous Waste Profile</SUB> for each unique type of dangerous waste[ not less than [45][20] 
days from scheduled removal from Government property].  Profiles are to be completed and signed by an EPA-permitted TSDF.  The Government will 
approve and co-sign profiles.  Approval of each dangerous waste profile must be complete before manifesting.  Accumulate in an approved satellite 
or 90-day accumulation area meeting the requirements set forth in <RID>WAC-173-303</RID>.  Waste Determination Documentation must be submitted and dangerous 
waste must be designated before removal from Government property.  Submit a copy of the applicable EPA and state permit(s), manifest(s), Land Disposal 
Restriction (LDR) forms, and license(s) for transportation, treatment, storage, and disposal of hazardous and regulated waste by permitted facilities.  <SUB>
Dangerous waste manifests</SUB> must be reviewed, signed, and approved by the Government before the Contractor may ship waste.  To obtain specific disposal 
instructions, coordinate with the Activity environmental office.  Labels will be supplied by the Government.</TXT><BRK/>
<BRK/>
]</SPT>[<SPT><TTL>Contractor-Generated Hazardous Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this subparagraph for projects at NBK Bangor or Indian Island.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Identify and turn in dangerous Contractor-Generated Hazardous Waste to the Government as encountered waste.  Follow all encountered waste procedures 
in paragraph ENCOUNTERED WASTE below.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Encountered Waste</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this subparagraph for projects at NBK Bangor or Indian Island.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Identify, minimize, segregate, contain, package, label and turn in dangerous and industrial encountered waste to the Government in accordance with 
the approved Environmental Protection Plan.  Contractor-generated dangerous or industrial waste must be disposed of by the Government at Contractor's 
expense.  On base disposal of Contractor generated waste is prohibited.</TXT><BRK/>
<BRK/>
<TXT>Follow originator disposal instructions provided in NAVBASEKITSAPINST 5090.3(Series) and on side 2 of the[ Waste Information Specification][ Waste 
Information Sheet].  Package according to 49 CFR specifications and attach a completed SUBASE Bangor Originator Label when instructed.  Properly 
stage and transfer encountered waste to a Government-approved accumulation area within 7 miles of the project site.  Transportation to the Government 
site must be within 72 hours of generation.  Provide the Project Number on Crew/Code line of the Originator Label.  Turning in encountered waste 
to the Government, in accordance with[ Waste Information Specification][ Waste Information Sheet] instructions, is not considered disposal.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL><SUB>Certificate of Final Disposal</SUB> (CFD)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this subparagraph for projects at Whidbey Island.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Within 10 working days after final disposal of dangerous waste, submit the CFD to the Contracting Officer.  Final disposal means disposal of dangerous 
waste and any residues from the treatment of the waste prior to disposal.  The CFD includes, at a minimum the following:</TXT><BRK/>
<OLG><BRK/>
<OLI>Waste Profile Sheet Number, Government Manifest Number, and Shipment Date</OLI><BRK/>
<BRK/>
<OLI>Unit of Measure</OLI><BRK/>
<BRK/>
<OLI>Quantity of Disposal</OLI><BRK/>
<BRK/>
<OLI>Waste that required land disposal, including effluents from treatment systems.</OLI><BRK/>
<BRK/>
<OLI>Disposal facility's (Facilities') EPA ID number, name, location, and phone.  In addition, include the name, address, phone number, and 
EPA ID number of each TSDF the waste was taken to for any intermediate steps for final disposal.</OLI><BRK/>
<BRK/>
<OLI>Disposal Method</OLI><BRK/>
<BRK/>
<OLI>Date of Final Disposal</OLI><BRK/>
<BRK/>
<OLI>Signature of the person responsible for adequate and appropriate disposition of the waste</OLI><BRK/></OLG>
<BRK/></SPT>
][<SPT><TTL>Regulated Waste Storage, Satellite Accumulation, and 90-Day Storage Areas</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include these paragraphs for work and NBK Bangor</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Prior to generating waste, submit an accumulation area registration form.  Waste stored in Central Accumulation Areas must be prepared for shipment 
within 45 days of generation.  Satellite accumulation over-water, such as on piers and dry docks, is not authorized unless waste is accumulated 
with secondary containment and is attended by a trained person.</TXT><BRK/>
<BRK/>
<TXT>Submit to the Contracting Officer once every 7 calendar days an Accumulation Area Inspection Record meeting the requirements set forth in <RID>WAC-173-303</RID>
.  Closure of 90-day areas require inspection and approval by the Government.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this subparagraph for work at Naval Hospital, Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Accumulate waste in the Contractor's satellite accumulation area or the Government's 90-Day accumulation area.  Contractor-operated 90-Day accumulation 
areas are prohibited at Naval Hospital, Bremerton.</TXT><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Include these subparagraphs for work at NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Prior to generating waste, submit an accumulation area registration form, known locally as <ATT><SUB>Contractor Request for 45/90-Day Hazardous Waste Accumulation 
Certification/Recertification</SUB></ATT> or <ATT><SUB>Contractor Request for Hazardous Waste Accumulation Area (SAA) Registration</SUB></ATT></TXT>.<BRK/>
<BRK/>
<TXT>90-Day areas are known locally as 45/90 day areas and such waste must be manifested prior to 45 days.  Satellite accumulation over-water, such 
as on piers and dry docks, is not authorized unless waste is accumulated with secondary containment and is attended by a trained person.  90-Day 
areas will not be authorized in dry docks, on piers, or on an over-water site.  Submit to the Contracting Officer once every 7 calendar days an <ATT><SUB>
Accumulation Area Inspection Record</SUB></ATT> meeting the requirements set forth in <RID>WAC-173-303</RID>.  Closure of 90-day areas require inspection and approval 
by the Government.</TXT><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Include this subparagraph for work at NBK Keyport.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Submit the <ATT><SUB>Hazardous Waste Accumulation Area Registration Form</SUB></ATT> as instructed in the "Hazardous Waste Site Manager/Alternate (Waste Generator)" 
training module.  Attach Site Plan to the Request.  Attach Waste Determination Documentation.</TXT><BRK/>
<BRK/>
]</SPT>][<SPT><TTL>Vacuum Cleaners</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this subparagraph for work at NBK Bremerton.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Container ID labeling requirements apply to vacuums used onsite.  Vacuum cleaners must be empty when they arrive at the BNC, and emptied into approved 
containers in accordance this section.  If a vacuum cleaner cannot be emptied at the end of the shift, it must be managed as a hazardous waste 
container and stored in a registered satellite accumulation area.  Hazardous waste container labeling and storage requirements of this section 
apply to vacuum cleaners used for pickup and storage of hazardous waste.</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Class I and Class II ODS Prohibition</TTL><BRK/>
<BRK/>
<TXT>Turn over to the Government Class I and II ODS reclaimed as a part of this Contract with analysis documentation, upon the completion of the work 
covered by this Contract.  Mixed refrigerant cannot be accepted and must be recycled by a refrigerant recycler meeting the requirements of 40 CFR 
82.</TXT><BRK/>
<BRK/>
<TXT>Certified technicians must perform refrigerant work using EPA-approved recovery equipment.  Releases of ODS or refrigerants to the atmosphere is 
strictly prohibited.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Noise</TTL><BRK/>
<BRK/>
<TXT>Conduct work in full compliance with <RID>WAC-173-60</RID>.</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Drinking Water</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Many Navy activities in Washington State, including, but not limited to, Whidbey Island, NBK Bangor, NBK 
Keyport, MWR Pacific Beach, Naval Radio Station (t) Jim Creek, NAVORDCEN Det Port Hadlock, and NBK Bremerton are 
regulated as public water system purveyors.  Delete this paragraph if there is no potable water system change, 
or the change is listed as one of the exceptions in accordance with WAC-246-290.  For projects which involve applicable 
construction, repair, or alteration of a drinking water system, ensure the work is covered in the activity's Water 
System Plan (WSP).</NPR><BRK/>
<BRK/>
<NPR>For Design-Build projects, choose the first sentence in first paragraph; this sentence is tailored for DESIGN-BUILD.  
Include the Project Report in the Design Build Requirements to accommodate this evaluation.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<SPT><TTL><SUB>Project Report</SUB></TTL><BRK/>
<BRK/>
<TXT><TAI OPT="DESIGN-BUILD">[Submit a <SUB>Project Report</SUB>, in accordance with <RID>WAC-246-290</RID>-110(2).  ]</TAI>[This project includes work on a potable water[ treatment,][ storage,][ and][ 
distribution] system that is regulated by <RID>WAC-246-290</RID>.][  The design specifications have been reviewed and approved by the Washington State Department 
of Health.][  The design specifications conform to the activity's approved Water System Plan.][  Do not use any materials of construction or construction 
practices that deviate from the approved water system design.]</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Public Works Department Permit</TTL><BRK/>
<BRK/>
<TXT>Obtain permit from the Public Works Department prior to any connections or changes to the potable drinking water system, or access to fire hydrants.  
Do not access any part of the potable water system (including fire hydrants) without obtaining a connection permit from the Government.  Connections 
or work pertaining to the potable water system as part of the Contract must be in accordance with the instructions specified in the connection 
permit and in compliance with state and federal regulations.  Submit an Inspection Report to the Government for acceptance.  Include the most recent 
annual calibration inspection report for the test assembly to be used.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Project Completion Report</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:   If the project is not identified in the Water System Plan and is not exempted according to WAC-246-290-125, 
the construction manager must submit a Project Completion Report to the Washington Department of Health within 
60 days after completion of the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Within 15 days after completion of an approved water system project, submit a <SUB>Project Completion Report</SUB> in accordance with <RID>WAC-246-290</RID>-120(5).  
The <URL HREF="http://www.doh.wa.gov/ehp/dw/forms/forms.htm">report</URL> must be signed by a Washington State-registered professional engineer.  This report is required for new construction on exterior building 
potable water system components.  Any significant changes from the approved water system design must receive prior approval of the Contracting 
Officer and written approval from the Department of Health in accordance with <RID>WAC-246-290</RID>-120 prior to use.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Disinfection of Water System Components</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for work at NBK Bremerton when Section <SRF>33 11 00</SRF> WATER UTILITY DISTRIBUTION PIPING 
is used.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Disinfect water system in accordance with paragraph DISINFECTION in Section <SRF>33 11 00</SRF> WATER UTILITY DISTRIBUTION PIPING.</TXT><BRK/>
<BRK/></SPT>
]</SPT>][<SPT><TTL>Contractor's Operation and Maintenance (O&amp;M) Plan</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Indian Island, choose ORCAA. For Whidbey Island, choose NWCAA.  For Everett and all Kitsap locations, 
choose PSCAA.  For additional information, see<BRK/>
<URL HREF="https://ecology.wa.gov/Air-Climate">https://ecology.wa.gov/Air-Climate</URL></NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Prior to using the types of air contaminant-generating equipment defined in[ <RID>PSCAA Regulation</RID>][ <RID>ORCAA Regulations</RID>][ <RID>NWCAA Regulation</RID>], develop 
and submit a <SUB>Contractor's Operation and Maintenance (O &amp; M) Plan</SUB>.  Maintain the O &amp; M Plan and any associated records on site for the duration 
of the project.  Be prepared to provide these records for review, within 30 minutes, when requested by regulatory agencies or the Contracting Officer.  
The O&amp;M Plan must contain at a minimum the following elements:</TXT><BRK/>
<OLG><BRK/>
<OLI>Maintain equipment in good working order.  Follow manufacturer's O &amp; M recommendations, at a minimum.</OLI><BRK/>
<BRK/>
<OLI>Maintain records of any repairs made, including records of preventive maintenance and chemicals used, including SDSs.</OLI><BRK/>
<BRK/>
<OLI>Inspect periodically, including, but not limited to, evidence of fugitive emissions.  If fugitive emissions are found, determine whether 
reasonable precautions are being taken to minimize such emissions. List requirements to repair the equipment or shut down operations, when 
reasonable precautions are not being taken to minimize fugitive emissions or unreasonable odors.</OLI><BRK/>
<BRK/>
<OLI>Ensure deficiencies are promptly repaired.  Secure operation of such equipment if immediate repairs are not feasible.</OLI><BRK/>
<BRK/>
<OLI>List any requirements noted under "Conditions" on the Order of Approval for the equipment.</OLI><BRK/>
<BRK/>
<OLI>Generate records that list any actions (for example, inspections, maintenance, shut down) that have been taken or completed, including 
the location, date, time, and name of person(s) completing the actions. Records may be maintained in the form of a logbook.  Submit <SUB>Operation 
and Maintenance Records</SUB> at Contract completion.</OLI><BRK/>
<BRK/>
<OLI>Maintain records of operating permit(s) and related permit compliance records.</OLI><BRK/></OLG>
<BRK/></SPT>
]<SPT><TTL>Emission Standards</TTL><BRK/>
<BRK/>
<TXT>Opacity from Contractor equipment and operations must be in compliance with[ <RID>PSCAA Regulation</RID> I, Section 9.03] [_____] including but not limited 
to Visual Emissions (Opacity), Odor, Fugitive Dust, Spray Coating, Crushing, and Maintenance of Equipment.</TXT><BRK/>
<BRK/>
<SPT><TTL>Volatile Organic Compound Emission Control</TTL><BRK/>
<BRK/>
<TXT>Do not leave containers of paint, epoxy, or solvent open to the atmosphere unless they are being used.  Secure containers at the end of each shift. 
Do not use evaporation as a means of minimizing or disposing of hazardous waste.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT></TAI><TAI OPT="NAVFAC SE"><SPT><TTL>SOUTHEAST</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This Article is tailored for NAVFAC SE.  Use this paragraphs and subparagraphs for NAVFAC SE projects only.  
Delete for other projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Florida</TTL><BRK/>
<BRK/>
[<SPT><TTL>Laboratory Analysis</TTL><BRK/>
<BRK/>
<TXT>Test soil and groundwater that will be disposed under this Contract in accordance with the paragraph LABORATORY ANALYSIS.</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Waste Storage/Satellite Accumulation</TTL><BRK/>
<BRK/>
<TXT>For Hazardous Waste accumulation areas, submit weekly <SUB>hazardous waste inspection logs</SUB> to the Station Hazardous Waste Manager via the Contracting 
Officer and maintain compliance with <RID>40 CFR 265</RID>.16 personnel training requirements.  Ensure containers are kept closed (except when adding or removing 
waste) and that containers remain in good condition and are properly labeled by PWC Jacksonville or the Station.  Store Regulated waste for up 
to 190 day.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Control and Management of Hazardous Waste</TTL><BRK/>
<BRK/>
<SPT><TTL>Universal Waste</TTL><BRK/>
<BRK/>
<TXT>Dispose of lead-acid batteries that are not damaged or leaking at the NAS Jacksonville MWR Recycling Center or at a state-approved battery-recycling 
facility.  For lead-acid batteries that are leaking or have cracked casings, dispose of the battery by calling PWC Jacksonville for disposal.  
Collect and segregate alkaline batteries, non-alkaline batteries, lithium batteries, metal hydride batteries, and nickel-cadmium batteries by type 
for turn-in to the activity for disposal or recycling.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Mercury Containing Materials</TTL><BRK/>
<BRK/>
<TXT>Prior to starting work, remove bulbs, thermostats, switches, and other components that contain mercury.  Upon removal, place items containing mercury 
in DOT approved containers, label, and turn over to the activity for disposal or recycling.  For projects at NAS Jacksonville, fluorescent bulbs 
are to be turned in to Self-Help for recycling.  For projects at Naval Aviation Depot and Naval Hospital Jacksonville, turn in fluorescent bulbs 
in to the appropriate environmental office as directed by the Contracting Officer.  Bulbs must be boxed, stenciled with the words "spent mercury-containing 
devices for recycling", and marked with the date of accumulation.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Aerosol Cans Management and Disposal</TTL><BRK/>
<BRK/>
<TXT>Do not dispose of aerosol cans as solid waste or construction and demolition debris.  Collect aerosol cans and segregate from other waste in a 
suitable container on site.  Label the container "aerosol cans for recycling" and turn it in to the General HM Locker at Building 102.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Disposal of Regulated Waste</TTL><BRK/>
<BRK/>
<TXT>In accordance with Station requirements, accumulate regulated waste in DOT-approved containers.  Ensure containers remain closed except when adding 
or removing waste and they are marked with the appropriate Non-hazardous Waste Label, which will be provided by PWC Jacksonville or the Station.  
Air-drying any containers to render them empty is prohibited.  Dispose of regulated waste, except for asbestos and petroleum-contaminated waste, 
through PWC Jacksonville and do not take them off Station.  Pay disposal costs in accordance with PWC Jacksonville's published rates.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Disposal of Petroleum Contaminated Waste</TTL><BRK/>
<BRK/>
<TXT>Provide the completed Non-hazardous Waste Manifest for offsite disposal of petroleum-contaminated waste to the Contracting Officer within 7 days 
of disposal.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Dumpsters</TTL><BRK/>
<BRK/>
<TXT>Equip dumpsters with a secure cover and paint the standard installation color.  Keep dumpster covers closed, except when being loaded with trash 
and debris.  Locate dumpsters behind the construction fence or out of the public view.  Empty site dumpsters at least once a week, or as needed 
to keep the site free of debris and trash.  If necessary, provide<MET> 208 liter</MET><ENG> 55 gallon</ENG> trash containers painted the darker installation color to 
collect debris in the construction site area.  Locate the trash containers behind the construction fence or out of the public view.  Empty trash 
containers at least once a day.  For large demolitions, large dumpsters without lids are acceptable, but should not have debris higher than the 
sides before emptying.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Cuba</TTL><BRK/>
<BRK/>
<SPT><TTL>Fish and Wildlife Resources</TTL><BRK/>
<BRK/>
<TXT>Ensure compliance, including off-duty hours with <RID>1710.10</RID>.  Ensure employees comply with prohibitions on feeding and raising indigenous wildlife 
and feral animals during working and non-working hours.  Specifically, direct or indirect feeding of iguanas resulting in the domestication or 
semi-domestication of these animals is strictly prohibited.  Further, direct or indirect feeding of feral chickens, cats, dogs, goats, or other 
feral domestic animals is strictly prohibited.  Prohibitions of this section apply to living and working areas.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Protection of Erodible Soils</TTL><BRK/>
<BRK/>
<TXT>Use endemic or regionally native and drought and heat-tolerant grass species as specified by the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Control and Management of Solid Waste</TTL><BRK/>
<BRK/>
<TXT>Dispose of solid waste generated at locations as directed by the Contracting Officer.  Solid waste disposal service is available from the BOS contractor 
on a cost-reimbursable basis.  Refer to Section <SRF>01 14 00</SRF> WORK RESTRICTIONS, for more information.</TXT><BRK/>
<BRK/>
<SPT><TTL>Disposal of Solid Waste and Debris</TTL><BRK/>
<BRK/>
<TXT>Dispose of solid waste, debris, and metal containers in accordance with the requirements specified herein.</TXT><BRK/>
<BRK/>
<SPT><TTL>Base Sanitary Landfill and Concrete Areas</TTL><BRK/>
<BRK/>
<TXT>Only authorized solid waste approved for deposit by the landfill attendant or equipment operator may be dumped at a designated area in the Windward 
Landfill.  Deposit demolition material such as grading or excavated materials at the designated area, provided such material does not contain segregated 
metals, as directed by Landfill Attendant.  Landfill hours of operation are Monday through Saturday, 7:30 A.M. to 11:00 A.M., and 12:30 P.M. to 
4:00 P.M.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Disposal of Rubbish and Debris</TTL><BRK/>
<BRK/>
<TXT>Self-hauling of garbage and municipal solid waste (MSW) to the landfill is at the discretion of the BOS contractor.  An approved Landfill Access 
Pass must be presented prior to entry into the landfill.Arrange MSW collection and disposal services for jobsites and berthing areas with the BOS 
contractor.</TXT><BRK/>
<BRK/>
<SPT><TTL>Permitted Material in Landfill</TTL><BRK/>
<BRK/>
<TXT>A Landfill Access Pass must be obtained prior to transporting asbestos-containing materials to the Asbestos Landfill in accordance with <RID>5090.4</RID>.  
The Landfill Access Pass must be approved by Hazardous Waste Facility personnel (Bldg. 850). Materials that may be deposited in the landfill include 
the following:</TXT><BRK/>
<TAB>
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="17">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="380.25"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="380.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="19.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">CATEGORY</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">CONSTRUCTION/DEMOLITION WASTE</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="54.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Mixed Debris</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">The following materials may be placed in the landfill in a location designated by the landfill operator.  These items may be mixed together.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="34.50">
         <CEL STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Gypsum board panels, plaster, glass.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="34.50">
         <CEL STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Non-asbestos insulation-(bag fiberglass and mineral wool).</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="34.50">
         <CEL STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Packing paper, Styrofoam, and cardboard boxes.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="34.50">
         <CEL STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Painted wood such as doors, windows, siding, and trim.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="44.25">
         <CEL STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Plastic and fiberglass such as pipe, electrical boxes, cover plates, and similar.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="41.25">
         <CEL STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Ceramic and vinyl flooring or tile, ceiling tile.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="47.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Shingles</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Non-asbestos roofing materials such as shingles built-up and single roofing.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="65.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Masonry and Concrete</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Concrete, block, brick, mortar to the landfill separate from any other items, and place in a location designated by the landfill operator.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="28.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Pallets</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Place in a location designated by the Landfill Operator.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="63.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Treated Lumber</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Treated wood, and such as piling and power poles, to the landfill separated from any other items and place in C/D Landfill.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="47.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Fiberglass/Poly Containers</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Triple wash tanks before delivery to landfill.<MET> 208 liter</MET><ENG> 55 gallons</ENG> or less are turned in at recycling.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="22.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Asphalt Pavement</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Deliver to Windward Landfill.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="90.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Construction Debris</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Separate each category of construction debris at the construction site and deliver separately to the landfill. Place each category of construction debris in the landfill at a location designated by the Landfill Operator.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="93.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Asbestos</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Place in designated area of the landfill. Transport asbestos-containing materials in covered vehicles, wetted, double bagged, and properly marked and documented.  Obtain a Landfill Access Pass at the Hazardous Waste Facility.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="228.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Lead Based Paint and Materials</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Dispose of building components and materials removed that have lead-based paint (LBP) at the construction waste cell at the C/D Landfill. Dispose of abatement waste, such as blast material, paint chips, paint stripper scrapings, and similar, where the LBP has been removed from a substrate in approved drums and deliver material to the Hazardous Waste Facility, Building 850, properly marked and documented for proper analysis and potential disposal in the United States at Contractor expense.</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/></SPT>
<SPT><TTL>Metals Disposal</TTL><BRK/>
<BRK/>
<TXT>Metals will not be accepted at the landfill in the regular or C/D waste. Recycling Center personnel/scale attendant <BRK/>
will inspect metals and provide driver with instructions.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT><SPT><TTL>Sewage</TTL><BRK/>
<BRK/>
<TXT>Dispose of sewage through connection to a station sanitary sewage system or the Lizard Island treatment pump station as directed by the BOS Contractor.  
Where such a system is not available, use chemical toilets or comparable effective units and periodically empty waste into a pump station designated 
by the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Control and Disposal of Hazardous Waste</TTL><BRK/>
<BRK/>
<TXT>Disposal of hazardous waste at the Windward Landfill and C/D area is prohibited.</TXT><BRK/>
<BRK/>
<SPT><TTL>Hazardous Waste Generation</TTL><BRK/>
<BRK/>
<TXT>Handle generated hazardous waste in accordance with the Overseas Environmental Baseline Guidance Document (OEBGD), Final Governing Standards (FGS) 
and base requirements..</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Hazardous Waste Disposal</TTL><BRK/>
<BRK/>
<TXT>Dispose of hazardous waste in accordance with federal and station regulations, especially <RID>40 CFR 260</RID>, <RID>40 CFR 261</RID>, <RID>40 CFR 262</RID>, <RID>40 CFR 263</RID>, <RID>40 CFR 264</RID>
, <RID>40 CFR 265</RID>, the <RID>FGS</RID> and <RID>5090.1</RID>.  Do not bring hazardous waste onto the Station.  In accordance with <RID>5090.1</RID> turn in hazardous waste for disposal 
to the Hazardous Waste Facility (Bldg. 850).  Obtain containers for hazardous waste or oily waste from Hazardous Waste Facility.  Waste in containers 
must meet DOT shipping container requirements in accordance with <RID>49 CFR 178</RID>.  Package the containers in accordance with <RID>49 CFR 171</RID> for waste.  
Knowingly mismanaging or disposing of hazardous waste are grounds for immediate debarment and administrative/criminal action.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Hazardous Waste Accumulation</TTL><BRK/>
<BRK/>
<TXT>Accumulate and manage hazardous waste in accordance with federal and station regulations, <RID>40 CFR 261</RID>, <RID>40 CFR 262</RID>, <RID>FGS</RID>, <RID>5090.1</RID>, and revisions.  
Properly identify, package, and label hazardous waste in accordance with <RID>49 CFR 172</RID> and <RID>5090.1</RID> and turn it in for disposal to the Hazardous Waste 
Facility (Bldg. 850).  Obtain containers for hazardous waste and used oil from the Hazardous Waste Facility.  Containerize and transport the waste 
to the Hazardous Waste Facility.  If hazardous materials are mismanaged so they become hazardous waste, or if a hazardous waste is not managed 
properly and costs more for disposal because of contamination, the Contractors' Special Deposit Account will be charged for sampling, analysis, 
and disposal rates as specified or identified.  Itemized statements will be provided to the Contractor via the Contracting Officer.</TXT><BRK/>
<BRK/>
<SPT><TTL>Site Storage</TTL><BRK/>
<BRK/>
<TXT>In accordance with <RID>5090.1</RID>, store hazardous waste near the point of generation up to a total quantity of one quart of acutely hazardous waste or<MET>
 208 liter</MET><ENG> 55 gallons</ENG> of hazardous waste.  Deliver waste exceeding these quantities to the Hazardous Waste Storage Area (Bldg. 850) within three 
days..  Prior to generating hazardous waste, contact the Hazardous Waste Facility for labeling requirements for the accumulation of hazardous waste.  
Accumulate hazardous waste (no longer than 90 days) in containers in accordance with <RID>49 CFR 178</RID> and Station instructions.  Identify hazardous waste 
in accordance with <RID>40 CFR 261</RID>, <RID>40 CFR 262</RID>, and Station instructions.  Ensure hazardous waste is properly labeled and segregated.  Every effort 
must be made to ensure used oil is not contaminated.  Used oil generated must be containerized and delivered to the Hazardous Waste Facility (Bldg. 
850) for disposal.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Turn-In</TTL><BRK/>
<BRK/>
<TXT>Hazardous waste must be turned into the Hazardous Waste Facility for shipment or disposal off Station.  At the conclusion of the project, turn 
in all unused hazardous materials to the Consolidated Hazardous Material Reutilization and Inventory Management Program for reuse.  Exceptions 
to this will be hold back of minor amounts for possible warranty work.  Properly dispose of waste generated from a project at the conclusion of 
each task order or project.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Spills of Oil and Hazardous Materials</TTL><BRK/>
<BRK/>
<TXT>Package, transport, and dispose of contaminated material, equipment, and any PPE generated during the spill cleanup process at the Hazardous Waste 
Storage Area (Bldg. 850), which must be at no additional cost to the Government in accordance with <RID>5090.1</RID> and <RID>5090.7</RID>.  Provide SDSs to the Contracting 
Officer to ensure material is properly identified for disposal, or reimburse the Government for analytical data (to include labor and costs of 
analysis) should data be required to properly identify the waste.</TXT><BRK/>
<BRK/>
<TXT>Complete the spill report provided in <RID>5090.7</RID> and submit it to the Contracting Officer within 24 hours of spill occurrence.  Base environmental 
notification is required immediately upon discovery of spill regardless of volume.  Contractor's special deposit account will be charged for disposal 
of spilled material and associated waste.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Oily and Hazardous Substances</TTL><BRK/>
<BRK/>
<TXT>Limit the storage of fuels, lubricants, solvents, paints, and hazardous substances to a total of less than<MET> 208 liter</MET><ENG> 55 gallons</ENG> onsite unless preapproved 
by the Government.  Bulk storage of fuel is prohibited.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Lead-Acid Batteries</TTL><BRK/>
<BRK/>
<TXT>Dispose of lead-acid batteries that are not damaged or leaking through the BOS Contractor.  For lead-acid batteries that are leaking or have cracked 
casings, turn in battery at the Hazardous Waste Facility (Bldg. 850).</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Mercury Controls</TTL><BRK/>
<BRK/>
<TXT>Prior to starting work, remove thermostats, switches, fluorescent tubes, and other components that contain mercury.  Prior to removal, obtain proper 
containers from the Hazardous Waste Facility (Bldg. 850).</TXT><BRK/>
<BRK/>
<SPT><TTL>Management and Disposal of Low Level Radioactive Waste (LLRW)</TTL><BRK/>
<BRK/>
<TXT>Prior to starting work, coordinate collection and delivery of LLRW items, such as smoke detectors, with the NAVFAC Safety Engineering Technician 
(E.T.).</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Petroleum Products</TTL><BRK/>
<BRK/>
<TXT>Dispose of petroleum products and oily water at the Hazardous Waste Facility (Bldg. 850).</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Refrigerants, Including Class I and Class II Ozone Depleting Substances (ODS)</TTL><BRK/>
<BRK/>
<TXT>Transfer ODS and other refrigerants to DOT-approved recovery cylinders.  Properly label identifying refrigerant and deliver to the Hazardous Waste 
Facility (Bldg. 850) at the conclusion of the Task Order or project.  Do not mix different refrigerants in the same cylinder.</TXT><BRK/>
<BRK/>
<TXT>Certified technicians must perform refrigerant work using EPA-approved recovery equipment.  Releases of ODS or refrigerants to the atmosphere is 
strictly prohibited.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Vegetation</TTL><BRK/>
<BRK/>
<TXT>Remove trees and other landscape features scarred or damaged by equipment operations, and replace with equivalent, undamaged trees and landscape 
features.  Obtain Contracting Officer's approval before removal/replacement, Environmental Office will evaluate removal of all mature trees.  Replace 
trees on a one-to-one basis.  Use Regionally native plants as specified by the station Integrated Natural Resources Management Plan (INRMP) as 
replacement landscape features.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Contract Completion and Close-Out</TTL><BRK/>
<BRK/>
<TXT>At project completion, remove any hazardous material brought onto the Station.  Account for the quantity of hazardous material brought to the station, 
the quantity used or expended during job, and the leftover quantity that (1) may have additional useful life as a hazardous material and must be 
removed by the Contractor, or (2) may be a hazardous waste, which must then be removed as specified herein.  The sale of any hazardous material 
to other Contractors (or Base entity) must be specifically approved in writing by the Contracting Officer prior to the sale.  Abandoned hazardous 
materials and waste will be properly disposed of and all associated costs charged to the Contractor.</TXT><BRK/>
<BRK/>
<TXT>Laydown areas, vehicle storage and repair facilities, and similar that were <NED/>Contractor operated and controlled must be returned to a condition 
similar to the time of the contract award.  This includes the removal of break shacks, kitchens, gardens, and similar.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT></SPT></TAI></PRT>    <END/><BRK/></SEC>