<?xml version="1.0" encoding="windows-1252"?><SEC xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="http://si.ksc.nasa.gov/sidownloads/xml/specsintactSEC.xsd"><MTA NAME="SUBFORMAT" CONTENT="NEW"/><MTA NAME="AUTONUMBER" CONTENT="TRUE"/><HDR><AST/><TAB BORDERS="0">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="4">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="366.75"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="364.50"/>
      <ROW AUTOHEIGHT="0" HEIGHT="14.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">USACE / NAVFAC / AFCEC</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">UFGS-01 50 00 (November 2020)</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="12.00">
         <CEL MERGEDOWN="1" STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Change 3 - 08/24</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="12.00">
         <CEL INDEX="2" STYLEID="s50">
<DTA TYPE="STRING"><HL3>------------------------------------</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="45.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Preparing Activity:  <PRA>USACE</PRA></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Superseding<BRK/>UFGS-01 50 00 (May 2018)<BRK/>UFGS-01 50 00.05 20 (November 2007)</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<HL4>UNIFIED FACILITIES GUIDE SPECIFICATIONS</HL4><BRK/>
<BRK/>
<HL4>References are in agreement with UMRL dated July 2025</HL4><BRK/>
<AST/><BRK/></HDR>
<BRK/>
<SCN>SECTION 01 50 00</SCN><BRK/>
<BRK/>
<STL>TEMPORARY CONSTRUCTION FACILITIES AND CONTROLS</STL><BRK/>
<DTE>11/20, CHG 3: 08/24</DTE><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This specification covers the requirements for <SCP>temporary construction facilities, safety systems, construction 
traffic provisions, construction signage, jobsite Wi-Fi, and controls over Contractor operations required for 
use in all projects.</SCP></NPR><BRK/>
<BRK/>
<NPR>Adhere to <URL HREF="https://www.wbdg.org/dod/ufc/ufc-1-300-02">UFS 1-300-02</URL> Unified Facilities Guide Specifications (UFGS) Format Standard when editing this guide 
specification or preparing new project specification sections.  Edit this guide specification for project specific 
requirements by adding, deleting, or revising text.  For bracketed items, choose applicable item(s) or insert 
appropriate information.</NPR><BRK/>
<BRK/>
<NPR>Remove information and requirements not required in respective project, whether or not brackets are present.</NPR><BRK/>
<BRK/>
<NPR>Comments, suggestions and recommended changes for this guide specification are welcome and should be submitted 
as a <URL HREF="https://www.wbdg.org/dod/ufgs">Criteria Change Request (CCR)</URL>.</NPR><BRK/>
<BRK/>
<NPR>This guide specification includes tailoring for ARMY, NAVY, AIR FORCE, NAVFAC ML, NAVFAC FE, NAVFAC LANT, NAVFAC 
PAC, NAVFAC HAWAII, NAVFAC SE and NAVY DESIGN-BUILD projects.  Where an Editor's Note states a paragraph is tailored 
for a Service or project type, the content of the paragraph, or a portion of the paragraph, is suited specifically 
to be included only for that Service or project type.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<PRT><TTL>PART 1   GENERAL</TTL><BRK/>
<TAI OPT="NAVY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  To download UFGS Forms, Graphics, and Tables, go to: <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables">https://www.wbdg.org/dod/ufgs/ufgs-forms-graphics-tables</URL><BRK/>
On the drawings, show:<BRK/>
<BRK/>
1.  Location of temporary buildings and storage areas, if specified;<BRK/>
<BRK/>
2.  Location of temporary utility connections, if specified.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<SPT><TTL>REFERENCES</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is used to list the publications cited in the text of the guide specification.  The publications 
are referred to in the text by basic designation only and listed in this paragraph by organization, designation, 
date, and title.<BRK/>
<BRK/>
Use the Reference Wizard's Check Reference feature when you add a Reference Identifier (RID) outside of the Section's 
Reference Article to automatically place the reference in the Reference Article.  Also use the Reference Wizard's 
Check Reference feature to update the issue dates.<BRK/>
<BRK/>
References not used in the text will automatically be deleted from this section of the project specification when 
you choose to reconcile references in the publish print process.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The publications listed below form a part of this specification to the extent referenced.  The publications are referred to within the text by 
the basic designation only.</TXT><BRK/>
<BRK/>
<REF><ORG>AMERICAN WATER WORKS ASSOCIATION (AWWA)</ORG><BRK/>
<BRK/>
<RID>AWWA C511</RID><RTL>(2017; R 2021) Reduced-Pressure Principle Backflow Prevention Assembly</RTL><BRK/>
<BRK/></REF>
<REF><ORG>NATIONAL FIRE PROTECTION ASSOCIATION (NFPA)</ORG><BRK/>
<BRK/>
<RID>NFPA 70</RID><RTL>(2023; ERTA 1 2024; TIA 24-1; TIA 25-2) National Electrical Code</RTL><BRK/>
<BRK/>
<RID>NFPA 241</RID><RTL>(2022; ERTA 22-1) Standard for Safeguarding Construction, Alteration, and Demolition 
Operations</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. ARMY CORPS OF ENGINEERS (USACE)</ORG><BRK/>
<BRK/>
<RID>EM 385-1-1</RID><RTL>(2024) Safety -- Safety and Occupational Health (SOH) Requirements</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. FEDERAL HIGHWAY ADMINISTRATION (FHWA)</ORG><BRK/>
<BRK/>
<RID>MUTCD</RID><RTL>(2023) Manual on Uniform Traffic Control Devices</RTL><BRK/>
<BRK/></REF>
</SPT><SPT><TTL>SUBMITTALS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Review submittal description (SD) definitions in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES and edit the following 
list, and corresponding submittal items in the text, to reflect only the submittals required for the project.  
The Guide Specification technical editors have classified those items that require Government approval, due to 
their complexity or criticality, with a "G."  Generally, other submittal items can be reviewed by the Contractor's 
Quality Control System.  Only add a “G” to an item, if the submittal is sufficiently important or complex in context 
of the project.<BRK/>
<BRK/>
<TAI OPT="ARMY">For Army projects, fill in the empty brackets following the "G" classification, with a code of up to three characters 
to indicate the approving authority.  Codes for Army projects using the Resident Management System (RMS) are:  
"AE" for Architect-Engineer; "DO" for District Office (Engineering Division or other organization in the District 
Office); "AO" for Area Office; "RO" for Resident Office; and "PO" for Project Office.  </TAI>Codes following the "G" 
typically are not used for Navy and Air Force projects.<BRK/>
<BRK/>
The "S" classification indicates submittals required as proof of compliance for sustainability Guiding Principles 
Validation or Third Party Certification and as described in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
<TAI OPT="NAVY DESIGN-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Navy Design-Build projects, delete <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES, and replace with UFGS 01 33 00.05 
20 CONSTRUCTION SUBMITTAL PROCEDURES and UFGS 01 33 10.05 20 DESIGN SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Government approval is required for submittals with a "G" or "S" classification.<TAI OPT="AIR FORCE,NAVY">  Submittals not having a "G" or "S" classification are for Contractor 
Quality Control approval.</TAI><TAI OPT="ARMY">  Submittals not having a "G" or "S" classification are for information only.  When used, a code following the "G" classification 
identifies the office that will review the submittal for the Government.</TAI>  Submit the following in accordance with Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES:</TXT><BRK/>
<BRK/>
<LST><SUB>SD-01 Preconstruction Submittals</SUB></LST><BRK/>
<TAI OPT="NAVFAC PAC"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects in the NAVFAC PAC Area of Operation, and for the submittals identified as SD-01 Preconstruction 
Submittals, remove the "G" designation.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<BRK/>
<ITM><SUB>Construction Site Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Traffic Control Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Haul Road Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Contractor Computer Cybersecurity Compliance Statements</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Contractor Temporary Network Cybersecurity Compliance Statements</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<TAI OPT="NAVFAC SE"><LST><SUB>SD-03 Product Data</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Backflow Preventers</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM></TAI><BRK/>
<BRK/>
<LST><SUB>SD-06 Test Reports</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Backflow Preventer Tests</SUB></ITM><BRK/>
<BRK/>
<LST><SUB>SD-07 Certificates</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Backflow Tester</SUB> Certification</ITM><BRK/>
<BRK/>
<ITM><SUB>Backflow Preventers</SUB> Certificate of Full Approval</ITM><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>CONSTRUCTION SITE PLAN</SUB></TTL><BRK/>
<BRK/>
<TXT>Prior to the start of work, submit for Government approval a site plan showing the locations and dimensions of temporary facilities (including 
layouts and details, equipment and material storage area (onsite and offsite), and access and haul routes, avenues of ingress/egress to the fenced 
area and details of the fence installation.  Identify any areas which may have to be graveled to prevent the tracking of mud.  Indicate if the 
use of a supplemental or other staging area is desired. Show locations of safety and construction fences, site trailers, construction entrances, 
trash dumpsters, temporary sanitary facilities, and worker parking areas.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>BACKFLOW PREVENTERS</SUB> CERTIFICATE</TTL><BRK/>
<BRK/>
<SPT><TTL>Backflow Tester Certificate</TTL><BRK/>
<BRK/>
<TXT>Prior to testing, submit to the Contracting Officer certification issued by the State or local regulatory agency attesting that the <SUB>backflow tester</SUB>
 has successfully completed a certification course sponsored by the regulatory agency.  Tester must not be affiliated with a company participating 
in other phases of this Contract.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Backflow Prevention Training Certificate</TTL><BRK/>
<BRK/>
<TXT>Submit a certificate recognized by the State or local authority that states the Contractor has completed at least 10 hours of training in backflow 
preventer installations.  The certificate must be current.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>CONDITION OF READINESS (COR) LEVELS FOR WEATHER</TTL><BRK/>
<BRK/>
<TXT>The Condition of Readiness (COR) is based on the weather forecast and the potential for sustained winds 50 knots (<MET>93 km/hr</MET><ENG>58 mph</ENG>) or greater.  
Contact the Contracting Officer for the current COR.</TXT><BRK/>
<BRK/>
<TXT>Monitor weather conditions a minimum of twice a day and take appropriate actions according to the approved Emergency Plan in the accepted Accident 
Prevention Plan, <RID>EM 385-1-1</RID> Emergency Plan requirements and the instructions below.</TXT><BRK/>
<BRK/>
<TXT>Unless otherwise directed by the Contracting Officer, comply with:</TXT><BRK/>
<OLG><BRK/>
<OLI>Condition FOUR (Sustained winds of<MET> 93 km/hr</MET><ENG> 58 mph</ENG> or greater expected within 72 hours):  Normal daily jobsite cleanup and good housekeeping 
practices.  Collect and store in piles or containers scrap lumber, waste material, and rubbish for removal and disposal at the close of 
each work day.  Maintain the construction site including storage areas, free of accumulation of debris.  Stack form lumber in neat piles 
less than<MET> one m</MET><ENG> 3.3 feet</ENG> high.  Remove all debris, trash, or objects that could become missile hazards.  Review requirements pertaining 
to "Condition THREE" and continue action as necessary to attain "Condition FOUR" readiness.  Contact Contracting Officer for weather and 
COR updates and completion of required actions.</OLI><BRK/>
<BRK/>
<OLI>Condition THREE (Sustained winds of<MET> 93 km/hr</MET><ENG> 58 mph</ENG> or greater expected within 48 hours):  Maintain "Condition FOUR" requirements and commence 
securing operations necessary for "Condition ONE" which cannot be completed within 18 hours.  Cease all routine activities which might 
interfere with securing operations.  Commence securing and stow all gear and portable equipment.  Make preparations for securing buildings.  
Reinforce or remove formwork and scaffolding.  Secure machinery, tools, equipment, materials, or remove from the jobsite.  Expend every 
effort to clear all missile hazards and loose equipment from general base areas.  Contact Contracting Officer for weather and COR updates 
and completion of required actions.  Review requirements pertaining to "Condition TWO" and continue action as necessary to attain "Condition 
THREE" readiness.  </OLI><BRK/>
<BRK/>
<OLI>Condition TWO (Sustained winds of<MET> 93 km/hr</MET><ENG> 58 mph</ENG> or greater expected within 24 hours):  Secure the jobsite, and leave Government premises.</OLI><BRK/>
<BRK/>
<OLI>Condition ONE.  (Sustained winds of<MET> 93 km/hr</MET><ENG> 58 mph</ENG> or greater expected within 12 hours):  Contractor access to the jobsite and Government 
premises is prohibited.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>CYBERSECURITY DURING CONSTRUCTION</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The requirements in this subpart are included to provide a basic level of "cyber hygiene" during the construction 
process, and the controls that they are related to are still noted for reference.  Paragraphs in this Article 
contain text in curly braces ("{" and "}") indicating which cybersecurity control and control correlation identifier 
(CCI) the requirements of the subpart relate to.  The text inside these curly braces is for Government reference 
only, and enables coordination of the requirements of this Article with the RMF process throughout the design 
and construction process.  Text in curly braces are not contractor requirements. </NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>{For Reference Only:  This subpart (and its subparts) relates to AC-18, SA-3, CCI-00258.}  Meet the following requirements throughout the construction 
process.</TXT><BRK/>
<BRK/>
<SPT><TTL>Contractor Computer Equipment</TTL><BRK/>
<BRK/>
<TXT>Contractor owned computers may be used for construction.  When used, contractor computers must meet the following requirements:</TXT><BRK/>
<BRK/>
<SPT><TTL>Operating System</TTL><BRK/>
<BRK/>
<TXT>The operating system must be an operating system currently supported by the manufacturer of the operating system.  The operating system must be 
current on security patches and operating system manufacturer required updates.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Anti-Malware Software</TTL><BRK/>
<BRK/>
<TXT>The computer must run anti-malware software from a reputable software manufacturer.  Anti-malware software must be a version currently supported 
by the software manufacturer, must be current on all patches and updates, and must use the latest definitions file.  All computers used on this 
project must be scanned using the installed software at least once per day. </TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Passwords and Passphrases</TTL><BRK/>
<BRK/>
<TXT>The passwords and passphrases for all computers must be changed from their default values.  Passwords must be a minimum of eight characters with 
a minimum of one uppercase letter, one lowercase letter, one number and one special character.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>Contractor Computer Cybersecurity Compliance Statements</SUB></TTL><BRK/>
<BRK/>
<TXT>Provide a single submittal containing completed Contractor Computer Cybersecurity Compliance Statements for each company using contractor owned 
computers.  Contractor Computer Cybersecurity Compliance Statements must use the template published at <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-01-50-00">https://www.wbdg.org/dod/ufgs/ufgs-01-50-00</URL>
.  Each Statement must be signed by a cybersecurity representative for the relevant company.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Temporary IP Networks</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The allowance of connection to "Government furnished IP networks provided for this purpose" covers the 
case of there being a "guest" network the contractor can use.  This is likely not available in many cases, but 
is covered here for the instances in which it is offered by the project site.</NPR><BRK/>
<BRK/>
<NPR>Use the first bracketed option if Contractor furnished Wi-Fi network is optional.  Use the second bracketed option 
if the Contractor must provide a Wi-Fi network for Government use.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[Temporary Contractor-installed IP networks may be used during construction.][  Provide Government access to Contractor furnished temporary IP 
networks during construction.]  When used, temporary contractor-installed IP networks must meet the following requirements:</TXT><BRK/>
<BRK/>
<SPT><TTL>Network Boundaries and Connections</TTL><BRK/>
<BRK/>
<TXT>The network must not extend outside the project site and must not connect to any IP network other than IP networks provided under this project 
or Government furnished IP networks provided for this purpose.  Any and all network access from outside the project site is prohibited.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Government Access to Network</TTL><BRK/>
<BRK/>
<TXT>Government personnel, as defined, prescribed, and identified by the Contracting Officer, must be allowed to have complete and immediate access 
to the network at any time in order to verify compliance with this specification.  If there is a Government agency responsible for network access, 
identify that agency.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Temporary Wireless IP Networks</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Contractor provided Wi-Fi network option provides capability for the Government to have access to Wi-Fi 
for use with mobile devices in the field.  Edit the option in paragraph TEMPORARY IP NETWORKS to select the second 
bracketed option and include the bracketed option in paragraph CONTRACTOR PROVIDED WI-FI NETWORK below.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Contractor Provided Wi-Fi Network  </TTL><BRK/>
<BRK/>
<TXT>Provide standalone Wi-Fi network for authorized Government personnel.  Network access must be available throughout the jobsite and for the entire 
Contract period.  The Government will use the Wi-Fi service for coordination in the field and related activities.  Do not attach or connect the 
temporary Wi-Fi network to Government networks or systems unrelated to construction activities.</TXT><BRK/>
<BRK/>
<TXT>Password information must adhere to requirements outlined in Paragraph PASSWORDS AND PASSPHRASES.  Provide password and Wi-Fi network name (SSID) 
to the Contracting Officer for Government personnel access.  Wi-Fi performance must be capable of handling bandwidth to support Government and 
Contractor activities, including drawing and model access onsite.  Provide a point of contact for reporting Wi-Fi outages.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Temporary Wireless IP Networks Security</TTL><BRK/>
<BRK/>
<TXT>In addition to the other requirements on temporary IP networks, temporary wireless IP (WiFi) networks must not interfere with existing wireless 
network and must use WPA2 security.  Network names (SSID) for wireless networks must be changed from their default values.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Passwords and Passphrases</TTL><BRK/>
<BRK/>
<TXT>The passwords and passphrases for all network devices and network access must be changed from their default values.  Passwords must be a minimum 
8 characters with a minimum of one uppercase letter, one lowercase letter, one number and one special character.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL><SUB>Contractor Temporary Network Cybersecurity Compliance Statements</SUB></TTL><BRK/>
<BRK/>
<TXT>Provide a single submittal containing completed Contractor Temporary Network Cybersecurity Compliance Statements for each company implementing 
a temporary IP network.  Contractor Temporary Network Cybersecurity Compliance Statements must use the template published at <URL HREF="https://www.wbdg.org/dod/ufgs/ufgs-01-50-00">https://www.wbdg.org/dod/ufgs/ufgs-01-50-00</URL>
.  Each Statement must be signed by a cybersecurity representative for the relevant company.  If no temporary IP networks will be used, provide 
a single copy of the Statement indicating this.</TXT><BRK/>
<BRK/></SPT>
</SPT></PRT><PRT><TTL>PART 2   PRODUCTS</TTL><BRK/>
<BRK/>
<SPT><TTL>TEMPORARY SIGNAGE</TTL><BRK/>
<BRK/>
<SPT><TTL>Bulletin Board</TTL><BRK/>
<BRK/>
<TXT>Prior to the commencement of work activities, provide a clear weatherproof covered bulletin board not less than<MET> 915 by 1220 mm</MET><ENG> 36 by 48 inches</ENG> 
in size for displaying the Equal Employment Opportunity poster, a copy of the wage decision contained in the Contract, Wage Rate Information poster, 
Safety and Health Information as required by <RID>EM 385-1-1</RID> and other information approved by the Contracting Officer.  Coordinate requirements herein 
with <SRF>01 35 26</SRF> GOVERNMENTAL SAFETY REQUIREMENTS.  Locate the bulletin board at the project site in a conspicuous place easily accessible to all 
employees, and in location as approved by the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Project Identification Signs</TTL><BRK/>
<BRK/>
<TXT>The requirements for the signs, their content, and location are [as indicated][ and ][as specified in Section <SRF>01 58 00</SRF> PROJECT IDENTIFICATION]. 
Erect signs within 15 days after receipt of the notice to proceed.  Correct the data required by the safety sign daily, with light colored metallic 
or non-metallic numerals.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Warning Signs</TTL><BRK/>
<BRK/>
<TXT>Post temporary signs, tags, and labels to give workers and the public adequate warning and caution of construction hazards according to the <RID>EM 385-1-1</RID>
.  Attach signs to the perimeter fencing every 150 feet warning the public of the presence of construction hazards.  Signs must require unauthorized 
persons to keep out of the construction site. Correct the data required by safety signs daily.  Post signs at all points of entry designating the 
construction site as a hard hat area.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>TEMPORARY TRAFFIC CONTROL</TTL><BRK/>
<BRK/>
<SPT><TTL>Haul Roads</TTL><BRK/>
<TAI OPT="NAVFAC PAC"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects in the NAVFAC PAC Area of Operation, remove the bracketed portion "by the Contracting Officer" 
in the 6th sentence. </NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Construct access and haul roads necessary for proper prosecution of the work under this Contract in accordance with <RID>EM 385-1-1</RID>.  Construct with 
suitable grades and widths; avoid sharp curves, blind corners, and dangerous cross traffic.  Submit <SUB>haul road plan</SUB> for approval.  Provide necessary 
lighting, signs, barricades, and distinctive markings for the safe movement of traffic.  The method of dust control, although optional, must be 
adequate to ensure safe operation at all times.  Location, grade, width, and alignment of construction and haul roads are subject to approval[ 
by the Contracting Officer].  Lighting must be adequate to assure full and clear visibility for full width of haul road and work areas during any 
night work operations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Barricades</TTL><BRK/>
<BRK/>
<TXT>Erect and maintain temporary barricades to limit public access to hazardous areas.  Barricades are required whenever safe public access to paved 
areas such as roads, parking areas or sidewalks is prevented by construction activities or as otherwise necessary to ensure the safety of both 
pedestrian and vehicular traffic.  Securely place barricades clearly visible with adequate illumination to provide sufficient visual warning of 
the hazard during both day and night.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>FENCING</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Evaluate fencing requirements based on the exposure potential of the construction site to the public.  
The public is considered as any non-construction personnel.  Minimum fencing may range from nylon fabric (reinforced 
by a top supporting cable to provide adequate strength to provide needed physical protection) to<MET> 2400 mm</MET><ENG> 8 foot</ENG>
 chain link fencing.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the second (optional) paragraph if projects require special privacy fencing based on project size, 
scope, complexity, and visibility.  Coordinate with the supporting local USACE District for Army projects and 
NAVFAC FEAD or ROICC office for Navy projects to determine if a privacy fence is required.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide fencing along the construction site and at all open excavations and tunnels to control access by unauthorized personnel.  Safety fencing 
must be highly visible to be seen by pedestrians and vehicular traffic.  All fencing must meet the requirements of <RID>EM 385-1-1</RID>.  Remove the fence 
upon completion and acceptance of the work.</TXT><BRK/>
<BRK/>
[<TXT>To block public view of the construction, enclose the project work area and Contractor lay-down area with a<MET> 2400 mm</MET><ENG> 8 ft</ENG> high [shadow-box type, 
wooden fence and gates][chain link fence and gates with brown, UV light resistant, plastic fabric mesh netting (similar to tennis court or other 
screening).]</TXT><BRK/>
<BRK/>
][<SPT><TTL>Polyethylene Mesh Safety Fencing</TTL><BRK/>
<BRK/>
<TXT>Temporary safety fencing must be a high visibility orange colored, high density polyethylene grid, a minimum of<MET> 1.2 m</MET><ENG> 48 inches</ENG> high and maximum 
mesh size of<MET> 50 mm</MET><ENG> 2 inches</ENG>.  Fencing must extend from the grade to a minimum of<MET> 1.2 m</MET><ENG> 48 inches</ENG> above the grade and be tightly secured to T-posts 
spaced as necessary to maintain a rigid and taut fence.  Fencing must remain rigid and taut with a minimum of<MET> 90.7 kilograms (kg)</MET><ENG> 200 pounds</ENG> of 
force exerted on it from any direction with less than<MET> 100 mm</MET><ENG> 4 inches</ENG> of deflection. </TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Chain Link Panel Fencing</TTL><BRK/>
<BRK/>
<NTE><AST/><BRK/>
<NPR>NOTE: Select 6 feet high chain link fencing unless 8 feet is needed for additional security. </NPR><BRK/>
<AST/><BRK/></NTE>
<TXT>Temporary panel fencing must be galvanized steel chain link panels [<MET>1.8 m</MET><ENG>6 feet</ENG>] [<MET>2.4 m</MET><ENG>8 feet</ENG>] high.  Multiple fencing panels may be linked together 
at the bases to form long spans as needed.  Each panel base must be weighted down using sand bags or other suitable materials in order for the 
fencing to withstand anticipated winds while remaining upright.  Fencing must remain rigid and taut with a minimum of<MET> 90.7 kg</MET><ENG> 200 pounds</ENG> of force 
exerted on it from any direction with less than<MET> 100 mm</MET><ENG> 4 inches</ENG> of deflection.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Post-Driven Chain Link Fencing</TTL><BRK/>
<BRK/>
<TXT>Temporary post-driven fencing must be galvanized chain link fencing [<MET>1.8 m</MET><ENG>6 feet</ENG>] [<MET>2.4 m</MET><ENG>8 feet</ENG>] high supported by an tightly secured to galvanized 
steel posts driven below grade.  Fence posts must be located on minimum<MET> 3 meter</MET><ENG> 10 foot</ENG> centers.  Posts may be set in various surfaces such as 
sand, soil, asphalt or concrete as necessary. Chain link fencing must remain rigid and taut with a minimum of<MET> 90.7 kg</MET><ENG> 200 pounds</ENG> of force exerted 
on it from any direction with less than<MET> 100 mm</MET><ENG> 4 inches</ENG> of deflection.  Completely remove fencing and posts at the completion of construction and 
restore surfaces disturbed or damaged to its original condition.  Locate and identify underground utilities prior to setting fence posts.  Equip 
fence with a lockable gate.  Gate must remain locked when construction personnel are not present.</TXT><BRK/>
<BRK/></SPT>
]</SPT><SPT><TTL>TEMPORARY WIRING</TTL><BRK/>
<BRK/>
<TXT>Provide temporary wiring in accordance with <RID>EM 385-1-1</RID>, <RID>NFPA 241</RID> and <RID>NFPA 70</RID>.  Include monthly inspection and testing of all equipment and apparatus.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>BACKFLOW PREVENTERS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following for all projects connecting to a potable water supply.</NPR><BRK/>
<BRK/>
<NPR>Consider using a lead free, brass body backflow preventer assembly on water lines<MET> 50 mm</MET><ENG> 2 inches</ENG> or smaller.  
For water lines greater than<MET> 50 mm</MET><ENG> 2 inches</ENG>, consider using a cast-iron body backflow preventer assembly.</NPR><BRK/>
<BRK/>
<NPR>Coordinate with Base Utilities/PWD for any approved list of backflow preventers and edit accordingly.  Add any 
specific testing or certification requirements to Part 3 Article for Backflow Preventers.</NPR><BRK/>
<BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Certificate of Full Approval from FCCCHR List, University of Southern California, attesting that the design, size and make of each backflow preventer 
has satisfactorily passed the complete sequence of performance testing and evaluation for the respective level of approval.  Certificate of Provisional 
Approval is not acceptable.</TXT><BRK/>
<BRK/>
<TXT>Reduced pressure principle type conforming to the applicable requirements <RID>AWWA C511</RID>.  Provide backflow preventers complete with <MET>[68 kg]</MET><ENG>[150 pound]</ENG>
 [_____] flanged [cast iron],[ ductile iron,] [bronze,][brass] mounted gate valve [and strainer], [304][_____] stainless steel or bronze, internal 
parts.</TXT><BRK/>
<BRK/></SPT>
</PRT><PRT><TTL>PART 3   EXECUTION</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Delete inapplicable paragraphs, selecting desired options for electricity, water, gas, heating and ventilating, 
sanitary, and fire protection facilities.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>EMPLOYEE PARKING</TTL><BRK/>
<BRK/>
<TXT>Construction Contract employees must park privately owned vehicles in an area designated by the Contracting Officer.  Employee parking must not 
interfere with existing and established parking requirements of the Government installation.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>AVAILABILITY AND USE OF UTILITY SERVICES</TTL><BRK/>
<BRK/>
<SPT><TTL>Temporary Utilities</TTL><BRK/>
<BRK/>
<TXT>Provide temporary utilities required for construction.  Materials may be new or used, must be adequate for the required usage, not create unsafe 
conditions, and not violate applicable codes and standards.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="ARMY,NAVY"><SPT><TTL>Payment for Utility Services</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraphs related to payment of utilities for Army and Navy projects only.  </NPR><BRK/>
<BRK/>
<NPR>Coordinate this paragraph with the Contracting Officer.  Coordinate with FAR 52.236-14 Availability and Use of 
Utility Services.  Choose one of the following options.<TAI OPT="NAVFAC LANT">  For NAVFAC, delete this set or paragraphs if utility 
service is covered in a paragraph "Utilities at (_____)"; used for some stations on a regional basis.</TAI></NPR><BRK/>
<BRK/>
<NPR>Government utilities listed in this paragraph may be furnished, if available without interfering with Government 
needs.  These services will not be made free of charge except: (1) on Air Force projects; (2) on other projects 
when administrative costs exceed the value of the services; or (3) when otherwise advantageous to the Government.  
Indicate the point at which the Government will deliver each utility specified and show pertinent data such as 
voltage,<MET> L/min</MET><ENG> gal/min</ENG>, and pipe sizes on the general layout plan or other appropriate drawing.  Information regarding 
the types of utilities available, the rates, the points of connection' and the quantities available should be 
obtained from the Government.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
<OLI>The Government will make all reasonably required utilities available from existing outlets and supplies, as specified in the Contract.  
Unless otherwise provided in the Contract, the amount of each utility service consumed will be charged to or paid at prevailing rates charged 
to the Government or, where the utility is produced by the Government, at reasonable rates determined by the Contracting Officer.  Carefully 
conserve utilities furnished without charge.</OLI><BRK/>
<BRK/>
<OLI>Reasonable amounts of the following utilities will be made available  [without charge.] [at the prevailing rates.] [at the following rates:]</OLI><BRK/>
<OLI><TAB>
<WBK>
   <STS>
      <STY SID="s50">
         <ALN HORIZONTAL="CENTER" VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="3" ROWCOUNT="9">
      <COL AUTOWIDTH="0" WIDTH="144.00"/>
      <COL AUTOWIDTH="0" WIDTH="144.00"/>
      <COL AUTOWIDTH="0" WIDTH="144.00"/>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL MERGEACROSS="2">
<DTA TYPE="STRING"><HL4>Utility Services</HL4></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Cost ($) per</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Unit</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL>
<DTA TYPE="STRING">Electricity</DTA>
         </CEL>
         <CEL/>
         <CEL/>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL>
<DTA TYPE="STRING">Potable Water</DTA>
         </CEL>
         <CEL/>
         <CEL/>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL>
<DTA TYPE="STRING">Salt Water</DTA>
         </CEL>
         <CEL/>
         <CEL/>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL>
<DTA TYPE="STRING">Compressed Air</DTA>
         </CEL>
         <CEL/>
         <CEL/>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL>
<DTA TYPE="STRING">Steam</DTA>
         </CEL>
         <CEL/>
         <CEL/>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL>
<DTA TYPE="STRING">Natural Gas</DTA>
         </CEL>
         <CEL/>
         <CEL/>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="47.25">
         <CEL>
<DTA TYPE="STRING">Sanitary Sewer</DTA>
         </CEL>
         <CEL/>
         <CEL/>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB></OLI><BRK/>
<OLI>The point at which the Government will deliver such utilities or services and the quantity available is [as indicated][must be coordinated 
with the Contracting Officer].  Pay all costs incurred in connecting, converting, and transferring the utilities to the work.  Make connections, 
including [providing backflow-preventing devices on connections to domestic water lines;] [providing meters;] and providing transformers; 
and make disconnections.  <TAI OPT="NAVFAC ML">Under no circumstances will taps to base fire hydrants be allowed for obtaining domestic water.</TAI></OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  If constraints prevent the Government from providing utilities, include the following paragraph and delete 
prior paragraphs applicable to provision of utilities by the Government.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>The Contractor must provide their own utilities.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Meters and Temporary Connections</TTL><BRK/>
<BRK/>
<TXT>Provide and maintain necessary temporary connections, distribution lines, and meter bases (Government will provide meters) required to measure 
the amount of each utility used for the purpose of determining charges.  Notify the Contracting Officer, in writing, 5 working days before final 
electrical connection is desired so that a utilities contract can be established.  The Government will provide a meter and make the final hot connection 
after inspection and approval of the Contractor's temporary wiring installation.  Do not make the final electrical connection.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Advance Deposit</TTL><BRK/>
<BRK/>
<TXT>An advance deposit for utilities consisting of an estimated month's usage or a minimum of $50.00 will be required.  The last monthly bills for 
the fiscal year will normally be offset by the deposit and adjustments will be billed or returned as appropriate.  Services to be rendered for 
the next fiscal year, beginning 1 October, will require a new deposit.  Notification of the due date for this deposit will be mailed prior to the 
end of the current fiscal year.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Final Meter Reading</TTL><BRK/>
<BRK/>
<TXT>Before completion of the work and final acceptance of the work by the Government, notify the Contracting Officer, in writing, 5 working days before 
termination is desired.  The Government will take a final meter reading, disconnect service, and remove the meters.  Then remove all the temporary 
distribution lines, meter bases, and associated appurtenances.  Pay all outstanding utility bills before final acceptance of the work by the Government.</TXT><BRK/>
<BRK/></SPT>
</TAI><TAI OPT="NAVY"><SPT><TTL>Utilities at Special Locations</TTL><BRK/>
<TAI OPT="NAVFAC LANT"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following set of paragraphs are tailored for use on NAVY projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For NAVFAC projects choose one of the following options.  The first subparagraph is tailored for use on 
NAVFAC LANT projects only.  For the first option, in the first set of brackets, insert the name of the activity 
to which application should be made.  Include the second bracketed expression for projects located at MCAS Cherry 
Point.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<LST INDENT="-0.33">a.  Reasonable amounts of utilities will be made available at the prevailing Government rates.  These rates may be obtained upon application 
to the Commanding Officer, [_____], by way of the Contracting Officer.  Make connections, provide transformers and meters, and make disconnections; 
and provide backflow preventer devices on connections to domestic water lines.  [Neither potable water nor sanitary facilities will be 
available at the main Contractor laydown area at Marine Corps Air Station (MCAS), Cherry Point, NC.]</LST>]</TAI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following option for projects located in Argentina and the Azores and for Air Force projects in 
the NAVFAC Atlantic Area of Responsibility.  Use this paragraph for other activities only when approved by the 
activity.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<LST INDENT="-0.33">b. Reasonable amounts of utilities will be made available without charge.  Make connections, provide transformers and meters, and make 
disconnections; and provide backflow preventer devices on connections to domestic water lines.  Under no circumstances will taps to base 
fire hydrants be allowed for obtaining domestic water.</LST>]<BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following option only for MCON funded and non-appropriated funds projects at Marine Corps Base, 
Camp Lejeune and Marine Corps Air Station (Helicopter (H)), New River.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<LST INDENT="-0.33">c.  Reasonable amounts of utilities will be made available at the prevailing Government rates and may be obtained upon application to the 
Base Maintenance Officer, Bldg. 1202, Marine Corps Base, Camp Lejeune.  A refundable security deposit to the Resident Officer in Charge 
of Construction must be made prior to application for services.  Provide transformers, meter bases, electrical service poles and drops 
for electrical services, and backflow preventer devices on connections to domestic water lines.  Final taps and tie-ins to the Government 
utility grid will be made by Base Maintenance who will also provide and seal a 120 or 208 volt, three-wire kWh meter.  Tap-in cost, if 
any, is the responsibility of the Contractor.  Tampering or movement of a sealed meter without notification to base maintenance is grounds 
for discontinuance of electrical service.  Provide larger meters required if they are not available from the Government.  The Contractor 
is responsible for the cost of utility services required until the date of Government acceptance. Under no circumstances will taps to base 
fire hydrants be allowed for obtaining domestic water.</LST>]<BRK/>
<BRK/>
<TAI OPT="NAVFAC PAC"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following set of subparagraphs are tailored for use on NAVFAC PAC projects only.  Include the bracketed 
options as applicable.</NPR><BRK/>
<AST/><BRK/></NTE>
[<SPT><TTL>Utilities at Guam by Contractor for Special Projects</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this subparagraph for projects in Guam.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<BRK/>
<TXT>Contact the Government of Guam for water and electricity.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Utility Services at Midway</TTL><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following subparagraphs for projects at Midway.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLG><BRK/>
<OLI>Potable water is rationed during dry periods and not available for construction purposes during the months of June and July.</OLI><BRK/>
<BRK/>
<OLI>Electrical power available, primary voltage is 2400 volt 3 phase, 3 wire, 60 cycle AC.  Secondary voltages may be 120/208 or 120/240 volts.</OLI><BRK/>
<BRK/>
<OLI>Provide new meters for potable water, brackish water and electricity.  The cost of utility services furnished may be reduced by the cost 
the Government would normally pay for comparable meters if, at the end of the job, the meters are delivered to the Government in good condition.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI></SPT><TAI OPT="NAVFAC FE"><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following set of paragraphs are tailored for use on NAVFAC FE projects only.  Include the bracketed 
options as applicable.</NPR><BRK/>
<AST/><BRK/></NTE>
[<SPT><TTL>Utility Services for Diego Garcia Projects</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraphs for  Diego Garcia projects.  Contact the local Public Works office and insert 
the prevailing utility rates at the time of the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLG><BRK/>
<OLI>Potable water will be made available to Contractor's office and housing.  The prevailing rate for potable water is [$_____] per<MET> 3800 L</MET><ENG> 
thousand gallons</ENG>.</OLI><BRK/>
<BRK/>
<OLI>No charge for brackish water.</OLI><BRK/>
<BRK/>
<OLI>Electrical power available is primary, 2400 volt 3 phase, 3 wire, 60 cycle AC, secondary voltages may be 120/208 or 120/240 volts.  The 
prevailing rate for electricity is [$_____] per kilowatt hour (KWH).</OLI><BRK/>
<BRK/>
<OLI>Sewage costs at [$_____] per<MET> 3800 L</MET><ENG> KGAL</ENG>.</OLI><BRK/>
<BRK/>
<OLI>Provide new meters for potable water and electricity.  The cost of utility services furnished may be reduced by the cost the Government 
would normally pay for comparable meters if, at the end of the job, the meters are delivered to the Government in good condition.</OLI><BRK/></OLG>
<BRK/>
[<SPT><TTL>Contractor-Owned and Operated Radio Telecommunications</TTL><BRK/>
<BRK/>
<TXT><TST>A transmitter/receiver and antenna may be erected upon approval by the Contracting Officer. Submit for approval, 30 calendar days prior to the 
use of the equipment, the type of radio equipment power and band width of the equipment.</TST></TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Off-Island</TTL><BRK/>
<BRK/>
<TXT>The Government will provide military message communication from Diego Garcia at no cost.  The Contractor is responsible for the cost of retransmitting 
messages through commercial sources.  Process messages through the Contracting Officer.  Messages will be screened and limited use of communication 
facilities will be permitted.  Private messages will be permitted only for emergencies.  The Navy voice communication system is no longer available 
for use. A local vendor provides commercial voice and teletype services for [$_____] per minute.</TXT><BRK/>
<BRK/></SPT>
]</SPT>]<SPT><TTL>Utility Services for Wake Island</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraphs for Wake Island projects.  Contact the local Public Works office and insert 
the prevailing utility rates at the time of the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<BRK/>
<LST INDENT="-0.33">[a.  Potable water may not be available for construction during dry periods.  Desalinized water available during dry periods at [$_____] 
per day for<MET> 114-150 kL</MET><ENG> 30,000-40,000 gallons</ENG> per day.</LST><BRK/>
<BRK/>
<LST INDENT="-0.33">b.  Available primary voltage is 4160 volts, 3 phase, 3 wire, 60 cycle.   Secondary voltage is 120/208 volts, 3 phase, 60 cycle.]</LST><BRK/>
<BRK/></SPT>
[<SPT><TTL>Telephones at Midway, Wake, and Diego Garcia</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraph for Midway, Wake Island, and Diego Garcia projects only.  Contact the local 
Public Works office and insert the prevailing utility rates at the time of the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<BRK/>
<TXT>On-Island service may be obtained if lines are available.  Make arrangements through the Contracting Officer.  The prevailing rate for cable or 
wireless is [$_____] per phone.  There is no charge for on-island telephone service.  [Current rates are [$_____] per month for each private telephone 
line plus an installation charge of [$_____] for each instrument and [$_____] per month for two-party lines plus [$_____] per month for each extension.  
Pay for the cost of the wiring on runs in excess of two spans].  Long distance services are usually available at commercial rates.  The Navy Radio 
Communication System or Defense Switch Network will not be available for use.  [Limited teletypewriter circuit service is available.]</TXT><BRK/>
<BRK/></SPT>
]</TAI></TAI><SPT><TTL>Sanitation</TTL><BRK/>
<BRK/>
<TXT>Provide and maintain within the construction area minimum field-type sanitary facilities in accordance with <RID>EM 385-1-1</RID>.  Locate the facilities 
behind the construction fence or out of the public view.  Clean units and empty wastes at least once a week or more frequently into a municipal, 
district, or station sanitary sewage system, or remove waste to a commercial facility.  Obtain approval from the system owner prior to discharge 
into a municipal, district, or commercial sanitary sewer system.  Penalties or fines associated with improper discharge will be the responsibility 
of the Contractor. Coordinate with the Contracting Officer and follow station regulations and procedures when discharging into the station sanitary 
sewer system.  Maintain these conveniences at all times.  Include provisions for pest control and elimination of odors. Government toilet facilities 
will not be available to Contractor's personnel.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Telephone</TTL><BRK/>
<BRK/>
<TXT>Make arrangements and pay all costs for telephone facilities desired.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Fire Protection</TTL><BRK/>
<BRK/>
<TXT>Provide temporary fire protection equipment for the protection of personnel and property during construction.  Remove debris and flammable materials  
[daily][weekly][monthly] to minimize potential hazards.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>STATION OPERATION AFFECT ON CONTRACTOR OPERATIONS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph on all projects involving potential conflicts with operating conditions other than utilities 
or where the work must be pursued in a particular sequence.   Clearly detail the permissible extent of sequencing 
or duration of interruptions to station operation.  Obtain information from the Government.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<BRK/>
<TXT>[    ].</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>TRAFFIC PROVISIONS</TTL><BRK/>
<BRK/>
<SPT><TTL>Maintenance of Traffic</TTL><BRK/>
<OLG><BRK/>
<OLI>Conduct operations in a manner that will not close a thoroughfare or interfere with traffic on railways or highways except with written 
permission of the Contracting Officer at least 15 calendar days prior to the proposed modification date, and provide a <SUB>Traffic Control 
Plan</SUB> for Government approval detailing the proposed controls to traffic movement for approval.  The plan must be in accordance with State 
and local regulations and the <RID>MUTCD</RID>, Part VI.  [Make all notifications and obtain all permits required for modification to traffic movements 
outside Station's jurisdiction.].  Contractor may move oversized and slow-moving vehicles to the worksite provided requirements of the 
highway authority have been met.</OLI><BRK/>
<BRK/>
<OLI>Conduct work so as to minimize obstruction of traffic, and maintain traffic on at least half of the roadway width at all times.  Obtain 
approval from the Contracting Officer prior to starting any activity that will obstruct traffic.</OLI><BRK/>
<BRK/>
<OLI>Provide, erect, and maintain, at Contractor's expense, lights, barriers, signals, passageways, detours, Life Safety Signage, overhead protection, 
and other items that may be required by the authority having jurisdiction.</OLI><BRK/>
<BRK/>
<OLI>Provide cones, signs, barricades, lights, or other traffic control devices and personnel required to control traffic.  Do not use foil-backed 
material for temporary pavement marking because of its potential to conduct electricity during accidents involving downed power lines.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Protection of Traffic</TTL><BRK/>
<BRK/>
<TXT>Maintain and protect traffic on all affected roads during the construction period except as otherwise specifically directed by the Contracting 
Officer.  Measures for the protection and diversion of traffic, including the provision of watchmen and flagmen, erection of barricades, placing 
of lights around and in front of equipment the work, and the erection and maintenance of adequate warning, danger, and direction signs, will be 
as required by the State and local authorities having jurisdiction.  Provide self-illuminated (lighted) barricades during hours of darkness.  All 
personnel working in roadways will wear brightly-colored vests or other high visibility apparel in accordance with <RID>EM 385-1-1</RID>.  Protect the traveling 
public from damage to person and property.  Minimize the interference with public traffic on roads selected for hauling material to and from the 
site.  Investigate the adequacy of existing roads and their allowable load limit.  Contractor is responsible for the repair of damage to roads 
caused by construction operations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Rush Hour Restrictions</TTL><BRK/>
<BRK/>
<TXT>Do not interfere with the peak traffic flows preceding and during normal operations[ for [_____]] without notification to and approval by the Contracting 
Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Dust Control</TTL><BRK/>
<BRK/>
<TXT>Dust control methods and procedures must be approved by the Contracting Officer.  Coordinate dust control methods with <SRF>01 57 19 </SRF>TEMPORARY ENVIRONMENTAL 
CONTROLS.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>REDUCED PRESSURE BACKFLOW PREVENTERS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following for all projects connecting to a potable water supply.<BRK/>
<BRK/>
Coordinate with Base Utilities/PWD for any specific testing or certification requirements and edit accordingly.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<BRK/>
<TXT>Provide an approved reduced pressure backflow prevention assembly at each location where the Contractor taps into the Government potable water 
supply.</TXT><BRK/>
<BRK/>
<TXT>Perform <SUB>backflow preventer tests</SUB> using test equipment, procedures, and certification forms conforming to those outlined in the latest edition of 
the Manual of Cross-Connection Control published by the FCCCHR Manual.  Test and tag each reduced pressure backflow preventer upon initial installation 
(prior to continued water use) and[ quarterly][ monthly][    ] thereafter.  Tag must contain the following information:   make, model, serial number, 
dates of tests, results, maintenance performed, and signature of tester.  Record test results on certification forms conforming to requirements 
cited earlier in this paragraph.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>CONTRACTOR'S TEMPORARY FACILITIES</TTL><BRK/>
<BRK/>
<TXT>Contractor is responsible for security of their property.  Provide adequate outside security lighting at the temporary facilities.  Trailers must 
be anchored to resist high winds and meet applicable state or local standards for anchoring mobile trailers.  Coordinate anchoring with <RID>EM 385-1-1</RID>
.  The Contract Clause entitled "FAR 52.236-10, Operations and Storage Areas" and the following apply:</TXT><BRK/>
<BRK/>
<SPT><TTL>Administrative Field Offices</TTL><BRK/>
<BRK/>
<TXT>Provide and maintain administrative field office facilities within the construction area at the designated site.  Government office and warehouse 
facilities will [not] be available to the Contractor's personnel.</TXT><BRK/>
<BRK/>
<TXT>In the event a new building is constructed for the temporary project field office, it must be a minimum<MET> 3.6 m</MET><ENG> 12 feet</ENG> in width,<MET> 5 m</MET><ENG> 16 feet</ENG> in 
length and have a minimum of<MET> 2.1 m</MET><ENG> 7 feet</ENG> headroom.  Equip the building with approved electrical wiring, at least one double convenience outlet 
and the required switches and fuses to provide 110-120 volt power.  Provide a work table with stool, desk with chair, two additional chairs, and 
one legal size file cabinet that can be locked.  The building must be waterproof, supplied with a heater, have a minimum of two doors, electric 
lights, a telephone, a battery-operated smoke detector alarm, a sufficient number of adjustable windows for adequate light and ventilation, and 
a supply of approved drinking water.  Provide approved sanitary facilities.  Screen the windows and doors and provide the doors with deadbolt type 
locking devices or a padlock and heavy-duty hasp bolted to the door.  Door hinge pins must be non-removable.  Arrange the windows to open and to 
be securely fastened from the inside.  Protect glass panels in windows by  bars or heavy mesh screens to prevent easy access.  In warm weather, 
provide air conditioning capable of maintaining the office at 50 percent relative humidity and a room temperature<MET> 11 degrees C</MET><ENG> 20 degrees F</ENG> below 
the outside temperature when the outside temperature is<MET> 35 degrees C</MET><ENG> 95 degrees F</ENG>.  Unless otherwise directed by the Contracting Officer, remove 
the building from the site upon completion and acceptance of the work.</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Quality Control Manager Records and Field Office</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph when project has separate QC Manager and project Superintendent. Edit to suit the 
size and location of the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<BRK/>
<TXT>Provide on the jobsite an office with approximately<MET> [9][18][_____] square meter</MET><ENG> [100][200][_____] square feet</ENG> of useful floor area for the exclusive 
use of the QC Manager.  Provide a weathertight structure with adequate [heating and cooling,] toilet facilities, lighting, ventilation, a<MET> 1200 
by 2400 mm</MET><ENG> 4 by 8 foot</ENG> plan table, a standard size office desk and chair, computer station, and working communications facilities.  [Provide  either 
a 1,500 watt radiant heater and a window-mounted air conditioner rated at<MET> 2.6 kW</MET><ENG> 9,000 Btus</ENG> minimum or a window-mounted heat pump of the same minimum 
heating and cooling ratings.]  Provide a door with a cylinder lock and windows with locking hardware.  Make utility connections.  Locate [as directed][where 
indicated].  File quality control records in the office and make available at all times to the Government.  After completion of the work, remove 
the entire structure from the site.</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Storage Area</TTL><BRK/>
<BRK/>
<TXT>Construct a temporary<MET> 1.8 m</MET><ENG> 6 foot</ENG> high chain link fence around trailers and materials.  Include plastic strip inserts, colored [green][brown], 
so that visibility through the fence is obstructed.  Fence posts may be driven, in lieu of concrete bases, where soil conditions permit.  Do not 
place or store trailers, materials, or equipment outside the fenced area unless such trailers, materials, or equipment are assigned a separate 
and distinct storage area by the Contracting Officer away from the vicinity of the construction site but within the installation boundaries.  Trailers, 
equipment, or materials must not be open to public view with the exception of those items which are in support of ongoing work on the current day.  
Do not stockpile materials outside the fence in preparation for the next day's work.  Park mobile equipment, such as tractors, wheeled lifting 
equipment, cranes, trucks, and like equipment within the fenced area at the end of each work day.</TXT><BRK/>
<BRK/>
<TXT>Keep fencing in a state of good repair and proper alignment.  If the Contractor elects to traverse grassed or unpaved areas which are not established 
roadways with construction equipment or other vehicles, cover the grassed or unpaved areas with a layer of gravel as necessary to prevent rutting 
and the tracking of mud onto paved or established roadways; gravel gradation must be at the Contractor's discretion.  Mow and maintain grass located 
within the boundaries of the construction site for the duration of the project.  Grass and vegetation along fences, structures, under trailers, 
and in areas not accessible to mowers must be edged or trimmed neatly.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Supplemental Storage Area</TTL><BRK/>
<BRK/>
<TXT>Upon request, and pending availability, the Contracting Officer will designate another or supplemental area for the use and storage of trailers, 
equipment, and materials.  This area may not be in close proximity of the construction site but will be within the installation boundaries.  Maintain 
the area in a clean and orderly fashion and secured if needed to protect supplies and equipment. Utilities will not be provided to this area by 
the Government.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Appearance of Trailers</TTL><BRK/>
<OLG><BRK/>
<OLI>Trailers must be roadworthy and comply with all appropriate state and local vehicle requirements.  Trailers which are rusted, have peeling 
paint or are otherwise in need of repair will not be allowed on Installation property. Trailers must present a clean and neat exterior 
appearance and be in a state of good repair. </OLI><BRK/>
<BRK/>
<OLI>Maintain the temporary facilities.  Failure to do so will be sufficient reason to require their removal at the Contractor's expense.</OLI><BRK/></OLG>
<BRK/></SPT>
<TAI OPT="NAVFAC LANT"><SPT><TTL>Trailers or Storage Buildings</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for use on NAVY projects only.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
<OLI>Trailers or storage buildings will be permitted, where space is available, subject to the approval of the Contracting Officer.</OLI><BRK/>
<BRK/>
<OLI>Mount a sign not smaller than<MET> 350 by 350 mm</MET><ENG> 13.78 by 13.78 inches</ENG> on the trailer or building that shows the company name, business phone 
number, emergency phone number and conforms to the following requirements and sketch:<BRK/>
<TAB HEADERROWS="0">
<WBK>
   <STS/>
   <TDA COLUMNCOUNT="2" ROWCOUNT="4">
      <COL AUTOWIDTH="0" WIDTH="216.75"/>
      <COL AUTOWIDTH="0" WIDTH="215.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="22.50">
         <CEL>
<DTA TYPE="STRING">Graphic panel</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Aluminum, painted blue</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="22.50">
         <CEL>
<DTA TYPE="STRING">Copy</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Screen painted or vinyl die-cut, white</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="22.50">
         <CEL>
<DTA TYPE="STRING">Typeface</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Univers 65 u/lc</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="27.75">
         <CEL MERGEACROSS="1">
<DTA TYPE="STRING">See Sketch No. 01500 (graphic).</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB></OLI><BRK/></OLG>
<BRK/></SPT>
</TAI><SPT><TTL>Safety Systems</TTL><BRK/>
<BRK/>
<TXT>Protect the integrity of all installed safety systems or personnel safety devices.  Obtain prior approval from the Contracting Officer if entrance 
into systems serving safety devices is required.  If it is temporarily necessary to remove or disable personnel safety devices in order to accomplish 
Contract requirements, provide alternative means of protection prior to removing or disabling any permanently installed safety devices or equipment 
and obtain approval from the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="NAVY">[<SPT><TTL>Special Storage Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following subparagraphs are tailored for use on Navy projects only to designate any special storage 
requirements.  Coordinate with the supporting local NAVFAC FEAD or ROICC office to determine these special requirements 
and select the appropriate bracketed options, or insert other requirements, as applicable.  If no special storage 
requirements apply to the project delete this bracketed set of subparagraphs in its entirety.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<BRK/>
<TXT>The following special storage requirements apply:</TXT><BRK/>
<BRK/>
[<SPT><TTL>Storage Size and Location</TTL><BRK/>
<BRK/>
<TXT>The [roofed][enclosed][open] site available for storage must be [confined to the indicated operations area][within<MET> 300 m</MET><ENG> 1,000 feet</ENG> of the operations 
area][as indicated].  The storage area will be approximately [____]<MET> square meter</MET><ENG> square feet</ENG>.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Storage in Existing Buildings</TTL><BRK/>
<BRK/>
<TXT>The Contractor will be working [in][around] existing building[s]; the storage of material [will be allowed in a [____]<MET> square meter</MET><ENG> square foot</ENG>
 area][where indicated][will not be allowed in the building[s]].  [Provide<MET> 2.4 m</MET><ENG> 8 foot</ENG> high-security fence with a lockable gate around the storage 
area.  Remove at the completion of work.]</TXT><BRK/>
<BRK/></SPT>
]</SPT>]</TAI><SPT><TTL>Weather Protection of Temporary Facilities and Stored Materials</TTL><BRK/>
<BRK/>
<TXT>Take necessary precautions to ensure that roof openings and other critical openings in the building are monitored carefully.  Take immediate actions 
required to seal off such openings when rain or other detrimental weather is imminent, and at the end of each workday.  Ensure that the openings 
are completely sealed off to protect materials and equipment in the building from damage.</TXT><BRK/>
<BRK/>
<SPT><TTL>Building and Site Storm Protection</TTL><BRK/>
<BRK/>
<TXT>When a warning of gale force winds is issued, take precautions to minimize danger to persons, and protect the work and nearby Government property.  
Precautions must include, but are not limited to, closing openings; removing loose materials, tools and equipment from exposed locations; and removing 
or securing scaffolding and other temporary work.  Close openings in the work when storms of lesser intensity pose a threat to the work or any 
nearby Government property.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT>[<TAI OPT="AIR FORCE,ARMY"><SPT><TTL>GOVERNMENT FIELD OFFICE</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph for ARMY and AIR FORCE.  Do not use for NAVY projects.  This paragraph is tailored for 
ARMY and AIR FORCE.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Resident Engineer's Office</TTL><BRK/>
<BRK/>
<TXT>Provide the [Government Resident Engineer] [Government Engineer] with an office, approximately<MET> 19 square meters</MET><ENG> 200 square feet</ENG> in floor area, 
located where directed and providing space heat, [air conditioning unit,] electric light and power, and toilet facilities consisting of one lavatory 
and one water closet complete with connections to water and sewer mains.  Provide a mail slot in the door or a lockable mail box mounted on the 
surface of the door.  Include a<MET> 1200 by 2400 mm</MET><ENG> 4 by 8 foot</ENG> plan table,[ computer work space] a standard size office desk and chair, and telephone. 
At completion of the project, the office will remain the property of the Contractor and be removed from the site.  Utilities must be connected 
and disconnected in accordance with local codes and to the satisfaction of the Contracting Officer.  Compliance with safety and appearance requirements 
for temporary facilities stated in previous paragraphs is required.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Trailer-Type Mobile Office</TTL><BRK/>
<BRK/>
<TXT>The option is available to, furnish and maintain a trailer-type mobile office acceptable to the Contracting Officer to meet the requirements of 
the minimum facilities specified above.  Securely anchor the trailer to the ground at all four corners to guard against movement during high winds. 
Coordinate requirements for proper anchoring with <RID>EM 385-1-1</RID>. </TXT><BRK/>
<BRK/></SPT>
</SPT></TAI>]<SPT><TTL>PLANT COMMUNICATIONS</TTL><BRK/>
<BRK/>
<TXT>Whenever the individual elements of the plant are located so that operation by normal voice between these elements is not satisfactory, install 
a satisfactory means of communication, such as telephone or other suitable devices and make available for use by Government personnel.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>TEMPORARY PROJECT SAFETY FENCING</TTL><BRK/>
<BRK/>
<TXT>As soon as practicable, but not later than 15 days after the date established for commencement of work, furnish and erect temporary project safety 
fencing at the work site.  Maintain the safety fencing during the life of the Contract and, upon completion and acceptance of the work, remove 
from the work site.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="NAVFAC SE"><SPT><TTL>DUMPSTERS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This Aryicle is tailored for use on NAVFAC SE projects only.  Use the bracketed item where visibility to 
the public is an issue.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Equip dumpsters with a secure cover and paint the standard installation color.  Keep dumpster closed, except when being loaded with trash and debris.[  
Locate dumpsters behind the construction fence or out of the public view.]  Empty site dumpsters at least once a week, or as needed to keep the 
site free of debris and trash.  If necessary, provide<MET> 200 liter</MET><ENG> 55 gallon</ENG> trash containers painted the darker installation color to collect debris 
in the construction site area.  For large demolitions, large dumpsters without lids are acceptable, but must not have debris higher than the sides 
before emptying.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>CLEANUP</TTL><BRK/>
<BRK/>
<TXT>Remove construction debris, waste materials, packaging material and the like from the work site daily.  Any dirt or mud which is tracked onto paved 
or surfaced roadways must be cleaned away.  Store all salvageable materials resulting from demolition activities within the fenced area described 
above or at the supplemental storage area.  Neatly stack stored materials not in trailers, whether new or salvaged.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>RESTORATION OF STORAGE AREA</TTL><BRK/>
<BRK/>
<TXT>Upon completion of the project remove the bulletin board, signs, barricades, haul roads, and all other temporary products from the site.  After 
removal of trailers, materials, and equipment from within the fenced area, remove the fence.  Restore areas used during the performance of the 
Contract to the original or better condition.  Remove gravel used to traverse grassed areas and restore the area to its original condition, including 
top soil and seeding as necessary.</TXT><BRK/>
<BRK/></SPT>
</PRT>    <END/><BRK/></SEC>
