<?xml version="1.0" encoding="windows-1252"?><SEC xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="http://si.ksc.nasa.gov/sidownloads/xml/specsintactSEC.xsd"><MTA NAME="SUBFORMAT" CONTENT="NEW"/><MTA NAME="AUTONUMBER" CONTENT="TRUE"/><HDR><AST/><TAB BORDERS="0">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="4">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="366.00"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="365.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="14.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">USACE / NAVFAC / AFCEC</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">UFGS-01 33 29 (February 2021)</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="12.00">
         <CEL MERGEDOWN="1" STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Change 1 - 08/25</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="12.00">
         <CEL INDEX="2" STYLEID="s50">
<DTA TYPE="STRING"><HL3>------------------------------------</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="45.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Preparing Activity:  <PRA>NAVFAC</PRA></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Superseding<BRK/>UFGS-01 33 29 (February 2017)<BRK/>UFGS-01 33 29.05 20 (March 2019)</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<HL4>UNIFIED FACILITIES GUIDE SPECIFICATIONS</HL4><BRK/>
<BRK/>
<HL4>References are in agreement with UMRL dated July 2025</HL4><BRK/>
<AST/><BRK/></HDR>
<BRK/>
<SCN>SECTION 01 33 29</SCN><BRK/>
<BRK/>
<STL>SUSTAINABILITY REQUIREMENTS AND REPORTING</STL><BRK/>
<DTE>02/21, CHG 1: 08/25</DTE><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This guide specification covers the requirements for <SCP>providing sustainability documentation for Guiding 
Principles Validation (GPV) and Third-Party Certification (TPC)</SCP>.  GPV is equivalent to meeting the requirements 
of UFC 1-200-02 "HIGH PERFORMANCE AND SUSTAINABLE BUILDING REQUIREMENTS."  All projects must meet the requirements 
of UFC 1-200-02.</NPR><BRK/>
<BRK/>
<NPR>For building scopes that do not meet the minimum requirements or thresholds as cited by UFC 1-200-02 Table 1-1, 
ensure the project delivery team completes the initial High Performance and Sustainable Building (HPSB) Checklist 
for each building in the project, to determine the crosswalk of scope items with criteria in the UFC.</NPR><BRK/>
<BRK/>
<NPR>Specifications are chosen by the project delivery team.  UFGS 01 33 29 is not required for all projects, based 
on UFC 1-200-02 thresholds, but can be utilized, based on the project team's consideration.</NPR><BRK/>
<BRK/>
<NPR>This guide specification includes tailoring for both DESIGN-BUILD and DESIGN-BID-BUILD.</NPR><BRK/>
<BRK/>
<NPR>This guide specification includes tailoring for ARMY.  Deselect the ARMY tailoring option for Navy projects.  
Air Force projects must use tailoring for the Service that is executing the project and choose bracketed options 
per Editor's Notes.</NPR><BRK/>
<BRK/>
<NPR>Use a properly edited version of this guide specification for projects that contain one or more buildings that 
meet one of the following:</NPR><BRK/>
<BRK/>
<NPR>a)  For Army and Navy, new buildings or stand-alone additions greater than or equal to 25,000 GSF (2323 GSM); 
for Air Force, all new buildings or stand-alone additions.</NPR><BRK/>
<BRK/>
<NPR>b)  Comprehensive replacement in an existing building that is greater than or equal to 25,000 GSF (2323 GSM), 
with total cost (includes new work, renovation, operations and maintenance, sustainment, restoration, and modernization 
associated with and existing building renovation) greater than $4M and 50-percent or more Estimated Replacement 
Cost (ERC).</NPR><BRK/>
<BRK/>
<NPR>Use the HPSB Checklist for the Service who will maintain the building asset in their Real Property Record.  Complete 
an HPSB Checklist for each applicable building in the project, before attaching to this specification. Checklist(s) 
must be completely filled out before being used in a solicitation.  Check with the user Command for additional 
requirements.  Each Component’s HPSB Checklist may be found at:  <URL HREF="https://www.wbdg.org/dod/sustainability/tracking-reporting">www.wbdg.org/dod/sustainability/tracking-reporting</URL></NPR><BRK/>
<BRK/>
<NPR>(Where Internet address appears on multiple lines, copy full address into Internet browser.)</NPR><BRK/>
<BRK/>
<NPR>Adhere to <URL HREF="https://www.wbdg.org/dod/ufc/ufc-1-300-02">UFS 1-300-02</URL> Unified Facilities Guide Specifications (UFGS) Format Standard when editing this guide 
specification or preparing new project specification sections.  Edit this guide specification for project specific 
requirements by adding, deleting, or revising text.  For bracketed items, choose applicable item(s) or insert 
appropriate information.</NPR><BRK/>
<BRK/>
<NPR>Remove information and requirements not required in respective project, whether or not brackets are present.</NPR><BRK/>
<BRK/>
<NPR>Comments, suggestions and recommended changes for this guide specification are welcome and should be submitted 
as a <URL HREF="https://www.wbdg.org/dod/ufgs">Criteria Change Request (CCR)</URL>.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<PRT><TTL>PART 1   GENERAL</TTL><BRK/>
<BRK/>
<SPT><TTL>REFERENCES</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is used to list the publications cited in the text of the guide specification.  The publications 
are referred to in the text by basic designation only and listed in this paragraph by organization, designation, 
date, and title.</NPR><BRK/>
<BRK/>
<NPR>Use the Reference Wizard's Check Reference feature when you add a Reference Identifier (RID) outside of the Section's 
Reference Article to automatically place the reference in the Reference Article.  Also use the Reference Wizard's 
Check Reference feature to update the issue dates.</NPR><BRK/>
<BRK/>
<NPR>References not used in the text will automatically be deleted from this section of the project specification when 
you choose to reconcile references in the publish print process.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The publications listed below form a part of this specification to the extent referenced.  The publications are referred to within the text by 
the basic designation only. For references without a year, use the current published version.</TXT><BRK/>
<BRK/>
<REF><ORG>COUNCIL ON ENVIRONMENTAL QUALITY (CEQ) (WHITE HOUSE)</ORG><BRK/>
<BRK/>
<RID>HPSB Guiding Principles</RID><RTL>Guiding Principles for Sustainable Federal Buildings and Determining Compliance 
with the Guiding Principles for Sustainable Federal Buildings</RTL><BRK/>
<BRK/></REF>
<REF><ORG>GREEN BUILDING INITIATIVE (GBI)</ORG><BRK/>
<BRK/>
<RID>GBI DOD GP Compliance</RID><RTL>GBI Department of Defense Guiding Principles Compliance Program for New Construction</RTL><BRK/>
<BRK/>
<RID>GBI Green Globes for NC</RID><RTL>Green Globes(tm) for New Construction Technical Reference Manual</RTL><BRK/>
<BRK/></REF>
<REF><ORG>GREEN BUSINESS CERTIFICATION INC. (GBCI)</ORG><BRK/>
<BRK/>
<RID>GBCI GP Assessment (DOD)</RID><RTL>Guiding Principles Assessment for Department of Defense</RTL><BRK/>
<BRK/></REF>
<REF><ORG>INTERNATIONAL CODE COUNCIL (ICC)</ORG><BRK/>
<BRK/>
<RID>ICC IgCC</RID><RTL>(2018) International Green Construction Code</RTL><BRK/>
<BRK/></REF>
<REF><ORG>SHEET METAL AND AIR CONDITIONING CONTRACTORS' NATIONAL ASSOCIATION (SMACNA)</ORG><BRK/>
<BRK/>
<RID>ANSI/SMACNA 008</RID><RTL>(2007) IAQ Guidelines for Occupied Buildings Under Construction, 2nd Edition</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. DEPARTMENT OF AGRICULTURE (USDA)</ORG><BRK/>
<BRK/>
<RID>FSRIA 9002</RID><RTL>Farm Security and Rural Investment Act Section 9002 (USDA BioPreferred Program)</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. DEPARTMENT OF DEFENSE (DOD)</ORG><BRK/>
<BRK/>
<RID>UFC 1-200-02</RID><RTL>(2020; Change 2, 2022) High Performance and Sustainable Building Requirements</RTL><BRK/>
<BRK/>
<RID>UFC 3-410-01</RID><RTL>(2013; with Change 9, 2024) Heating, Ventilating, and Air Conditioning Systems</RTL><BRK/>
<BRK/>
<RID>UFC 3-600-01</RID><RTL>(2016; with Change 6, 2021) Fire Protection Engineering for Facilities</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. DEPARTMENT OF ENERGY (DOE)</ORG><BRK/>
<BRK/>
<RID>Energy Star</RID><RTL>Energy Star Energy Efficiency Labeling System (FEMP)</RTL><BRK/>
<BRK/>
<RID>FEMP</RID><RTL>Federal Energy Management Program (FEMP) Energy-Efficient Product Procurement</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. GREEN BUILDING COUNCIL (USGBC)</ORG><BRK/>
<BRK/>
<RID>LEED BD+C</RID><RTL>LEED Building Design and Construction</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. NATIONAL ARCHIVES AND RECORDS ADMINISTRATION (NARA)</ORG><BRK/>
<BRK/>
<RID>10 CFR 433.300</RID><RTL>Subpart C - Green Building Certification for Federal Buildings</RTL><BRK/>
<BRK/>
<RID>40 CFR 247</RID><RTL>Comprehensive Procurement Guideline for Products Containing Recovered Materials</RTL><BRK/>
<BRK/></REF>
</SPT><SPT><TTL>SUMMARY</TTL><BRK/>
<BRK/>
<TXT>This section includes requirements for Sustainability documentation and reporting submittals per the federally mandated High Performance and Sustainable 
Building (HPSB) or HPSB "Guiding Principles" (GP),[ and Third-Party Certification (TPC) requirements,] in accordance with <RID>UFC 1-200-02</RID> High Performance 
and Sustainable Building Requirements, and other identified requirements.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>SUBMITTALS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Review Submittal Description (SD) definitions in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES and edit the following 
list, and corresponding submittal items in the text, to reflect only the submittals required for the project.  
The Guide Specification technical editors have classified those items that require Government approval, due to 
their complexity or criticality, with a "G."  Generally, other submittal items can be reviewed by the Contractor's 
Quality Control System.  Only add a "G" to an item if the submittal is sufficiently important or complex in context 
of the project.</NPR><BRK/>
<BRK/>
<NPR><TAI OPT="ARMY">For Army projects, fill in the empty brackets following the "G" classification, with a code of up to three characters 
to indicate the approving authority.  Codes for Army projects using the Resident Management System (RMS) are:  
"AE" for Architect-Engineer; "DO" for District Office (Engineering Division or other organization in the District 
Office); "AO" for Area Office; "RO" for Resident Office; and "PO" for Project Office.  </TAI>Codes following the "G" 
typically are not used for Navy and Air Force projects.</NPR><BRK/>
<BRK/>
<NPR>The "S" classification indicates submittals required as proof of compliance for sustainability Guiding Principles 
Validation or Third-Party Certification and as described in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Sustainability requirements have been identified in many of the technical performance sections.  Include 
additional sustainability requirements throughout the technical specification sections according to goals of this 
project.  Identify products and other submittals required for Guiding Principle Validation (GPV) and Third-Party 
Certification (TPC) where applicable, with an "S" next to the submittal item.  Use the following format to add 
submittal items in the technical sections to comply with the requirements of this section:</NPR><BRK/>
<BRK/>
<NPR>&lt;ITM&gt;&lt;SUB&gt;Insert Submittal Item&lt;/SUB&gt;; &lt;SUB&gt;S&lt;/SUB&gt;&lt;/ITM&gt;</NPR><BRK/>
<BRK/>
<NPR>Make corresponding edits in technical sections' Part 1, Part 2 Products or in Part 3 Execution to differentiate 
those pieces of equipment, products, or activities related to GPV and TPC.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the following bracketed paragraph for all projects except Navy DESIGN-BUILD.</NPR><BRK/>
<BRK/>
<NPR>Choose the first bracketed item for all DESIGN-BID-BUILD projects.  Choose the second bracketed item for Navy 
DESIGN-BUILD only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Government approval is required for submittals with a "G" or "S" classification.<TAI OPT="AIR FORCE,NAVY">  Submittals not having a "G" or "S" classification are for Contractor 
Quality Control approval.</TAI><TAI OPT="ARMY">  Submittals not having a "G" or "S" classification are for information only.  When used, a code following the "G" classification 
identifies the office that will review the submittal for the Government.</TAI>  Submit the following in accordance with [Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES][Section 
01 33 00.05 20 CONSTRUCTION SUBMITTAL PROCEDURES and Section 01 33 10.05.20 DESIGN SUBMITTAL PROCEDURES]:</TXT><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  For Air Force only:  For every Air Force DESIGN-BUILD project, keep all bracketed SD-01, SD-05, and SD-11 
submittals.  For every Air Force DESIGN-BID-BUILD project, keep all SD-01 and SD-11 submittals</NPR><BRK/>
<BRK/>
<NPR>Add other Checklist and Sustainability eNotebook submittals to match the number of design submissions, based on 
the project scope, and add requirements paragraphs in Part 1.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<LST><SUB>SD-01 Preconstruction Submittals</SUB></LST><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Navy projects in the NAVFAC PAC Area of Operation only: remove the "G" designation from all SD-01 Preconstruction 
Submittals.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>Preliminary High Performance and Sustainable Building Checklist</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]<ITM><SUB>Sustainability Action Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Preliminary Sustainability eNotebook</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]<TAI OPT="DESIGN-BUILD"><LST><SUB>SD-05 Design Data</SUB></LST><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following four Submittals are tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>Interim Design High Performance and Sustainable Building Checklist</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Interim Design Sustainability eNotebook</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Final Design High Performance and Sustainable Building Checklist</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Final Design Sustainability eNotebook</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]</TAI><LST><SUB>SD-06 Test Reports</SUB></LST><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For DESIGN-BID-BUILD projects, delete the following submittal if it is not part of the contractor's scope.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>Third-Party Certification Design Compliance Report</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]<LST><SUB>SD-11 Closeout Submittals</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Final High Performance and Sustainable Building Checklist</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Final Sustainability eNotebook</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
[<ITM><SUB>Amended Final Sustainability eNotebook</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
][<ITM><SUB>Amended Final High Performance and Sustainable Building Checklist</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Choose bracketed option for "Third-Party Certification Certificate, Assessment, or Validation and Compliance 
Report" for TPC projects that require the Contractor to obtain the TPC certification.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<ITM><SUB>Third-Party Certification Certificate, Assessment, or Validation and Compliance Report</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
]</SPT><SPT><TTL>GUIDING PRINCIPLES VALIDATION (GPV)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  GUIDING PRINCIPLES VALIDATION (GPV) is required in accordance with UFC 1-200-02 HIGH PERFORMANCE SUSTAINABLE 
BUILDING REQUIREMENTS and the notes under this specification's title above.</NPR><BRK/>
<BRK/>
<NPR>Complete Preliminary HPSB Checklist and include at the end of this specification.  For projects with multiple 
buildings, attach HPSB Checklist for each building.  See the notes under this specification's title above.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Guiding Principles Validation (GPV) is the project delivery team's self-assessment of <RID>UFC 1-200-02</RID> compliance requirements, which includes meeting 
Federally-required tracking and reporting requirements, in order to report a sustainable Federal building.  The use of a third-party certification 
is an additional and separate requirement.</TXT><BRK/>
<BRK/>
<TXT>Provide the following sustainability activities and documentation to verify achievement of <RID>HPSB Guiding Principles</RID> Validation (GPV):</TXT><BRK/>
<OLG><BRK/>
<OLI>Analysis of each Guiding Principle Requirement and how project complies.  Include final government approved narrative(s) in the HPSB Checklist 
submittal.  Multiple checklists indicate multiple buildings that require individual HPSB Checklist tracking.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose first bracket for all projects except Navy DESIGN-BUILD.  Choose second bracket for Navy DESIGN-BUILD 
only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>No changes to the HPSB Checklist are allowed without approval from the Contracting Officer, in accordance with Section[ <SRF>01 33 00</SRF> SUBMITTAL 
REQUIREMENTS][ 01 33 00.05 20 CONSTRUCTION SUBMITTAL PROCEDURES and Section 01 33 10.05 20 DESIGN SUBMITTAL PROCEDURES, paragraph DESIGN 
CHANGE AND VARIATION].  Immediately bring to the attention of the Contracting Officer any project changes that impact meeting the approved <RID>
HPSB Guiding Principles</RID> Requirements for this project.  Demonstrate the change will not increase the life-cycle cost and maintains or improves 
the building performance.</OLI><BRK/>
<BRK/>
<OLI>Documentation of all work required to incorporate the applicable <RID>HPSB Guiding Principles</RID> requirements indicated on the HPSB Checklist and 
in this contract, including all "S" submittals.</OLI><BRK/>
<BRK/>
<OLI>Sustainability Action Plan.</OLI><BRK/>
<TAI OPT="DESIGN-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Design and construction related documentation for the project Sustainability eNotebook and keep updated with regularly-scheduled Construction 
Quality Control Meetings.  Include design and construction related documentation containing the following components:</OLI><BRK/></TAI>
<TAI OPT="DESIGN-BID-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for DESIGN-BID-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Construction related documentation for the project Sustainability eNotebook and keep updated with regularly-scheduled Construction Quality 
Control Meetings.  Include construction related documentation containing the following components:</OLI><BRK/></TAI>
<BRK/>
<OLI LEVEL="2">HPSB Checklist(s)</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Sustainability Action Plan</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Documentation illustrating <RID>HPSB Guiding Principles</RID> Requirements compliance, including "S" submittals</OLI><BRK/></OLG>
<BRK/>
<SPT><TTL><SUB>Sustainability Action Plan</SUB></TTL><BRK/>
<BRK/>
<TXT>Include the following information in the Sustainability Action Plan:</TXT><BRK/>
<OLG><BRK/>
<OLI>Analysis of each <RID>HPSB Guiding Principles</RID> Requirement and how project will comply.  Final government approved narrative(s) must be included 
in the HPSB Checklist submittal.</OLI><BRK/>
<BRK/>
<OLI>Name and contact information for: Contractor's Point of Contact (POC) ensuring sustainability goals are accomplished and documentation 
is assembled.  For TPC that include on-site visit by third party representative, provide list of required attendees.</OLI><BRK/>
<BRK/>
<OLI>Indoor Air Quality plan.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Calculations</TTL><BRK/>
<TAI OPT="DESIGN-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide all design data, calculations, product data, labels and product certifications required in this specification to demonstrate compliance 
with the <RID>HPSB Guiding Principles</RID> Requirements.</TXT><BRK/></TAI>
<TAI OPT="DESIGN-BID-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for DESIGN-BID-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide all calculations, product data, labels and product certifications required in this specification to demonstrate compliance with the <RID>HPSB Guiding Principles</RID>
 Requirements.</TXT><BRK/></TAI>
<BRK/></SPT>
</SPT><SPT><TTL>SUSTAINABILITY SUBMITTALS</TTL><BRK/>
<BRK/>
<TXT>Provide HPSB Checklist and other documentation in the Sustainability eNotebook to indicate compliance with the sustainability requirements of the 
project.</TXT><BRK/>
<BRK/>
<SPT><TTL>High Performance Sustainable Building (HPSB) Checklist</TTL><BRK/>
<BRK/>
<TXT>Provide construction documentation that provides proof of, and supports compliance with, the completed HPSB Checklist.</TXT><BRK/>
<BRK/>
<SPT><TTL>HPSB Checklist Submittals</TTL><BRK/>
<BRK/>
<TXT>Submit updated HPSB Checklist with each Sustainability eNotebook submittal.  Include the final HPSB Checklist(s) with the interim DD1354 Real Property 
Record Submittal.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>"S" Submittals for Sustainability Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the bracketed phrases below for projects required to obtain TPC.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>"S" submittals are the sustainability documentation requirements cited in the various sections of this contract.  Submit the GPV[ and TPC] sustainability 
documentation required in this section as "S" submittals in all affected UFGS Sections.</TXT><BRK/>
<OLG><BRK/>
<OLI>Highlight GPV[ and TPC] compliance data in "S" submittal.</OLI><BRK/>
<BRK/>
<OLI>Add "S" submittals to the Sustainability eNotebook only after submittal approval, and bookmark them as required in paragraph SUSTAINABILITY 
ENOTEBOOK below.</OLI><BRK/>
<BRK/>
<OLI>Ensure all approved "S" submittals are included in each Sustainability eNotebook submittal.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Sustainability eNotebook</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the bracketed TPC phrases for projects required to obtain TPC.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Sustainability eNotebook is an electronic organizational file that serves as a repository for all required sustainability submittals.  To support 
documentation of compliance with an approved HPSB[ and TPC] checklist, provide and maintain a comprehensive and current Sustainability eNotebook.  
Include all required data in Sustainability eNotebook, to support full compliance with the <RID>HPSB Guiding Principles</RID> Requirements, including:</TXT><BRK/>
<OLG><BRK/>
<OLI>HPSB checklist</OLI><BRK/>
<BRK/>
<OLI>Sustainability Action Plan</OLI><BRK/>
<BRK/>
<OLI>Calculations</OLI><BRK/>
<BRK/>
<OLI>Labels</OLI><BRK/>
<BRK/>
<OLI>"S" submittals</OLI><BRK/>
<BRK/>
[<OLI>Certifications, assessments, or validations and compliance report</OLI><BRK/>
<BRK/>
][<OLI>TPC documentation required in paragraph THIRD-PARTY CERTIFICATION (TPC).</OLI><BRK/></OLG>
<BRK/>
]<SPT><TTL>Sustainability eNotebook Format</TTL><BRK/>
<BRK/>
<TXT>Provide Sustainability eNotebook in the form of an Adobe PDF file; bookmark each <RID>HPSB Guiding Principles</RID> Requirement[, and each TPC requirement,] 
and sub-bookmark at each document.  Match format to <RID>HPSB Guiding Principles</RID> numbering system indicated herein.  Maintain up-to-date information, 
such as spreadsheets, templates, with each current submittals.[  For TPC projects, provide a second Table of Contents using TPC numbering system, 
for maintaining documentation unique to TPC.]</TXT><BRK/>
<BRK/>
<TXT>Contracting Officer may deduct from the monthly progress payment accordingly if Sustainability eNotebook information is not current and on track 
per project goals.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Sustainability eNotebook Submittal Schedule</TTL><BRK/>
<BRK/>
<TXT>Provide Sustainability eNotebook Submittals at the following milestones of the project:</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose submittal paragraphs, based on scope of project.  In each of the following paragraphs, include the 
first bracketed phrase for projects required to obtain TPC.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
[<OLI><SUB>Preliminary Sustainability eNotebook</SUB></OLI><BRK/>
<BRK/>
<OLI>Submit preliminary Sustainability eNotebook with updated <SUB>Preliminary High Performance and Sustainable Building Checklist</SUB>[ and TPC checklist] 
at the first post award meeting in accordance with Section <SRF>01 30 00</SRF> ADMINISTRATIVE REQUIREMENTS.</OLI><BRK/>
]<TAI OPT="DESIGN-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following two paragraphs are tailored for DESIGN-BUILD.</NPR><BRK/>
<BRK/>
<NPR>Choose submittal paragraphs, based on scope of project.  In each of the following paragraphs, include the first 
bracketed phrase for projects required to obtain TPC.  Include the second bracketed phrase for Navy DESIGN-BUILD 
only.  In paragraph d., add the submittal stage in the blank brackets (for example: [Design Development]).</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI><SUB>Interim Design Sustainability eNotebook</SUB></OLI><BRK/>
<BRK/>
<OLI>Submit updated Sustainability eNotebook with updated <SUB>Interim Design High Performance and Sustainable Building Checklist</SUB>[ with TPC Checklist] 
with the [_____] design[, in accordance with Section 01 33 10.05 20 DESIGN SUBMITTAL PROCEDURES].  If issues relating to achieving the 
sustainability goals of the project are subsequently identified, identify reasons and mitigation from DOR, and resubmit to the Contracting 
Officer for approval.</OLI><BRK/>
<BRK/>
][<OLI><SUB>Final Design Sustainability eNotebook</SUB></OLI><BRK/>
<BRK/>
<OLI>Submit updated Sustainability eNotebook with updated <SUB>Final Design High Performance and Sustainable Building Checklist</SUB>[ with TPC Checklist] 
with the final design[, in accordance with Section 01 33 10.05 20 DESIGN SUBMITTAL PROCEDURES].  If issues relating to achieving the sustainability 
goals of the project are subsequently identified, identify reasons and mitigation from DOR, and resubmit to the Contracting Officer for 
approval.</OLI><BRK/>
]</TAI><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects required to obtain TPC, include the bracketed paragraph when seeking approval of TPC design 
requirements.  This is the preferred method to obtain TPC, and it is preferred this report is obtained prior to 
construction award.  For DESIGN-BID-BUILD projects, delete this report if it is not part of the contractor's scope.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI><SUB>Third-Party Certification Design Compliance Report</SUB></OLI><BRK/>
<BRK/>
<OLI>Obtain Third-Party Certification Design Compliance Report after final design submittal is approved.  Submittal must indicate 100 percent 
compliance with applicable design requirements.  File approved submittal in the Sustainability eNotebook.</OLI><BRK/>
]<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:   Include the bracketed phrases for projects required to obtain TPC.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Construction Quality Control Meetings.</OLI><BRK/>
<BRK/>
<OLI>Provide up-to-date GP[ and TPC] documentation in the Sustainability eNotebook[ and TPC Online tool] for each meeting.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the first bracketed phrase for projects required to obtain TPC.</NPR><BRK/>
<BRK/>
<NPR>Include the second bracketed phrase for Navy DESIGN-BUILD only.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI><SUB>Final Sustainability eNotebook</SUB></OLI><BRK/>
<BRK/>
<OLI>Submit updated Sustainability eNotebook with updated <SUB>Final High Performance and Sustainable Building Checklist</SUB>[ with TPC Checklist][, in 
accordance with Section 01 33 00.05 20 CONSTRUCTION SUBMITTAL PROCEDURES] at Beneficial Occupancy Date (BOD).  Final progress payment retainage 
may be held by Contracting Officer until Final Sustainability construction phase documentation is complete.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following paragraph when an amended Sustainability eNotebook is required (due to post-construction 
activities such as commissioning).  Include the first bracketed phrase for projects required to obtain TPC.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI><SUB>Amended Final Sustainability eNotebook</SUB></OLI><BRK/>
<BRK/>
<OLI>Amend and resubmit the Amended Final Sustainability eNotebook with <SUB>Amended Final High Performance and Sustainable Building Checklist</SUB>[ and 
amended TPC Checklist], to include post-occupancy corrections, updates, and requirements.  Final progress payment retainage may be held 
by Contracting Officer until amended final sustainability documentation is complete.  Submit electronic copy of the Amended Final Sustainability 
eNotebook Submittal to the Contracting Officer no later than 30 days after final GP[, TPC] determination.</OLI><BRK/></OLG>
<BRK/>
]</SPT></SPT></SPT><SPT><TTL>DOCUMENTATION REQUIREMENTS</TTL><BRK/>
<OLG><BRK/>
<OLI>Incorporate each of the following <RID>HPSB Guiding Principles</RID> requirements into project and provide documentation that proves compliance with 
each listed requirement.  Items below are organized by <RID>HPSB Guiding Principles</RID>.  For life-cycle cost analysis requirements, one document 
with all analyses is acceptable, with Contracting Officer approval.</OLI><BRK/>
<BRK/>
<OLI>For each of the following paragraphs that require the use of products listed on Government-required websites, provide documentation of 
the process used to select products, or process used to determine why listed products do not meet project performance requirements.</OLI><BRK/></OLG>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following subparagraphs provide Guiding Principle Requirements.</NPR><BRK/>
<BRK/>
<NPR>Choose requirements that can be fully achieved, or partially achieved to the greatest degree possible.  For partially 
achievable requirements, track them as "yes" only with one of the following justifications:</NPR><BRK/>
<BRK/>
<NPR>1.  Life-cycle cost-effectiveness and energy model;<BRK/>
2.  Mission restriction (ex: 24/7 operation);<BRK/>
3.  Location/regional restriction (ex: availability of high-efficiency equipment service);<BRK/>
4.  Locale restriction (ex: proximity of existing buildings restricts daylighting).</NPR><BRK/>
<BRK/>
<NPR>Delete requirements that are not applicable to the project.  Non-applicability requires one of the following justifications:</NPR><BRK/>
<BRK/>
<NPR>1.  Life-cycle cost-effectiveness and energy model;<BRK/>
2.  Mission exclusion (ex: no daylighting in a theater or a SCIF);<BRK/>
3.  Location/regional exclusion (ex: no local recycling facility); or<BRK/>
4.  Locale exclusion (ex: there is no steam to meter).</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>Integrated Design Process</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For the submittal documentation below, demonstrate compliance with <RID>UFC 1-200-02</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<OLG><BRK/>
<OLI>List the sustainability integrated design team, and a description of their roles in all stages of a project's planning and delivery:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Include Contractor's Sustainability Coordinators; Architecture and Engineering disciplines involved on the project, and the DOR 
in charge of the overall project and each discipline; Construction Subcontractors and the company representatives that align 
with each architectural and engineering discipline, Planning, Public Works, Environmental Specialist and other appropriate installation 
personnel.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Describe their roles and responsibilities and plan-of-action for how each team member will be involved to achieve the project 
sustainability requirements, and how the Contractor will coordinate with Government personnel.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Maintain an up-to-date list with descriptions throughout the project.</OLI><BRK/>
<BRK/>
<OLI>Provide narratives that:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Indicate each performance goal cited in <RID>UFC 1-200-02</RID> paragraph "Integrated Design Process", along with other comprehensive design 
goals and ensures incorporation and integration of these goals throughout the planning, design, construction, and life cycle 
of the building..</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Demonstrate integration of the goals into design and construction.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Demonstrate collaboration with other providers, such as Commissioning Provider[ and Third- Party Certifier].</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>Commissioning (Cx)</TTL><BRK/>
<BRK/>
<TXT>Develop and incorporate Commissioning requirements into the documents, and provide final commissioning report.  Refer to Section <SRF>01 91 00.15</SRF> BUILDING 
COMMISSIONING and related documents for commissioning requirements.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>Optimize Energy Performance</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For the submittal documentation below, demonstrate compliance with <RID>UFC 1-200-02</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For determining energy consumption reduction levels, comply with UFC 1-200-02 HIGH PERFORMANCE AND SUSTAINABLE 
BUILDING REQUIREMENTS, Chapter 1 paragraph titled "Life-Cycle Cost Analysis," Chapter 2 paragraph titled "Optimized 
Energy Performance," Chapter 4 "Energy Optimization, Modeling, and LCCA Process Integration," and Chapter 5 paragraph 
titled  "Energy Compliance Analysis."</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
<OLI>Narrative that provides a summary of:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The decision-making process for considering and implementing passive strategies prior to designing active and mechanical systems.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The decision-making process leading to the selection of at least three energy-efficient solutions (for each system contributing 
to the energy footprint of the building) to be analyzed; and the selected design solution(s)</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The specific energy standard and version utilized; and the software used in the analysis</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The calculated energy consumption and energy use intensity (EUI in kBTU/sf/yr) of the baseline building and the proposed design 
alternatives</OLI><BRK/>
<BRK/>
<OLI>A minimum of the following energy modeling files and summaries for the baseline and proposed alternatives:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Input, schedules and libraries; and output</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Calculated energy use by energy type<BRK/></OLI>
<BRK/>
<OLI LEVEL="2">Calculated energy use by building system</OLI><BRK/>
<BRK/>
<OLI>The life-cycle cost analysis input and output files for the baseline and the proposed alternatives</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Construction Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Provide revised energy modeling for actual system constructed.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>Energy Efficient Products</TTL><BRK/>
<BRK/>
<TXT>Provide only energy-using products that are <RID>Energy Star</RID> Certified by the Environmental Protection Agency (EPA) or that meet or exceed the efficiency 
standard designated by the Federal Energy Management Program (<RID>FEMP</RID>).  Where <RID>Energy Star</RID> or <RID>FEMP</RID> requirements have not been established, provide 
most efficient products that are life-cycle cost-effective.  Provide only energy using products that meet <RID>FEMP</RID> requirements for low standby power 
consumption.  Energy efficient products can be found at: <URL HREF="https://www.energystar.gov">https://www.energystar.gov/</URL>.</TXT><BRK/>
<BRK/>
<TXT>For construction submittal documentation, provide proof that product is labeled energy efficient and complies with the cited requirements.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>On-Site Renewable Energy Generation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<BRK/>
<NPR>In order to inform the cost and scope of the DESIGN-BUILD request for proposal (RFP), it is preferred that the 
LCCA is performed prior to issuance (RFP.)</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For the submittal documentation below, demonstrate compliance with <RID>UFC 1-200-02</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Provide life-cycle cost analysis (LCCA).  When found to be LCCE, do one of the following options:</TXT><BRK/>
<OLG><BRK/>
<OLI>Provide design drawings and calculations that demonstrate total on-site renewable energy as an annual percentage of proposed building energy 
consumption in kBTU/year; and provide equipment ratings, and calculations that demonstrate the generation capacity of the system in kBTU/year 
for thermal and kwh for electricity.</OLI><BRK/>
<BRK/>
<OLI>Provide documentation that renewable energy development at the Installation level is planned.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></TAI><TAI OPT="DESIGN-BUILD"><SPT><TTL>Solar Domestic Hot Water (SDHW)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For the submittal documentation below, demonstrate compliance with <RID>UFC 1-200-02</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Provide life-cycle cost analysis (LCCA).  When found to be LCCE, provide design drawings and calculations that demonstrate total on-site renewable 
energy as an annual percentage of proposed building energy consumption in kBTU/year; and provide equipment ratings, and calculations that demonstrate 
the generation capacity of the system in kBTU/year for thermal.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>Building-level Power Metering</TTL><BRK/>
<BRK/>
<TXT>Provide building-level meters for electricity, natural gas, and steam where applicable.</TXT><BRK/>
<BRK/>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide design drawings that highlight meter locations on the site.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Construction Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Provide documentation of meter communication with the base-wide meter monitoring system, and manufacturer's data validating compatibility with 
base-wide system and component advanced meter requirements.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Indoor Water Use</TTL><BRK/>
<BRK/>
<TXT>Provide Construction Documentation proof that fixtures are labeled EPA WaterSense, for products available with EPA WaterSense labeling; for all 
other fixtures, proof they comply with EPA WaterSense efficiency requirements.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Indoor Water Metering</TTL><BRK/>
<BRK/>
<TXT>Provide building-level meters for potable water use.  Provide the requirements cited in the following paragraphs:</TXT><BRK/>
<BRK/>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide design drawings that highlight meter locations on the site.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Construction Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Provide documentation of meter communication with the base-wide meter monitoring system, and manufacturer's data validating compatibility with 
base-wide system and component advanced meter requirements.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Outdoor Water Use</TTL><BRK/>
<BRK/>
<TXT>When there is no permanent irrigation system beyond plant establishment period, this element is met.</TXT><BRK/>
<BRK/>
<TXT>Where new irrigation is required beyond plant establishment period, provide only non-potable sources.  Provide meters.  Provide the requirements 
cited in the following paragraphs:</TXT><BRK/>
<BRK/>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
<OLI>Provide design drawings and analysis that identify the non-potable water source used and demonstrate the non-potable water source is appropriate 
for landscape irrigation, and that highlight meter locations on the site.</OLI><BRK/>
<BRK/>
<OLI>Provide life-cycle cost analysis (LCCA).</OLI><BRK/></OLG>
<BRK/></SPT>
</TAI><SPT><TTL>Construction Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Provide documentation of meter communication with the base-wide meter monitoring system, and manufacturer's data validating compatibility with 
base-wide system and component advanced meter requirements.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Outdoor Water Meters</TTL><BRK/>
<BRK/>
<TXT>Provide meters for outdoor systems that use potable water.  Provide the requirements cited in the following paragraphs:</TXT><BRK/>
<BRK/>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
<OLI>Provide design drawings that highlight meter locations on the site.</OLI><BRK/>
<BRK/>
<OLI>Provide life-cycle cost analysis (LCCA).</OLI><BRK/></OLG>
<BRK/></SPT>
</TAI><SPT><TTL>Construction Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Provide documentation of meter communication with the base-wide meter monitoring system, and manufacturer's data validating compatibility with 
base-wide system and component advanced meter requirements.</TXT><BRK/>
<BRK/></SPT>
</SPT><TAI OPT="DESIGN-BUILD"><SPT><TTL>Alternative Water</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Use alternative sources of water to replace potable water usage, when life-cycle cost-effective and to the extent permitted by local laws and regulations.</TXT><BRK/>
<BRK/>
<SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<OLG><BRK/>
<OLI>Provide design drawings and calculations that demonstrate the alternative water sources used, potable water savings as compared to non-alternative 
water sourcing, and projected annual potable water savings.</OLI><BRK/>
<BRK/>
<OLI>Provide life-cycle cost analysis (LCCA).</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></TAI><TAI OPT="DESIGN-BUILD"><SPT><TTL>Stormwater Management</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Develop and incorporate stormwater requirements into the documents.  Service processes, as proof of this tracking requirement.</TXT><BRK/>
<BRK/></SPT>
</TAI><TAI OPT="DESIGN-BUILD"><SPT><TTL>Ventilation and Thermal Comfort</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For the submittal documentation below, demonstrate compliance with <RID>UFC 1-200-02</RID> and <RID>UFC 3-410-01</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Provide design drawings and calculations that demonstrate HVAC systems and the building envelope have been designed to meet the requirements.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><TAI OPT="DESIGN-BUILD"><SPT><TTL>Daylighting</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For the submittal documentation below, demonstrate compliance with <RID>UFC 1-200-02</RID>.</TXT><BRK/>
<BRK/>
<SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<OLG><BRK/>
<OLI>Provide floor plans and elevations that demonstrates all required illumination levels, including automated and daylighting controls, and 
daylighting where people regularly occupy and gather.</OLI><BRK/>
<BRK/>
<OLI>Provide design analysis delineating requirements, to include compliant reflective surface locations and shading devices (where applicable).</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>Moisture Control</TTL><BRK/>
<BRK/>
<TXT>Provide the following: </TXT><BRK/>
<BRK/>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>Design Submittal Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide drawings of building envelope details, HVAC humidity controls, and design calculations..</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Construction Submittal Documentation</TTL><BRK/>
<BRK/>
<TXT>Ensure construction materials are separated and protected in accordance with other sections in this contract document, with adequate humidity controls 
during construction.  In accordance with Section <SRF>01 78 23</SRF> OPERATION AND MAINTENANCE DATA, includes plan for ongoing building moisture control.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Reduce Volatile Organic Compounds (VOC) (Low-Emitting Materials)</TTL><BRK/>
<BRK/>
<TXT>Meet the requirements of Table 3-1 at the end of this specification.</TXT><BRK/>
<BRK/>
<TXT>For Construction submittal documentation, provide certifications or labels that demonstrate compliance with cited requirements, based on the attached 
TABLE 3-1.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Indoor Air Quality During Construction</TTL><BRK/>
<BRK/>
<TXT>Prior to construction, create indoor air quality plan.  Develop and implement an IAQ construction management plan during construction and flush 
building air before occupancy.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the first bracketed sentence for new construction or renovation projects in buildings that are not 
occupied during construction.</NPR><BRK/>
<BRK/>
<NPR>Include the second bracketed sentence for Navy only.</NPR><BRK/>
<BRK/>
<NPR>Choose the third bracketed sentence for renovation projects in buildings that remain occupied during construction.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[For new construction and for renovation of unoccupied existing buildings, meet the requirements of <RID>ICC IgCC</RID> 1001.3.1.5 (10.3.1.5) Indoor Air Quality 
(IAQ) Construction Management.] [Coordinate with moisture control requirements in Section <SRF>01 45 00</SRF> QUALITY CONTROL.] [For renovation of occupied 
existing buildings, meet the requirements of <RID>ICC IgCC</RID> 1001.4.4 (10.4.4) Construction Activity Pollution Prevention:  Protection of Occupied Areas.  
Refer to <RID>ANSI/SMACNA 008</RID> IAQ Guidelines for Occupied Buildings Under Construction for additional best practices.]</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose "building" for all new construction projects, and for renovation projects that substantially replace 
the building from the foundation up.  Choose "area" for all other renovation projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide documentation showing that after construction ends and prior to occupancy, HVAC filters were replaced and[ building][ area] air was flushed 
out in accordance with the cited standard.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Recycled Content</TTL><BRK/>
<BRK/>
<TXT>Comply with <RID>40 CFR 247</RID>.  Refer to: <URL HREF="https://www.epa.gov/smm/comprehensive-procurement-guideline-cpg-program">https://www.epa.gov/smm/comprehensive-procurement-guideline-cpg-program</URL> for assistance identifying products 
cited in <RID>40 CFR 247</RID>.  Selected products must comply with non-proprietary requirements of the Federal Acquisition Regulation and must meet performance 
requirements.</TXT><BRK/>
<BRK/>
<SPT><TTL>Construction Submittal Documentation</TTL><BRK/>
<OLG><BRK/>
<OLI>Provide manufacturers' documents stating the recycled content by material, or written justification for claiming one of the exceptions 
allowed on the cited website.</OLI><BRK/>
<BRK/>
<OLI>Substitutions: Submit for Government approval for proposed alternative products or systems that provide equivalent performance and appearance 
and have greater contribution to project recycled content requirements.  For all such proposed substitutions, submit with the Sustainability 
Action Plan accompanied by product data demonstrating equivalence.</OLI><BRK/>
<BRK/>
<OLI>In order to complete compliance with FAR 52.223-9 Estimate of Percentage of Recovered Material Content for EPA Designated Items, refer 
to submittal requirement for recycled/recovered material content in Section <SRF>01 78 00</SRF> CLOSEOUT SUBMITTALS.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT><SPT><TTL>Bio-Based Products</TTL><BRK/>
<BRK/>
<TXT>Provide products and materials composed of the highest percentage of bio-based materials (including rapidly renewable resources and certified sustainably 
harvested products), consistent with <RID>FSRIA 9002</RID> USDA BioPreferred Program, to the maximum extent possible without jeopardizing the intended end 
use or detracting from the overall quality delivered to the end user and when available at a reasonable cost.  Use only supplies and materials 
of a type and quality that conform to applicable specifications and standards.</TXT><BRK/>
<BRK/>
<TXT>Comply with <RID>FSRIA 9002</RID> USDA BioPreferred Program.  Refer to <URL>www.biopreferred.gov</URL> for the product categories and BioPreferred Catalog.  Selected 
products must comply with non-proprietary requirements of the Federal Acquisition Regulation and must meet performance requirements.  Provide the 
following documentation:</TXT><BRK/>
<OLG><BRK/>
<OLI>USDA BioPreferred label for each product; for bio-based products used on project but not listed with BioPreferred program, provide bio-based 
content and percentage.</OLI><BRK/>
<BRK/>
<OLI>In order to complete compliance with FAR 52.223-1 Biobased Product Certification, refer to submittal requirement for biobased products 
in Section <SRF>01 78 00</SRF> CLOSEOUT SUBMITTALS, paragraphs CERTIFICATION OF EPA DESIGNATED ITEMS and CERTIFICATION OF USDA DESIGNATED ITEMS.</OLI><BRK/></OLG>
<BRK/></SPT>
<TAI OPT="DESIGN-BUILD"><SPT><TTL>Waste Material Management (Recycling – Design)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For the submittal documentation below, demonstrate compliance with <RID>UFC 1-200-02</RID>.</TXT><BRK/>
<BRK/>
<TXT>For design submittal documentation, provide drawing showing an appropriately sized and placed dedicated storage area for recyclables.</TXT><BRK/>
<BRK/></SPT>
</TAI><SPT><TTL>Waste Material Management (Recycling – Construction)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Verify division percentage in Section <SRF>01 74 19</SRF> CONSTRUCTION WASTE MANAGEMENT AND DISPOSAL.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Divert demolition and construction debris in accordance with Section <SRF>01 74 19</SRF> CONSTRUCTION WASTE MANAGEMENT AND DISPOSAL.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="DESIGN-BUILD">[<SPT><TTL>Address Risk</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<BRK/>
<NPR>Address only government-provided, specific scope direction related to the following paragraph.  If none has been 
provided in the DD1391 or scope, delete this paragraph, and document on HPSB Checklist and other required tracking 
locations as "N/A due to location/regional exclusion".</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For design submittal documentation, provide narrative of decisions for design associated with scoped requirements.</TXT><BRK/>
<BRK/></SPT>
]</TAI>[<SPT><TTL>Additional Sustainability Requirements</TTL><BRK/>
<BRK/>
<TXT>Provide the additional sustainability requirements cited in this paragraph.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  In addition to GPV and Sustainability eNotebook, Third-Party Certification (TPC) is required for projects 
that meet the thresholds cited in Table 1-1 of UFC 1-200-02.</NPR><BRK/>
<BRK/>
<NPR>1.  New building or stand-alone addition greater than or equal to 25,000 GSF (2323 GSM), with construction cost 
greater than $3M.</NPR><BRK/>
<BRK/>
<NPR>2.  Comprehensive replacement in an existing building that is greater than or equal to 25,000 GSF (2323 GSM), 
with total cost greater than $3M and 50-percent or more ERC.</NPR><BRK/>
<BRK/>
<NPR>TPC is the generic term for a third-party product that provides either certification of the third party vendor's 
proprietary product requirements (examples LEED, Green Globes), or a validation program by the third party vendor 
that UFC 1-200-02 requirements have been met (examples: Guiding Principles Assessment, Guiding Principles Compliance).</NPR><BRK/>
<BRK/>
<NPR>For each building that meets item 1 or item 2 above, choose one of the following paragraphs titled "Third-Party 
Certification (TPC) Documentation" below, based on how TPC is executed, and delete the others.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TAI OPT="DESIGN-BUILD">[<SPT><TTL>Third-Party Certification (TPC) Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Third-Party Certification certificate, assessment, or validation, and compliance report requirements are in addition to all requirements under 
header above GUIDING PRINCIPLES VALIDATION (GPV).</TXT><BRK/>
<BRK/>
<SPT><TTL>TPC Registration Required</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the rating system below that best assists with Guiding Principles Validation and delete the others.  
Verify rating systems approved for use by Service.</NPR><BRK/>
<BRK/>
<NPR>Obtain, fill out, and include TPC checklist with this section.  For projects with multiple buildings, attach completed 
TPC Checklist for each building that requires TPC.</NPR><BRK/>
<BRK/>
<NPR>For certifications, assessments, or validations that include a plaque, include the bracketed phrase in the first 
paragraph.</NPR><BRK/>
<BRK/>
<NPR>For Air Force ONLY:  Choose one of the following methods for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For Guiding Principles Assessment for Department of Defense (by GBCI), choose "GBCI GP Assessment (DOD)", 
use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>b.  For Green Building Initiative (GBI) Department of Defense Guiding Principles Compliance, or "GBI DOD GP Compliance", 
use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>For Army projects ONLY:  Choose only the following method for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For USGBC LEED, choose "LEED", and enter "Silver" in the bracket.  For use of alternate certification systems, 
a waiver must be submitted per the current Army Sustainable Design and Development Policy.</NPR><BRK/>
<BRK/>
<NPR>For Navy ONLY:  Choose one of the following methods for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For USGBC LEED, choose "LEED", and enter the target level in the bracket.</NPR><BRK/>
<BRK/>
<NPR>b.  For Guiding Principles Assessment for Department of Defense (by GBCI), choose "GBCI GP Assessment (DOD)", 
use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>c.  For Green Building Initiative (GBI) Department of Defense Guiding Principles Compliance, or "GBI DOD GP Compliance", 
use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>d.  For "GBI Green Globes for NC", enter the target level in the bracket.</NPR><BRK/>
<BRK/>
<NPR>e.  For an alternate certification system, use only those that comply with the minimum requirements of 10 CFR 
433.300 Subpart C — Green Building Certification for Federal Buildings, and insert the name of the compliant system 
in the empty bracket.  Facilities Engineering Command (FEC) Capital Improvements (CI) Core must authorize the 
use of alternative system.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Register and achieve Third-Party Certification (TPC), by meeting all TPC and project requirements to achieve[ <RID>LEED BD+C</RID> [_____]][ <RID>GBCI GP Assessment (DOD)</RID>
][ <RID>GBI DOD GP Compliance</RID>][ <RID>GBI Green Globes for NC</RID> [_____]] [[_____][_____]], or Government-approved equivalent TPC sustainability certification, 
assessment, or validation.  An equivalent TPC organization must demonstrate equivalency for Government consideration and meet the requirements 
of <RID>10 CFR 433.300</RID>, prior to use on the project.  Third-Party Certification is met when Government receives TPC organization certificate, assessment, 
or validation and compliance report[ and plaque].</TXT><BRK/>
<BRK/>
<TXT>Register project with TPC organization using the following format and content:</TXT><BRK/>
<OLG><BRK/>
<OLI>Project Title First Line: Building Owner (US Army, US Air Force, US Navy or US Marine Corps), Building Name (if known)</OLI><BRK/>
<BRK/>
<OLI>Project Title Second Line: MILCON P#, DD1391 Project Name</OLI><BRK/>
<BRK/>
<OLI>Project Address: UIC (Installation code), Category code, RPUID (Real Property Unique Identifier) Number</OLI><BRK/>
<BRK/>
<OLI>Project Owner Organization: US Army, US Air Force, US Navy or US Marine Corps</OLI><BRK/>
<BRK/>
<OLI>Primary Contact, Project Owner: Executing DOD Service's Project Manager or Design Manager</OLI><BRK/>
<BRK/>
<OLI>Building Owner Organization: US Army, US Air Force, US Navy or US Marine Corps</OLI><BRK/>
<BRK/>
<OLI>Building Owner Organization Project Number</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose first bracket for Air Force projects and delete the others.  Choose second bracket for Army projects 
and delete the others.  Choose third bracket for Navy projects and delete the others.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Additional Contact, Building Owner: [ Base Civil Engineer][ Department of Public Works][ Public Works Officer] or Designee.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>TPC Management and Certification</TTL><BRK/>
<BRK/>
<TXT>Execute the following TPC Certification, assessment, or validation requirements:</TXT><BRK/>
<OLG><BRK/>
<OLI>Refer to TPC Checklist at the end of this specification section.  (Multiple checklists indicate multiple buildings that require TPC.)</OLI><BRK/>
<BRK/>
<OLI>Immediately bring to the attention of the Contracting Officer any project changes that impact meeting the approved TPC Requirements for 
this project.  Demonstrate the change will not increase the life-cycle cost and maintains or improves the building performance.</OLI><BRK/>
<BRK/>
<OLI>Complete all design and construction work to incorporate the applicable TPC Requirements.</OLI><BRK/>
<BRK/>
<OLI>Maintain the design and construction related information in the Sustainability eNotebook pertaining to additions and changes to the approved 
sustainability requirements.  Maintain the Sustainability eNotebook in electronic format.  Refer to explanation in the paragraph SUSTAINABILITY 
eNOTEBOOK.  Provide the following components in the Sustainability eNotebook, in addition to the GPV components listed above:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC Checklist</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Completed TPC forms. Transmit by the method required by TPC organization.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Copy of all correspondence with the TPC organization. Provide proof of TPC registration.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Documentation illustrating compliance with TPC requirements and additional documentation as requested by the Third Party certifier.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC Award Certificate, assessment or validation and compliance report.</OLI><BRK/>
<BRK/>
<OLI>Provide the following information in the Sustainability Action Plan.  Provide this TPC information in addition to the Sustainability Action 
Plan items above:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Planned method to achieve each TPC requirement.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Provide analysis of each TPC credit and how project will comply.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Provide names and contact information for: Contractor sustainability point of contact (POC) and other names of sustainability 
professionals on the Contractor's Staff responsible for ensuring TPC sustainability goals are accomplished and documentation 
is assembled.  It is recommended the construction team has a member with a current TPC credential, when available, that matches 
the TPC system and variation specialty pursued for the certification.  When retained, this team member must be engaged and keep 
this credential current over the duration of the entire project schedule.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC vendor's project identification and number.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For certifications, assessments, or validations that include a plaque, included the bracketed phrase.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Bear all costs associated with designing, constructing, demonstrating, and documenting that project complies with approved TPC requirements, 
including but not limited to:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Registration, review, certification, assessment, or validation[ and plaque] fees.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Online (or offline with secure facilities) TPC management and documentation.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Obtaining TPC certification, assessment, or validation based on Government-approved sustainability goals.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Design and construction work required to incorporate TPC requirements.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Submittals required to demonstrate compliance with Government approved TPC checklists.</OLI><BRK/>
<BRK/>
<OLI>Provide all design data, calculations, product data, and certifications, assessments, or validations required in this specification to 
demonstrate compliance with the TPC Requirements.</OLI><BRK/>
<BRK/>
<OLI>Provide all online (or offline, with secure facilities) TPC management and documentation.</OLI><BRK/>
<BRK/>
<OLI>Provide all required responses to third party organization.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the bracketed paragraph below for TPC that includes required site visit by a TPC representative.  
Coordinate with the TPC representative, Project Manager, Design Manager, and Construction Manager to determine 
participating team members.  Include commissioning provider on applicable projects.</NPR><BRK/>
<BRK/>
<NPR>For projects that require the Construction Contractor to obtain TPC, the Construction Contractor’s designated 
Sustainability POC is responsible to coordinate the TPC site visit.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>Facilitate and participate in required TPC site visit.  Coordinate with the Executing DOD Service's Project Manager and Design Manager, 
to determine participating team members.  Include Commissioning provider on applicable projects.</OLI><BRK/>
]<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the bracketed paragraph below for TPC that include a certification, assessment, or validation.  
For TPC that include a plaque, include the bracketed phrases.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>Provide TPC [Plaque and ]Certificate, assessment, or validation.  Provide TPC compliance report that includes level achieved and reasons 
for non-compliance or not applicable elements.  Use the following format to create the Plaque, Certificate, assessment, or validation, 
compliance report, and Letter of Congratulations.  Forward to parties designated by Contracting Officer:</OLI><BRK/>
<BRK/>
[<OLI LEVEL="2">Plaque:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Name: Final Building Name.  If unknown, use the Form DD1391 Project Name.</OLI><BRK/>
<BRK/>
]<OLI LEVEL="2">Certificate, Assessment, or Validation:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Project title, first line: P-(X); (1391 Project Name).  Project title, second line: UIC (installation code)</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Letter of Congratulation (when provided):</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Address letter to the Facility's Installation Commander Name. Address the letter to an individual person.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Compliance Report:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Title page must cite Project title: P-(X); (1391 Project Name); Final Building Name if known; UIC (installation code); Owner 
Service; User organization if known; date of compliance.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Include TPC scoresheet if applicable.</OLI><BRK/>
]<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose first bracket for Air Force projects. Choose second bracket for Army projects. Choose third bracket 
for Navy projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Once Final Certification is achieved, turn over Administrative rights to online TPC to the [Base Civil Engineer][ Department of Public 
Works][ Public Works Office] or designee, contact information provided by the Contracting Officer.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT>]</TAI><TAI OPT="DESIGN-BID-BUILD">[<SPT><TTL>Third-Party Certification (TPC) Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose this DESIGN-BID-BUILD "Third-Party Certification (TPC) Documentation" paragraph for Third-Party 
Certification, assessment, or validation when the Designer of Record is responsible for the entire TPC process, 
with the Construction Contractor providing the construction documentation.  This is the preferred method of TPC 
execution for DESIGN-BID-BUILD (DBB)  Delete the other DESIGN-BID-BUILD "Third-Party Certification (TPC) Documentation" 
paragraph option.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Third-Party Certification certificate, assessment, or validation, and compliance report requirements are in addition to all requirements under 
header above GUIDING PRINCIPLES VALIDATION (GPV).</TXT><BRK/>
<BRK/>
<SPT><TTL>TPC Registration</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the rating system below that best assists with Guiding Principles Validation, complies with Component 
policy, and delete the others.</NPR><BRK/>
<BRK/>
<NPR>Obtain, fill out, and include TPC checklist with this section.  For projects with multiple buildings, attach TPC 
Checklist for each building that requires TPC.</NPR><BRK/>
<BRK/>
<NPR>For certifications, assessments or validations that include a plaque, include the bracketed phrase in the first 
paragraph.</NPR><BRK/>
<BRK/>
<NPR>For Air Force ONLY:  Choose one of the following methods for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For Guiding Principles Assessment for Department of Defense (by GBCI), choose "GBCI GP Assessment (DOD)", 
use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>b.  For Green Building Initiative (GBI) "Department of Defense Guiding Principles Compliance", or "GBI DOD GP 
Compliance", use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>For Army projects ONLY:  Choose only the following method for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For USGBC LEED, choose "LEED", and enter "Silver" in the bracket.  For use of alternate certification systems, 
a waiver must be submitted per the current Army Sustainable Design and Development Policy.</NPR><BRK/>
<BRK/>
<NPR>For Navy ONLY:  Choose one of the following methods for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For USGBC LEED, choose "LEED", and enter the target level in the bracket.</NPR><BRK/>
<BRK/>
<NPR>b.  For Guiding Principles Assessment for Department of Defense (by GBCI), choose "GBCI GP Assessment (DOD)", 
use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>c.  For Green Building Initiative (GBI) "Department of Defense Guiding Principles Compliance", or "GBI GP DOD 
Compliance", use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>d.  For Green Building Initiative (GBI) Green Globes, choose "GBI Green Globes for NC", and enter the target level 
in the bracket.</NPR><BRK/>
<BRK/>
<NPR>e.  For an alternate certification system, use only those that comply with the minimum requirements of 10 CFR 
433.300 Subpart C — Green Building Certification for Federal Buildings, and insert the name of the compliant system 
in the empty bracket.  Facilities Engineering Command (FEC) Capital Improvements (CI) Core must authorize the 
use of alternative system.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>This project has been designed for, and must be constructed to achieve[ <RID>LEED BD+C</RID> [_____]][ <RID>GBCI GP Assessment (DOD)</RID>][ <RID>GBI DOD GP Compliance</RID>] [<RID>
GBI Green Globes for NC</RID> [_____]] [_____].  Project is already registered with the TPC Organization.  Provide construction related sustainability 
documentation, in the format required by the TPC Organization, to the Contracting Officer for approval, and for final approval by the TPC organization.  
Third-Party Certification is met when Government receives TPC organization certificate, assessment, or validation and compliance report[ and plaque].  
Execute the following:</TXT><BRK/>
<OLG><BRK/>
<OLI>Refer to TPC Checklist at the end of this specification section.  (Multiple checklists indicate multiple buildings that require TPC.)</OLI><BRK/>
<BRK/>
<OLI>Immediately bring to the attention of the Contracting Officer any project changes that impact meeting the approved TPC Requirements for 
this project.  Demonstrate the change will not increase the life-cycle cost and maintains or improves the building performance.</OLI><BRK/>
<BRK/>
<OLI>Complete all work required to incorporate the applicable TPC Requirements.</OLI><BRK/>
<BRK/>
<OLI>Maintain the construction related information in the Sustainability eNotebook pertaining to additions and changes to the approved sustainability 
requirements.  Maintain the Sustainability eNotebook in electronic format.  For more explanation, refer to paragraph SUSTAINABILITY eNOTEBOOK.  
Provide the following components in the Sustainability eNotebook, in addition to the GPV components above:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC Checklist</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Provide construction documentation required to achieve third-party certification</OLI><BRK/>
<BRK/>
<OLI>Provide the following information in the Sustainability Action Plan.  Provide this TPC information in addition to the GPV Action Plan items 
above:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Planned method to achieve each TPC requirement.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">For each TPC requirement that is attempted but not achieved, provide narrative explaining how mission or activity precludes achieving 
specific sustainability requirement or goal.  Provide analysis of particular requirement and level to which project is able to 
comply.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Provide name and contact information for: Sustainability Point of Contact (POC) and other names of sustainability professionals 
responsible for ensuring TPC sustainability goals are accomplished and documentation is assembled.  Sustainability POCs are also 
responsible for ensuring GPV required in paragraph GUIDING PRINCIPLES VALIDATION (GPV) above.  It is recommended construction 
team has a member with a current TPC credential, when available, that matches the TPC system and variation specialty pursued 
for the certification.  When retained, this team member must be engaged and keep this credential current over the duration of 
the entire project schedule.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC vendor's project identification and number.</OLI><BRK/>
<BRK/>
<OLI>Bear all costs associated with construction changes that affect sustainability design requirements, constructing, demonstrating, and documenting 
that project complies with approved TPC requirements, including but not limited to:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC coordination with Government's AE and other consultants, TPC website requirements, and management for construction related 
documentation.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Construction work required to incorporate TPC requirements.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Submittals required to demonstrate compliance with Government approved TPC checklists.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Documentation illustrating compliance with TPC requirements and additional documentation required by the TPC.</OLI><BRK/>
<BRK/>
<OLI>Provide all calculations, product data, and certifications, assessments, or validations required in this contract to demonstrate compliance 
with the TPC Requirements of this section.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT>]</TAI><TAI OPT="DESIGN-BID-BUILD">[<SPT><TTL>Third-Party Certification (TPC) Documentation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose this DESIGN-BID-BUILD "Third-Party Certification (TPC) Documentation" paragraph, if the Construction 
Contractor is responsible for achieving the final TPC.  Use of this method is discouraged.  Delete the previous 
DESIGN-BID-BUILD "Third-Party Certification (TPC) Documentation" paragraph option.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Third-Party Certification certificate, assessment, or validation, and compliance report requirements are in addition to all requirements under 
header above GUIDING PRINCIPLES VALIDATION (GPV).</TXT><BRK/>
<BRK/>
[<SPT><TTL>TPC Registration Required</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose this bracketed paragraph if the Designer of Record (DOR) has not registered the project with a TPC 
organization, and the Construction Contractor must do so.  Delete the second bracketed paragraph.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the rating system below that best assists with Guiding Principles Validation complies with Component 
policy and delete the others.</NPR><BRK/>
<BRK/>
<NPR>Obtain, fill out, and include TPC checklist with this section.  For projects with multiple buildings, attach TPC 
Checklist for each building that requires TPC.</NPR><BRK/>
<BRK/>
<NPR>For certifications, assessments, or validations that include a plaque, include the bracketed phrases below.</NPR><BRK/>
<BRK/>
<NPR>For Air Force ONLY:  Choose one of the following methods for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For Guiding Principles Assessment by USGBC/GBCI (DOD Version), choose "GBCI GP Assessment", use only DOD version, 
and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>b.  For Green Building Initiative (GBI) "Department of Defense Guiding Principles Compliance", or "GBI GP DOD 
Compliance", use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>For Army projects ONLY:  Choose only the following method for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For USGBC LEED, choose "LEED", and enter "Silver" in the bracket.  For use of alternate certification systems, 
a waiver must be submitted per the current Army Sustainable Design and Development Policy.</NPR><BRK/>
<BRK/>
<NPR>For Navy ONLY: Choose one of the following methods for executing TPC:</NPR><BRK/>
<BRK/>
<NPR>a.  For USGBC LEED, choose "LEED", and enter the target level in the bracket.</NPR><BRK/>
<BRK/>
<NPR>b. For Guiding Principles Assessment for Department of Defense (by GBCI), choose "GBCI GP Assessment (DOD)", use 
only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>c. For Green Building Initiative (GBI) "Department of Defense Guiding Principles Compliance", or "GBI GP DOD Compliance", 
use only DOD version, and ask for it when registering.</NPR><BRK/>
<BRK/>
<NPR>d. For Green Building Initiative (GBI) Green Globes, choose "GBI Green Globes for NC", and enter the target level 
in the bracket.</NPR><BRK/>
<BRK/>
<NPR>e. For an alternate certification system, use only those that comply with the minimum requirements of 10 CFR 433.300 
Subpart C — Green Building Certification for Federal Buildings, and insert the name of the compliant system in 
the empty bracket.  Facilities Engineering Command (FEC) Capital Improvements (CI) Core must authorize the use 
of alternative system.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Pay all fees associated with registration and achievement of Third-Party Certification (TPC), by meeting all TPC and project requirements to achieve[ <RID>
LEED BD+C</RID> [_____]][ <RID>GBCI GP Assessment (DOD)</RID>][ <RID>GBI DOD GP Compliance</RID>][ <RID>GBI Green Globes for NC</RID> [_____]], or Government-approved equivalent TPC 
sustainability certification, assessment, or validation.  An equivalent TPC organization must demonstrate equivalency for Government consideration 
and meet the requirements of <RID>10 CFR 433.300</RID>, prior to use on the project.  Third-Party Certification is met when Government receives TPC organization 
certificate, assessment, or validation and compliance report[ and plaque.]</TXT><BRK/>
<BRK/>
<TXT>Register project with TPC organization using the following format and content:</TXT><BRK/>
<OLG><BRK/>
<OLI>Project Title First Line: Building Owner (US Army, US Air Force, US Navy or US Marine Corps), Building Name (if known)</OLI><BRK/>
<BRK/>
<OLI>Project Title Second Line: MILCON P#, DD1391 Project Name</OLI><BRK/>
<BRK/>
<OLI>Project Address: UIC (Installation code), Category code, RPUID (Real Property Unique Identifier) Number</OLI><BRK/>
<BRK/>
<OLI>Project Owner Organization: US Army, US Air Force, US Navy or US Marine Corps</OLI><BRK/>
<BRK/>
<OLI>Primary Contact, Project Owner: Component Project Manager</OLI><BRK/>
<BRK/>
<OLI>Building Owner Organization: US Army, US Air Force, US Navy or US Marine Corps</OLI><BRK/>
<BRK/>
<OLI>Building Owner Organization Project Number</OLI><BRK/>
<BRK/>
<OLI>Additional Contact, Building Owner: Department of Public Works, Public Works Officer, Base Civil Engineer, or Designee</OLI><BRK/></OLG>
<BRK/></SPT>
][<SPT><TTL>TPC Already Registered</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose this bracketed paragraph if the DOR has registered the project with a TPC organization and will 
pass the responsibility for final TPC documentation and certification, assessment, or validation to the Construction 
Contractor.  Delete the previous bracketed paragraph.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Obtain, fill out, and include TPC checklist with this section.  For projects with multiple buildings, attach 
TPC Checklist for each building that requires TPC.</NPR><BRK/>
<BRK/>
<NPR>For certifications, assessments, or validations that include a plaque, include the bracketed phrases below.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Project is already registered with TPC organization to achieve[ <RID>LEED BD+C</RID> [_____]][ <RID>GBCI GP Assessment (DOD)</RID>][ <RID>GBI DOD GP Compliance</RID>][ <RID>GBI Green Globes for NC</RID>
 [_____]] [_____].  When applicable, request TPC online access turnover from Government.  Manage and provide all documentation for requirements 
of TPC and obtain Final Certification or validation.  Third-Party Certification is met when Government receives TPC organization certificate, assessment, 
or validation and compliance report[ and plaque].</TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>TPC Management and Certification</TTL><BRK/>
<BRK/>
<TXT>Execute the following TPC Certification, assessment, or validation requirements:</TXT><BRK/>
<OLG><BRK/>
<OLI>Refer to TPC Checklist at the end of this specification section.  (Multiple checklists indicate multiple buildings that require TPC.)</OLI><BRK/>
<BRK/>
<OLI>Immediately bring to the attention of the Contracting Officer any project changes that impact meeting the approved TPC Requirements for 
this project.  Demonstrate the change will not increase the life-cycle cost and maintains or improves the building performance.</OLI><BRK/>
<BRK/>
<OLI>Complete all work required to incorporate the applicable TPC Requirements.</OLI><BRK/>
<BRK/>
<OLI>Maintain the construction related information in the Sustainability eNotebook pertaining to additions and changes to the approved sustainability 
requirements.  When construction changes are made that affect design sustainability requirements, provide all required updates to affected 
design requirements and update in the Sustainability eNotebook.  Maintain the Sustainability eNotebook in electronic format.  For more 
explanation, refer to paragraph SUSTAINABILITY eNOTEBOOK.  Provide the following components in the Sustainability eNotebook, in addition 
to the GPV components above:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC Checklist</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Completed TPC forms.  Transmit by the method required by the TPC organization.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Copy of all correspondence with the TPC organization including proof of TPC registration</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Documentation illustrating compliance with TPC requirements and additional documentation as requested by the TPC</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC Award Certificate, assessment, or validation and compliance report.</OLI><BRK/>
<BRK/>
<OLI>Provide the following information in the Sustainability Action Plan.  Provide this TPC information in addition to the Sustainability Action 
Plan items above:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Planned method to achieve each TPC requirement.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">For each TPC requirement that is attempted but not achieved, provide narrative explaining how mission or activity precludes achieving 
specific sustainability requirement or goal.  Provide analysis of particular requirement and level to which project is able to 
comply.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Provide name and contact information for:  Sustainability point of contact (POC) and other names of sustainability professionals 
responsible for ensuring TPC sustainability goals are accomplished and documentation is assembled.  Sustainability POCs are also 
responsible for ensuring GPV required in paragraph GUIDING PRINCIPLES VALIDATION (GPV) above.  It is recommended construction 
team has a member with a current TPC credential, when available, that matches the TPC system and variation specialty pursued 
for the certification.  When retained, this team member must be engaged and keep this credential current over the duration of 
the entire project schedule</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">TPC vendor's project identification and number.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For certifications, assessments, or validations that include a plaque, included the bracketed phrase.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Bear all costs associated with construction changes that affect sustainability design requirements, constructing, demonstrating, and documenting 
that project complies with approved TPC requirements, including but not limited to:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Final TPC review, certification, assessment, or validation[ and plaque] fees.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Online (or offline with secure facilities) TPC management and documentation.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Obtaining TPC certification or validation based on Government-approved sustainability goals.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Construction work required to incorporate TPC requirements.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Submittals required to demonstrate compliance with Government approved TPC checklists.</OLI><BRK/>
<BRK/>
<OLI>Provide all calculations, product data, and certifications, assessments, or validations required in this specification to demonstrate compliance 
with the TPC Requirements.</OLI><BRK/>
<BRK/>
<OLI>Provide all TPC management and documentation. Transmit TPC requirements by the method required by TPC organization.</OLI><BRK/>
<BRK/>
<OLI>Provide all required responses to third party organization.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the bracketed paragraph below for TPC that includes required site visit by a TPC representative 
(this is typically required for GBI provided TPC).  The Government Executing Agent's Project Manager is responsible 
to coordinate the TPC site visit.  Project Manager must coordinate with the TPC representative, Design Manager, 
and Construction Manager to determine participating team members.  Include commissioning provider on applicable 
projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>Facilitate and participate in required TPC site visit.  Coordinate with the Contract Officer to determine participating team members.  
Include Commissioning provider on applicable projects.</OLI><BRK/>
]<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the following paragraph for TPC that includes a certificate, assessment, or validation.  For TPC 
that include a plaque, include the bracketed phrases.</NPR><BRK/>
<AST/><BRK/></NTE>
[<OLI>Provide TPC [Plaque and ]Certificate, assessment, or validation. Provide TPC compliance report that includes level achieved and reasons 
for non-compliance or not applicable elements. Use format below to create the Plaque, Certificate, assessment or validation, compliance 
report, and Letter of Congratulations (when provided).  Forward to parties designated by Contracting Officer:</OLI><BRK/>
<BRK/>
[<OLI LEVEL="2">Plaque:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Name: Final Building Name.  If unknown, provide Form DD1391 Project Name.</OLI><BRK/>
<BRK/>
]<OLI LEVEL="2">Certificate, Assessment or Validation:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Project Title, first line: P-(X); Form DD1391 Project Name).</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Project Title, second line: UIC (Installation code)</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Letter Congratulations (when provided):</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Address letter to Facility's Installation Commander Name.  Address the letter to an individual person.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Compliance Report:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Title page must cite Project title: P-(X); (1391 Project Name); Final Building Name if known; UIC (installation code); Owner 
Service; User organization if known; date of compliance.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Include TPC scoresheet if applicable.</OLI><BRK/>
]<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose first bracket for Air Force projects and delete the others. Choose second bracket for Army projects 
and delete the others. Choose third bracket for Navy projects and delete the others.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Once Final Certification is achieved, turn over Administrative rights to online TPC to the [Base Civil Engineer] [Department of Public 
Works] [Public Works Office] or designee, contact information provided by the Contracting Officer.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT>]</TAI></SPT>][<SPT><TTL>Additional Sustainability Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this bracketed paragraph when there are additional sustainability requirements, including additional 
TPC requirements.  TPC optional requirements that align with HPSB requirements are mandatory.  Add them as requirements 
in the following paragraph.  Coordinate language throughout affected UFGS Sections in this project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The following requirements are included, as required by the project scope or the applied sustainability Third-Party Certification program:</TXT><BRK/>
<BRK/>
<TXT>[_____]</TXT><BRK/>
<BRK/></SPT>
]</SPT></PRT><PRT><TTL>PART 2   PRODUCTS</TTL><BRK/>
<BRK/>
<TXT>Not used.</TXT><BRK/>
<BRK/></PRT>
<PRT><TTL>PART 3   EXECUTION</TTL><BRK/>
<BRK/>
<SPT><TTL>SUSTAINABILITY COORDINATION</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose all the bracketed options below for projects required to obtain TPC certification, assessment, or 
validation.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide sustainability focus and coordination at all meetings to achieve sustainability goals.  Coordinate meeting requirements with other UFGS 
Sections meeting requirements in this project.  Ensure the designated [TPC accredited ]sustainability professional responsible for GP [and TPC 
]documentation participates in these meetings to coordinate documentation completion.  Review GP[ and TPC] sustainability requirements, HPSB Checklist[ 
and TPC] documentation, Sustainability Action Plan, and completeness status of Sustainability eNotebook[, and TPC status] at the following meetings:</TXT><BRK/>
<OLG><BRK/>
<OLI>Pre-Construction Conference</OLI><BRK/>
<BRK/>
<OLI>Construction Quality Control Meetings</OLI><BRK/>
<TAI OPT="DESIGN-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following three items are tailored for DESIGN-BUILD.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Refer to Section <SRF>01 30 00</SRF> ADMINISTRATIVE PROCEDURES for Post Award Meetings.</OLI><BRK/>
<BRK/>
<OLI>Post Award Meeting</OLI><BRK/>
<BRK/>
<OLI>Design Quality Assurance Meetings</OLI><BRK/>
<BRK/>
<OLI>Design Complete Review Meetings</OLI><BRK/>
<BRK/>
<OLI>Conduct review no later than 60 days after final design complete submission and identify any outstanding issues that affect correct completion 
of all documentation requirements, and actions that will achieve requirements. Conduct corrective actions.</OLI><BRK/></TAI>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose the following bracketed sentences for TPC that require on-site visit.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>TPC On-site Visit</OLI><BRK/>
<BRK/>
<OLI>Execute, coordinate, and facilitate on-site visit by third-party representative no later than 60 days before final turnover, or as required 
by TPC organization, whichever is greater.</OLI><BRK/>
<BRK/>
]<OLI>Facility Turnover Meetings</OLI><BRK/>
<BRK/>
<OLI>Conduct review no later than 60 days before final turnover and identify any outstanding issues that affect correct completion of all documentation[ 
and final TPC certification, assessment or validation], and actions that will achieve requirements. Conduct corrective actions prior to 
turnover, to ensure all requirements are achieved.</OLI><BRK/></OLG>
<BRK/></SPT>
[<SPT><TTL><SUB>THIRD-PARTY CERTIFICATION CERTIFICATE, ASSESSMENT, OR VALIDATION AND COMPLIANCE REPORT</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Choose this bracketed paragraph for projects that require the Contractor to obtain the TPC certification.</NPR><BRK/>
<BRK/>
<NPR>For certifications, assessments, or validations that include a plaque, include the bracketed phrase for the plaques.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Finalize the process requirements and obtain the TPC [Plaque and ]Certificate, assessment, or validation, and compliance report, indicating completion 
of the project's sustainability goals.  Include TPC compliance report with final TPC scoresheet as applicable.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Choose the first bracketed sentence when the contract documents give specific instruction for placement 
of the plaque.</NPR><BRK/>
<BRK/>
<NPR>Choose the second bracketed sentence if the Contracting Officer has verified the building occupant wants a framed 
certificate, assessment, or validation, and what kind of framing.</NPR><BRK/>
<BRK/>
<NPR>For certification that include a plaque, include the last bracketed phrase.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[Provide and hang Plaque in accordance with contract documents.  ][Provide one original framed copy of the certificate, assessment, or validation, 
mounted in<MET> 25 mm</MET><ENG> 1 inch</ENG> deep metal frames, with double matt, and wire hangers, in location approved by Contracting Officer.  ]Deliver [one][_____] 
original certificate, assessment, or validation, and compliance report to Contractor Officer, unless otherwise instructed.[  Provide and hang Plaque 
in a prominent interior location approved by the Contracting Officer.]</TXT><BRK/>
<PGE/><BRK/></SPT>
]<SPT><TTL>TABLE 3-1 VOLATILE ORGANIC COMPOUNDS (VOC) (LOW EMITTING MATERIALS) REQUIREMENTS</TTL><BRK/>
<BRK/>
<TAB HEADERROWS="2">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="5" ROWCOUNT="13">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="189.00"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="197.25"/>
      <COL AUTOWIDTH="0" WIDTH="57.75"/>
      <COL AUTOWIDTH="0" WIDTH="189.00"/>
      <COL AUTOWIDTH="0" WIDTH="186.00"/>
      <ROW AUTOHEIGHT="0" HEIGHT="63.00">
         <CEL MERGEACROSS="4" STYLEID="s50">
<DTA TYPE="STRING"><HL3>TABLE 3-1  Volatile Organic Compounds (VOC) (Low Emitting Materials) <HL4>Requirements</HL4></HL3><BRK/><BRK/><HL4>Source: <RID>ICC IgCC</RID> Chapter 8 (Materials) (Interior Applications Only)</HL4></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="44.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>MATERIAL CATEGORY</HL3></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>EMISSIONS REQUIREMENT</HL3></DTA>
         </CEL>
         <CEL/>
         <CEL>
<DTA TYPE="STRING"><HL3>MATERIALS WITH ADDED VOC REQUIREMENT</HL3></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL3>EMISSIONS REQUIREMENTS</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="171.00">
         <CEL MERGEDOWN="1" STYLEID="s50">
<DTA TYPE="STRING"><HL3>Adhesives and Sealants</HL3></DTA>
         </CEL>
         <CEL MERGEDOWN="1" STYLEID="s50">
<DTA TYPE="STRING"><HL3>CDPH/EHLB/Standard method V1.1 (California Section 01350)</HL3><BRK/>(Use "office" or "classroom" space limits for all applications)<BRK/></DTA>
         </CEL>
         <CEL MERGEDOWN="1">
<DTA TYPE="STRING"><HL4>or</HL4></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Adhesives<BRK/>(carpet, resilient, wood flooring; base cove; ceramic tile; drywall and panel; primers)<BRK/>Sealants<BRK/>(acoustical; firestop; HVAC Air duct; primers)<BRK/>Caulks<BRK/></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL3>SCAQMD Rule 1168</HL3><BRK/>(Use "other" category for HVAC duct sealant)<BRK/>(for firestop adhesive, <RID>UFC 3-600-01</RID> overrides conflicting requirements)<BRK/></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="244.50">
         <CEL INDEX="4">
<DTA TYPE="STRING">Aerosol adhesives</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL3>Section 3 of Green Seal Standard GS-36</HL3><BRK/>(except: cleaners, solvent cements, and primers used with plastic piping and conduit in plumbing, fire suppression, and electrical systems; HVAC air duct sealants when the application space air temp is less than 40 F (4.5 C).<BRK/></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="315.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>Paints and Coatings</HL3></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>CDPH/EHLB/Standard method V1.1 (California Section 01350)</HL3><BRK/>(Use "office" or "classroom" space limits for all applications)<BRK/></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL4>or</HL4></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Flat and nonflat, nonflat high-gloss, specialty, basement specialty, fire-resistive, floor, low-solids, rust preventative, wood, reflective wall coatings; concrete/masonry sealers; primers; sealers; undercoaters; shellacs (clear and opaque); stains; varnishes; conjugated oil varnish; lacquer; clear brushing lacquer</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL3>Green Seal Standard GS-11</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="281.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>Paints and Coatings</HL3></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>CDPH/EHLB/Standard method V1.1 (California Section 01350)</HL3><BRK/>(Use "office" or "classroom" space limits for all applications)<BRK/></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL4>or</HL4></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Concrete curing compounds; dry fog, faux finishing, graphic arts (sign paints), industrial maintenance, mastic texture, metallic pigmented, multicolor, recycled coatings; pretreatment wash primers, reactive penetrating sealers; specialty primers, wood preservatives, and zinc primers</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL3>California Air Resources Board (CARB) Suggested Control Measure for Architectural Coatings</HL3><BRK/>or<BRK/><HL3>SCAQMD Rule 1113r</HL3><BRK/></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="125.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>Paints and Coatings</HL3></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>CDPH/EHLB/Standard method V1.1 (California Section 01350)</HL3><BRK/>(Use "office" or "classroom" space limits for all applications)</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL4>or</HL4></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">High-temperature coatings; stone consolidants; swimming-pool coatings; tub- and tile-refining coatings; and waterproofing membranes</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL3>California Air Resources Board (CARB) Suggested Control Measure for Architectural Coatings</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="172.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>Floor Covering Materials</HL3></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">For carpet, all locations:<BRK/><HL3>CDPH/EHLB/Standard Method V1.1 (California Section 01350)</HL3><BRK/>or<BRK/>label for <HL3>Section 9</HL3> of <HL3>CDPH/EHLB/Standard Method V1.1 (California Section 01350)</HL3><BRK/><BRK/></DTA>
         </CEL>
         <CEL/>
         <CEL>
<DTA TYPE="STRING">none</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">none</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="108.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>Insulation</HL3></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>CDPH/EHLB/Standard method V1.1</HL3> (California Section 01350)<BRK/>(Use "office" or "classroom" space limits for all applications)<BRK/></DTA>
         </CEL>
         <CEL/>
         <CEL>
<DTA TYPE="STRING">none</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">none</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="184.50">
         <CEL MERGEDOWN="1" STYLEID="s50">
<DTA TYPE="STRING"><HL3>Composite Wood, Wood Structural Panel, and Agrifiber Products</HL3>, no added urea- formaldehyde resins<BRK/>including laminating adhesives for composite wood and agrifiber assemblies -<BRK/>particleboard,<BRK/>medium density fiberboard (MDF),<BRK/>wheatboard,<BRK/>strawboard,<BRK/>panel substrates,<BRK/>door cores<BRK/></DTA>
         </CEL>
         <CEL MERGEDOWN="1" STYLEID="s50">
<DTA TYPE="STRING">Third-party certification (approved by CARB) of <HL3>California Air Resource Board's (CARB) regulation</HL3>, Airborne Toxic Control Measure to Reduce Formaldehyde Emissions from Composite Wood Products</DTA>
         </CEL>
         <CEL MERGEDOWN="1">
<DTA TYPE="STRING"><HL4>or</HL4></DTA>
         </CEL>
         <CEL MERGEDOWN="1">
<DTA TYPE="STRING">none</DTA>
         </CEL>
         <CEL MERGEDOWN="1">
<DTA TYPE="STRING"><HL3>CDPH/EHLB/Standard method V1.1</HL3> (California Section 01350)<BRK/>(Use "office" or "classroom" space limits for all applications)<BRK/>(except: Structural panel components such as plywood, particle board, wafer board, and oriented strand board identified as "EXPOSURE 1," "EXTERIOR," or "HUD-APPROVED" are considered acceptable for interior use.)<BRK/></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="84.00"/>
      <ROW AUTOHEIGHT="0" HEIGHT="182.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>Office Furniture Systems and Seating</HL3><BRK/>installed prior to occupancy</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>ANSI/BIFMA X7.1</HL3><BRK/><HL3>ANSI/BIFMA X7.1:</HL3><BRK/>(95-percent of installed office furniture system workstations and seating units)<BRK/><BRK/><HL3>Section 7.6.2 of ANSI/BIFMA e3</HL3><BRK/>(50-percent
 of office furniture system workstations and seating units)</DTA>
         </CEL>
         <CEL/>
         <CEL>
<DTA TYPE="STRING">none</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">none</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="195.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>Ceiling and Wall</HL3> assemblies and systems including: acoustical treatments; ceiling panels and tiles; tackable wall panels and coverings; wall coverings; wall and ceiling paneling and planking</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL3>CDPH/EHLB/Standard method V1.1 (California Section 01350)</HL3><BRK/>(Use "office" or "classroom" space limits for all applications)</DTA>
         </CEL>
         <CEL/>
         <CEL>
<DTA TYPE="STRING">none</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">none</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/></SPT>
<NTE><BRK/>
<AST/><BRK/>
<NPR>Attach completed draft "High Performance and Sustainable Building (HPSB) Checklist".  For Army and Navy, this 
is required when project exceeds threshold defined in notes under this section’s title.  For Air Force, this is 
required for every project.  For projects with multiple buildings, attach completed draft HPSB Checklist for each 
building.</NPR><BRK/>
<BRK/>
<NPR>Attach completed draft TPC checklist.  This is required when project exceeds threshold defined in note above the 
paragraph THIRD-PARTY CERTIFICATION <NED/>(TPC) DOCUMENTATION.  For projects with multiple buildings, attach completed 
draft TPC Checklist for each building that requires TPC.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/></PRT>
    <END/><BRK/></SEC>
