<?xml version="1.0" encoding="windows-1252"?><SEC xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="http://si.ksc.nasa.gov/sidownloads/xml/specsintactSEC.xsd"><MTA NAME="SUBFORMAT" CONTENT="NEW"/><MTA NAME="AUTONUMBER" CONTENT="TRUE"/><HDR><AST/><TAB BORDERS="0">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="4">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="366.00"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="365.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="14.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">USACE / NAVFAC / AFCEC</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">UFGS-01 74 19 (February 2019)</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="12.00">
         <CEL MERGEDOWN="1" STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Change 3 - 11/21</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="12.00">
         <CEL INDEX="2" STYLEID="s50">
<DTA TYPE="STRING"><HL3>------------------------------------</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="33.00">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Preparing Activity:  <PRA>USACE</PRA></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Superseding<BRK/>UFGS-01 74 19 (January 2007)</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<HL4>UNIFIED FACILITIES GUIDE SPECIFICATIONS</HL4><BRK/>
<BRK/>
<HL4>References are in agreement with UMRL dated July 2025</HL4><BRK/>
<AST/><BRK/></HDR>
<BRK/>
<SCN>SECTION 01 74 19</SCN><BRK/>
<BRK/>
<STL>CONSTRUCTION WASTE MANAGEMENT AND DISPOSAL</STL><BRK/>
<DTE>02/19, CHG 3: 11/21</DTE><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This guide specification covers the requirements for <SCP>the management of non-hazardous construction waste 
and demolition debris/waste materials</SCP>.<BRK/>
<BRK/>
Every project must use a properly edited version of this guide specification.<BRK/>
<BRK/>
This guide specification contains tailoring for AIR FORCE, ARMY, NAVY, NAVFAC PAC, and NAVFAC SE. Select/deselect 
tailoring prior to editing.<BRK/>
<BRK/>
This specification section must be coordinated with Section <SRF>02 41 00</SRF> [DEMOLITION][ AND ][DECONSTRUCTION] and Section 
<SRF>01 57 19</SRF>, TEMPORARY ENVIRONMENTAL CONTROLS, and when included, Section <SRF>01 33 29</SRF>, SUSTAINABILITY REQUIREMENTS AND REPORTING.<BRK/>
<BRK/>
Requirements in this guide specification apply to all DoD installations (including government owned / contractor 
operated installations and tenant activities) regardless of the funding source.<BRK/>
<BRK/>
Adhere to <URL HREF="https://www.wbdg.org/dod/ufc/ufc-1-300-02">UFS 1-300-02</URL> Unified Facilities Guide Specifications (UFGS) Format Standard when editing this guide 
specification or preparing new project specification sections.  Edit this guide specification for project specific 
requirements by adding, deleting, or revising text.  For bracketed items, choose applicable item(s) or insert 
appropriate information.<BRK/>
<BRK/>
Remove information and requirements not required in respective project, whether or not brackets are present.<BRK/>
<BRK/>
Comments, suggestions and recommended changes for this guide specification are welcome and should be submitted 
as a <URL HREF="https://www.wbdg.org/dod/ufgs">Criteria Change Request (CCR)</URL>.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<PRT><TTL>PART 1   GENERAL</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The DOD Integrated (Non-Hazardous) Solid Waste Management Policy, requires all facilities to meet a non-hazardous 
solid waste diversion goal of 60% Construction and Demolition Diversion.  This guide specification should be used 
to identify requirements necessary to meet construction waste management requirements under government construction 
or demolition contract.<BRK/>
<BRK/>
Coordinate the requirements of this specification with the installation's waste management programs where the 
project is located.  Where available, include information about access to recycling centers and storage areas 
in the technical content for better coordination with the contract requirements.<BRK/>
<BRK/>
Disposal of hazardous waste or toxic waste materials is specified in Section <SRF>02 81 00</SRF> TRANSPORTATION AND DISPOSAL 
OF HAZARDOUS MATERIALS and Section <SRF>01 57 19</SRF> TEMPORARY ENVIRONMENTAL CONTROLS.<BRK/>
<BRK/></NPR>
<BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>REFERENCES</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is used to list the publications cited in the text of the guide specification.  The publications 
are referred to in the text by basic designation only and listed in this paragraph by organization, designation, 
date, and title.<BRK/>
<BRK/>
Use the Reference Wizard's Check Reference feature when you add a Reference Identifier (RID) outside of the Section's 
Reference Article to automatically place the reference in the Reference Article.  Also use the Reference Wizard's 
Check Reference feature to update the issue dates.<BRK/>
<BRK/>
References not used in the text will automatically be deleted from this section of the project specification when 
you choose to reconcile references in the publish print process.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The publications listed below form a part of this specification to the extent referenced.  The publications are referred to within the text by 
the basic designation only.</TXT><BRK/>
<BRK/>
<REF><ORG>U.S. NATIONAL ARCHIVES AND RECORDS ADMINISTRATION (NARA)</ORG><BRK/>
<BRK/>
<RID>40 CFR 273</RID><RTL>Standards for Universal Waste Management</RTL><BRK/>
<BRK/>
<RID>49 CFR 173</RID><RTL>Shippers - General Requirements for Shipments and Packagings</RTL><BRK/>
<BRK/>
<RID>49 CFR 178</RID><RTL>Specifications for Packagings</RTL><BRK/>
<BRK/></REF>
</SPT><SPT><TTL>DEFINITIONS</TTL><BRK/>
<BRK/>
<SPT><TTL>Co-mingle</TTL><BRK/>
<BRK/>
<TXT>The practice of placing unrelated materials together in a single container, usually for benefits of convenience and speed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Construction Waste</TTL><BRK/>
<BRK/>
<TXT>Waste generated by construction activities, such as scrap materials, damaged or spoiled materials, temporary and expendable construction materials, 
and other waste generated by the workforce during construction activities.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Demolition Debris/Waste</TTL><BRK/>
<BRK/>
<TXT>Waste generated from demolition activities, including minor incidental demolition waste materials generated as a result of Intentional dismantling 
of all or portions of a building, to include clearing of building contents that have been destroyed or damaged.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Disposal</TTL><BRK/>
<BRK/>
<TXT>Depositing waste in a solid waste disposal facility, usually a managed landfill or incinerator, regulated in the US under the Resource Conservation 
and Recovery Act (RCRA).</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Diversion</TTL><BRK/>
<BRK/>
<TXT>The practice of diverting waste from disposal in a landfill or incinerator, by means of eliminating or minimizing waste, or reuse of materials.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Final Construction Waste Diversion Report</TTL><BRK/>
<BRK/>
<TXT>A written assertion by a material recovery facility operator identifying constituent materials diverted from disposal, usually including summary 
tabulations of materials, weight in short-ton.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Recycling</TTL><BRK/>
<BRK/>
<TXT>The series of activities, including collection, separation, and processing, by which products or other materials are diverted from the solid waste 
stream for use in the form of raw materials in the manufacture of new products sold or distributed in commerce, or the reuse of such materials 
as substitutes for goods made of virgin materials, other than fuel.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Reuse</TTL><BRK/>
<BRK/>
<TXT>The use of a product or materials again for the same purpose, in its original form or with little enhancement or change.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Salvage</TTL><BRK/>
<BRK/>
<TXT>Usable, salable items derived from buildings undergoing demolition or deconstruction, parts from vehicles, machinery, other equipment, or other 
components.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Source Separation</TTL><BRK/>
<BRK/>
<TXT>The practice of administering and implementing a management strategy to identify and segregate unrelated waste at the first opportunity.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>CONSTRUCTION WASTE (INCLUDES DEMOLITION DEBRIS/WASTE)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  All projects are required to divert at least 60 percent of their non-hazardous solid wastes from the waste 
stream (including waste from construction, demolition, or deconstruction operations).</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Divert a minimum of [60][_____] percent by weight of the project construction waste and demolition debris/waste from the landfill or incinerator.  
Follow applicable industry standards in the management of waste.  Apply sound environmental principles in the management of waste.  (1) Practice 
efficient waste management when sizing, cutting, and installing products and materials and (2) use all reasonable means to divert construction 
waste and demolition debris/waste from landfills and incinerators and to facilitate the recycling or reuse of excess construction materials.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>CONSTRUCTION WASTE MANAGEMENT</TTL><BRK/>
<BRK/>
<TXT>Implement a Construction Waste Management Program for the project.  Take a pro-active, responsible role in the management of construction waste, 
recycling process, disposal of demolition debris/waste, and require all subcontractors, vendors, and suppliers to participate in the Construction 
Waste Management Program.  Establish a process for clear tracking, and documentation of construction waste and demolition debris/waste.</TXT><BRK/>
<BRK/>
<SPT><TTL>Implementation of Construction Waste Management Program</TTL><BRK/>
<BRK/>
<TXT>Develop and document how the Construction Waste Management Program will be implemented in a Construction Waste Management Plan.  Submit a Construction 
Waste Management Plan to the Contracting Officer for approval.  Construction waste and demolition debris/waste materials include un-used construction 
materials not incorporated in the final work, as well as demolition debris/waste materials from demolition activities or deconstruction activities.  
In the management of waste, consider the availability of viable markets, the condition of materials, the ability to provide material in suitable 
condition and in a quantity acceptable to available markets, and time constraints imposed by internal project completion mandates.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Oversight</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Army Project select the first bracketed option.</NPR><BRK/>
<BRK/>
<NPR>For Air Force Project being designed and administered by Army, select the first<BRK/>
bracketed option.</NPR><BRK/>
<BRK/>
<NPR>For Navy Projects, select the second bracketed option.</NPR><BRK/>
<BRK/>
<NPR>For Air Force Project being designed and administered by Navy, select the second bracketed option.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT><TAI OPT="AIR FORCE,ARMY">[The Quality Control Manager, as specified in Section <SRF>01 45 00</SRF> QUALITY CONTROL, is responsible for overseeing and documenting results from executing 
the Construction Waste Management Plan for the project.]</TAI><TAI OPT="NAVY">[The Environmental Manager, as specified in Section <SRF>01 57 19</SRF> TEMPORARY ENVIRONMENTAL CONTROLS, 
is responsible for overseeing and documenting results from executing the Construction Waste Management Plan for the project.]</TAI></TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Special Programs</TTL><BRK/>
<BRK/>
<TXT>Implement special programs involving rebates or similar incentives related to recycling of construction waste and demolition debris/waste materials.  
Retain revenue or savings from salvaged or recycling, unless otherwise directed.  Ensure firms and facilities used for recycling, reuse, and disposal 
are permitted for the intended use to the extent required by federal, state, and local regulations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Special Instructions</TTL><BRK/>
<BRK/>
<TXT>Provide on-site instruction of appropriate separation, handling, recycling, salvage, reuse, and return methods to be used by all parties at the 
appropriate stages of the projects.  Designation of single source separating or commingling will be clearly marked on the containers.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Waste Streams</TTL><BRK/>
<BRK/>
<TXT>Delineate waste streams and characterization, including estimated material types and quantities of waste, in the Construction Waste Management 
Plan.  Manage all waste streams associated with the project.  Typical waste streams are listed below.  Include additional waste steams not listed:</TXT><BRK/>
<OLG><BRK/>
<OLI>Land Clearing Debris</OLI><BRK/>
<BRK/>
<OLI>Asphalt</OLI><BRK/>
<BRK/>
<OLI>Masonry and CMU</OLI><BRK/>
<BRK/>
<OLI>Concrete</OLI><BRK/>
<BRK/>
<OLI>Metals (Includes, but is not limited to, banding, stud trim, ductwork, piping, rebar, roofing, other trim, steel, iron, galvanized, stainless 
steel, aluminum, copper, zinc, bronze.)</OLI><BRK/>
<BRK/>
<OLI>Wood (nails and staples allowed)</OLI><BRK/>
<BRK/>
<OLI>Glass</OLI><BRK/>
<BRK/>
<OLI>Paper</OLI><BRK/>
<BRK/>
<OLI>Plastics (PET, HDPE,PVC,LDPE,PP,PS, Other)</OLI><BRK/>
<BRK/>
<OLI>Gypsum</OLI><BRK/>
<BRK/>
<OLI>Non-hazardous paint and paint cans</OLI><BRK/>
<BRK/>
<OLI>Carpet</OLI><BRK/>
<BRK/>
<OLI>Ceiling Tiles</OLI><BRK/>
<BRK/>
<OLI>Insulation</OLI><BRK/>
<BRK/>
<OLI>Beverage Containers</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT><SPT><TTL>SUBMITTALS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Review submittal description (SD) definitions in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES and edit the following 
list, and corresponding submittal items in the text, to reflect only the submittals required for the project.  
The Guide Specification technical editors have classified those items that require Government approval, due to 
their complexity or criticality, with a "G."  Generally, other submittal items can be reviewed by the Contractor's 
Quality Control System.  Only add a “G” to an item, if the submittal is sufficiently important or complex in context 
of the project.<BRK/>
<BRK/>
<TAI OPT="ARMY">For Army projects, fill in the empty brackets following the "G" classification, with a code of up to three characters 
to indicate the approving authority.  Codes for Army projects using the Resident Management System (RMS) are:  
"AE" for Architect-Engineer; "DO" for District Office (Engineering Division or other organization in the District 
Office); "AO" for Area Office; "RO" for Resident Office; and "PO" for Project Office.  </TAI>Codes following the "G" 
typically are not used for Navy and Air Force projects.<BRK/>
<BRK/>
The "S" classification indicates submittals required as proof of compliance for sustainability Guiding Principles 
Validation or Third Party Certification and as described in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
<TAI OPT="NAVY DESIGN-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Navy Design-Build projects, delete <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES, and replace with UFGS 01 33 00.05 
20 CONSTRUCTION SUBMITTAL PROCEDURES and UFGS 01 33 10.05 20 DESIGN SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Government approval is required for submittals with a "G" or "S" classification.<TAI OPT="AIR FORCE,NAVY">  Submittals not having a "G" or "S" classification are for Contractor 
Quality Control approval.</TAI><TAI OPT="ARMY">  Submittals not having a "G" or "S" classification are for information only.  When used, a code following the "G" classification 
identifies the office that will review the submittal for the Government.</TAI>  Submit the following in accordance with Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES:</TXT><BRK/>
<BRK/>
<LST><SUB>SD-01 Preconstruction Submittals</SUB></LST><BRK/>
<TAI OPT="NAVFAC PAC"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects in the NAVFAC PAC Area of Operation, the submittals identified as SD-01 Preconstruction Submittal 
for this spec section, remove the “G” designation.  The preconstruction submittal(s) in this spec section must 
be approved by the Contractor’s Quality Control System.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<ITM><SUB>Construction Waste Management Plan</SUB>; <SUB>G<TAI OPT="ARMY">, [_____]</TAI></SUB></ITM><BRK/>
<BRK/>
<TAI OPT="AIR FORCE,ARMY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The following three submittals are tailored for AIR FORCE and ARMY.</NPR><BRK/>
<AST/><BRK/></NTE>
<LST><SUB>SD-06 Test Reports</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Quarterly Reports</SUB></ITM><BRK/>
<BRK/>
<ITM><SUB>Annual Report</SUB></ITM></TAI><BRK/>
<BRK/>
<LST><SUB>SD-11 Closeout Submittals</SUB></LST><BRK/>
<BRK/>
<ITM><SUB>Final Construction Waste Diversion Report</SUB>; <SUB>S</SUB></ITM><BRK/>
<BRK/></SPT>
<SPT><TTL>MEETINGS</TTL><BRK/>
<BRK/>
<TXT>Conduct Construction Waste Management meetings.  After award of the Contract and prior to commencement of work, schedule and conduct a meeting 
with the Contracting Officer to discuss the proposed Construction Waste Management Plan and to develop a mutual understanding relative to the management 
of the Construction Waste Management Program and how waste diversion requirements will be met.</TXT><BRK/>
<BRK/>
<TXT>The requirements of this meeting may be fulfilled during the coordination and mutual Understanding meeting outlined in Section <SRF>01 45 00</SRF> QUALITY 
CONTROL.  At a minimum, discuss  and document waste management goals at following meetings:</TXT><BRK/>
<OLG><BRK/>
<OLI>[Preconstruction][Pre-demolition] meeting.</OLI><BRK/>
<BRK/>
<OLI>Regular [site][Quality Control] meetings.</OLI><BRK/>
<BRK/>
<OLI>Work safety meeting (if applicable).</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL><SUB>CONSTRUCTION WASTE MANAGEMENT PLAN</SUB></TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<TAI OPT="NAVFAC PAC"><NPR>NOTE:  For projects in the NAVFAC PAC Area of Operation, for DBB projects select the first bracketed sentences 
(1st and 2nd sentence), and edit this first sentence by selecting "45" and "calendar" and "contract award", and 
delete the second bracketed sentences.  For DB project select the second bracketed (3rd and 4th sentence) sentences 
and remove the first bracketed sentences.</NPR><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC SE"><NPR>For projects in the NAVFAC Southeast Area of Operation, the requirements for the Contractor's Waste Management 
Plan must be coordinated with the waste management plan for the Installation. Revise the paragraph as necessary 
to meet the Installation's requirements. Verify that items are able to be desposed of as specified herein. The 
contractor may include specified items in item (i) below if explanation or justification exists, when approved 
by the Contracting Officer.</NPR></TAI><BRK/>
<AST/><BRK/></NTE>
<TXT>[Submit Construction Waste Management Plan within [15] [45] [calendar] days after [contract award][notice to proceed].  Revise and resubmit Construction 
Waste Management Plan as necessary, in order for construction to begin.].  [Submit Construction Waste Management Plan not less than 60 calendar 
days before scheduled final site or building design approval.  Revise and resubmit Construction Waste Management Plan until it receives final approval 
from the Contracting Officer, in order for construction to begin.]  Execute demolition or deconstruction activities in accordance with Section 
<SRF>02 41 00</SRF> [DEMOLITION] [AND] [DECONSTRUCTION].  Manage demolition debris/waste or deconstruction materials in accordance with the approved construction 
waste management plan.</TXT><BRK/>
<BRK/>
<TXT>An approved Construction Waste Management Plan will not relieve the Contractor of responsibility for compliance with applicable environmental regulations 
or meeting project cumulative waste diversion requirement.  Ensure all subcontractors receive a copy of the approved Construction Waste Management 
Plan.  The plan demonstrates how to meet the project waste diversion requirement.  Also, include the following in the plan:</TXT><BRK/>
<OLG><BRK/>
<OLI>Identify the names of individuals responsible for waste management and waste management tracking, along with roles and responsibilities 
on the project.</OLI><BRK/>
<BRK/>
<OLI>Actions that will be taken to reduce solid waste generation, including coordination with subcontractors to ensure awareness and participation.</OLI><BRK/>
<BRK/>
<OLI>Description of the regular meetings to be held to address waste management.</OLI><BRK/>
<BRK/>
<OLI>Description of the specific approaches to be used in recycling/reuse of the various materials generated, including the areas on site and 
equipment to be used for processing, sorting, and temporary storage of materials.</OLI><BRK/>
<BRK/>
<OLI>Name of landfill and incinerator to be used.</OLI><BRK/>
<BRK/>
<OLI>Identification of local and regional re-use programs, including non-profit organizations such as schools, local housing agencies, and organization 
that accept used materials such as material exchange networks and resale stores. Include the name, location, phone number for each re-use 
facility identified, and provide a copy of the permit or license for each facility.</OLI><BRK/>
<BRK/>
<OLI>List of specific materials, by type and quantity, that will be salvaged for resale, salvaged and reused on the current project, salvaged 
and stored for reuse on a future project, or recycled.  Identify the recycling facilities by name, address, and phone number.</OLI><BRK/>
<BRK/>
<OLI>Identification of materials that cannot be recycled or reused with an explanation or justification, to be approved by the Contracting Officer.</OLI><BRK/>
<BRK/>
<OLI>Description of the means by which materials identified in item (g) above will be protected from contamination.</OLI><BRK/>
<BRK/>
<OLI>Description of the means of transportation of the recyclable materials (whether materials will be site-separated and self-hauled to designated 
centers, or whether mixed materials will be collected by a waste hauler and removed from the site).</OLI><BRK/>
<BRK/>
<OLI>Copy of training plan for subcontractors and other services to prevent contamination by co-mingling materials identified for diversion 
and waste materials.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include list items below when required by Third Party Certification (TPC).  Refer to section <SRF>01 33 29</SRF> SUSTAINABILITY 
REQUIREMENTS AND REPORTING for third party certification requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>Identification of at least [5] [_____] construction or demolition material streams for diversion.<BRK/></OLI>
]<BRK/>
<BRK/>
[<OLI>Detailed plan and distribution of waste diversion between buildings, when project is a part of a campus.</OLI>]<BRK/>
<BRK/>
[<OLI>Facilities or subcontractors offering construction waste transport on-site or off-site must ensure that proper shipping orders, bill of 
lading, manifests, or other shipping documents containing waste diversion information meet requirements of <RID>40 CFR 273</RID> Universal Waste Management, <RID>
49 CFR 173</RID> Shippers - General Requirements for Shipments and Packagings, and <RID>49 CFR 178</RID> Specifications for Packaging.  Individuals signing 
manifests or other shipping documents should meet the minimum training requirements.</OLI>]<BRK/>
<BRK/>
[<OLI>List each supplier who deliver construction materials, in bulk, or package products in returnable containers or returnable packaging, or 
have take-back programs.  List each program and the applicable material to actively monitor and track to assist in meeting waste diversion 
requirements on the project.</OLI>]<BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include items below when a project is located outside the Continental United States (OCONUS) and is subject 
to known host nation agreements.  Delete the additional items below, if the project is inside the United States 
and not subject to Host Nation Agreements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>Identify local jurisdiction requirements for waste management.  Include local requirements and points of contact.]</OLI><BRK/></OLG>
<BRK/>
<TXT>Distribute copies of the waste management plan to each subcontractor, <TAI OPT="AIR FORCE,ARMY">Quality Control Manager</TAI> <TAI OPT="NAVY">Environmental Manager</TAI>, and the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>RECORDS (DOCUMENTATION)</TTL><BRK/>
<BRK/>
<SPT><TTL>General</TTL><BRK/>
<BRK/>
<TXT>Maintain records to document the types and quantities of waste generated and diverted though re-use, recycling and sale to third parties; through 
disposal to a landfill or incinerator facility.  Provide explanations for materials not recycled, reused or sold.  Collect and retain manifests, 
weight tickets, sales receipts, and invoices specifically identifying diverted project waste materials or disposed materials.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Accumulated</TTL><BRK/>
<BRK/>
<TXT>Maintain a running record of materials generated and diverted from landfill disposal, including accumulated diversion rates for the project. Make 
records available to the Contracting Officer during construction or incidental demolition activities. Provide a copy of the diversion records to 
the Contracting Officer upon completion of the construction, incidental demolitions or minor deconstruction activities.</TXT><BRK/>
<BRK/></SPT>
</SPT><TAI OPT="AIR FORCE,ARMY"><SPT><TTL>REPORTS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for Armyand Air Force.</NPR><BRK/>
<BRK/>
<NPR>For Army projects, waste reports go to the SWARS Coordinator or Department of Public Works (DPW) Solid Waste Manager.</NPR><BRK/>
<BRK/>
<NPR>For Air Force projects, coordinate with the Base and identify the appropriate person to receive this data.</NPR><BRK/>
<BRK/>
<BRK/>
<NPR>Edit the bracket selection for Quarterly Reporting and insert the appropriate office/point of contact that will 
receive the waste reports.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>General</TTL><BRK/>
<BRK/>
<TXT>Maintain current construction waste diversion information on site for periodic inspection by the Contracting Officer.  Include in the quarterly 
reports, annual reports and final reports:  the project name, contract information, information for waste generated, diverted and disposed of for 
the current reporting period and show cumulative totals for the project.  Reports must identify quantifies of waste by type and disposal method.  
Also include in each report, supporting documentation to include manifests, weigh tickets, receipts, and invoices specifically identifying the 
project and waste material type and weighted sum.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Quarterly Reporting</TTL><BRK/>
<BRK/>
<TXT>Provide cumulative reports at the end of each quarter (December, March, June, and September, corresponding with the federal fiscal year for reporting 
purposes).  Submit <SUB>quarterly reports</SUB> not later than 15 calendar days after the preceding quarter has ended.  [Submit Quarterly Reports to the appropriate 
office or identified point of contact.]<BRK/></TXT>
<BRK/>
<BRK/></SPT>
<SPT><TTL>Annual Reporting</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Edit bracketed option to tell Contractor where additional copies of annual report is required to be submitted.</NPR><BRK/>
<BRK/>
<NPR>Identify who the appropriate installation POC is and insert in the bracketed option.  Delete bracketed option 
if not applicable.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide a cumulative construction waste diversion report annually.  Submit <SUB>annual report</SUB> not later than 30 calendar days after the preceding fourth 
quarter has ended.[  Provide copy of annual construction waste diversion report to the installation POC.]</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>FINAL CONSTRUCTION WASTE DIVERSION REPORT</TTL><BRK/>
<BRK/>
<TXT>A Final Construction Waste Diversion Report is required at the end of the project.  Provide <SUB>Final Construction Waste Diversion Report</SUB> [60] [_____] 
days prior to the Beneficial Occupancy Date (BOD).  The final Construction Waste Diversion Report must be included in the Sustainability eNotebook 
in accordance with Section <SRF>01 33 29</SRF> SUSTAINABILITY REQUIREMENTS AND REPORTING.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>COLLECTION</TTL><BRK/>
<BRK/>
<TXT>Collect, store, protect, and handle reusable and recyclable materials at the site in a manner which prevents contamination, and provides protection 
from the elements to preserve their usefulness and monetary value. Provide receptacles and storage areas designated specifically for recyclable 
and reusable materials and label them clearly and appropriately to prevent contamination from other waste materials.  Keep receptacles or storage 
areas neat and clean.</TXT><BRK/>
<BRK/>
<TXT>Train subcontractors and other service providers to either separate waste streams or use the co-mingling method as described in the Construction 
Waste Management Plan.  Handle hazardous waste and hazardous materials in accordance with applicable regulations and coordinate with Section 
<SRF>01 57 19</SRF> TEMPORARY ENVIRONMENTAL CONTROLS and Section <SRF>02 81 00</SRF> TRANSPORTATION AND DISPOSAL OF HAZARDOUS MATERIALS.  Separate materials by one of 
the following methods:</TXT><BRK/>
<BRK/>
<SPT><TTL>Source Separation Method</TTL><BRK/>
<BRK/>
<TXT>Separate waste products and materials that are recyclable from trash and sort as described below into appropriately marked separate containers 
and then transport to the respective recycling facility for further processing.  Deliver materials in accordance with recycling or reuse facility 
requirements (e.g., free of dirt, adhesives, solvents, petroleum contamination, and other substances deleterious to the recycling process).  Separate 
materials into the category types as defined in the Construction Waste Management Plan.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Contact local recycling centers or Installation POC if the Installation has a recycling program to determine 
if Co-Mingled Method is allowed.  Include the following section if applicable.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/></SPT>
[<SPT><TTL>Co-Mingled Method</TTL><BRK/>
<BRK/>
<TXT>Place waste products and recyclable materials into a single container and then transport to an authorized recycling facility, which meets all applicable 
requirements to accept and dispose of recyclable materials in accordance with all applicable local, state and federal regulations.  The Co-mingled 
materials must be sorted and processed in accordance with the approved Construction Waste Management Plan. </TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Other Methods</TTL><BRK/>
<BRK/>
<TXT>Other methods proposed by the Contractor may be used when approved by the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>DISPOSAL</TTL><BRK/>
<BRK/>
<TXT>Control accumulation of waste materials and trash.  Recycle or dispose of collected materials off-site at intervals approved by the Contracting 
Officer and in compliance with waste management procedures as described in the waste management plan.  Except as otherwise specified in other sections 
of the specifications, dispose of in accordance with the following:</TXT><BRK/>
<BRK/>
<SPT><TTL>Reuse</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Determine if sale of recovered materials is allowed at the Installation, and choose the appropriate bracketed 
phrase.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Give first consideration to reusing construction and demolition materials as a disposition strategy.  Recover for reuse materials, products, and 
components  as described in the approved Construction Waste Management Plan.  Coordinate with the Contracting Officer to identify onsite reuse 
opportunities or material sales or donation available through Government resale or donation programs.  Sale of recovered materials [is] [is not] 
allowed on the Installation.   Consider the use of surplus industrial supply broker services, who match entities with reusable or repurpose industrial 
materials with entities with need of such materials.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Recycle</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Crushing lamps on site creates a hazardous waste stream, which has additional handling and disposal requirements.  
If this process is required based on the facility type, make adjustments in the associated text. </NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Recycle non-hazardous construction and demolition/debris materials that are not suitable for reuse.  Track rejection of contaminated recyclable 
materials by the recycling facility.  Rejected recyclables materials will not be counted as a percentage of diversion calculation.  Recycle all 
fluorescent lamps, HID lamps, mercury (Hg) -containing thermostats and ampoules, and PCBs-containing ballasts and electrical components as directed 
by the Contracting Officer.  Do not crush lamps on site as this creates a hazardous waste stream with additional handling requirements. </TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include bracket paragraph if a composting pile can remain on site after construction is completed or if 
the Installation has a Composting Program or partners with a local composting venue.  Verify if advertised composting 
opportunities are still available at the time of the contract and remove if no longer available.  Construction 
Waste Management Plan should expressly address the strategy to utilize composting or not to utilize composting, 
if the opportunity exists.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/></SPT>
[<SPT><TTL>Compost</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  If a compost pile can remain on site after construction is complete, and if there is a use for the finished 
compost, employ composting practices throughout the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Consider composting on site if a reasonable amount of compostable materials will be available and a utilization of compostable material can be 
determined and appropriately planned for.  Compostable materials include plant materials, sawdust and certain food scraps.  Composting as a strategy 
must be explicitly addressed in the Construction Waste Management Plan submitted for approval to ensure it is feasible. </TXT><BRK/>
<BRK/></SPT>
]<SPT><TTL>Waste</TTL><BRK/>
<BRK/>
<TXT>Dispose by landfill or incineration only those waste materials with no practical use, economic benefit, or recycling opportunity.</TXT><BRK/>
<BRK/></SPT>
</SPT></PRT><PRT><TTL>PART 2   PRODUCTS</TTL><BRK/>
<BRK/>
<TXT>Not used.</TXT><BRK/>
<BRK/></PRT>
<PRT><TTL>PART 3   EXECUTION</TTL><BRK/>
<BRK/>
<TXT>Not used.</TXT></PRT>   <END/><BRK/></SEC>
