<?xml version="1.0" encoding="windows-1252"?><SEC xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="http://si.ksc.nasa.gov/sidownloads/xml/specsintactSEC.xsd"><MTA NAME="SUBFORMAT" CONTENT="NEW"/><MTA NAME="AUTONUMBER" CONTENT="TRUE"/><HDR><AST/><TAB BORDERS="0">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="4">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="225.00"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="225.00"/>
      <ROW AUTOHEIGHT="0" HEIGHT="15.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">USACE / NAVFAC / AFCEC</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">UFGS-01 14 00 (November 2022)</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="21.00">
         <CEL MERGEDOWN="1" STYLEID="s50"/>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Change 5 - 05/25</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="18.00">
         <CEL INDEX="2" STYLEID="s50">
<DTA TYPE="STRING"><HL3>------------------------------------</HL3></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="64.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Preparing Activity:  <PRA>NAVFAC</PRA></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Superseding<BRK/>UFGS-01 14 00 (November 2011)</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<HL4>UNIFIED FACILITIES GUIDE SPECIFICATIONS</HL4><BRK/>
<BRK/>
<HL4>References are in agreement with UMRL dated July 2025</HL4><BRK/>
<AST/><BRK/></HDR>
<BRK/>
<SCN>SECTION 01 14 00</SCN><BRK/>
<BRK/>
<STL>WORK RESTRICTIONS</STL><BRK/>
<DTE>11/22, CHG 5: 05/25</DTE><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This guide specification covers the requirements for <SCP>work and site restrictions</SCP>
.</NPR><BRK/>
<BRK/>
<NPR>Adhere to <URL HREF="https://www.wbdg.org/dod/ufc/ufc-1-300-02">UFS 1-300-02</URL> Unified Facilities Guide Specifications (UFGS) Format 
Standard when editing this guide specification or preparing new project specification 
sections.  Edit this guide specification for project specific requirements by 
adding, deleting, or revising text.  For bracketed items, choose applicable 
item(s) or insert appropriate information.</NPR><BRK/>
<BRK/>
<NPR>Remove information and requirements not required in respective project, whether 
or not brackets are present.</NPR><BRK/>
<BRK/>
<NPR>Comments, suggestions and recommended changes for this guide specification are 
welcome and should be submitted as a <URL HREF="https://www.wbdg.org/dod/ufgs">Criteria Change Request (CCR)</URL>.</NPR><BRK/>
<BRK/>
<NPR>This guide specification includes a variety of tailoring options for ease of 
initially editing the section.  Selection or deselection of a tailoring option 
will include or exclude that option in the section but editing the resulting 
section to fit the project is still required.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<PRT><TTL>PART 1   GENERAL</TTL><BRK/>
<BRK/>
<SPT><TTL>REFERENCES</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is used to list the publications cited in the text of 
the guide specification.  The publications are referred to in the text by basic 
designation only and listed in this paragraph by organization, designation, 
date, and title.</NPR><BRK/>
<BRK/>
<NPR>Use the Reference Wizard's Check Reference feature when you add a Reference 
Identifier (RID) outside of the Section's Reference Article to automatically 
place the reference in the Reference Article.  Also use the Reference Wizard's 
Check Reference feature to update the issue dates.</NPR><BRK/>
<BRK/>
<NPR>References not used in the text will automatically be deleted from this section 
of the project specification when you choose to reconcile references in the 
publish print process.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The publications listed below form a part of this specification to the extent referenced.  The publications are 
referred to within the text by the basic designation only.</TXT><BRK/>
<BRK/>
<REF><ORG>AIR-CONDITIONING, HEATING AND REFRIGERATION INSTITUTE (AHRI)</ORG><BRK/>
<BRK/>
<RID>ANSI/AHRI 210/240</RID><RTL>(2008; Add 1 2011; Add 2 2012) Performance Rating 
of Unitary Air-Conditioning &amp; Air-Source 
Heat Pump Equipment</RTL><BRK/>
<BRK/></REF>
<REF><ORG>AMERICAN SOCIETY OF CIVIL ENGINEERS (ASCE)</ORG><BRK/>
<BRK/>
<RID>ASCE 7-16</RID><RTL>(2017; Errata 2018; Supp 1 2018) Minimum Design 
Loads and Associated Criteria for Buildings 
and Other Structures</RTL><BRK/>
<BRK/></REF>
<REF><ORG>FLORIDA ADMINISTRATIVE CODE (FAC)</ORG><BRK/>
<BRK/>
<RID>FAC Chapter 15C-1</RID><RTL>Department of Highway Safety and Motor Vehicles</RTL><BRK/>
<BRK/></REF>
<REF><ORG>INSTRUCTIONS AND STANDARDS FOR NAVBASE GUANTANAMO BAY CUBA (COMNAVBASEGTMOINST)</ORG><BRK/>
<BRK/>
<RID>11300.3</RID><RTL>Base Energy Conservation Regulations</RTL><BRK/>
<BRK/></REF>
<REF><ORG>INTERNATIONAL CODE COUNCIL (ICC)</ORG><BRK/>
<BRK/>
<RID>ICC IBC</RID><RTL>(2024) International Building Code</RTL><BRK/>
<BRK/></REF>
<REF><ORG>NATIONAL FIRE PROTECTION ASSOCIATION (NFPA)</ORG><BRK/>
<BRK/>
<RID>NFPA 70</RID><RTL>(2023; ERTA 1 2024; TIA 24-1; TIA 25-2) National 
Electrical Code</RTL><BRK/>
<BRK/>
<RID>NFPA 90A</RID><RTL>(2024) Standard for the Installation of Air 
Conditioning and Ventilating Systems</RTL><BRK/>
<BRK/>
<RID>NFPA 101</RID><RTL>(2024) Life Safety Code</RTL><BRK/>
<BRK/></REF>
<REF><ORG>NAVAL FACILITIES ENGINEERING AND EXPEDITIONARY WARFARE CENTER (NAVFAC EXWC)</ORG><BRK/>
<BRK/>
<RID>NFESC UG-2029-ENV</RID><RTL>(1998) Cross-Connection Control and Backflow 
Prevention Program Implementation at Shore Facilities, 
User's Guide</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. ARMY CORPS OF ENGINEERS (USACE)</ORG><BRK/>
<BRK/>
<RID>EM 385-1-1</RID><RTL>(2024) Safety -- Safety and Occupational Health 
(SOH) Requirements</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. Code (USC)</ORG><BRK/>
<BRK/>
<RID>8 USC 1101</RID><RTL>Definitions</RTL><BRK/>
<BRK/>
<RID>10 USC 6011</RID><RTL>Navy Regulations</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. DEPARTMENT OF DEFENSE (DOD)</ORG><BRK/>
<BRK/>
<RID>UFC 3-301-01</RID><RTL>(2023; with Change 3, 2025) Structural Engineering</RTL><BRK/>
<BRK/></REF>
<REF><ORG>U.S. DEPARTMENT OF HOUSING AND URBAN DEVELOPMENT (HUD)</ORG><BRK/>
<BRK/>
<RID>24 CFR 3280</RID><RTL>(2019) Manufactured Home Construction and Safety 
Standards</RTL><BRK/>
<BRK/></REF>
</SPT><TAI OPT="NAVFAC MARIANAS">[<SPT><TTL>DEFINITIONS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC MARIANAS.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>State</TTL><BRK/>
<BRK/>
<TXT>"State" when used in reference to states of the United States also includes the Territory of Guam.</TXT><BRK/>
<BRK/></SPT>
</SPT>]</TAI>[<SPT><TTL>SUBMITTALS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Review Submittal Description (SD) definitions in Section <SRF>01 33 00</SRF> SUBMITTAL 
PROCEDURES and edit the following list, and corresponding submittal items in 
the text, to reflect only the submittals required for the project.  The Guide 
Specification technical editors have classified those items that require Government 
approval, due to their complexity or criticality, with a "G."  Generally, other 
submittal items can be reviewed by the Contractor's Quality Control System.  
Only add a "G" to an item if the submittal is sufficiently important or complex 
in context of the project.</NPR><BRK/>
<BRK/>
<NPR><TAI OPT="ARMY">For Army projects, fill in the empty brackets following the "G" classification, 
with a code of up to three characters to indicate the approving authority.  
Codes for Army projects using the Resident Management System (RMS) are:  "AE" 
for Architect-Engineer; "DO" for District Office (Engineering Division or other 
organization in the District Office); "AO" for Area Office; "RO" for Resident 
Office; and "PO" for Project Office.  </TAI>Codes following the "G" typically are 
not used for Navy and Air Force projects.</NPR><BRK/>
<BRK/>
<NPR>The "S" classification indicates submittals required as proof of compliance 
for sustainability Guiding Principles Validation or Third Party Certification 
and as described in Section <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The items in this Submittals Article contain tailoring for NAVFAC FE, 
NAVFAC MARIANAS, NAVFAC, SW, and NAVFAC SE.  If the project is not at any of 
these locations, and no additional submittals are added, delete this Submittals 
Article altogether.</NPR><BRK/>
<AST/><BRK/></NTE>
<TAI OPT="NAVY DESIGN-BUILD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Navy Design-Build projects, delete <SRF>01 33 00</SRF> SUBMITTAL PROCEDURES, 
and replace with UFGS 01 33 00.05 20 CONSTRUCTION SUBMITTAL PROCEDURES and UFGS 
01 33 10.05 20 DESIGN SUBMITTAL PROCEDURES.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Government approval is required for submittals with a "G" or "S" classification.<TAI OPT="AIR FORCE,NAVY">  Submittals not having a "G" 
or "S" classification are for Contractor Quality Control approval.</TAI><TAI OPT="ARMY">  Submittals not having a "G" or "S" classification 
are for information only.  When used, a code following the "G" classification identifies the office that will 
review the submittal for the Government.</TAI>  Submit the following in accordance with Section <SRF>01 33 00</SRF> SUBMITTAL 
PROCEDURES:</TXT><BRK/>
<BRK/>
<LST><SUB>SD-01 Preconstruction Submittals</SUB></LST><BRK/>
<BRK/>
<TAI OPT="NAVFAC FE"><ITM><SUB>Meal Signature Record Book (MSRB)</SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC FE"><ITM><SUB>Dining And Lodging Requirements</SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC FE"><ITM><SUB>Housing Plan</SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC PAC"><ITM><SUB>Medical Plan</SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC FE"><ITM><SUB>Contractor Regulations</SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC FE"><ITM><SUB>Transportation of Personnel, Materials, and Equipment</SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC FE"><ITM><SUB>Purchase Orders</SUB></ITM><BRK/>
<BRK/></TAI>
<ITM><SUB>List of Contact Personnel</SUB></ITM><BRK/>
<BRK/>
<TAI OPT="NAVFAC PAC,NAVFAC SW"><ITM><SUB>Personnel List</SUB></ITM><BRK/>
<BRK/></TAI>
<TAI OPT="NAVFAC SE"><ITM><SUB>Entry Approval for Employees</SUB>; G<TAI OPT="ARMY">, [_____]</TAI></ITM><BRK/>
<BRK/></TAI>
<LST><SUB>SD-07 Certificates</SUB></LST><BRK/>
<TAI OPT="ARMY"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For Army and Army National Guard projects, require 3Rs Explosive Safety 
Education Training Certificate to be submitted annually.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<ITM><SUB>3Rs Explosive Safety Education Training Certificate</SUB> (annual submission required)</ITM><BRK/></TAI>
<BRK/>
<TAI OPT="NAVFAC EURAFCENT">[<ITM><SUB>Proof of IMD Ordnance Work Authorization</SUB>; G<TAI OPT="ARMY">, [_____]</TAI></ITM><BRK/>
<BRK/>
]</TAI></SPT>][<SPT><TTL>SPECIAL SCHEDULING REQUIREMENTS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  If there are special requirements, use those portions of the following 
paragraph which apply to the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
<OLI>[_____] must be ready for operation as approved by Contracting Officer before work is started on [_____] 
which would interfere with normal operation.</OLI><BRK/>
<BRK/>
<OLI>Have materials, equipment, and personnel required to perform the work at the site prior to the commencement 
of the work.  Specific items of work to which this requirement applies include:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">[_____]</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">[_____]</OLI><BRK/>
<BRK/>
<OLI>The [_____] will remain in operation during the entire construction period.  Conduct operations so as 
to cause the least possible interference with normal operations of the activity.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use 30 calendar days in bracket below for NBK Bangor, WA.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Permission to interrupt any Activity roads, railroads, or utility service must be requested in writing 
a minimum of [15] [_____] calendar days prior to the desired date of interruption.</OLI><BRK/>
<BRK/>
[<OLI>The work under this contract requires special attention to the scheduling and conduct of the work in 
connection with existing operations.  Identify on the construction schedule each factor which constitutes 
a potential interruption to operations.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The following conditions apply:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">[_____]</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">[_____]</OLI><BRK/>
<BRK/>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Use this paragraph on all projects involving potential conflicts with 
operating conditions other than utilities or where the work must be pursued 
in a particular sequence.   Clearly detail the permissible extent of sequencing 
or duration of interruptions to station operation.  Obtain information from 
the Government.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<OLI>Restricted Access Areas.  The Government will monitor work in areas[ listed below][ indicated].  Notify 
Contracting Officer at least 14 calendar days prior to starting work in these areas.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">[_____]</OLI><BRK/></OLG>
<BRK/>
]</SPT>]<SPT><TTL>CONTRACTOR ACCESS AND USE OF PREMISES</TTL><BRK/>
<BRK/>
<SPT><TTL>Activity Regulations</TTL><BRK/>
<TAI OPT="NAVFAC HI"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Include the first bracketed sentence for projects at MCBH Kaneohe Bay.  
The two bracketed sentences are tailored for use at NAVFAC Hawaii.</NPR><BRK/>
<AST/><BRK/></NTE>
</TAI><BRK/>
<TXT>Ensure that Contractor personnel employed on the Activity become familiar with and obey Activity regulations 
including safety, fire, traffic and security regulations.  Keep within the limits of the work and avenues of 
ingress and egress.<TAI OPT="NAVFAC HI">[  Ingress and egress of Contractor vehicles at the Activity is limited to the H-3 gate.][  
To minimize traffic congestion, delivery of materials must be outside of peak traffic hours (6:30 to 8:00 a.m. 
and 3:30 to 5:00 p.m.) unless otherwise approved by the Contracting Officer.]</TAI>  Wear appropriate personal protective 
equipment (PPE) in designated areas.  Do not enter any restricted areas unless required to do so and until cleared 
for such entry.  Ensure all Contractor equipment, including delivery vehicles, are clearly identified with their 
company name.</TXT><BRK/>
<BRK/>
<SPT><TTL>Subcontractors and Personnel Contacts</TTL><BRK/>
<BRK/>
<TXT>Provide a <SUB>list of contact personnel</SUB> of the Contractor and subcontractors including addresses and telephone numbers 
for use in the event of an emergency.  As changes occur and additional information becomes available, correct 
and change the information contained in previous lists.</TXT><BRK/>
<BRK/></SPT>
<TAI OPT="NAVY">[<SPT><TTL>Additional Personnel Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include the following for projects that have a Sensitive Compartmented 
Information Facilities (SCIF) or Special Access Program Facilities (SAPF).  
For SCIF and SAPF, coordinate personnel requirements with the Site Security 
Manager and the Construction Security Plan.  These requirements apply to the 
SCIF or SAPF and not the entire facility unless the entire facility is the SCIF 
or SAPF.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for Navy use only.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for projects within the U.S. and its territories.  
Include Sitework, utilities, foundations, structure when the entire facility 
is a SCIF or SAPF.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<SPT><TTL>General Construction and Finish Work</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  U.S. citizens or U.S. persons should be the default for projects within 
the U.S. and its territories.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>General construction and finish work of the [secure area][controlled area][_____] must be performed by U.S. firms 
using U.S. citizens[ or U.S. persons].  General construction includes construction activities such as [building 
sitework, utilities, foundations, structure, and ]enclosure or shell, including doors, windows and façade work.  
Finish Work includes construction activities such as insulation, floor, partition, and ceiling systems; cabinet 
work; conveyor systems; specialties; building furnishings, fixtures, and equipment; and mechanical and electrical 
services and equipment including those specialized for fire protection, security, communication, control, energy 
conservation, safety, comfort, convenience, and similar purposes.</TXT><BRK/>
<BRK/></SPT>
]<NTE><AST/><BRK/>
<NPR>NOTE:  Include the following paragraphs for projects outside the U.S. and its 
territories.  Include Sitework, utilities, foundations, structure when the entire 
facility is a SCIF or SAPF.  Refer to the Construction Security Plan to determine 
whether U.S. SECRET or TOP SECRET-cleared workers are required for finish work.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<SPT><TTL>General Construction</TTL><BRK/>
<BRK/>
<TXT>General construction of the [secure area][controlled area][_____] must be performed by U.S. firms using U.S. 
citizens.  General construction includes construction activities such as [building sitework, utilities, foundations, 
structure, and ]enclosure or shell, including doors, windows and façade work.  Utility work that penetrates the 
[secure area][controlled area][_____] and installation of doors in these areas are not general construction.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Finish Work</TTL><BRK/>
<BRK/>
<TXT>Finish Work within the [secure area][controlled area][_____] must be accomplished by [U.S. SECRET-cleared][U.S. 
TOP SECRET-cleared] personnel.  Finish Work includes construction activities such as insulation, floor, partition, 
and ceiling systems; cabinet work; conveyor systems; specialties; building furnishings, fixtures, equipment; 
and  mechanical and electrical services and equipment including those specialized for fire protection, security, 
communication, control, energy conservation, safety, comfort, convenience, and similar purposes.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Electronic Security Systems Equipment</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For projects that include Electronic Security Systems for the protection 
of areas such as Secure Rooms (Secret or Top Secret Open Storage), Sensitive 
Compartmented Information Facilities (SCIF) or Special Access Program Facilities 
(SAPF) include the following personnel requirements.</NPR><BRK/>
<BRK/>
<NPR>1.  For Secure Rooms (Secret or Top Secret Open Storage) select the first bracketed 
option.</NPR><BRK/>
<BRK/>
<NPR>2.  For SCIF and SAPF within the U.S., its possessions or territories, select 
the second bracketed option.</NPR><BRK/>
<BRK/>
<NPR>3.  For SCIF and SAPF outside the U.S., its possessions or territories, choose 
the third or fourth bracketed option.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Electronic Security Systems equipment such as processing control units, workstations, field panels, sensors, 
high security locks, card readers, cable installation, and system programming, testing and training must be performed 
by [U.S. citizens who have been subjected to a trustworthiness determination] [U.S. companies using U.S. citizens 
who have been subjected to a trustworthiness determination] [[U.S. companies using U.S. TOP SECRET-cleared personnel] 
[U.S. companies using U.S. SECRET-cleared personnel]].</TXT><BRK/>
<BRK/></SPT>
]</SPT>]</TAI><TAI OPT="NAVY"><SPT><TTL>Installation Access</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph for Navy and Marine Corps installations, with the 
exception of overseas locations that do not employ the Defense Biometric Identification 
System (DBIDS).  Confirm with installation security office and tailor DBIDS 
project requirements to local policy.  This paragraph is tailored for Navy.</NPR>  <BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Obtain access to Navy installations through participation in the Defense Biometrics Identification System (DBIDS).  
Requirements for Contractor employee registration, and transition for employees currently under Navy Commercial 
Access Control System (NCACS), are available at <URL HREF="https://www.cnic.navy.mil/Operations-and-Management/Base-Support/DBIDS">https://www.cnic.navy.mil/Operations-and-Management/Base-Support/DBIDS/</URL>
.  No fees are associated with obtaining a DBIDS credential.</TXT><BRK/>
<BRK/>
<TXT>Participation in the DBIDS is not mandatory, and Contractor personnel may apply for One-Day Passes at the Base 
Visitor Control Office to access an installation.</TXT><BRK/>
<BRK/>
<SPT><TTL>Registration for DBIDS</TTL><BRK/>
<BRK/>
<TXT>Registration for DBIDS is available at <URL HREF="https://www.cnic.navy.mil/Operations-and-Management/Base-Support/DBIDS">https://www.cnic.navy.mil/Operations-and-Management/Base-Support/DBIDS/</URL>
.  Procedure includes:</TXT><BRK/>
<OLG><BRK/>
<OLI>Present a letter or official award document (i.e. DD Form 1155 or SF 1442) from the Contracting Officer, 
that provides the purpose for access, to the base Visitor Control Center representative.</OLI><BRK/>
<BRK/>
<OLI>Present valid identification, such as a passport or Real ID Act-compliant state driver's license.</OLI><BRK/>
<BRK/>
<OLI>Provide completed SECNAV FORM 5512/1 to the base Visitor Control Center representative to obtain a background 
check.  This form is available for download at <URL HREF="https://www.cnic.navy.mil/Operations-and-Management/Base-Support/DBIDS">https://www.cnic.navy.mil/Operations-and-Management/Base-Support/DBIDS/</URL>
.</OLI><BRK/>
<BRK/>
<OLI>Upon successful completion of the background check, the Government will complete the DBIDS enrollment 
process, which includes Contractor employee photo, fingerprints, base restriction and several other assessments.</OLI><BRK/>
<BRK/>
<OLI>Upon successful completion of the enrollment process, the Contractor employee will be issued a DBIDS 
credential, and will be allowed to proceed to worksite.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>DBIDS Eligibility Requirements</TTL><BRK/>
<BRK/>
<TXT>Throughout the length of the contract, the Contractor employee must continue to meet background screen standards. 
Periodic background screenings are conducted to verify continued DBIDS participation and installation access 
privileges.  DBIDS access privileges will be immediately suspended or revoked if at any time a Contractor employee 
becomes ineligible.</TXT><BRK/>
<BRK/>
<TXT>An adjudication process may be initiated when a background screen failure results in disqualification from participation 
in the DBIDS, and Contractor employee does not agree with the reason for disqualification.  The Government is 
the final authority.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>DBIDS Notification Requirements</TTL><BRK/>
<OLG><BRK/>
<OLI>Immediately report instances of lost or stolen badges to the Contracting Officer.</OLI><BRK/>
<BRK/>
<OLI>Immediately collect DBIDS credentials and notify the Contracting Officer in writing under the following 
circumstances:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">An employee has departed the company without having properly returned or surrendered their 
DBIDS credentials.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">There is a reasonable basis to conclude that an employee, or former employee, might pose a 
risk, compromise, or threat to the safety  or security of the Installation or anyone therein.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>One-Day Passes</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This subpart is not applicable at NS Guantanamo Bay and should be deleted.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Personnel applying for One-Day passes at the Base Visitor Control Office are subject to daily mandatory vehicle 
inspection, and will have limited access to the installation.  The Government is not responsible for any cost 
or lost time associated with obtaining daily passes or added vehicle inspections incurred by non-participants 
in the DBIDS.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><TAI OPT="NAVFAC WASH">[<SPT><TTL>Additional Badge Requirements - NAS Patuxent River</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Use the following paragraph for projects at the Naval Air Station, Patuxent 
River, MD.  This paragraph is tailored for NAVFAC WASH.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Identification badges will be issued to the Contractor and his employees in accordance with the Naval Air Station 
Security Regulations.  A copy of the security regulations may be obtained from the security office.  All badges 
must be returned or accounted for to the department of Public Safety's Pass and Identification Office upon expiration 
of the badge or contract, or termination of the employee.</TXT><BRK/>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC WASH">[<SPT><TTL>Employee List</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for projects at Naval Air Station, Patuxent River 
, Maryland.  This paragraph is tailored for NAVFAC WASH.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  </NPR><BRK/>
<AST/><BRK/></NTE>
<TXT>Provide to the Contracting officer, in writing, the names of two designated representatives authorized to request 
personnel and vehicle passes for employees and subcontractor's employees prior to commencement of work under 
this contract.  Adhere to the requirements of "Important Clarifications - Contractors - How to Gain Access," 
dated 31 October 1995, in obtaining access to the Naval Air Station complex for the life of the contract.  A 
copy of these requirements will be provided at the preconstruction meeting.</TXT><BRK/>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC WASH">[<SPT><TTL>Personnel Entry Approval</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include this paragraph for projects at Naval Air Station, Patuxent River, 
MD.  This paragraph is tailored for NAVFAC WASH.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Failure to obtain entry approval will not affect the contract price or time of completion.</TXT><BRK/>
<BRK/></SPT>
]</TAI><SPT><TTL>No Smoking Policy</TTL><BRK/>
<BRK/>
<TXT>Smoking is prohibited within and outside of all buildings on installation,  except in designated smoking areas.  
This applies to existing buildings, buildings under construction and buildings under renovation.  Discarding 
tobacco materials other than into designated tobacco receptacles is considered littering and is subject to fines.  
The Contracting Officer will identify designated smoking areas.</TXT><BRK/>
<BRK/></SPT>
</SPT><TAI OPT="NORFOLK NAVAL SHIPYARD">[<SPT><TTL>Emergency Response Requirement</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Add the following paragraphs for projects at Norfolk Naval Shipyard (NNSY)</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The Norfolk Naval Shipyard has instituted a requirement for all personnel to take shelter for personal safety 
in the event of certain emergencies.  This policy includes Contractors, Subcontractors, and any person who is 
employed by the Contractor.</TXT><BRK/>
<BRK/>
<TXT>The most appropriate protective action for certain emergencies is to take shelter.  Personnel must immediately 
seek shelter while an assessment is made of the threat and determinations are being made regarding subsequent 
actions such as "all clear" or selected building evacuations.  The following procedures have been put in place 
in the event of an emergent condition.</TXT><BRK/>
<OLG><BRK/>
<OLI LEVEL="2">NOTIFICATION:  The primary means of alerting personnel will be emergency alert signals.  The 
alerting signal to seek shelter will be three steady tones that last for thirty seconds separated 
by ten seconds of silence.  The notification for "all clear" will be three short tones repeated 
three times.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">SHELTERING:  When personnel hear the alert signal, the area of work must be secured in a manner 
that will leave the site in safe condition.  Personnel must seek shelter in the nearest occupied 
building in calm and orderly manner.  If possible, secure all windows and doors and shut off 
ventilation.  If working aboard ship, proceed into the interior of the ship and wait for further 
directions from official personnel.  If in a vehicle, park the vehicle so that it does not 
block the normally traveled portion of the road and proceed into the nearest occupied building.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">EVACUATION:  In the event of an evacuation, personnel will receive directions from team members 
of the Crowd Control Center (CCC) or the building custodian acting on the directions from the 
CCC.  Contract personnel must comply with instructions given at all times.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI><TAI OPT="NORFOLK NAVAL SHIPYARD">[<SPT><TTL>Shipyard Regulations</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Add the following paragraphs for projects at Norfolk Naval Shipyard (NNSY). </NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Ensure that Contractor personnel employed on the Shipyard become familiar with and obey Shipyard regulations.  
Wear appropriate personal protective equipment (PPE) in designated areas.  Do not enter any restricted areas 
unless required to do so and until cleared for such entry.  The Contractor's equipment must be conspicuously 
marked for identification.  Comply with the following conditions:</TXT><BRK/>
<OLG><BRK/>
<OLI>Restrict employees/representatives to the work site and control travel directly to and from the work 
site</OLI>.<BRK/>
<BRK/>
<OLI>Restore all traffic/parking/security signs and markings, including space numbers, designations, and lines, 
to their original form if such signs/markings are defaced or deleted during construction/repair.</OLI><BRK/>
<BRK/>
<OLI>Be responsible for control and security of Contractor-owned equipment and materials at the work site.  
Report immediately missing/lost/stolen property to the Shipyard Police Department (phone 396-7266) as 
each case occurs.</OLI><BRK/>
<BRK/>
<OLI>Ensure that no material is stacked within<MET> 3 meters</MET><ENG> 10 feet</ENG> of the Controlled Industrial Area (CIA) perimeter.  
Remove from the work site, or secure ladders or other such equipment which could be used to climb the 
CIA perimeter fence.  Ensure that no vehicles are parked within<MET> 3 meters</MET><ENG> 10 feet</ENG> of the CIA perimeter.</OLI><BRK/>
<BRK/>
<OLI>Ensure that no openings in the roof/walls/windows/fence of the building exist at the end of the workday 
and do not exist where penetration is possible during non-working hours.  If the building cannot be secured 
at the end of the workday, coordinate action with the Contracting Office to notify the cognizant code 
to arrange for a security watch by their personnel.</OLI><BRK/>
<BRK/>
<OLI>Seventy-two hours prior to making any penetrations (such as tunneling under, cutting through a fence 
or building) in a restricted area, contact the Shipyard Security Office to make arrangements for a security 
guard or other measures required to meet all security requirements.  Cost of security guard will be charged 
to the Contractor.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI><TAI OPT="NORFOLK NAVAL SHIPYARD"><SPT><TTL>Entry to Radiologically Controlled Areas</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Add the following paragraphs for projects at Norfolk Naval Shipyard (NNSY).</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Contractor personnel must not, under any circumstances, enter a radiologically controlled area or cross any posted 
radiological boundary.  This paragraph applies to all phases of contract work.  Radiation areas are posted with 
signs consistent with OSHA requirements.  Ensure that employees are familiar with the radiation signs and symbols.  
All personnel entering the shipyard for the first time are required to receive radiological indoctrination training.</TXT><BRK/>
<BRK/>
<TXT>Should contract workers encounter radiological postings or boundaries which appear to limit their ability to 
access or carry out their intended work, they must notify their contract administrator for resolution of the 
problem.</TXT><BRK/>
<BRK/>
<SPT><TTL>Radioactive Materials and Equipment</TTL><BRK/>
<BRK/>
<TXT>All testing equipment, containing a radioactive source, must be operated in accordance with an approved radioactive 
equipment plan.  This plan must be submitted to the Contracting Officer and approved by the Radiation Officer 
(Code 105.5), prior to bringing the equipment into the shipyard.  This plan must include:</TXT><BRK/>
<OLG><BRK/>
<OLI>The name and type of equipment.</OLI><BRK/>
<BRK/>
<OLI>The type and size of radiation source.</OLI><BRK/>
<BRK/>
<OLI>The dates and locations of the equipment's usage.</OLI><BRK/>
<BRK/>
<OLI>The radiological controls that the Contractor will use while operating the equipment.</OLI><BRK/></OLG>
<BRK/>
<TXT>A different radioactive equipment plan will be required for each different type of equipment, type of radioactive 
source, or size of radioactive source.  A data sheet of for each piece of new radioactive equipment must be submitted 
to the Contracting Officer to forward to the shipyard's Radiation Safety Officer.  The data sheet must contain 
the following information:</TXT><BRK/>
<OLG><BRK/>
<OLI>Name of equipment.</OLI><BRK/>
<BRK/>
<OLI>Name and address of equipment manufacturer.</OLI><BRK/>
<BRK/>
<OLI>Type and size of radiation source.</OLI><BRK/>
<BRK/>
<OLI>The location of the installed radioactive equipment (i.e. building no., floor, code/shop area).</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></TAI><SPT><TTL>Working Hours</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  When there is a need for special work periods, such as occupied family 
housing or when working in locations with non-traditional workdays such as Bahrain 
or Djibouti, modify this paragraph accordingly.  Consult with the supported 
command or FEAD/ROICC office.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Regular working hours will consist of an [8 1/2 hour] [[_____] hour] period [established by the Contracting Officer], 
between [7 a.m. and 3:30 p.m.,] [[_____] a.m. and [_____] p.m.,] [Monday through Friday] [[_____] through [_____]], 
[and 7 a.m. to 3:30 p.m. on Saturday] [[_____] a.m. and [_____] p.m. on Saturday], excluding Government holidays.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Work Outside Regular Hours</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Discuss with the Contracting Officer when work outside regular hours 
is anticipated since it generally requires overtime pay for Government employees.  
When there is a need for special work periods, such in occupied family housing, 
modify this paragraph accordingly.</NPR><BRK/>
<BRK/>
<NPR>For MCBH Kaneohe Bay, use 30 calendar days in bracketed option.</NPR><BRK/>
<BRK/>
<NPR>For NAVFAC PAC and NAVFAC Hawaii, include the last bracketed item.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Work outside regular working hours requires Contracting Officer approval.  Make application [15] [_____] calendar 
days prior to such work to allow arrangements to be made by the Government for inspecting the work in progress, 
giving the specific dates, hours, location, type of work to be performed, contract number and project title.  
Based on the justification provided, the Contracting Officer may approve work outside regular hours.  During 
periods of darkness, the different parts of the work must be lighted in accordance with requirements of <RID>EM 385-1-1</RID>
.[  Make utility cutovers after normal working hours or on Saturdays, Sundays, and Government holidays unless 
directed otherwise.]</TXT><BRK/>
<BRK/></SPT>
[<SPT><TTL>Exclusionary Period</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Only use this paragraph and edit accordingly, only if project must shut 
down during certain, known dates or times.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>No work may be performed during the period [_____] to [_____], inclusive, without prior written approval of the 
Contracting Officer.  This period has not been considered in computing the time allowed for the performance of 
this contract.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Occupied<TAI OPT="NAVFAC WASH"> and Existing</TAI> Building[s]</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Edit for all projects as appropriate.  Delete this paragraph and its 
subparagraphs unless the work is in or around existing occupied buildings or 
unless Activity operations will materially affect the Contractor's operations.  
In most projects, the Government will remove furniture and equipment before 
the Contractor begins work.  In this case the last subparagraph should be used.  
Examples of Activity operations materially affecting Contractor's operations 
include:</NPR><BRK/>
<BRK/>
<NPR>1.  Restrictions regarding the time of day (or other period) or the duration 
of work in an area</NPR><BRK/>
<BRK/>
<NPR>2.  Interruptions of work in an area for operations, one time or periodic</NPR><BRK/>
<BRK/>
<NPR>3.  Interruption of work for a specific time for operations</NPR><BRK/>
<BRK/>
<NPR>4.  Location or restrictions on location of construction equipment</NPR><BRK/>
<BRK/>
<NPR>5.  Maintaining access.</NPR><BRK/>
<BRK/>
<NPR>Contact the Government to determine the complete details of scheduling restraints 
which may impact on the successful bidder's time or cost of performance of the 
work, and incorporate such details in this paragraph.  Note that this paragraph 
defines the impact of Activity operations upon the Contractor.  If the Contractor 
affects Activity operations, include that information in paragraph SPECIAL SCHEDULING 
REQUIREMENTS and not in this paragraph.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Work will be [in an existing building] [around existing buildings] which [is][are] occupied.[  Do not enter the 
building[s] without prior approval of the Contracting Officer.]</TXT><BRK/>
<BRK/>
[<TXT>The existing buildings and their contents must be kept secure at all times.  Provide temporary closures as required 
to maintain security as directed by the Contracting Officer.</TXT><BRK/>
<BRK/>
][<TXT>Provide dust covers or protective enclosures to protect existing work that remains, and Government material located 
in the [_____] during the construction period.</TXT><BRK/>
<BRK/>
]<TXT>[Relocate movable furniture [approximately<MET> [1.8 m]</MET><ENG> [6 feet]</ENG> [_____] away from the Contractor's working area] 
[as required to perform the work], protect the furniture, and replace the furniture in [its] [their] original 
location[s] upon completion of the work.][  Leave attached equipment in place, and protect [it] [them] against 
damage, or temporarily disconnect, relocate, protect, and reinstall [it] [them] at the completion of the work.]</TXT><BRK/>
<BRK/>
[<TXT>The Government will remove [and relocate] other Government property in the areas of the building[s] scheduled 
to receive work.</TXT><BRK/>
<BRK/>
]</SPT>]<SPT><TTL>Utility Cutovers and Interruptions</TTL><BRK/>
<OLG><BRK/>
<OLI>Make utility cutovers and interruptions after normal working hours or on Saturdays, Sundays, and Government 
holidays.  Conform to procedures required in paragraph WORK OUTSIDE REGULAR HOURS.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the next two paragraphs on all projects involving potential conflicts 
with existing utility systems.  Clearly detail the permissible extent, the sequencing, 
or the duration of outages.  Contact the Government to determine the complete 
details of outage or scheduling restraints which may impact on the successful 
bidder's time or cost of performance of the work, and incorporate such details 
in this paragraph.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Ensure that new utility lines are complete, except for the connection, before interrupting existing service.</OLI><BRK/>
<BRK/>
<OLI>Interruption to water, sanitary sewer, storm sewer, telephone service, electric service, air conditioning, 
heating, fire alarm, compressed air, and [_____] are considered utility cutovers pursuant to the paragraph 
WORK OUTSIDE REGULAR HOURS.[  Such interruptions are further limited to [_____] hours.  This time limit 
includes time for deactivation and reactivation.]</OLI><BRK/>
<BRK/>
[<OLI>Operation of Station Utilities:  Do not operate nor disturb the setting of control devices in the station 
utilities system, including water, sewer, electrical, and steam services.  The Government will operate 
the control devices as required for normal conduct of the work.  Notify the Contracting Officer giving 
reasonable advance notice when such operation is required.</OLI><BRK/>
<BRK/>
]<TAI OPT="NAVY"><NTE><AST/><BRK/>
<NPR>NOTE:  The following paragraph is tailored for Navy use only.  Coordinate with 
Installation to determine if permit is required and if so, time period required 
prior to connection.  Edit Section <SRF>33 30 00</SRF> SANITARY SEWERAGE to specify permits 
and requirements for connections to existing sanitary sewer lines.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Connection to Existing Sanitary Sewer Line:  Provide positive verification that the existing line conveys 
sanitary sewer; verify line is not incorrectly connected to a storm drain.[  Obtain Installation's Sanitary 
Sewer Connection Permit[ 2 weeks][ _____] prior to connection and in accordance with Section 
<SRF>33 30 00</SRF> SANITARY SEWERAGE.]</OLI><BRK/>
<BRK/></TAI>
</OLG></SPT><TAI OPT="NAVY">[<SPT><TTL>Shipyard Area Work Clearance Request</TTL><BRK/>
<TAI OPT="NAVFAC HI"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Include for Pearl Harbor Shipyard projects. This paragraph is tailored 
for NAVFAC HI.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT><TST>Coordinate excavation and electrical work, including testing and troubleshooting of circuits, within the NAVFAC 
Hawaii Utilities Management (UM) and PHNSY&amp;IMF via the Contracting Officer.</TST>  Furnish the:</TXT><BRK/>
<OLG><BRK/>
<OLI>Contract title and number</OLI><BRK/>
<BRK/>
<OLI>Specific location of work</OLI><BRK/>
<BRK/>
<OLI>Reason for work</OLI><BRK/>
<BRK/>
<OLI>Duration of work</OLI><BRK/></OLG>
</TAI><BRK/>
[<SPT><TTL>Shipyard Hazardous Areas</TTL><BRK/>
<BRK/>
<TXT>Do not enter into work areas where Shipyard personnel are using protective equipment such as respirator and masks 
or marked boundary areas without prior approval.</TXT><BRK/>
<BRK/></SPT>
]</SPT>]</TAI><TAI OPT="NAVFAC PAC,NORFOLK NAVAL SHIPYARD">[<SPT><TTL>Restrictions on Use of Yellow[, Orange-Yellow, Red, and Magenta] Materials</TTL><BRK/>
<TAI OPT="NORFOLK NAVAL SHIPYARD"><NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Add the following for projects at Norfolk Naval Shipyard (NNSY).  This 
paragraph is tailored for NNSY.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Refrain from use of yellow or orange-yellow materials for the following purposes:  sheeting, tarpaulins, polyethylene 
bottles or other containers, tapes, bags, banding of identification marks on tools, boundary markers such as 
ribbons.  Contractor generated yellow waste materials such as torn foul weather gear must be disposed of by the 
Contractor off-yard.  Shipyard dumpsters and trash cans must not be used for disposal of Contractor generated 
yellow waste materials.  Yellow colored items such as described above are of specific significance within the 
shipyard and are subject to strict controls.</TXT><BRK/>
<BRK/>
]</TAI><TAI OPT="NAVFAC PAC"><NTE><AST/><BRK/>
<NPR>NOTE:  Add the following for shipyard projects at NAVFAC PAC.  This paragraph 
is tailored for NAVFAC PAC.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>The use of yellow, yellow-orange, red and magenta materials for the following purposes is prohibited: sheeting, 
tarpaulins, polyethylene bottles or other containers, tapes, bags, banding of identification marks on tools, 
and boundary markers such as ribbons.  Obtain Contracting Officer's prior approval for use of such colored materials 
for other purposes, such as buried vapor barrier membranes.</TXT><BRK/>
<BRK/>
]</TAI></SPT>]</TAI></SPT>[<SPT><TTL>SECURITY REQUIREMENTS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Add special or extraordinary security requirements which are unique to 
the station at which the work is to be performed because of the location of 
the project site on the station.  This information will be made available by 
the station through the Government.  For NAVFAC ML, include if the project involves 
Contractor access to "Classified" information or "Classified" areas.</NPR><BRK/>
<BRK/>
<NPR>This paragraph is tailored for several NAVFAC FECs.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Contract Clause FAR 52.204-2 Security Requirements and Alternate II and the following apply:</TXT><BRK/>
<BRK/>
<ITM INDENT="-0.33">Dual citizenship is not permitted. [_____].</ITM><BRK/>
<BRK/>
]<TAI OPT="NAVFAC WASH">[<SPT><TTL>Naval Air Station (NAS), Patuxent River, MD</TTL><BRK/>
<BRK/>
<TXT>Foreign Nationals:  The Contractor is responsible for notifying the Contracting Officer, at least five days in 
advance, of any foreign nationals coming into a restricted area so that proper clearance and escort procedures 
may be initiated.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Naval Observatory(NOBSY), Washington, DC, Quarters "A"</TTL><BRK/>
<BRK/>
<TXT>Provide full name, date of birth, and Social Security number of all employees and representatives of the Contractor 
who need access to the Quarters "A" compound to the Contracting Officer at least 7 days in advance of the date 
on which access is desired.  The Contractor will be advised should any of the proposed employees not meet security 
requirements for access to the Quarters "A" compound.  For individual cases, access to the Quarters "A" compound 
can occasionally be obtained with a 4-hour advance notice; however, the Contracting Officer reserves the right 
to utilize the full 7 days should he determine it necessary.</TXT><BRK/>
<OLG><BRK/>
[<OLI>Personal identification:  Before entering the Quarters "A" compound, all persons must furnish personal 
identification and receive a badge furnished by the Government.  Badges must be worn so they are clearly 
visible at all times.  Return badges to the issuing office when leaving the Quarters "A" compound.</OLI><BRK/>
<BRK/>
][<OLI>Security processing:  Allow for a processing period of [15] [_____] minutes as employees enter the Quarters 
"A" compound at the beginning of each workday.  All materials entering or in the Quarters "A" compound 
will be subject to search.</OLI><BRK/></OLG>
<BRK/>
]</SPT>][<SPT><TTL>Naval Surface Warfare Center (NSWC), Dahlgren, VA</TTL><BRK/>
<BRK/>
<TXT>A copy of the security regulations may be obtained from the security office of the station.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Naval Surface Warfare Center (NSWC), Indian Head, MD</TTL><BRK/>
<BRK/>
<TXT>No employee or representative of the Contractor will be admitted to the work site unless he furnishes satisfactory 
proof that he is a citizen of the United States or is specifically authorized admittance by the OICC.</TXT><BRK/>
<OLG><BRK/>
<OLI>Identification Badges - A list of all employees to be engaged in the performance of work must be furnished 
to the Security Department.  In the event employees are hired or discharged, a corrected list of employees 
must be furnished reflecting the change in personnel.  Identification badges for the Contractor and his 
employees will be furnished by the Security Department, Indian Head Division, Naval Surface Warfare Center, 
Indian Head, MD.  Immediately report instances of lost or stolen badges to the Contracting Officer.  
Upon completion of the contract or termination of the service of any employee, return the badges to the 
Security Pass Office.  Compliance with this requirement is mandatory and certification thereof to the 
Contracting Officer is required prior to submitting final invoices.  Failure to return badges will hold 
up Contractor's final payment.</OLI><BRK/>
<BRK/>
<OLI>Vehicles and Equipment - In addition to other conditions and requirements set forth hereinbefore, attention 
is invited to the fact that vehicles and equipment admitted to the Indian Head Division, Naval Surface 
Warfare Center, Indian Head, MD will be required to meet standards established be the Station Safety 
Department.  The vehicular and equipment conditions must satisfactorily meet the following provisions:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Steering mechanism must be satisfactory and safe condition.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Horns and warning devices must be operable.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Windshield wipers must be satisfactory in place, clean and unbroken.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Rearview mirrors must be satisfactory in place, clean and unbroken.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">General body conditions:  Body must be satisfactory tight including fenders, bumpers, doors 
and latches thereto, and other parts which might become dislocated during travel.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Lights:  All lights required by the type of vehicle/equipment in use must be functional with 
satisfactory bulbs and lenses.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Exhaust Systems:  Exhaust systems must be completely functional with no leaks.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Fuel system must be free of leaks and show no evidence of loss of fuel or fumes.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Brakes:  All brakes must be functional and give evidence of the ability to halt the loaded 
vehicles within safe distances.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Tires need not be new but must contain sufficient tread to indicate safety at operating speed 
with vehicle loaded.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Electric Wiring:  All wiring must be completely insulated as required, and in cases considered 
appropriate, waterproofing of wiring is required.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Motors must be reasonably clean from excess grease, dust, and dirt, and if required must be 
steam cleaned to the satisfaction of the inspection personnel.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Where applicable, inspection will include other such items as gauges, thermometers, controls, 
relief valves, piping, mechanical locks, limit switches, connectors, and other safety related 
devices associated with vehicles and equipment admitted to the Station.</OLI><BRK/></OLG>
<BRK/></SPT>
][<SPT><TTL>NSS, Washington, DC</TTL><BRK/>
<BRK/>
<TXT>The station is a secured facility:</TXT><BRK/>
<OLG><BRK/>
<OLI>Application:  Furnish to the Contracting Officer a list showing, for employees and representatives to 
be engaged at the site, the name, address, date and place of birth, Social Security number, and, for 
anyone who is not a United States citizen, an alien registration number.  Update the list with each addition 
and deletion to such engagement.</OLI><BRK/>
<BRK/>
<OLI>Passes and badges:  Each individual engaged at the site must obtain a temporary pass each day.  Car passes 
will be issued for parking on the station.  Allow 15 minutes for this procedure at the beginning of each 
day.  Additionally, expect to lose 25 crew hours over the duration of the contract due to delays in obtaining 
an escort while working in the inner compound.  For the purpose of definition, a crew is defined as the 
size of the Contractor's workforce during any given workday.  (If the Contractor has a crew of 10 men 
delayed 30 minutes on a given day, the delay period is one-half crew hour). Such delays will be at no 
additional cost to the Government.</OLI><BRK/>
<BRK/>
[<OLI>Escort:  Work in or around Building[s] No. [_____] is in the inner compound and includes areas where 
an escort furnished by the Government must accompany the Contractor and his representatives and employees 
at all times.</OLI><BRK/></OLG>
<BRK/>
]</SPT>][<SPT><TTL>Naval Research Laboratory (NRL), Washington, DC</TTL><BRK/>
<BRK/>
<TXT>The Contractor is working in highly secured areas.  These areas include [_____].  Furnish notice to the Contracting 
Officer 30 days prior to working in these areas.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Marine Corps Base Quantico (MCBQ), Quantico, VA</TTL><BRK/>
<BRK/>
<TXT>All Contractor and its employees performing services on Marine Corps Base, Quantico (MCBQ) requiring physical 
access to the installation must be properly screened.  Screening consists of identity proofing and vetting in 
accordance with the standards set forth in Marine Corps Base Order 4200.3 (28 JUL 10).  Request a copy of this 
policy from the Contracting Officer.</TXT><BRK/>
<BRK/>
<TXT>Hangars 2102 and 2103 are secured areas.  Comply with the following security requirements:</TXT><BRK/>
<BRK/>
<TXT>[_____].</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Naval Support Facility, Thurmont, MD</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Obtain information needed from  NAVFAC WASH, Code 09F.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The station is a secured facility.  Comply with the following security requirements.</TXT><BRK/>
<BRK/>
<TXT>[_____].</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Joint Base Anacostia-Bolling (JBAB), Washington, DC</TTL><BRK/>
<BRK/>
<TXT>No employee or representative of the Contractor will be admitted to the work site unless he furnishes satisfactory 
proof that he is a citizen of the United States or is specifically authorized admittance by the OICC.</TXT><BRK/>
<OLG><BRK/>
<OLI>Personnel Information - All duty authorized non-military personnel utilizing the base are required to 
have in their possession at all times a Base Entry Pass.  This pass is issued by the Visitors Control 
Center at the South Gate.  Visitors Control is open Monday through Friday, 6:00 a.m. to 3:00 p.m.  A 
minimum of 5 working days prior to start of work, furnish to the Joint Base Anacostia-Bolling (JBAB), 
Washington, DC, Security Department, via the Contracting Officer, the following information for Contractor 
and subcontractor personnel required to enter the Station:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Name of the company</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Name of the employee</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Social Security number</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Proof of U.S. citizenship</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A completed Contractor/Vendor Criminal History Record Request</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A completed application for Base Entry Pass</OLI><BRK/>
<BRK/>
<OLI>Proof of Citizenship - Proof of citizenship will consist of copies of birth certificates, military dependent 
ID card, or naturalization papers, which will be returned once entered into the security computer system.  
The Security Department will run a criminal history check on Contractor employees and, as a condition 
of employment, each employee must willingly sign an authorization form allowing the Security Department 
to conduct the criminal history check.  Subject authorization form will be maintained on file by the 
Security Officer.  Based on proof of U.S. citizenship and the results of the criminal history check, 
the Security Officer will or will not grant entry to the Station.  If entry is denied, the Contractor 
will be immediately notified.</OLI><BRK/>
<BRK/>
<OLI>Contractor Responsibility for Employees - The Contractor is responsible for employees under his employment.  
Ensure that employees are familiar with and obey station traffic, safety, and security regulations.</OLI><BRK/>
<BRK/>
<OLI>Motor Vehicle Operation - Ingress and egress of personnel will be subject to the security regulations 
of the Station.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">All personnel must be made aware of the base speed limits:</OLI><BRK/>
<BRK/>
<ITM>Housing areas       5 mph</ITM><BRK/>
<ITM>Parking areas      10 mph</ITM><BRK/>
<ITM>All other areas    25 mph (unless otherwise posted)</ITM><BRK/>
<BRK/>
<OLI LEVEL="2">Parking is in designed areas only, between two white lines.  No parking is permitted in fire 
lanes, on seeded areas, in parking slots reserved for general officers and handicapped personnel.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Traffic accidents should be reported immediately to the Security Police Law Enforcement Desk 
by calling 767-5000, 5001.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">All personnel entering the installation are subject to random vehicle inspections.  The purpose 
of these inspections is to detect the theft of Government and private property, and to detect 
contraband or illegal drugs.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Required Information on Privately Owned Vehicles - Advise company employees who desire to use 
their privately owned vehicles to personally bring the vehicle, vehicle registration, copy 
of vehicle insurance policy, valid state inspection documentation, and driver's license to 
the Visitor Control Center at the South Gate.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Access to Restricted Areas - Base entry passes allow access to designated areas on the installation 
only.  Entry into off limits areas is prohibited unless the contract requires it.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Current Information - Contractors will be responsible for keeping the vehicle and employee 
lists current, and for securing and returning identification cards belonging to terminated 
employees to the Command Manager's Officer.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Base Entry Passes - Contractor base entry passes will be valid for each entry aboard Joint 
Base Anacostia-Bolling (JBAB) from 6:00 a.m. to 6:00 p.m., Monday through Friday only, unless 
prior arrangements have been made with the Resident Officer in Charge of Construction, NDW, 
and the Base Security Officer, Joint Base Anacostia-Bolling (JBAB), has been notified.  The 
passes are the property of the base and are to be returned to Visitors Control at the South 
Gate upon completion of the contract or termination of employment.  Replacement passes must 
be requested in writing and be accomplished by written authorization from the Contracting Officer.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Providing Information to Subcontractors - Prime Contractors are responsible for ensuring that 
subcontractors receive security information.  Failure to comply with the specified requirements 
will result in prime contractors and subcontractors being denied access to the construction 
site.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC ML">[<SPT><TTL>Naval Weapons Station, Yorktown, VA</TTL><BRK/>
<OLG><BRK/>
<OLI>Personnel information.  A minimum of 5 working days prior to start of work, the Contractor will furnish 
to the Naval Weapons Station (NWS), Yorktown, Security Department, via the Contracting Officer, the following 
information for Contractor and subcontractor personnel required to enter the station:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Name of company</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Name of the employee</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Social Security number</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Proof of U.S. citizenship</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Completed Contractor/Vendor Criminal History Record Request</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Completed application for gate badge</OLI><BRK/>
<BRK/>
<OLI>Proof of citizenship.  Proof of citizenship may consist of copies of birth certificate, military dependent 
identification card (ID), or naturalization papers, which will be returned once entered into the security 
computer system.  The Security Department will run a criminal history check on Contractor employees and, 
as a condition of employment, each employee must willingly sign an authorization form allowing the Security 
Department to conduct the criminal history check.  Subject authorization form will be maintained on file 
by the Security Officer.  Based on proof of U.S. citizenship and results of the criminal history check, 
the Security Officer will or will not grant entry to the station.  If entry is denied, the Contractor 
will be immediately notified.</OLI><BRK/>
<BRK/>
<OLI>Contractor responsibility for employees.  The Contractor is responsible for employees under his employment.  
Ensure that employees are familiar with and obey station traffic, safety, and security regulations.</OLI><BRK/>
<BRK/>
<OLI>Motor vehicle operation.  Ingress and egress of personnel are subject to the security regulations of 
the station.  Motor vehicles operated within the NWS, Yorktown, must comply with the vehicle codes of 
Virginia which are incorporated into NWS Instruction 5510.5G, "Security and Traffic Regulations."  Copies 
may be obtained from the Resident Officer in Charge of Construction, NWS, Yorktown, VA.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC ML">[<SPT><TTL>Armed Forces Experimental Training Activity, Williamsburg, VA</TTL><BRK/>
<BRK/>
<TXT>This activity operates under strict security regulations and persons admitted to this activity will be accompanied 
by a military police escort or an official escort designated by the Security Officer, at all times.  The activity 
Security Officer will authorize issuance of badges to selected responsible employees of the Contractor which 
permits the person issued the badge to act as an escort for other Contractor personnel on the activity.</TXT><BRK/>
<BRK/></SPT>
]</TAI><TAI OPT="NORFOLK NAVAL SHIPYARD">[<SPT><TTL>Norfolk Naval Shipyard, Portsmouth, VA</TTL><BRK/>
<BRK/>
<TXT>Contractor employees and representatives performing work under this contract are required to be United States 
citizens.  If naturalized, the individual must present his naturalization papers to the Security Officer for 
inspection.  Foreign born personnel must present evidence of citizenship regardless of citizenship of parents, 
as required by immigration laws.  Contractors and Contractor personnel are the subject of a local police records 
check.  Contractor personnel who possess a security clearance issued by the Defense Industrial Security Clearance 
Office (DISCO) will be issued a shipyard badge in the appropriate category.  Each Contractor employee is required 
at the time of issuance of a personnel badge to submit a signed Privacy Act Release Form, in duplicate, to complete 
the local police check.  Requested information must be furnished.  Individuals who have felony convictions (e.g., 
murder, rape, drug offences, of theft) or who are deemed untrustworthy by the Security Department, Norfolk Shipyard 
will be denied access to the shipyard and their personnel badge will be recalled.</TXT><BRK/>
<BRK/>
<SPT><TTL>Shipyard CIA and Sensitive Areas</TTL><BRK/>
<BRK/>
<TXT>All Contractor or visitor personnel requesting access to the Controlled Industrial Area (CIA0) will be required 
to view an orientation videotape prior to receiving a badge.  The videotape is 20 minutes in length and includes 
radiological indoctrination training as well as security, environmental, safety and health issues.</TXT><BRK/>
<BRK/>
<TXT>Entry into the CIA for those listed with the Contracting Officer may be authorized under one of the following 
conditions.</TXT><BRK/>
<OLG><BRK/>
<OLI>Contractors having a DOD Facility Security clearance and whose employees have a DOD security clearance 
may be badged for immediate unescorted access into the CIA.</OLI><BRK/>
<BRK/>
<OLI>Employees and representatives having current Shipyard ID badges authorizing CIA access will be permitted 
entry into the CIA.</OLI><BRK/>
<BRK/>
<OLI>Employees not holding a current DOD security clearance or current CIA access badge must establish suitability 
and eligibility prior to being badged for unescorted CIA access.  Provide a Completed Special Access 
Determination (NAVSEA 5510/15) (Apr 90) for each employee.</OLI><BRK/>
<BRK/>
<OLI>For situations other than the above, US citizens who are employees or representatives requiring a CIA 
access may be issued an "Escort Required" ("ER") pass for CIA access under the escort of a cleared individual 
employed by the activity.  Processing of "ER" passes may take up to 5 days.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The initial submittal of Visit Request forms need not be all inclusive.  It may be expanded 
to meet essential requirements of the Contractor.  Each individual added to the list, however, 
are subject to the same pre-entry screening requirements as outlined above.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Shipyard ID badge will be issued by the Shipyard pass and Identification Office (Pass and ID 
Office).</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Vehicle Regulations in the Shipyard CIA</TTL><BRK/>
<BRK/>
<TXT>No vehicle will be permitted access to a work site in the CIA without a DOD vehicle sticker and a valid Shipyard 
vehicle pass.  The Shipyard vehicle passes are issued by the Shipyard Pass and ID Office.  Shipyard vehicle passes 
will not be issued unless a DOD vehicle sticker has been obtained and proof of vehicle registration to the Contractor's 
company has been presented to Shipyard Pass and ID.  Vehicles are required to conform to Shipyard traffic regulations.  
The speed limit is 15 mph in the CIA.  Outside the CIA, the speed limit is as posted or marked.  No privately 
owned vehicles are allowed inside the CIA with the exceptions of handicap, CO/XO/CMC of ships.</TXT><BRK/>
<BRK/>
<TXT>Only those Contractor vehicles meeting the following criteria will be allowed to enter the CIA with the Shipyard 
vehicle pass:</TXT><BRK/>
<OLG><BRK/>
<OLI>Vehicles must clearly display an authorized company sign or logo.</OLI><BRK/>
<BRK/>
<OLI>Vehicles must be company or commercial vehicles used to transport heavy equipment or material to the 
job site or to conduct bona fide and required inspections and surveillance at the job site.  Privately 
owned vehicles will not be used to transport employees to the job site and will not be allowed in the 
CIA.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Commercial Vehicles</TTL><BRK/>
<BRK/>
<TXT>Vehicle passes will be issued to each commercial vehicle that is required for the job, authorizing entry and 
parking within the CIA.  Every vehicle entering the CIA will display the pass on the dashboard or visor (facing 
outward).  The pass will be visible at all times while in the CIA.  Parking is limited to those areas that are 
specifically identified on the pass.  If additional passes are required, present adequate justification to the 
Pass and ID Office via the Contracting officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Parking</TTL><BRK/>
<BRK/>
<TXT>Prohibited on any piers and dry dock/waterfront areas.  Do not park on or block the marked fire lanes or crane 
rail traveling zones (marked in yellow) at any time.  Vehicles may stop on the piers or dry dock/waterfront areas 
for 15 minutes for loading and unloading.  An exception may be made for vehicles which are part of the equipment 
needed to do the required work and are attached or connected to the pier of ship; for example, a truck which 
uses a mounted generator or a vehicle with built-in equipment.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Vehicle Searches</TTL><BRK/>
<BRK/>
<TXT>Vehicles are subject to search while entering, remaining in, or leaving the Shipyard.  Government material being 
transported out of the CIA must be covered by a Property Pass (OP-7), issued and signed by the Security Officer.  
Material found without a Property Pass will be confiscated and a police officer offense report issued.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Escort</TTL><BRK/>
<BRK/>
<TXT>For entrance to and work inside any building inside the CIA, the cognizant Shipyard code will provide escort 
services in the affected area.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Areas Not Covered by Contract</TTL><BRK/>
<BRK/>
<TXT>Contractor personnel will not be permitted to enter Shipyard buildings, spaces, and areas not covered by this 
contract except on prior approval of the Shipyard department/office/shop having jurisdiction of the areas.  Coordinate 
action with the Contracting officer to obtain such entry approval.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Access to Unclassified Information</TTL><BRK/>
<BRK/>
<TXT>Access to unclassified U.S. Navy shipbuilding, conversion, or repair technology and related technical information 
manuals, documents, drawings, plans, specifications, and other unclassified information is restricted to official 
need-to-know basis, designated by physical markings to show the appropriate control designations.  Handle, control, 
and safeguard to prevent oral, visual, and documentary disclosure to the public, to foreign sources, and to personnel 
not having an official need-to-know.  Return this information to the naval Shipyard upon completion of contracted 
work, except when specific retention authorization is granted by the Contracting Officer's Security Representative.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Photographs</TTL><BRK/>
<BRK/>
<TXT>Unofficial photograph is prohibited in the Naval Shipyard.  When operationally required, submit a written request 
containing specific justification and details to the Security Officer prior to release.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Identification Badges</TTL><BRK/>
<BRK/>
<TXT>In addition to the requirements specified in Section <SRF>01 30 00</SRF> ADMINISTRATIVE REQUIREMENTS, comply with the following:</TXT><BRK/>
<OLG><BRK/>
<OLI>Submit a Visit Request (VR) and Special Access Determination (SAD) for each person listed to the Security 
Officer (Code 1125.2) via the Contracting Officer at least 6 weeks prior to the start date.</OLI><BRK/>
<BRK/>
<OLI>Employees and representatives requiring access are U.S. citizens or U.S.  Nationals.</OLI><BRK/>
<BRK/>
<OLI>Under no circumstances may personnel hand carry their own visit request.</OLI><BRK/>
<BRK/>
<OLI>Employees must provide documented proof of U.S. citizenship to the Pass and ID Office prior to being 
issued a Shipyard badge.</OLI><BRK/>
<BRK/>
<OLI>Employees must be available for interviews upon request by the Shipyard Personnel Security Specialist.</OLI><BRK/>
<BRK/>
<OLI>Employees must wear and display the Shipyard badge in the chest area at all times while entering, remaining 
in, and exiting Shipyard spaces and each badge may be used only by the specific individual named on the 
badge.</OLI><BRK/>
<BRK/>
<OLI>Maintain strict accountability over identification badges and passes issued by the Pass and ID Office.  
Return badges/passes to the Pass Office immediately upon termination of any employee, expiration, completion 
of contract, or when no longer required.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT>]</TAI><TAI OPT="NAVFAC ML">[<SPT><TTL>Naval Air Station, Oceana, Virginia Beach, VA</TTL><BRK/>
<BRK/>
<TXT>Contractor personnel are required to obtain personnel identification badges.  In accordance with Section 
<SRF>01 30 00</SRF> ADMINISTRATIVE REQUIREMENTS,  paragraph SUBCONTRACTORS AND PERSONNEL, submit, in triplicate, a list 
of his subcontractors and the work each is to perform.  On this listing must appear the names of the key personnel 
of the Contractor and subcontractors.  A copy of the list of key personnel will be forwarded to the Naval Air 
Station, Oceana, Security Department by the Contracting Officer.  The key personnel are responsible for identifying 
other Contractor and subcontractor personnel for the purpose of obtaining identification badges.  Contractors 
working in restricted work areas are also required to obtain special identification badges for personnel requiring 
access to the restricted work areas.  Immediately after award, submit a letter to the Contracting Officer with 
the following information for each employee:  Company name, employee's name, Social Security number, height, 
and weight.  Also, indicate the names of persons authorized to vouch for additional employees requiring badges.</TXT><BRK/>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC ML">[<SPT><TTL>Fleet Trng Cntr Atlantic (FTCLANT), Dam Neck, Virginia Beach, VA</TTL><BRK/>
<OLG><BRK/>
<OLI>Required Company Information.  Furnish the FTCLANT Base Security Officer (Code 14) with the following 
information on company letterhead:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Contract number and duration of contract.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">List of make, model, and license number of company vehicles requiring decals.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Copy of insurance policy covering company vehicles, indicating the Virginia State minimum insurance 
requirements have been met.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">List of employees who will require ID cards with normal work hours.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Name and sample signature of the representative responsible for obtaining and returning ID 
cards.</OLI><BRK/>
<BRK/>
<LST>The preceding information must be received by the Commanding Officer, Fleet Training Center Atlantic, 
Dam Neck, Virginia Beach, VA 23461-5000, Attn:  Base Security Officer (Code N31, Bldg. 543); or brought 
to the Base Security Office located in Building 448, prior to the first day of work.</LST><BRK/>
<BRK/>
<OLI>Required Information on Privately Owned Vehicles.  Advise company employees who desire to use their privately 
owned vehicles to personally bring the vehicle, vehicle registration, copy of vehicle insurance policy, 
valid State inspection documentation, and driver's license to the pass and decal office located at the 
main gate.</OLI><BRK/>
<BRK/>
<OLI>Current Information.  Contractors are responsible for keeping the vehicle and employee lists current, 
and for securing and returning identification cards belonging to terminated employees to the command 
security manager's office.</OLI><BRK/>
<BRK/>
<OLI>Valid ID Cards.  Contractor ID cards must be valid for each entry aboard FTCLANT from 6 a.m. to 6 p.m., 
Monday through Friday only, unless prior arrangements have been made with the Resident Officer in Charge 
of Construction, Naval Air Station Oceana, and the Base Police Officer, FTCLANT, has been notified.</OLI><BRK/>
<BRK/>
<OLI>Providing Information to Subcontractors.  Prime Contractors are responsible for ensuring that subcontractors 
receive security information.  Failure to comply with specified requirements will result in prime Contractors 
and subcontractors being denied access to construction sites.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC ML">[<SPT><TTL>Naval Station Norfolk, Norfolk, VA</TTL><BRK/>
<OLG><BRK/>
<OLI>Contractor registration.  Register with the Base Police Truck Investigation Team, located behind pass 
and ID Office (Bldg CD-9) on Hampton Boulevard, Naval Station Norfolk, Norfolk, VA 23511-5000, telephone 
number 757-322-2979.</OLI><BRK/>
<BRK/>
<OLI>Storage and office trailer registration.  Register storage and office trailers to be used on base with 
the truck investigation team.  Trailers must meet State law requirements and must be in good condition.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Trailers must be lockable and must be locked when not in use.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Trailers must have a sign in the lower left hand corner of left door of trailer with the following 
information:  Company name, address, registration number of trailer or vehicle identification 
number, location on base, duration of contract or stay on base, contract number, local on-base 
phone number, off-base phone number of main office, and emergency recall person and phone number.</OLI><BRK/>
<BRK/>
<OLI>Equipment markings.  Equipment owned or rented by the company must have the company name painted or stenciled 
on the equipment in a conspicuous location.  Rented equipment is to be conspicuously marked with a tag 
showing who rented the equipment.  Register the equipment with the truck investigation team.</OLI><BRK/>
<BRK/>
<OLI>Procedure information.  For additional information regarding registration procedures, contact the Officer 
in Charge of Construction at 757-445-1463 or Base Police at 757-444-8856.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC ML">[<SPT><TTL>Naval Security Group Activity (NSGA), Northwest, Chesapeake, VA</TTL><BRK/>
<OLG><BRK/>
<OLI>All Contractor personnel and vehicles must report to Truck Control upon initial visit.  All Contractors 
working at NSGA Northwest must have activity badges.  Inform the Truck Control of the expected duration 
of the contract and its location.  Truck Control hours are 6:00 a.m. to 5:00 p.m., Monday through Friday.  
Contractors required to work past 5:00 p.m. must notify Truck Control in person or by telephone at 421-8383, 
no later than 2:00 p.m. of that day.  Contractors required to work weekends, or on Government holidays, 
must notify Truck Control no later than 11:30 a.m. the preceding normal workday.</OLI><BRK/>
<BRK/>
<OLI>The pass/ID clerk will issue an identification badge upon completion of part A of the activity pass application 
form.  This outlines proper procedures and instructions to be followed when issuing activity badges and 
vehicle passes to Contractors.  The following procedures apply:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Contractors must submit to the Security Office via the Contracting Officer, an access list 
of all personnel who will be working on the contract job.  Present a valid picture ID that 
the pass clerk can compare against the access list.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A blue activity pass with photo will be issued for no longer than one year and no less than 
thirty days, corresponding with the length of time listed on the access list.  Activity passes 
without photo will be issued to Contractors who will be at the job site for less than twenty-nine 
days.  Contractors who will be at the job site for less than five days are required to check 
in and out through Truck Control daily, between the hours of 6:00 a.m. and 5:00 p.m.  A Department 
of Defense decal with a black NSGA decal will be issued to the Contractor vehicles that will 
be utilized on-site for over ninety days.  This will be verified by the company or the designated 
on-site supervisor.  All privately owned vehicles and company vehicles used on-site less than 
ninety  days will be issued temporary passes, renewable as required,</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Renewal of activity/vehicle passes, or decals will be done after verifying applicant against 
a valid access list.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Replacement of a lost or stolen pass will be granted after the applicant completes a signed 
statement outlining the circumstances.  The applicant will be verified against a valid access 
list.</OLI><BRK/>
<BRK/>
<OLI>All vehicle operators must have a valid state driver's license.  All Contractor vehicles must meet the 
state law requirements of the state in which it is registered.</OLI><BRK/>
<BRK/>
<OLI>All Contractors will be issued a badge/pass and it must be returned to Truck Control upon completion 
of the contract.</OLI><BRK/>
<BRK/>
<OLI>Any construction materials being removed from the NSGA Northwest base must be accompanied by a property 
pass signed with an original authorized signature.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC ML">[<SPT><TTL>AEGIS Systems Combat Center, Wallops Island, VA</TTL><BRK/>
<OLG><BRK/>
<OLI>The Contractor will be working in the AEGIS Combat Systems Center (ACSC), a Navy facility.  As soon as 
possible, and before work begins, submit to the Contracting Officer a list of all employees who will 
work on the project, including names, Social Security numbers, and dates and places of birth.  Verify 
that all employees are not known felons nor have felony charges pending.  Only United States citizens 
will be admitted to the work site.</OLI><BRK/>
<BRK/>
<OLI>At all times, while on Government property, the Contractor, subcontractors, and their employees must 
wear badges, and vehicle passes are required to access the jobsite.  These badges and passes will be 
issued for the Navy by the Wallops Flight Facility Security Office at the direction of the Contracting 
Office.  Make application for badges to the Navy Contracts Office.  Badges previously issued by NASA 
for NASA projects may not be used to access Navy jobsites.  Upon entering the AEGIS Combat Systems Center 
facility, employees and their gear are subject to inspection.</OLI><BRK/>
<BRK/>
<OLI>The Contractor is held accountable for identification badges and vehicle passes for the life of the contract.  
The Contractor is required to report badge loss or theft immediately to the Contracting Officer.  Failure 
to surrender all badges and passes at the contract's end may result in the retainment of funds or the 
withholding of final payment by the Contracting Officer.</OLI><BRK/></OLG>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC SW">[<SPT><TTL>Employment Restrictions For NAVFAC SW</TTL><BRK/>
<BRK/>
<TXT>Do not employ any person, for any work required by this contract, who: (1)is a non-immigrant as described in 
section 101(a)(15)(H)(ii) of the Immigration and Nationality Act <RID>8 USC 1101</RID>(a)(15)(H)(ii), (2)is an alien having 
a residence in a foreign country which he has no intention of abandoning and who is coming to the United States 
to perform temporary services or labor.</TXT><BRK/>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC MARIANAS"><SPT><TTL>Employment Restrictions For Guam</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph and its subparagraphs ONLY for contracts for base 
operations support (BOS) on Guam that: (1) Are awarded as a result of a competition 
conducted under OMB Circular A-76; and (2) Are entered into or modified on or 
after November 18, 1997.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Do not employ any person, for any work required by this contract, who: (1)is a non-immigrant as described in 
section 101(a)(15)(H)(ii) of the Immigration and Nationality Act (8 U.S.C. 1101(a)(15)(H)(ii), (2) is an alien 
having a residence in a foreign country which he has no intention of abandoning and who is coming to the United 
States to perform temporary services or labor.</TXT><BRK/>
<BRK/></SPT>
</TAI><TAI OPT="NAVFAC PAC"><SPT><TTL><SUB>Personnel List</SUB></TTL><BRK/>
<BRK/>
<TXT><TST>Submit for approval, at least 15 days prior to the desired date of entry, an original alphabetical list of personnel 
who require entry into Government property to perform work on the project.</TST>  Furnish for each person:</TXT><BRK/>
<OLG><BRK/>
<OLI>Name</OLI><BRK/>
<BRK/>
<OLI>Date and place of birth</OLI><BRK/>
<BRK/>
<OLI>Citizenship</OLI><BRK/>
<BRK/>
<OLI>Home address</OLI><BRK/>
<BRK/>
[<OLI>Social Security number</OLI><BRK/>
<BRK/>
][<OLI>Current pass expiration date</OLI><BRK/>
<BRK/>
][<OLI>Naturalization or Alien Registration number</OLI><BRK/>
<BRK/>
][<OLI>Passport number, place of issue, and expiration date</OLI><BRK/>
<BRK/>
][<OLI>Guam Police clearance report for last six months</OLI><BRK/></OLG>
<BRK/>
][<TXT>The request for personnel passes must be accompanied with the following certification:</TXT><BRK/>
<BRK/>
<TXT>"I hereby certify that all personnel on this list are either born U.S. citizens, naturalized U.S. citizens with 
the naturalization number shown[, or legal aliens with the alien registration number indicated]."</TXT><BRK/>
<BRK/>
<TXT>Signature/Firm Name</TXT><BRK/>
<BRK/>
]<SPT><TTL>Citizenship Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Verify with the Activity on the security requirements for Contractor's 
personnel.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>[Aliens will not be admitted to the work site without approval.][Aliens are not allowed on the project site.  
][Clearance for aliens may require approximately 20 workdays for approval.  ][Work under this contract is restricted 
to U.S. citizens.]</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><TAI OPT="NAVFAC SE"><SPT><TTL>Guantanamo Bay, Cuba</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This Article is tailored for NAVFAC SE.  Use and edit for projects at 
Guantanamo Bay, Cuba.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Work Force</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Fill in the brackets when more specific direction is required.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Due to the sensitive locale of the U.S. Naval Base, Guantanamo Bay, Cuba, foreign nationals from dissident political 
areas may be excluded and denied entry approval.  In general, foreign nationals may be used [_____].  The Contractor 
agrees to dismiss from the site, when directed by the Contracting Officer, any individual whose continued employment 
is deemed to be contrary to the public interest or inconsistent with the best interest of the national security.</TXT><BRK/>
<BRK/>
<SPT><TTL><SUB>Entry Approval for Employees</SUB></TTL><BRK/>
<BRK/>
<TXT>No employee or representative of the Contractor will be admitted to the U.S. Naval Base, Guantanamo Bay, Cuba 
without prior entry approval.  The background of Contractor personnel will be screened prior to entry to the 
U.S. Naval Base, Guantanamo Bay, Cuba.  Submit to the Contracting Officer the full name, date and place of birth, 
Social Security number, and addresses of such persons.  This information must be received by the Contracting 
Officer 45 calendar days prior to the scheduled or desired arrival at the Naval Base.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Identification of Employees</TTL><BRK/>
<BRK/>
<TXT>The Contractor is responsible for furnishing to each employee and for requiring each employee to display such 
identification as may be approved and directed by the Contracting Officer.  Employees may be fingerprinted prior 
to employment as a condition of entry onto the Naval Base.  Prescribed Government identification cards must immediately 
be delivered to the Contracting Officer for cancellation upon release of any employee.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Local Labor</TTL><BRK/>
<BRK/>
<TXT>Proselytizing of labor, that is the hiring of Government or Contractor on-base employees by offering higher wages 
or other amenities, is not permitted unless a release from the employer is executed or the employee resigns and 
leaves the base for a minimum of 90 days.  Accordingly, labor which the Contractor proposes to use must be approved 
by the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Management Personnel</TTL><BRK/>
<BRK/>
<TXT>The Contractor is responsible for furnishing the personnel required, with the necessary skills and qualifications, 
to perform the work as described.  Additionally, provide an individual on-site, who is authorized to negotiate 
and financially commit change orders for the Principal.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Access Roads</TTL><BRK/>
<BRK/>
<TXT>Refrain from the use of roads, grounds, or other facilities which have not been specifically authorized for their 
use.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI></SPT>]<TAI OPT="NAVFAC EURAFCENT"><SPT><TTL>NAVFAC EURAFCENT REQUIREMENTS AND RESTRICTIONS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for NAVFAC EURAFCENT.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Building Entrance Restrictions</TTL><BRK/>
<BRK/>
<TXT>Contractor personnel are restricted from entering operational buildings or areas without the specific authorization 
of the Contracting Officer.  To perform work, where "security escorts" are required for access to a facility, 
coordinate with the Contracting Officer for access to such facilities.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Public Release of Information</TTL><BRK/>
<BRK/>
<TXT>There must be no public release of information or photographs concerning any aspect of the materials or services 
relating to this contract or other documents resulting therefrom without the prior written approval of the Contracting 
Officer.</TXT><BRK/>
<BRK/>
<TXT>The Contractor agrees to insert the substance of above paragraph in each subcontract and purchase order generated 
for this contract.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Responsibility for Physical Security</TTL><BRK/>
<BRK/>
<TXT>The Contractor is responsible for physical security of construction materials, supplies, and equipment of every 
description (including property which may be Government furnished or owned) provided or utilized in the execution 
of this contract.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Employment</TTL><BRK/>
<BRK/>
<TXT>Should the continued employment of any person in connection with this contract, or any subcontract thereunder, 
be deemed by the Contracting Officer to be prejudicial to the interests of the Government, that person must immediately 
be removed from the work.  In this connection the Contractor agrees that: </TXT><BRK/>
<OLG><BRK/>
<OLI>Cases which may involve disciplinary action against such persons, or the necessity of reassignment or 
termination of their services, will be investigated, processed, reported and disposed of, as directed 
by the Contracting Officer.</OLI><BRK/>
<BRK/>
<OLI>Employment contracts of all persons employed in connection with this contract, or any subcontract thereunder, 
will include clauses containing the substance of this clause.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Compliance</TTL><BRK/>
<BRK/>
<TXT>Compliance with the foregoing provisions of this clause by subcontractors is the responsibility of the Contractor.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Cultural Resources</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph and following paragraph covers special requirements for 
projects located in Italy.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Cultural resources such as archaeological remains or villa remains may be uncovered during construction excavation 
operations on and off the Installation.  If during excavations, suspected cultural remains are found, excavation 
operations must immediately cease and notify the Contracting Officer who will contact the Installation Environmental 
office.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Unexploded Ordnance</TTL><BRK/>
<BRK/>
<TXT>The Contractor is advised that unexploded ordnance may exist in areas where excavation work is required.  During 
the entire life of this Contract, perform both visual and electronic inspection of the work areas to prevent 
danger to personnel and loss of equipment from inadvertently exploding old ordnance.</TXT><BRK/>
<BRK/>
<TXT>During excavation work, use caution when unknown objects are encountered and thoroughly identify the object prior 
to removal.  Upon discovery of suspected unexploded ordnance in the course of contract work, immediately clear 
the area and contact the Contracting Officer.  Resultant exploratory and removal work may be subject to negotiations 
for a contract change in accordance with the Contract Clauses.</TXT><BRK/>
<BRK/>
[<SPT><TTL>Ordnance Removal Requirements</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Use this paragraph if Installation requires Contractor to have ordnance 
removal team on-call and perform ordnance removal.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Upon issuance of contract change and notice to proceed by the Contracting Officer, provide exploratory excavation 
and removal of suspected unexploded ordnance.  This work must be conducted only by a firm authorized by the Italian 
Ministry of Defense (IMD) to perform such work, and approved by the Contracting Officer.  Submit <SUB>proof of IMD 
ordnance work authorization</SUB> to the Contracting Officer for review and approval prior to conducting ordnance work.</TXT><BRK/>
<BRK/>
<TXT>Have the approved ordnance removal firm committed to an on-call basis in the event that suspected unexploded 
ordnance is encountered during contract work.</TXT><BRK/>
<BRK/></SPT>
]</SPT></SPT></TAI><TAI OPT="NAVFAC FE">[<SPT><TTL><SUB>CONTRACTOR REGULATIONS</SUB> FOR DIEGO GARCIA</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph for Diego Garcia projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Develop, promulgate and enforce operating regulations for campsite and other facilities and equipment under his 
control.  The regulations must include the maintenance of good discipline, security, sanitation, and a fire plan.  
Prepare and submit for approval after consultation with Navy authorities.</TXT><BRK/>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC FE">[<SPT><TTL>BRITISH INDIAN OCEAN TERRITORY (BIOT) LAWS FOR DIEGO GARCIA</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Use the following paragraphs for projects at Diego Garcia. </NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Applicable on Diego Garcia (DG) and enforced by the representative of the BIOT Commissioner on DG.</TXT><BRK/>
<BRK/>
[<SPT><TTL>BIOT Immigration Requirements</TTL><BRK/>
<BRK/>
<TXT>Third country Contractors and personnel must have valid passports.  Requirements for Contractor employees who 
are residents of the BIOT must be as specified by the Commissioner of the BIOT.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Contractor I.D.</TTL><BRK/>
<BRK/>
<TXT>Prepare and issue I.D. cards for each person with their equivalent General Schedule rating as prescribed in the 
JTR Manual Vol 11.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Contractor-Owned Vehicles</TTL><BRK/>
<BRK/>
<TXT>Approved Contractor-owned vehicles will be permitted on the site.  Motor scooters, mopeds, motorcycles, and privately 
owned vehicles are prohibited on DG.  Drivers must have a valid international driver's license.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Inspection</TTL><BRK/>
<BRK/>
<TXT>Personnel, equipment and plant are subject to customs inspection.  Personnel are also subject to physical searches 
at random intervals.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Business or Occupation on DG</TTL><BRK/>
<BRK/>
<TXT>Engaging in commercial enterprise or other than work covered by this contract is prohibited.  This prohibition 
includes, but is not limited to, commercial fishing, oil or mineral exploration, and production in or under those 
areas of the waters, Continental shelf, and seabed around DG over which the United Kingdom has sovereignty or 
exercises sovereign rights.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>BIOT Taxes and Customs Duties</TTL><BRK/>
<BRK/>
<TXT>Base bids on the assumption that the Contractor's firm and employees are exempt from BIOT taxes and customs duties.  
There are import and export controls applicable to the BIOT.  Personal household effects, privately-owned vehicles, 
drugs, firearms, and other controlled materials are not authorized.  Authorized goods and materials for a non-U.S. 
Contractor must be consigned in care of the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
]</SPT>]</TAI><TAI OPT="NAVFAC FE">[<SPT><TTL>BASE OPERATING SUPPORT (BOS) FOR WAKE ISLAND AND DIEGO GARCIA</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use for Wake, Johnston Island, and Diego Garcia projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT><TST>The BOS Contractor as mentioned herein is a private contractor retained by the Government for base operations 
support services.  Coordinate with the Contracting Officer for services available from the BOS Contractor.</TST></TXT><BRK/>
<BRK/></SPT>
]</TAI><TAI OPT="NAVFAC FE">[<SPT><TTL>FACILITIES AND SERVICES FOR WAKE ISLAND AND DIEGO GARCIA</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use for Wake, Johnston Island, and Diego Garcia projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Verify rates and available with the Activity.</TXT><BRK/>
<BRK/>
[<SPT><TTL>Meal Services for Diego Garcia</TTL><BRK/>
<BRK/>
<TXT>Available on a cost reimbursable basis.  U.S. expatriate (EXPAT) and Third Country Nationals (TCN) personnel 
may obtain meals from the Navy Support Facility Consolidated Dining Facility, and the BOS Contractor TCN Dining 
Facility, respectively.  Each employee must sign the Meal Signature Record Book (MSRB) before each meal.  Submit 
to the Contracting Officer the <SUB>Meal Signature Record Book (MSRB)</SUB> on a daily basis.  The Contractor will be charged 
by the number of personnel on island and not by the number of meals consumed.  Cost for three meals per day is 
$3.85 per person for TCNs and $5.65 per person for EXPATs.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Dining and Lodging Facilities for Wake Island</TTL><BRK/>
<BRK/>
<TXT>Meals and lodging facilities are available on a cost reimbursable basis.  This includes furniture, bed, linen, 
a towel, janitorial services and shower/toilet facilities. <TST>Submit <SUB>dining and lodging requirements</SUB> at least 60 
days prior to actual requirements for approval.</TST>  Rates and schedule:</TXT><BRK/>
<TAB WIDTH="79">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="3" ROWCOUNT="6">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="142.50"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="150.00"/>
      <COL AUTOWIDTH="0" WIDTH="215.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL1>MEAL</HL1></DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING"><HL1>RATES</HL1></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL1>SCHEDULE (DAILY)</HL1></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Breakfast</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$4.85</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">6:30 a.m. - 8:00 a.m.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Lunch</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$6.00</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">11:00 a.m. - 1:00 p.m.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Dinner</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$6.00</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">5:00 p.m. - 7:00 p.m.</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Box Lunch</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$2.50</DTA>
         </CEL>
         <CEL/>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="27.00">
         <CEL MERGEACROSS="2" STYLEID="s50">
<DTA TYPE="STRING">Lodging:  $4.00/Person/Day</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/></SPT>
][<SPT><TTL>Housing for Diego Garcia</TTL><BRK/>
<BRK/>
<TXT>Provide suitable housing for employees using the Splendidville/PWC Camp facilities or other locations as directed.  
Approval required to upgrade these seahuts through alteration or construction.  Develop and maintain a housing 
plan which reflects the actual use of housing assets under Contractor control.  The <SUB>housing plan</SUB> and any revisions 
thereto will be subject to approval.  Maintenance and repair of facilities are available on a cost reimbursable 
basis.  TCN housing must not be air-conditioned unless approved.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Medical Facilities for Wake and Diego Garcia</TTL><BRK/>
<BRK/>
<TXT>Limited medical facilities and services are available on a cost reimbursable basis.  Submit a <SUB>medical plan</SUB> and 
medical records of employees prior to transporting them to the Island.  The following conditions apply.</TXT><BRK/>
<OLG><BRK/>
<OLI>Medical plan:  Include narrative description that delineates the procedures for maintaining medical records; 
screening physical exams and immunization requirements; testing for contagious disease, such as dengue, 
malaria, tuberculosis; and other diseases that may be associated with the employee's country of origin.</OLI><BRK/>
<BRK/>
<OLI>Personnel must receive a thorough dental and physical examination and should bring unique medication/drugs 
and two pairs of prescription eyeglasses.</OLI><BRK/>
<BRK/>
<OLI>Rates:</OLI><BRK/>
<TAB HEADERROWS="0" WIDTH="49">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="3">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="158.25"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="156.75"/>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Out-patient Care</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$30.00 per visit</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">In-patient Care</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$100.00 per day</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="24.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Pharmacy</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Prevailing cost</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<NTE><AST/><BRK/>
<NPR>NOTE:  Also include this paragraph for Diego Garcia projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI>Government medical services are available in emergencies where life may be in danger and for infectious 
diseases. Treatment for long-term medical problems or those requiring hospitalization not available.  
When determined by the attending medical authorities, transfer patients to a non-Governmental medical 
facility as soon as possible.  [X-ray services are available for emergencies.]</OLI><BRK/>
<BRK/>
<OLI>The MEDEVAC point is Kadena, Okinawa.  The Contractor is responsible for transferring the patient from 
the air terminal to a private doctor or hospital.  In case of extreme emergency, patients may be transferred 
to a private hospital in Okinawa at the Contractor's expense.</OLI><BRK/></OLG>
<BRK/></SPT>
][<SPT><TTL>Dental Treatment for Diego Garcia</TTL><BRK/>
<BRK/>
<TXT>Limited to out-patient dispensary service, at $30.00 per visit, during regular working hours for relief of pain, 
contagious oral diseases or humanitarian reasons.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Retail Store</TTL><BRK/>
<BRK/>
<TXT>Limited items and quantities such as canned goods, bread, milk, produce, candy, toilet articles, magazines, and 
other such items, are available at the prevailing rates.  Luxury items are not available for purchase.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Alcohol and Gambling</TTL><BRK/>
<BRK/>
<TXT>[The Contractor may operate a combined mess and club where beer may be dispensed at authorized times.  ]Consumption 
of alcoholic beverages is only authorized in clubs, designated areas or quarters.  Gambling is prohibited.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Postal Services</TTL><BRK/>
<BRK/>
<TXT>Postal services via the U.S. Postal system are available to U.S. personnel. Foreign national employees may send 
letter mail to non-APO addressees and may receive letter mail.  Foreign nationals may neither send nor receive 
packages or purchase money orders through the U.S. Postal system.  Money orders are available.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Custodial Service for Diego Garcia</TTL><BRK/>
<BRK/>
<TXT>Custodial services for personnel housing and other facilities under the Contractor's control are available on 
a cost reimbursable basis.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Janitorial Services for Wake Island</TTL><BRK/>
<BRK/>
<TXT>Janitorial services, other than those included as part of the dining and lodging facilities, are available on 
a cost reimbursable basis.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Recreation Facilities</TTL><BRK/>
<BRK/>
<TXT>Existing recreation facilities and special services activities are available.  The Government retains the right 
to limit Contractor use or schedule such use so as not to interfere with Government employees.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Club Privileges</TTL><BRK/>
<BRK/>
<TXT>Club privileges may be granted by invitation from the various clubs on the basis of classification or grade of 
the employee.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Swimming and Fishing</TTL><BRK/>
<BRK/>
<TXT>Permitted.[  However, exercise caution in eating fish caught within the [Midway][Wake] reef area as certain species 
are poisonous.  Inform personnel of known species of poisonous fish.]</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Fuel for Wake Island</TTL><BRK/>
<BRK/>
[<TXT>JP-5 and MoGas are available at [$_____] and [$_____], respectively, plus a [_____] and [_____] percent surcharge, 
respectively.  Diesel fuel is not available.  The Government will not provide fuel storage facilities and will 
not be liable for damages and losses due to the use of JP-5 and MoGas purchased from the Government.</TXT><BRK/>
<BRK/>
]</SPT>][<SPT><TTL>Fuel for Diego Garcia</TTL><BRK/>
<BRK/>
[<TXT>JP-5, MoGas, and diesel are available at $0.71, $0.82, and $0.69 per gallon, respectively.  The Government will 
not provide fuel storage facilities and will not be liable for damages and losses due to the use of JP-5, MoGas, 
and diesel purchased from the Government.</TXT><BRK/>
<BRK/>
]</SPT>]</SPT>]</TAI><TAI OPT="NAVFAC FE">[<SPT><TTL><SUB>TRANSPORTATION OF PERSONNEL, MATERIALS, AND EQUIPMENT</SUB> FOR WAKE AND DIEGO GARCIA</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraphs as applicable for Wake and Diego Garcia 
projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Coordinate arrangements for transporting materials, equipment, and personnel with the Contracting Officer.[  
Rates shown were the latest available when this specification was prepared, and is furnished for informational 
purposes only.][  The Contractor will be charged rates in effect at the time the services are actually provided.]  
The Contractor has the option to use commercial or privately-owned transportation.</TXT><BRK/>
<BRK/>
[<SPT><TTL>Surface Transportation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Verify the availability and rates with the proper Government office.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Use of Government facilities are on a priority basis as determined by the Government.  Repair damaged Government 
property such as docks, buoys, lightering watercraft and equipment due to the Contractor's negligence at the 
Contractor's own expense.</TXT><BRK/>
<OLG><BRK/>
<OLI>Military Sealift Command (MSC):  [The current shipping cycle to Midway is approximately 90 days but is 
subject to change without notice].  [There is no regularly scheduled MSC service to [DG] [Wake]].  If 
the Contractor elects to use MSC services, the Contractor is responsible for costs incurred or delays 
encountered because of late or nondelivery of materials or equipment.  MSC services are subject to the 
following conditions:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Provided on a space available basis or if no commercial service is available.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Government has the right to reject cargo offered and to limit the quantities of materials 
accepted.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Government incurs no responsibility, expressed or implied, for return transportation, continued 
frequency, timeliness or reliability of the MSC service.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Pay in advance by means of a special deposit account to the Fleet and Industrial Supply Center 
(FISC), administering the services for transportation, stevedoring, handling, securing and 
local accessorial services.  For FISC [Pearl Harbor] rates are:</OLI><BRK/>
<TAB HEADERROWS="4" WIDTH="66">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
      <STY SID="s51">
         <ALN HORIZONTAL="RIGHT" VERTICAL="BOTTOM"/>
      </STY>
      <STY SID="s52">
         <ALN HORIZONTAL="CENTER"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="3" ROWCOUNT="6">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="140.25"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="86.25"/>
      <COL AUTOWIDTH="0" WIDTH="197.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL MERGEACROSS="2" STYLEID="s50">
<DTA TYPE="STRING"><HL4><HL1>Transportation,<MET> Tonne</MET><ENG> Ton</ENG></HL1></HL4></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="34.50">
         <CEL MERGEACROSS="2" STYLEID="s50">
<DTA TYPE="STRING"><MET><HL4><HL1>1.1 Cubic Meters Per Measurement</HL1></HL4></MET><ENG> <HL4><HL1>40 cubic feet Per Measurement</HL1></HL4></ENG></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s51"/>
         <CEL STYLEID="s51"/>
         <CEL STYLEID="s52">
<DTA TYPE="STRING"><HL1>Stevedoring</HL1></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">General Cargo</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$[_____]</DTA>
         </CEL>
         <CEL STYLEID="s52">
<DTA TYPE="STRING">$[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="23.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Special Cargo</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$[_____]</DTA>
         </CEL>
         <CEL STYLEID="s52">
<DTA TYPE="STRING">$[_____]</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="27.75">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">Cargo Trailer</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$[_____]</DTA>
         </CEL>
         <CEL STYLEID="s52">
<DTA TYPE="STRING">$[_____]</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<OLI LEVEL="2">The BOS Contractor's stevedoring/lighterage rates are:</OLI><BRK/>
<BRK/>
<ITM>Laborers:  [$_____] per hour</ITM><BRK/>
<BRK/>
<ITM>Operation Supervisor:  [$_____] per hour</ITM><BRK/>
<BRK/>
<ITM>Safety Supervisor:  [$_____] per hour</ITM><BRK/>
<BRK/>
<ITM>LCM-8 Boat Crew (5 Men per LCM-8):  [$_____] per hr/man</ITM><BRK/>
<BRK/>
<ITM>Crane Operator:  [$_____] per hour</ITM><BRK/>
<BRK/>
<ITM>Forklift Operator:  [$_____] per hour</ITM><BRK/>
<BRK/>
<ITM>Administrative Charges:  [$_____] per day</ITM><BRK/>
<BRK/>
<OLI LEVEL="2">Damages or loss due to handling, loading, securing, transporting, failure of, or delay in delivery 
will be borne by the Contractor.  Obtain adequate insurance against damage, loss or failure 
of, or delay in delivery, as appropriate, and include the Government as a named insurer.</OLI><BRK/>
<BRK/>
<OLI>Commercial vessel:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Lighterage operations are [normally 24 hours to avoid turnaround delay at Midway] [restricted 
to daylight hours unless approved otherwise at [Wake] [DG].]</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Contractor is liable for accidental injury or death of Contractor's personnel and damages 
to material and equipment during stevedoring operations performed by the Contractor.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Pay demurrage charges for barges and vessels not under Navy sponsorship, or vessels where delay 
results from the failure of the Contractor to perform specified stevedoring services. When 
demurrage is assessed to cargo belonging to several agencies, arrange with the agencies concerned 
in sharing such expenses.  No priority will be afforded the Contractor's cargo over others, 
and cargo will be handled as the ship's cargo master elects to unload, except that food or 
medical supplies will be given first priority.</OLI><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the text below for Wake projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<OLI LEVEL="2">Unload cargo from ships anchored offshore into BOS Contractor controlled watercraft and repair 
damages to Government lightering watercraft due to Contractor negligence.  The movement of 
the cargo from the dock to the jobsite is the Contractor's responsibility.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Contractor will not be charged for the use of the watercraft dockside crane and two forklifts 
for lighterage operations but will be charged for the labor involved at the prevailing labor 
rates.  Utilize the BOS Contractor's operators.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Government lightering watercraft consists of two LCM-8's.  The LCM-8's are<MET> 22.5 m long; 6.4 
m wide; 2.8 m side board;</MET><ENG> 73 feet 8 inches long; 21 feet wide; 9 feet 4 inches side board;</ENG><MET> 
one meter</MET><ENG> 3 feet 3 inches</ENG> draft light;<MET> 1.2 m</MET><ENG> 4 feet</ENG> draft loaded; have<MET> 53 tonnes</MET><ENG> 53 1/2 tons</ENG>
 load capacity, and<MET> 76.8 cubic meters</MET><ENG> 2742 cubic feet</ENG> cargo space.  The dockside crane capacity 
is<MET> 20,400 kg</MET><ENG> 45,000 pounds</ENG>.  Cargo that is not adequately crated/packed or cannot be safely 
handled by the LCMs or crane will not be unloaded by the Government.  Materials in bulk, such 
as aggregate, will not be transported or handled by the BOS Contractor unless bagged or otherwise 
contained for convenient handling.</OLI><BRK/></OLG>
<BRK/></SPT>
][<SPT><TTL><SUB>Purchase Orders</SUB> for Diego Garcia</TTL><BRK/>
<BRK/>
<TXT>Submit three copies of purchase orders for materials and equipment purchased from the U.S. prior to actual procurement 
for approval.  Also submit monthly three copies of subsequent revisions or amendments to the purchase orders 
with the MSR.  Purchase orders must refer to and contain the same nomenclature and item number as the corresponding 
item listed in the BM.</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Air Transportation</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the text in "a." below for Wake and Diego Garcia projects.  Verify 
the availability and rates with the proper Government office.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
<OLI>Air Mobility Command (AMC) [is not scheduled on a regular basis to [Wake] [DG].][  Service is subject 
to the following conditions:]</OLI><BRK/>
<BRK/>
<OLI>Commercial and private aircraft:  If approved, special commercial chartered flights and private aircraft 
will be permitted to land on [DG] [Wake].  Submit for approval at least 30 days prior to the flight date.</OLI><BRK/></OLG>
<BRK/></SPT>
][<SPT><TTL>Agreement</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this paragraph AGREEMENT for Wake and Diego Garcia projects.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT><TST>Submit prior to shipment of materials and equipment by Government air and surface transportation, an agreement 
in the following form:</TST></TXT><BRK/>
<BRK/>
<TXT>"In consideration of the carriage of the property described as follows: ___________________________________________________________________________ 
___________________________________________________________________________ (Description and maximum quantity 
to be shipped--the latter to be stated in both weight and measurement tons.)  I, ____________________________________ 
(Acting both individually and as the duly authorized agent of ______________________________________, the owner 
of said property) hereby agrees that neither the carrying vessels, nor the United States, nor an agent or agency 
incorporated or unincorporated thereof, will be liable for loss of, or damage of any nature whatsoever to, said 
property or for any failure to deliver above said property in the same quantity and in the same order and condition 
as when received by the initial carrying vessel, or for any delay in such delivery, whether said loss, damage 
or failure of or delay in delivery is occasioned by the negligence of the carrying vessel, the United States, 
or any employee or agency thereof, or by any cause whatsoever.  The owner of said property and [_____] hereby 
further agree to hold harmless and indemnify the United States for any loss or damage arising out of the carriage 
of the aforesaid property and also agree to pay for freight and terminal service charges as may be determined 
by the Government loading and discharging terminals."</TXT><BRK/>
<BRK/></SPT>
][<SPT><TTL>Packaging</TTL><BRK/>
<BRK/>
<TXT>Package in accordance with "Department of Defense Military, Standard Transportation and Movement Procedures" 
and the requirements of the Government shipping service.</TXT><BRK/>
<BRK/></SPT>
]</SPT>]</TAI><TAI OPT="NAVFAC SE"><SPT><TTL>TRANSPORTATION OF PERSONNEL, MATERIALS, AND EQUIPMENT FOR GUANTANAMO BAY</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use this Article for projects at Guantanamo Bay, Cuba.  This Article 
is tailored for NAVFAC SE.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Ocean Freight</TTL><BRK/>
<BRK/>
<TXT>Provide loading of freight and ocean freight, off-loading, and handling as required, based on the following:</TXT><BRK/>
<OLG><BRK/>
<OLI>Marine Insurance:  Marine insurance, to the extent required, must be provided by the Contractor.</OLI><BRK/>
<BRK/>
<OLI>Ship Arrival</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">No ships or vessels may enter the Guantanamo Bay Defense Sea Area except as approved by Commander, 
U.S. Naval Base, Guantanamo Bay, Cuba.  Not less than 48 hours prior to departure of vessel 
from the port of embarkation, provide to the Contracting Officer the following information:</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Name of vessel.</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Place of registry and registry number.</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Name, nationality, and address of owner.</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Name, nationality, and address of operator.</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Gross tonnage, length, beam, and draft of vessel.</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Nationality and numbers of officers and crew (include crew list).</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Number of passengers (include passenger list).</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Last port of call prior to entry into Guantanamo Bay Naval Defense Sea Area.</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Purpose of visit.</OLI><BRK/>
<BRK/>
<OLI LEVEL="3">Proposed date of entry and estimated duration of stay.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Passengers and crew are subject to Base regulations.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Commercial vessels will be permitted to discharge cargo at cargo docks to the extent that space 
is available.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Coordinate off-loading of barge materials with the Naval Station Guantanamo Bay port operations 
contractor.</OLI><BRK/>
<BRK/>
<OLI>Vessels on Contract to Government</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Contract for shipping service, scheduled every other week to and from Guantanamo Bay, Cuba 
and Jacksonville, Florida, is provided by Schuler Line Navigation Co. LLC., as the Government 
Carrier. Sailing schedule set at 14 days between Jacksonville, Florida and Guantanamo Bay.</OLI><BRK/>
<BRK/>
<ITM>Schuler Line Navigation Co. (SLNC) LLC</ITM><BRK/>
<ITM>130 Severn Ave, Ste 200</ITM><BRK/>
<ITM>Annapolis MD 21403, United States</ITM><BRK/>
<ITM>Office: (410) 216-9281</ITM><BRK/>
<ITM>Fax: (410) 216-6021</ITM><BRK/>
<ITM>Web: <URL>http://schulerline.com/cuba-liner-service</URL></ITM><BRK/>
<BRK/>
<ITM>   SLNC Broker:  Dome Chartering &amp; Trading Corp.</ITM><BRK/>
<ITM>   Office: (410) 216-6020</ITM><BRK/>
<ITM>   Fax: (410) 216-6021</ITM><BRK/>
<ITM>   Web: <URL HREF="http://www.domechartering.com">www.domechartering.com</URL></ITM><BRK/>
<ITM>   Email: <URL HREF="mailto:fix@domechartering.com">ops@domechartering.com</URL></ITM><BRK/>
<BRK/>
<ITM>   SLNC Jacksonville Port Agent: CB Agencies</ITM><BRK/>
<ITM>   Mr. Chuck Bridges</ITM><BRK/>
<ITM>   3565 Cardinal Point Drive</ITM><BRK/>
<ITM>   Jacksonville, FL 32257</ITM><BRK/>
<ITM>   Office: (904) 449-4714 (24 hrs)</ITM><BRK/>
<ITM>   Email: <URL HREF="mailto:cbagency@aol.com">cbagency@aol.com</URL></ITM><BRK/>
<BRK/>
<OLI LEVEL="2">Since these vessels are under Government contract, priority materials for Government agencies 
may delay receipt of Contractor's equipment and materials.  The cost of containerization, shipping, 
on-loading, and off-loading is at the Contractor's expense; and arrangements must be made directly 
with the shipping company.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Government Carrier is subject to change.  If a change in Government Carrier should occur, 
the Government is not liable for any additional costs which may be incurred by the Contractor 
for the construction contract.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Contractor is under no obligation to use the Government Carrier and may use others subject 
to the terms and conditions of this contract and U.S. Maritime law.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">The Contractor may ship materials and equipment by air or sea provided all clearances are met 
and approved in advance.  The Contractor may make use of the Government Carrier's barge service, 
if space is available, at the established commercial rates provided by the Government Carrier.  
The Government's material has priority over Contractor material on the Government Carrier's 
barge.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>On-Base Transportation</TTL><BRK/>
<BRK/>
<TXT>Provide necessary personnel, vehicles, and equipment required for on-base vehicular transportation, and bear 
the cost of required fuel, oil, lubricants, and maintenance there-for.  The vehicles must be operated only by 
Contractor's employees who possess a valid motor vehicle operator's identification card; and vehicular registration 
will be provided without cost by the Government.  Comply with the latest traffic safety program set forth in 
OPNAV Instruction 5100.12.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the bracketed paragraph below for projects within the JTF Area.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<TXT>Expect varying delays, up to 20 minutes, at security checkpoints when entering the JTF Area.</TXT><BRK/>
<BRK/>
]</SPT><SPT><TTL>Transportation of Personnel</TTL><BRK/>
<OLG><BRK/>
<OLI>Air travel to and from the base is limited, with demand often far in excess of supply.  Specifically:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Travel to and from Jacksonville, Florida; Norfolk, Virginia; and Kingston, Jamaica is provided 
by the Air Mobility Command (AMC) at the Contractor's expense, and passage will be in reserved 
seats.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Plane Fares to Guantanamo Bay, Cuba as of FY2024.  Rates are Subject to change.</OLI><BRK/>
<BRK/>
<TAB HEADERROWS="1" WIDTH="75">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN VERTICAL="BOTTOM"/>
      </STY>
      <STY SID="s51">
         <ALN HORIZONTAL="CENTER" VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="3">
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="303.75"/>
      <COL STYLEID="s50" AUTOWIDTH="0" WIDTH="266.25"/>
      <ROW AUTOHEIGHT="0" HEIGHT="22.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">From Norfolk, Virginia</DTA>
         </CEL>
         <CEL STYLEID="s51">
<DTA TYPE="STRING">$1128.00 Round Trip</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="22.50">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">From Jacksonville, Florida</DTA>
         </CEL>
         <CEL STYLEID="s51">
<DTA TYPE="STRING">$744.00 Round Trip</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="26.25">
         <CEL STYLEID="s50">
<DTA TYPE="STRING">From Kingston, Jamaica</DTA>
         </CEL>
         <CEL STYLEID="s51">
<DTA TYPE="STRING">$204.00 Round Trip</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<OLI LEVEL="2">Emergency leave travel for verified personal emergencies such as death or serious illness of 
a family member will be authorized to any destination on the next available flight, also chargeable 
to the Contractor at the international tariff rate.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT></TAI><TAI OPT="NAVFAC HI">[<SPT><TTL>EXTRAORDINARY SECURITY REQUIREMENTS FOR PEARL HARBOR</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Do not add information related to Activity regulations which are of a 
routine nature.  Unusual access provisions dictated by the needs of a particular 
project may be included, as directed.</NPR><BRK/>
<BRK/>
<NPR>For Pearl Harbor Naval Shipyard, coordinate with the Activity for security access 
requirements and add them to the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
[<SPT><TTL>Other Sensitive Areas</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  For areas other than Pearl Harbor Naval Shipyard or Naval Base, verify 
with the Activity if required for communication buildings or other sensitive 
areas.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Extraordinary Security Requirements</TTL><BRK/>
<OLG><BRK/>
<OLI>Vehicle searches.  All construction vehicles will be searched by the Marine sentry.</OLI><BRK/>
<BRK/>
<OLI>Photographs.  Photographs are prohibited in and around the building unless a written request containing 
specific justification and details is approved by the security officer via the Contracting Officer.  
Four days' advance notice is required.  Photographs, when approved, may only be taken in the presence 
of an activity escort.</OLI><BRK/>
<BRK/>
<OLI>Personnel restrictions.  Due to sensitivity of building operations, the following apply:</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">Restrict personnel to the designated work site.</OLI><BRK/>
<BRK/>
[<OLI LEVEL="2">Contractor's movements within the building will be restricted.  Contractor personnel will be 
escorted to and from designated work areas.  Contractor personnel are not permitted outside 
of designated work areas without being escorted by authorized personnel.[  Submit requests 
for entry into the building 4 days in advance with information required by paragraph PERSONNEL 
LIST for submission to the "Division Project Officer" through the Contracting Officer.]</OLI><BRK/></OLG>
<BRK/>
]</SPT></SPT>]</SPT>]</TAI><TAI OPT="NAVFAC NW"><SPT><TTL>EXTRAORDINARY SECURITY REQUIREMENTS FOR PUGET SOUND NAVAL SHIPYARD &amp; INTERMEDIATE MAINTENANCE FACILITY (PSNS 
&amp; IMF), NAVAL BASE KITSAP BREMERTON, WASHINGTON</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraphs for Puget Sound Naval Shipyard and Intermediate 
Maintenance Facility located at NBK Bremerton, WA.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Do not enter into work areas where Shipyard personnel are using protective equipment such as respirator and masks 
or marked boundary areas without prior approval from the Contracting Officer.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Do not add information related to Activity regulations which are of a 
routine nature.  Unusual access provisions dictated by the needs of a particular 
project may be included, as directed.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Vehicle Regulations in the Controlled Industrial Area (CIA) of Puget Sound Naval Shipyard &amp; Intermediate Maintenance 
Facility (PSNS &amp; IMF) Naval Base Kitsap, Bremerton, Washington and Sensitive Areas.</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  The provisions of these security requirements are applicable to the following 
area:  Controlled Industrial Area (CIA) within the boundaries of Puget Sound 
Naval Shipyard &amp; Intermediate Maintenance Facility (PSNS &amp; IMF) at NBK 
Bremerton, WA.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Contractor vehicles requiring admittance into the CIA must be submitted to the Puget Sound Naval Shipyard Security 
Office via a CIA Vehicle Pass Request (PSNS &amp; IMF 5530/25).  Allow five full working days for processing 
of the request.  CIA vehicle passes will not be issued unless a DOD vehicle sticker has been obtained and proof 
of vehicle registration to the Contractor's company has been submitted to the Pass and ID Office.  Only those 
Contractor vehicles meeting the following criteria will be allowed to enter the CIA with the Shipyard vehicle 
pass:</TXT><BRK/>
<OLG><BRK/>
<OLI>Vehicles must clearly display an authorized company sign or logo.</OLI><BRK/>
<BRK/>
<OLI>Vehicles must be a company or commercial vehicles used to transport heavy equipment or material to the 
job site or to conduct required inspections and surveillance at the job site.</OLI><BRK/>
<BRK/>
<OLI>Privately owned vehicles will not be used to transport employees to the job site and will not be allowed 
in the CIA area.</OLI><BRK/>
<BRK/>
<OLI>Upon approval of the CIA Vehicle Pass Request, the Contractor will bring the vehicle's registration and 
insurance document, or a photocopy, to the Pass and ID Office where one of two CIA Vehicle Permits will 
be issued.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A Laydown permit that authorizes the vehicle to be brought into the CIA and parked in the negotiated 
site/laydown area.  Each permit will include the company name, license plate number and expiration 
date.</OLI><BRK/>
<BRK/>
<OLI LEVEL="2">A Load/Unload permit that authorizes the vehicle to be brought into the CIA and parked in the 
negotiated site/lay down area.  Each Permit will include the company name, license plate number 
and expiration date.  Every vehicle entering the CIA will display the pass, visible at all 
times while in the CIA.  Parking is limited to those areas that are specifically identified 
on the pass.  If additional passes are required, present adequate justification to PSNS Security 
via the Contracting Officer.</OLI><BRK/>
<BRK/>
<OLI>Vehicles are required to conform to Shipyard traffic regulations.  The speed limit is 20 mph in the CIA.  
Outside the CIA, the speed limit is as posted or marked.  No privately owned vehicles are allowed inside 
the CIA with the exceptions of handicap, CO/XO/CMC of ships.  Parking is prohibited on any piers and 
dry dock/waterfront areas.  Do not park on or block the marked fire lanes or crane rail traveling zones 
(marked in yellow) at any time.  Vehicles may stop on the piers or dry dock/waterfront areas for 15 minutes 
for loading and unloading.  An exception may be made for vehicles which are part of the equipment needed 
to do the required work and are attached or connected to the pier of ship; for example, a truck which 
uses a mounted generator or a vehicle with built-in equipment.  Vehicles are subject to search while 
entering, remaining in, or leaving the Shipyard.  Government material being transported out of the CIA 
must be covered by a Property Pass (OP-7), issued and signed by the Security Officer.  Material found 
without a Property Pass will be confiscated and a police officer offense report issued.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Restrictions On Use Of Yellow, Orange-Yellow, Red, And Magenta Materials</TTL><BRK/>
<BRK/>
<TXT>Refrain from use of yellow or orange-yellow materials for the following purposes:  sheeting, tarpaulins, polyethylene 
bottles or other containers, tapes, bags, banding of identification marks on tools, boundary markers such as 
ribbons.  Contractor generated yellow waste materials such as torn foul weather gear must be disposed of by the 
Contractor off-yard.  Shipyard dumpsters and trash cans must not be used for disposal of Contractor generated 
yellow waste materials.  Yellow colored items such as described above are of specific significance within PSNS 
&amp; IMF and are subject to strict controls.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Tape Recorders </TTL><BRK/>
<BRK/>
<TXT>Tape Recorders are not allowed in Naval Base Kitsap (PSNS &amp; IMF), Bremerton unless prior written approval 
has been obtained from the Contracting Officer.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Laptop Computers</TTL><BRK/>
<BRK/>
<TXT>Contractor may bring laptop computers into the CIA provided they are processed through the Visitor Center (Pass 
&amp; ID) and receive a valid badge for personal entry.  They must also complete an AIS SURVEY FORM.  The completed 
form will be processed by the Contracting Officer, and a copy supplied to the Contractor upon approval.</TXT><BRK/>
<BRK/>
<TXT>The laptops:</TXT><BRK/>
<BRK/>
<LST>WILL NOT contain a network card and will not be connected to the Shipyard Local Area Network.</LST><BRK/>
<BRK/>
<LST>WILL NOT process or store Navy Nuclear Propulsion Information – NOFORN data nor will they be used in 
Controlled Nuclear Information Areas or Nuclear Work Areas.</LST><BRK/>
<BRK/>
<LST>WILL NOT use a MODEM inside the shipyard. Systems operating in the Shipyard that are not in compliance 
with this policy will be confiscated.</LST><BRK/>
<BRK/>
<LST>WILL NOT contain a webcam or other means of image capturing capability</LST>.<BRK/>
<BRK/></SPT>
<SPT><TTL>Prohibited Items</TTL><BRK/>
<BRK/>
<TXT>Pursuant to the authority contained in <RID>10 USC 6011</RID> and U.S Navy Regulations, Chapter 8, Article 0826, the following 
items are prohibited:</TXT><BRK/>
<OLG><BRK/>
<OLI>Personal photographic equipment of any kind, including but not limited to cameras (still and video), 
film and cellular telephones with cameras.</OLI><BRK/>
<BRK/>
<OLI>Weapons or other dangerous materials of any kind, including but not limited to firearms, ammunition, 
knives (with blades longer than 2 inches), explosives, incendiaries, personnel defense aerosols/sprays.</OLI><BRK/>
<BRK/>
<OLI>Personal reproduction equipment of any kind, including but not limited to photocopying, copying, and 
recording devices.</OLI><BRK/>
<BRK/>
<OLI>Alcoholic beverages of any kind.</OLI><BRK/>
<BRK/>
<OLI>Personally owned portable electronic devices (PEDs) used for storing data, including, but not limited 
to removable storage devices (e.g., memory sticks, rewriteable CDs and DVDs, Zip and floppy disks).</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Personally Owned Portable Electronic Device (PED) Functionality Matrix</TTL><BRK/>
<TAB WIDTH="94">
<WBK>
   <STS/>
   <TDA COLUMNCOUNT="3" ROWCOUNT="13">
      <COL AUTOWIDTH="0" WIDTH="246.00"/>
      <COL AUTOWIDTH="0" WIDTH="168.00"/>
      <COL AUTOWIDTH="0" WIDTH="189.75"/>
      <ROW>
         <CEL>
<DTA TYPE="STRING"><HL4><HL1><HL3>PED Functionality/Device Type</HL3></HL1></HL4></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL3><HL1><HL4>Example Device</HL4></HL1></HL3>    <BRK/><BRK/></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING"><HL4><HL3><HL1>PSNS &amp; IMF Work Areas</HL1></HL3></HL4></DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="39.00">
         <CEL>
<DTA TYPE="STRING">Any photographic or image capturing capability <BRK/></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Camera, Video Recorder Camera Cell Phone, Scanner</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Prohibited</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="14.25">
         <CEL>
<DTA TYPE="STRING">Single-function cell phone</DTA>
         </CEL>
         <CEL/>
         <CEL>
<DTA TYPE="STRING">Allowed</DTA>
         </CEL>
      </ROW>
      <ROW>
         <CEL>
<DTA TYPE="STRING">Multi-function cell phone</DTA>
         </CEL>
         <CEL/>
         <CEL>
<DTA TYPE="STRING">Allowed</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="39.00">
         <CEL>
<DTA TYPE="STRING">Wireless transmitting capabilities</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">WIFI, 802.xx, Bluetooth</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Allowed if<BRK/>turned off</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="39.00">
         <CEL>
<DTA TYPE="STRING">RF receivers</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Pager, AM/FM Radio, <BRK/>Satellite Radio</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Allowed</DTA>
         </CEL>
      </ROW>
      <ROW>
         <CEL>
<DTA TYPE="STRING">RF transmitter</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">RF Radio Transceiver</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Written</DTA>
         </CEL>
      </ROW>
      <ROW>
         <CEL>
<DTA TYPE="STRING">Walkie-talkie</DTA>
         </CEL>
         <CEL/>
         <CEL>
<DTA TYPE="STRING">Approval Required</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="39.00">
         <CEL>
<DTA TYPE="STRING">Primary function audio recording devices</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Digital voice recorders</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Prohibited</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="75.00">
         <CEL>
<DTA TYPE="STRING">Play-Only Devices without removable memory <BRK/></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">MP3 players, CD Players,<BRK/>Digital Picture Frames, Digital Books</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Allowed</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="63.00">
         <CEL>
<DTA TYPE="STRING">Removable storage media</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Memory Sticks, Thumb Drives, Flash Memory, SD Card</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Prohibited</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="51.00">
         <CEL>
<DTA TYPE="STRING">PEDs capable of connecting to government-owned systems without interface cables or cradles<BRK/><BRK/><BRK/></DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Built-in USB Adapter</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Prohibited</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="90.00">
         <CEL>
<DTA TYPE="STRING">Cables and cradles for privately owned PEDs connecting to a computer system</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">MP3 Player to USB Cable</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Prohibited</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/>
<TXT>No PED device is allowed within 10 ft of Classified Information/Work</TXT><BRK/>
<BRK/>
<TXT>The use of personally owned PEDs to process or store government data/information is prohibited.</TXT><BRK/>
<BRK/>
<TXT><HL1>Additional Definitions on PED Functionality/Device Types</HL1></TXT><BRK/>
<BRK/>
<TXT>Single-function cell phones are defined as cellular devices with no additional photographic or network capabilities 
(can only be used for voice or text message communications over a cellular network, storage of speed dial caller 
ID information, and limited voice recording).  SIM cards/embedded memory for cell phones are permitted.</TXT><BRK/>
<BRK/>
<TXT>Multi-function cell phone and PEDs with more than one functionality are controlled based on the most restrictive 
capability identified in this matrix.</TXT><BRK/>
<BRK/>
<TXT>An RF transmitter is defined as any radio frequency transmitter with the exception of single-function cell phones, 
which are addressed separately.</TXT><BRK/>
<BRK/>
<TXT>Amateur Radio Emergency Service (ARES)/Radio Amateur Civil Emergency Service (RACES) members must be approved 
in writing IAW ref (e) to carry hand-held transceivers.</TXT><BRK/>
<BRK/>
<TXT>CD Players capable of playing CD, CD-R, CD-RW, and MP3 formats are permitted.  Only commercially produced media 
is allowed.  No personally produced audio CDs are allowed within any PSNS and IMF facility.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Employment Restrictions For PSNS/IMF NBK Bremerton, WA.</TTL><BRK/>
<BRK/>
<TXT>Do not employ any person, for any work required by this contract, who is an alien having a residence in a foreign 
country.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><TAI OPT="NAVFAC NW"><SPT><TTL>CONTRACTED SERVICES FOR NBK BANGOR, SILVERDALE, WA.</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Use the following paragraph for escort services into the specific activity 
location of projects located at NBK, Bangor, WA.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Unarmed Escort Services</TTL><BRK/>
<BRK/>
<TXT>Unless noted otherwise in the contract, the contractor, vendors and deliveries will be required to have an unarmed 
escort provided by the Base Operations Support Contract (BOSC) for access to the SWFPAC Waterfront Restriction 
Area (WRA) and Main Limited Area (MLA).  The contractor will be required to contract and coordinate directly 
with the Base Operations Service Contractor (BOSC) for this service. Contact the EJB Contracts Manager at (360) 
396-6352 for escort requirements and to receive detailed information to cost a proposal.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI><TAI OPT="NAVFAC NW"><SPT><TTL>NAVAL BASE KITSAP BANGOR, WA OPERATIONS AREA/SWFPAC PRODUCTION AREA SECURITY/WATERFRONT RESTRICTED AREA/MAIN LIMITED</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraphs for projects located in the SWFPAC Operations 
Area at NBK Bangor, Silverdale, WA.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Contractor personnel will require a B9 Code on their security badge to gain access to the SWFPAC Operation Area.</TXT><BRK/>
<BRK/>
<SPT><TTL>SWFPAC Safety and Security Brief</TTL><BRK/>
<BRK/>
<TXT>A SWFPAC Safety and Security Brief is required for the contractor's complete crew before any work can begin.  
The brief is approximately 30 minutes and is provided in Building 1040 prior to picking up badges.</TXT><BRK/>
<BRK/>
<SPT><TTL>Vehicle Access</TTL><BRK/>
<BRK/>
<TXT>Only authorized company vehicles will be allowed access to the SWFPAC Production Area.  Prior to initial access, 
the individual driving the vehicle must stop by the SWFPAC Pass and ID Office and present the vehicle registration 
to obtain a vehicle pass for this area.  The location of the SWFPAC Pass and ID Office is next to the NBK Pass 
&amp; ID office in B1040, Naval Submarine Base Bangor (360-396-2440).  Vehicle must be owned and titled to the 
company and have a company decal displayed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Delays</TTL><BRK/>
<BRK/>
<TXT>Contractor operations are subject to reasonable delays, suspensions, and restrictions because of emergencies, 
alerts, drills, equipment movements and other such activities.  Contractor must expect 8 hours per month due 
to these delays.  Incorporate anticipated delay into construction schedule.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Searches and Inspections</TTL><BRK/>
<BRK/>
<TXT>Persons entering onto Government Property are, as a condition of access, subject to searches of all vehicles 
and personal belongings.  This includes briefcases, handbags, tool chests, boxes, sealed packages, and personal 
articles.  Random Administrative Vehicle Inspections are conducted by Security Police each day at various hours 
and locations on base.  If selected for a vehicle inspection, be prepared to open your glove box, hood, trunk, 
and other personal items requested by Security.  For the purpose of identification of unattended property, all 
hand carried bags and packages need to have identification tags attached.  Tags may be any type or color as long 
as they contain the individual's name, activity, and contact number.  Compliance with the security directions 
of SWFPAC Security Force Personnel is mandatory.</TXT><BRK/>
<BRK/>
<TXT>Loads or containers whose contents cannot be inspected visually are subject to inspection by Military Working 
Dog (MWD) teams.  MWD inspections must be coordinated in advance with the SWFPAC POC and Contracting Officer 
at least five working days in advance.  Loads that must be inspected by MWD's include, but are not limited to, 
concrete deliveries, asphalt deliveries, dirt loads, gravel loads, fuel trucks, and other enclosed work trucks.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Wireless Devices</TTL><BRK/>
<BRK/>
<TXT>Any commercial mobile wireless device or personal wearable device such as: cell phones, laptops, media devices, 
and smart watches, are prohibited in SWFPAC Areas.  If equipment that contains wireless capabilities are required 
for completion of contracted work, prior approval is required by SWFPAC.  Cell phones with cameras are not allowed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>HERO</TTL><BRK/>
<BRK/>
<TXT>Hazards of Electromagnetic Radiation to Ordnance (HERO) occurs when transmitting from any piece of equipment 
that emits a radio frequency (cell phone or radio (handheld or mobile)).  You are allowed to use your equipment 
while at your work location only, in accordance with HERO Restrictions.  Do not talk on your cell phone or radio 
while in transit within the Waterfront Restricted Area (WRA).  A copy of the HERO form must be carried by anyone 
with a radio or phone and must be presented upon request, provided by SWFPAC Project Manager.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Photography</TTL><BRK/>
<BRK/>
<TXT>Photography by the contractor is prohibited.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Smoking</TTL><BRK/>
<BRK/>
<TXT>Smoking is only permitted in designated smoking areas.  The SWFPAC Project Manager can provide the nearest designated 
smoking area upon request.  Escort may be required.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Flame Producing Devices</TTL><BRK/>
<BRK/>
<TXT>Matches, lighters, and other spark producing devices are not allowed without a Hot Work Permit</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Crane Operations</TTL><BRK/>
<BRK/>
<TXT>Coordinate with SWFPAC Project Manager regarding all work occurring inside contractor cranes operating envelope 
on appropriate safety precautions such as tagging, warning signage, and obstructions.  SWFPAC Safety and Cranes 
may direct tagging out the crane at any time.  The crane envelope is defined as the space the crane hook can 
travel and extending<MET> 152 mm</MET><ENG> 6 inches</ENG> above and beside the side of the crane.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Contracted Services</TTL><BRK/>
<BRK/>
<TXT>Coordinate with SWFPAC Project Manager and Contracting Officer regarding the current list of approved firms that 
are qualified to provide unarmed escorts.  This list is readily available upon request from the Contracting Officer.  
Additions/Omissions of firms to this list after award will not be cause for a claim or change order.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Main Limited Area (MLA) Security</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraphs for projects located in the Main Limited 
Area of NBK Bangor, Silverdale, WA.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The following requirements are in addition to those identified in the paragraph SWFPAC PRODUCTION AREA SECURITY</TXT><BRK/>
<BRK/>
<SPT><TTL>Exchange Badges</TTL><BRK/>
<BRK/>
<TXT>All personnel entering into the Main Limited Area are required to have an exchange badge.  Request Exchange Badges 
through the BAVR system.  Authorized Contractor personnel will be issued temporary uncleared visitor badges.  
Badges for the SWFPAC Main Limited Area will be issued by the SWFPAC Pass and ID Office.  Hours of Operation 
are 7:00 am to 2:00 pm, Monday thru Friday, excluding Holidays.  Pick up badges within 15 calendar days of the 
date of issue, except for emergencies.  Badges not picked up within this timeframe will no longer be valid, and 
the Contractor will resubmit the badge request.  The Contractor will ensure that each badge is returned to the 
SWFPAC Pass and ID Office, upon expiration of the badge or at the completion of the project, whichever occurs 
first.  Failure to do so may affect issuance of future badges.</TXT><BRK/>
<BRK/>
<TXT>For work inside the Main Limited Area, only Prime Contractor personnel will be issued Limited Area badges for 
the contract duration.  All other personnel will be issued Main Limited Area badges only for the period of time 
that their work is scheduled.  Due to the highly restrictive nature of the Main Limited Area, keep LA badge requests 
to the minimum personnel required to accomplish the work.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Flammable Materials</TTL><BRK/>
<BRK/>
<TXT>Flammable materials can be brought into the Main Limited Area with a signed Burn Permit.  Provide a written request, 
identifying the individuals who will be performing this work, a minimum of seven calendar days prior to required 
access, to the Contracting Officer for approval.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Vehicle Access</TTL><BRK/>
<BRK/>
<TXT>Only government and authorized company vehicles will be allowed access to the SWFPAC Production Area and Main 
Limited Area.  Prior to initial access into these areas, the individual driving the vehicle into the Areas must 
stop by the SWFPAC Pass and ID Office and present the vehicle registration in order to receive an additional 
MLA specific vehicle pass.  The location of the SWFPAC Pass and ID Office is the first floor of Building 6401, 
Naval Submarine Base Bangor (360-396-8426).</TXT><BRK/>
<BRK/>
<TXT>Every vehicle will be subject to an inspection and search by NBK Security each time access is requested and at 
any time after access to NBK Bangor is permitted.  Navy security personnel will search all vehicles entering 
and exiting the Main Limited Area.  Avoid transporting sealed containers (of a specific size, the real requirement 
is if the container is large enough to hide a person) into the Main Limited Area.  If such containers must be 
introduced into the area, prior coordination with the SWFPAC POC and Contracting Officer, is required.  Vehicle 
must be owned and titled to the company and have a company decal displayed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Vehicle Disabling</TTL><BRK/>
<BRK/>
<TXT>At the completion of each workday, all vehicles must be left unlocked in a location designated by the SWFPAC 
POC.  Construction equipment must be disabled (e.g., batteries disconnected).  Ignition keys for all vehicles 
left on the work site must be removed from the work site at the end of each workday.  Vehicles cannot be left 
on-site without prior permission from the Contracting Officer.  The request to leave vehicles overnight must 
be requested at least 10 days in advance.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Escorts</TTL><BRK/>
<BRK/>
<TXT>All personnel entering into the Main Limited Area (MLA) are required to have an exchange badge.  All uncleared 
visitors/contractors (denoted by a yellow or orange exchange badge) are required to be escorted at all times 
within the MLA.  Each escort may escort up to five uncleared personnel.  Each group of uncleared personnel must 
stay within visual range<MET> 22.8 m</MET><ENG> 25 yards</ENG> of their assigned escort at all times.  Each group must remain contiguous 
throughout each working day.</TXT><BRK/>
<BRK/>
<TXT>Uncleared personnel are allowed vehicles inside the MLA; however, there must be one escort per vehicle.  The 
escort must ride inside the vehicle of the personnel they are escorting.  The ratio of uncleared personnel to 
escort must not exceed five and is further limited to the number of personnel that can be safely seated inside 
the same vehicle.  The only exemption to this rule is in the case of heavy construction equipment where only 
one operator my safely sit in the vehicle.  Escorts are allowed to walk along side of, or follow in a separate 
vehicle, earth moving equipment such as excavators, rollers, loaders.  Uncleared personnel must be attentive 
to and follow the direction of assigned escorts at all times.</TXT><BRK/>
<BRK/>
<TXT>Unarmed escort services must be obtained in accordance with the paragraph CONTRACTED SERVICES at the Contractor's 
expense.  Prior coordination with the SWFPAC POC and Contracting Officer is required.  A minimum of 5 working 
days notice is required for Military Escort coordination.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Smoking Area</TTL><BRK/>
<BRK/>
<TXT>There is no smoking in the Main Limited Area.  The closest designated smoking area is outside of Alpha Gate (Building 
6024).</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Restrooms</TTL><BRK/>
<BRK/>
<TXT>Use Building 6594 for restrooms while working in the Main Limited Area.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Delays at India Gate</TTL><BRK/>
<BRK/>
<TXT>Due to extraordinary security requirements for Main Limited Area access, all vehicles and their contents will 
be searched by Marine Guard Force personnel on both ingress and egress at India Gate.  This often results in 
vehicle delays of 30 minutes per gate transit, for each vehicle.  Expect delays during morning rush hour (0700-0800) 
up to 60 minutes per gate transit, for each vehicle.  Expect personnel delays during morning rush hour up to 
30 minutes per gate transit, for each person.  The Contractor may leave a cleared company passenger vehicle within 
the Limited Area to serve as a shuttle to the job site(s).  These delays will not be the cause for a claim or 
change order.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Delays Inside Main Limited Area</TTL><BRK/>
<BRK/>
<TXT>Due to extraordinary security requirements for the Main Limited Area and the Waterfront Restricted Area, delays 
due to security drills, alerts, or missile movements can be expected to be more frequent and longer duration 
than would be expected elsewhere on the base.  There is no predictable pattern, but delays averaging up to 8 
hours per month are to be expected and will be considered an existing site condition.</TXT><BRK/>
<BRK/>
<TXT>Due to extraordinary security requirements for the Main Limited Area and the Waterfront Restricted Area access, 
all vehicles and their contents will be searched by Guard Force personnel.  This often results in vehicle delays 
of 30 minutes per gate transit, for each vehicle.  Expect delays at any time with emphasis during morning rush 
hour (0630-0830) up to 60 minutes per gate transit, for each vehicle.  Expect personnel delays at any time with 
emphasis during morning rush hour up to 30 minutes per gate transit, for each person.  Consider these delays 
an existing site condition.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Stockpiled Soil</TTL><BRK/>
<BRK/>
<TXT>Soil must not be stockpiled greater than<MET> 457 mm</MET><ENG> 18 inches</ENG> in height in the Main Limited Area.  All trenches in 
the Limited Area must be covered with traffic rated plates at the end of the work day </TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Clear Zone Requirements</TTL><BRK/>
<BRK/>
<TXT>The Limited Area Clear Zone is defined by a vertical plane, measured<MET> 9.1 m</MET><ENG> 30 ft</ENG> from the Limited Area fence, 
around the entire perimeter of the Limited Area.  There are Clear Zones on the interior and exterior of the Limited 
Area Fence perimeter.  Contractors must not enter this area without permission of the Contracting Officer and 
SWFPAC POC.  A minimum of three days noticed is required for this access to be coordinated.  Construction equipment 
(e.g., tower cranes) must not enter into this clear zone.  Soil must not be stockpiled greater than<MET> 203 mm</MET><ENG> 8 
inches</ENG> in height in the clear zone of the Limited Area.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Containers/Lockboxes</TTL><BRK/>
<BRK/>
<TXT>Contractor containers, lock boxes and equipment left overnight in the Production Area or Limited Area will be 
subject to search by SWFPAC Security Force Personnel.  Construction locks may be utilized but during security 
events Security Forces reserve the right to cut locks for the purposes of inspection without recourse.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Locking of Handholes /Manholes</TTL><BRK/>
<BRK/>
<TXT>All new handholes or manholes over<MET> 619 mm2</MET><ENG> 96 in2</ENG> will be locked and keyed alike with SWFPAC existing locks.  
The key code used will be provided via the SWFPAC Project Manager.</TXT><BRK/>
<BRK/>
<TXT>Existing hand hole and manholes are locked.  The key will be provided to the contractor, with prior coordination 
of at least 3 days, via the SWFPAC Project Manager.  Existing hand hole or manholes fitted with single use cable 
locks will have their locks replaced to match existing.  The specific make/model of cable lock currently being 
used can be provided via the SWFPAC Project Manager.  All hand hole and manholes will be relocked with the approved 
locking devices at the end of each working day.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Waterfront Restricted Area (WRA) Security</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Use the following paragraphs for projects located in the Waterfront Restricted 
Are (WRA) located at NBK Bangor, Silverdale, WA.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The following requirements are in addition to those identified in the paragraph SWFPAC PRODUCTION AREA SECURITY.</TXT><BRK/>
<BRK/>
<SPT><TTL>Vehicle Access</TTL><BRK/>
<BRK/>
<TXT>Only authorized company vehicles will be allowed access to the SWFPAC WRA.  Prior to initial access into these 
areas, the individual driving the vehicle into the WRA must stop by the SWFPAC Pass and ID Office and present 
the vehicle registration in order to receive an additional WRA specific vehicle access pass.  The location of 
the SWFPAC Pass and ID Office is the first floor of Building 6401, Naval Base Kitsap-Bangor (360-396-8426).  
They will need to obtain a WRA Vehicle pass for this area.  The vehicle must be owned and titled to the company 
and have a company decal displayed.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Escorts</TTL><BRK/>
<BRK/>
<TXT>All personnel entering into the Waterfront Restricted Area (WRA) are required to have FAD Clearance and a visitor 
badge with a W code.  All uncleared visitors/contractors are required to be escorted at all times within the 
WRA.  Each escort may escort up to five uncleared personnel.  Each group of uncleared personnel must stay within 
visual range<MET> 222.9 m</MET><ENG> 25 yards</ENG> of their assigned escort at all times.  Each group must remain contiguous throughout 
each working day.</TXT><BRK/>
<BRK/>
<TXT>Uncleared personnel are allowed vehicles inside the WRA; however, there must be one escort per vehicle.  The 
escort must ride inside the vehicle of the personnel they are escorting.  The ratio of uncleared personnel to 
escort must not exceed five and is further limited to the number of personnel that can be safely seated inside 
the same vehicle.  The only exemption to this rule is in the case of heavy construction equipment where only 
one operator my safely sit in the vehicle.  Escorts are allowed to walk along side of, or follow in a separate 
vehicle, earth moving equipment such as excavators, rollers, and loaders.</TXT><BRK/>
<BRK/>
<TXT>Unarmed escort services must be obtained in accordance with the paragraph CONTRACTED SERVICES at the Contractor's 
expense.  A minimum of 5 working days notice is required for Military Escort coordination.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Delays</TTL><BRK/>
<BRK/>
<TXT>Due to extraordinary security requirements for the Main Limited Area and the Waterfront Restricted Area, delays 
due to security drills, alerts, or missile movements can be expected to be more frequent and longer duration 
than would be expected elsewhere on the base.  There is no predictable pattern, but delays averaging up to eight 
hours per month are to be expected and will be considered an existing site condition.</TXT><BRK/>
<BRK/>
<TXT>Due to extraordinary security requirements for the Main Limited Area and the Waterfront Restricted Area access, 
all vehicles and their contents will be searched by Guard Force personnel.  This often results in vehicle delays 
of 30 minutes per gate transit, for each vehicle.  Expect delays at any time with emphasis during morning rush 
hour (0630-0830) up to 60 minutes per gate transit, for each vehicle.  Expect personnel delays at any time with 
emphasis during morning rush hour up to 30 minutes per gate transit, for each person.  Consider these delays 
an existing site condition.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Clear Zone Requirements</TTL><BRK/>
<BRK/>
<TXT>The Waterfront Restricted Area Clear Zone is defined by a vertical plane, measured<MET> 9.1 meters</MET><ENG> 30 feet</ENG> from the 
Limited Area fence, around the entire perimeter of the Limited Area.  There are Clear Zones on the interior and 
exterior of the Waterfront Restricted Area Fence perimeter.  Contractors must not enter this area without permission 
of the Contracting Officer and SWFPAC POC.  A minimum of three days noticed is required for this access to be 
coordinated.</TXT><BRK/>
<BRK/>
<TXT>Construction equipment (e.g., tower cranes) must not enter into this clear zone.  Soil must not be stockpiled 
greater than<MET> 203 mm</MET><ENG> 8 inches</ENG> in height in the clear zone of the Limited Area.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Containers/Lockboxes</TTL><BRK/>
<BRK/>
<TXT>Contractor containers, lock boxes, and equipment left overnight in the Production Area or Limited Area will be 
subject to search by SWFPAC Security Force Personnel.  Construction locks may be utilized, but during security 
events, Security Forces reserve the right to cut locks for the purposes of inspection without recourse.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Locking of Handholes /Manholes</TTL><BRK/>
<BRK/>
<TXT>All new handholes or manholes over<MET> 619 mm2</MET><ENG> 96 in2</ENG> will be locked and keyed alike with SWFPAC existing locks.  
The key code used will be provided via the SWFPAC Project Manager.</TXT><BRK/>
<BRK/>
<TXT>Existing hand hole and manholes are locked.  The key will be provided to the contractor, with prior coordination 
of at least 3 days, via the SWFPAC Project Manager.  Existing hand hole or manholes fitted with single use cable 
locks will have their locks replaced to match existing.  The specific make/model of cable lock currently being 
used can be provided via the SWFPAC Project Manager.  All hand hole and manholes will be relocked with the approved 
locking devices at the end of each working day.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT></TAI><TAI OPT="NAVFAC SE"><SPT><TTL>MATERIALS, FACILITIES, AND SERVICES FOR GUANTANAMO BAY</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This Article is tailored for NAVFAC SE. Use for projects at Guantanamo 
Bay, Cuba.</NPR><BRK/>
<AST/><BRK/></NTE>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate with Guantanamo Bay FEAD to update the prices for services 
and items, prior to PreFinal submittal.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>The availability of Government materials, equipment, and services addressed in the following paragraphs may vary 
subject to local supply priority requirements for operations and maintenance of the base.  Non-availability will 
not be considered as an excusable delay under the General Conditions Clause entitled "Changes."  The cost of 
Government materials, equipment, and services reflected in this specification are subject to fluctuation, revision, 
and adjustment.  Changes in rates or prices for goods and services in this and following paragraphs will not 
be used as a basis for a change to the contract.  Some materials and equipment may be furnished to the Contractor 
by the Government at current rates subject to 3 days' advance notice in writing.  Make all requests to the Contracting 
Officer.  Equipment will not be available for long-term rental.  Short-term equipment rental (1 to 2 days), one-time 
hauling service, and one-time crane service may be available if there is no conflict with Government workload.  
Government equipment will not be provided without Government operators.</TXT><BRK/>
<BRK/>
<SPT><TTL>Medical and Dental Services</TTL><BRK/>
<BRK/>
<TXT>Medical and dental services available to the Contractor's employees are limited in Guantanamo Bay.  The Naval 
Hospital and Dental Clinic are staffed to treat primarily DOD personnel.  Screen prospective employees with the 
objective to exclude those with admitted chronic disorders from traveling to Guantanamo Bay.  Advise prospective 
employees of the limited medical and dental services available in Guantanamo Bay; and explain the Contractor's 
policy concerning the extent of liability and coverage for required treatment.  Make every reasonable attempt 
to prevent personnel with chronic disorders, which may require treatment, such as cardiovascular defects, tuberculosis, 
mental health problems, and alcoholism, from being sent to Guantanamo Bay.  Provide and have available, both 
at the job site and in the berthing areas, first aid for minor and emergency treatment.  Government ambulance 
and medical care, when required, will be billed at the then current rates.  The Naval Hospital and Dental Clinic 
use CHAMPUS Maximum Allowable Charge (CMAC) rates.  These rates are reviewable at <URL HREF="http://www.tricare.mil/CMAC/home.aspx">Health.mil</URL>.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Post Exchange and Commissary Privilege and Recreation Facilities</TTL><BRK/>
<BRK/>
<TXT>Post Exchange and commissary privileges and recreation facilities are available to authorized Contractor personnel 
and dependents of Contractor personnel in accordance with current base regulations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Laundry and Dry Cleaning</TTL><BRK/>
<BRK/>
<TXT>The Government will make available laundry and dry cleaning facilities for Contractor personnel and dependents 
of Contractor personnel at current rates as set forth by the Navy Exchange, Guantanamo Bay, Cuba.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Food Facilities</TTL><BRK/>
<BRK/>
<TXT>Contractor personnel may eat at the Navy Exchange food outlets, or at other open food service facilities on a 
cash basis at current prices.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Contractor Debts</TTL><BRK/>
<BRK/>
<TXT>The Contractor is liable for debts to the Government incurred by their employees for personal services at Guantanamo 
Bay, Cuba, including but not limited to private telephone service, medical and dental services, and W.T. Sampson 
School expenses.  If an employee departs the Guantanamo Bay Naval Base without liquidating debts, sufficient 
funds to cover this type of obligation will be withheld from Contractor payments until the debts are paid.  Certify 
with every progress payment that all debts with the Naval Station are paid, including but not limited to, utility 
bills, HAZWASTE disposal charges, and Naval Hospital bills.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Energy Conservation</TTL><BRK/>
<BRK/>
<TXT>Observe and comply with the Base Energy Conservation Regulation, COMNAVBASEGTMO Instruction <RID>11300.3</RID> series.  
It is mandatory that the Contractor obtain a copy of this instruction and post it in a conspicuous location for 
the Contractor's employees to read.  Copies of the instructions are available from the ROICC office.  Ensure 
that employees comply with these regulations at all times.  It is suggested that an employee be appointed as 
energy monitor by the Contractor for buildings under the jurisdiction of the Contractor.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Drug Abuse by Contract Employees</TTL><BRK/>
<BRK/>
<TXT>The Secretary of the Navy has determined that the illegal possession and use of drugs and paraphernalia by civilian 
and contract employees in the military setting contributes directly to military drug abuse and undermines command 
efforts to eliminate drug abuse among military personnel.  The policy of the Department of the Navy, including 
the Marine Corps, is to deter and detect drug offenses by civilian and contract employees on military installations.  
Measures to be taken to identify drug offenses on military installations, and to prevent introduction of illegal 
drugs and paraphernalia include routine, random inspections of vehicles and personnel possessions on entry or 
exit, with drug detection dog teams, when available.  Where there is probable cause to believe that a civilian 
or contract employee on board a Naval or Marine Corps installation has been engaged in use, possession, or trafficking 
of drugs, that employee may be restricted or detained for the period necessary until that employee can be removed 
from the installation or can be turned over to local law enforcement authorities having jurisdiction, as appropriate.  
When illegal drugs are discovered during an inspection or search of a vehicle operated by a civilian or contract 
employee, the employee and vehicle may be detained for a reasonable period of time necessary to turn the employee 
and the vehicle over to appropriate civil law enforcement officials; action may be taken to suspend, revoke, 
or deny installation driving privileges.  Implicit with the acceptance of this contract is the Contractor's agreement 
to comply with Federal statutes, laws, and regulations, including those regulations issued by the commander of 
the military installation.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Government Utilities</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Coordinate with and add a reference to this paragraph in Section 01 50 
00 TEMPORARY CONSTRUCTION FACILITIES AND CONTROLS for utility services.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL>Rates</TTL><BRK/>
<BRK/>
<TXT>The contract Clause "Availability and Use of Utility Services" applies.  Water and electricity will be available 
at designated outlets at the prevailing Government rates.  Current rates (01 July 2023) are as follows:</TXT><BRK/>
<BRK/>
<ITM>Electricity - $ 412.37 per thousand kWh</ITM><BRK/>
<ITM>Water       - $ 18.37 per thousand gallons</ITM><BRK/>
<ITM>Sewage      - $ 2.74 per thousand gallons</ITM><BRK/>
<BRK/></SPT>
<SPT><TTL>Metering</TTL><BRK/>
<BRK/>
<TXT>Provide meters for power and water usage in office and shop areas.  The meters provided must be sealed and tagged 
to indicate last calibration date and name of the person performing the calibration.  The Government reserves 
the right to require the recalibration of the meters if erroneous readings are suspected.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Backflow Protection</TTL><BRK/>
<BRK/>
<TXT>Provide Backflow Protection at the source for temporary water connections used in accomplishment of this contract.  
Backflow device must be tested and pass certification prior to opening connection.  Person installing and certifying 
device must be trained in accordance with <RID>NFESC UG-2029-ENV</RID>.  Cross-Connection Control and Backflow Prevention 
Program Certification must be current prior to installation.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Port-a-let, Refuse Collection and Sanitary Sewage Trucking Service</TTL><BRK/>
<BRK/>
<TXT>These services are provided by the Base Maintenance Services Contractor, V2X.  For the current rates, call 830-273-0685.</TXT><BRK/>
<BRK/>
<TXT>Refuse containers will be furnished and serviced by the Government at living quarters.  Refuse collection service 
is mandatory.  Contractors are required to meet base regulations concerning collection and disposal of refuse.  
Pickup is scheduled and charged based on volume of the dumpster, not necessarily the volume of refuse.  Only 
refuse deposited in the Government-furnished containers will be collected.  This service does not include articles 
left outside of the containers.  This service is not available for construction or demolition sites.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Petroleum Products</TTL><BRK/>
<BRK/>
<TXT>Sales of petroleum products are made from Naval Station Supply Department Stocks under special deposit procedures 
based on prevailing stock ledger prices.  Prices are adjusted on average two times per year.  Fuel may be purchased 
in accordance with a Fuel Purchase Agreement between DLA Fuels and the Contractor.</TXT><BRK/>
<BRK/>
<TXT>Regular filling station pumps at the Navy Exchange (NEX) service station may be utilized by paying the current 
price at time of purchase.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Purchases From the Government</TTL><BRK/>
<BRK/>
<SPT><TTL>Sale of Government Supplies</TTL><BRK/>
<BRK/>
<TXT>Provisions and camp supplies other than petroleum products will be sold to the Contractor from Naval Station 
Supply Department Stocks under NAVSUP Fleet Logistics Center Jacksonville (NAVSUP FLC) regulations.  Miscellaneous 
construction materials may be sold to the Contractor under the same procedure if such sales are not detrimental 
to the Naval Station Supply Department stock position as determined by the Naval Station Supply Officer.  Materials 
other than petroleum products may be issued as required, during normal working hours.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Payment for Purchases From the Government</TTL><BRK/>
<BRK/>
<TXT>Invoices covering sales of equipment and materials specified must be charged to a special deposit account, to 
be established by the Contractor in advance.  Provide a cash deposit (only) to the Naval Station Comptroller 
prior to incurring charges.  Maintain a minimum balance in this account equal to two times the anticipated monthly 
expenditures or $200, whichever is greater.  Comply with directives governing special deposit accounts as established 
by the Comptroller, U.S. Naval Base, Guantanamo Bay, Cuba.  Failure to settle accounts due promptly will jeopardize 
the availability of goods and services.  The Government is entitled to withhold special deposit account arrearages 
from progress payments.</TXT><BRK/>
<BRK/></SPT>
</SPT><SPT><TTL>Electronic Invoices</TTL><BRK/>
<BRK/>
<TXT>Submit invoices electronically via e-mail or computer disc.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>E-mail and Internet</TTL><BRK/>
<BRK/>
<TXT>The Contractor must have e-mail and Internet service for their office on the base.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Available Living Quarters</TTL><BRK/>
<BRK/>
<SPT><TTL>Crew Berthing</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Check with the Public Works Office at U.S. Naval Base Guantanamo Bay, 
Cuba to determine where Contractor employees will be berthed and if berthing 
is available.  Use this paragraph for Crew Berthing requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>Provide temporary housing facilities (man camp) for prime and subcontractor workers.  Contractor is responsible 
to provide all required facilities for Contractor personnel at a site designated by the Contracting Officer's 
designated representative.  Tie into existing utilities at designated locations and maintain these utilities 
until completion of the project.  The Government will bill Contractor for utilities at prevailing rates.  Upon 
completion of the project, restore site to the original condition.</TXT><BRK/>
<BRK/>
<SPT><TTL>Codes</TTL><BRK/>
<BRK/>
<TXT>Temporary berthing units must be weather tight house trailers.  Design, construct, and erect the trailers in 
accordance with <RID>ICC IBC</RID>, the latest edition of the <RID>24 CFR 3280</RID>, <RID>ASCE 7-16</RID> and as modified herein.  Provide air 
conditioning units conforming to <RID>NFPA 90A</RID> and <RID>ANSI/AHRI 210/240</RID>.  Electrical work must conform to <RID>NFPA 70</RID>.  Design 
wind velocity must be in accordance with <RID>UFC 3-301-01</RID> for location of NS Guantanamo Bay.  Seismic loading criteria 
must be in accordance with NS Guantanamo Bay, of the referenced UFC.</TXT><BRK/>
<BRK/>
<TXT>Minimum furnishings must include a bed (single or bunked) and a wardrobe or dresser for each person.  Minimum 
house furnishings must also include a television, cable box, telephone, and refrigerator that are shared with 
other assigned housemates.  Two house mates may be assigned to one trailer.  Provide a house trailer with a minimum 
of<MET> 9.3 square meters</MET><ENG> 100 square feet</ENG> of useful floor area up and above the floor area required for the private 
furnishings and joint furnishings specified and the bathroom.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Description</TTL><BRK/>
<BRK/>
<TXT>The work includes delivery, erection, and removal of temporary berthing including all necessary furnishings adequate 
to house the Contractor's workforce for the duration of the project, complete and ready for use.  The work includes 
providing a group site with stairs, platforms, railings, walks, parking, lighting and utility connections to 
existing water supply, sanitary, and electrical systems.  Site must be properly drained.  Provide refuse collection.  
Provide temporary berthing and utility connections prior to workforce arriving.  Provide furnishings and equipment 
as required and specified.</TXT><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Confirm that the referenced documents are included in the project.</NPR><BRK/>
<AST/><BRK/></NTE>
<OLG><BRK/>
<OLI>Layout and Location:  Locate the trailers at a group site indicated on the drawings.</OLI><BRK/>
<BRK/>
<OLI>Shipping and Delivery:  Provide transportation for temporary house trailers and associated accessories 
to and from the Naval Station and to and from the temporary site location as determined by the Contracting 
Officer, bearing all costs incurred.  Delays in shipping must not cause an extension in the contract 
completion date, unless Contracting Officer determines otherwise.</OLI><BRK/>
<BRK/>
<OLI>Anchors, Piers and Tie-Down Components:  Provide anchors, piers and tie-down components, used in the 
installation of temporary housing units, tested, listed and approved by <RID>FAC Chapter 15C-1</RID>.</OLI><BRK/>
<BRK/>
<OLI>Stairs and Ramps:  Provide stairs, ramps, platforms and railings as required to facilitate access from 
finished grade to the temporary housing units.  Construct stairs, ramps, and railings in accordance with <RID>
NFPA 101</RID>.</OLI><BRK/>
<BRK/>
<OLI>Utility Connections:  The facility must be connected to existing sanitary collection, water distribution, 
and electrical systems.  Provide backflow protection in accordance with Section <SRF>01 50 00</SRF> TEMPORARY CONSTRUCTION 
FACILITIES AND CONTROL.  Meter power and water usage for temporary berthing with meters furnished and 
installed by, and at the expense of, the Contractor.  Costs associated with establishing utility connection 
are the responsibility of the Contractor.  Notify Contracting Officer 15 days prior to utility connections.</OLI><BRK/>
<BRK/>
<OLI>Refuse Collection:  Provide refuse collection through the Base Maintenance Service Contractor.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Installation</TTL><BRK/>
<OLG><BRK/>
<OLI>Erection:  Assemble, connect, and finish the facility in accordance with the <RID>24 CFR 3280</RID>, the manufacturer's 
written instructions, and in accordance with applicable codes and ordinances.  Provide temporary housing 
units with anchors, piers, and tie-down components in accordance with the minimum requirements of <RID>FAC Chapter 15C-1</RID>
.</OLI><BRK/>
<BRK/>
<OLI>Maintenance:  Maintain the site and temporary house trailers.  Suitably paint and maintain the temporary 
facilities.  Failure to do so is sufficient reason to require their removal.  Keep the site free of refuse 
and unused debris.  Provide a custodial service to clean each temporary berthing unit.</OLI><BRK/>
<BRK/>
<OLI>Removal:  Remove temporary housing units and associated sited improvements within 45 days after the contract 
is completed.  Notify Contracting Officer 15 days prior to disconnecting utilities.</OLI><BRK/>
<BRK/>
<OLI>Acceptance Testing:  Upon completion and before final acceptance of work, test each system to demonstrate 
compliance with the contract requirements, including testing of air conditioning, ventilation, lighting, 
and plumbing systems.  Adjust controls and balance systems prior to final acceptance of completed systems.  
Test controls through every cycle of operation.  Test safety controls to demonstrate performance of required 
function.  Correct defects in work and repeat tests.  Furnish instruments, connecting devices, and personnel 
for tests.  Flush and clean piping before placing in operation.  Clean equipment, piping, strainers, 
ducts, and provide new filters.</OLI><BRK/></OLG>
<BRK/></SPT>
</SPT><SPT><TTL>Contractor Management/Supervisory Housing</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE: Check with the Public Works Office at U.S. Naval Base Guantanamo Bay, 
Cuba to determine where contractor employees will be berthed and if berthing 
is available.  Use this paragraph if Contractor Management/Supervisory Housing 
is available.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For this contract, the Government will provide up to two housing units (based on availability) for the Contractor's 
use.  These units are reserved for use by accompanied or unaccompanied management/supervisory personnel only.</TXT><BRK/>
<BRK/>
<TXT>Housing is assigned as follows:  accompanied personnel by family composition with maximum family size of three 
dependents; unaccompanied personnel assignment will be made based on a minimum of one person per bedroom.  If 
house sharing, accompaniment by dependents will not be allowed.  The Government will provide family housing units 
with the following appliances:  refrigerator, stove, dishwasher, microwave, washer, and dryer.  All furnishings 
other than the listed appliances must be provided by the Contractor.  Issuance of these housing units and rental 
rates are controlled by the Housing Department, Building 2295, phone 757-458-4172.  Should the Contractor's assigned 
units not be fully occupied, the Housing Department will cancel the assignment and return the unit to inventory 
for other use.  Personnel must abide by Family Housing instructions, which are not part of the contract but available 
on request.  Contractors will pay rent under the Fair Market Rental (FMR) Program.  Rental rates include trash 
and maintenance costs.  Rental rates are normally adjusted annually based on market appraisal, utilities cost 
adjustment or the annual Consumer Price Index.  Family housing units are equipped with electric and water meters.  
Utilities cost is billed along with monthly rent and is based on established rates and actual consumption.  Rent 
is due in advance.  No personal checks accepted.  Remit payments via the Department of Treasury's web portal <URL>
www.pay.gov</URL>.  The Contractor is responsible for the applicable monthly rent above plus actual utilities.  Rates 
may be adjusted annually.  Current Fair Market Rental Rates as of March 2023:</TXT><BRK/>
<BRK/>
<TAB HEADERROWS="0" WIDTH="46">
<WBK>
   <STS>
      <STY SID="s50">
         <ALN HORIZONTAL="CENTER" VERTICAL="BOTTOM"/>
      </STY>
   </STS>
   <TDA COLUMNCOUNT="2" ROWCOUNT="6">
      <COL AUTOWIDTH="0" WIDTH="176.25"/>
      <COL AUTOWIDTH="0" WIDTH="120.00"/>
      <ROW AUTOHEIGHT="0" HEIGHT="13.50">
         <CEL>
<DTA TYPE="STRING">Rental</DTA>
         </CEL>
         <CEL>
<DTA TYPE="STRING">Rate</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="26.25">
         <CEL>
<DTA TYPE="STRING">2 Bedroom - 1 Bath</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$1,043 Month</DTA>
         </CEL>
      </ROW>
      <ROW>
         <CEL>
<DTA TYPE="STRING">2 Bedroom - 1.5 Bath</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$1,380 Month</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="31.50">
         <CEL>
<DTA TYPE="STRING">3 Bedroom - 1 Bath</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$1,249 Month</DTA>
         </CEL>
      </ROW>
      <ROW>
         <CEL>
<DTA TYPE="STRING">3 Bedroom - 2 Bath</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$1,380 Month</DTA>
         </CEL>
      </ROW>
      <ROW AUTOHEIGHT="0" HEIGHT="33.00">
         <CEL>
<DTA TYPE="STRING">4 Bedroom - 2.5 Bath</DTA>
         </CEL>
         <CEL STYLEID="s50">
<DTA TYPE="STRING">$1,649 Month</DTA>
         </CEL>
      </ROW>
   </TDA>
</WBK>
<BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/><BRL/></TAB><BRK/></SPT>
<SPT><TTL>Contractor Berthing Facilities (CBF)</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  Check with the Public Works Office at U.S. Naval Base Guantanamo Bay, 
Cuba to determine where Contractor employees will be berthed and if berthing 
is available.  Use this paragraph for Contractor Berthing Facilities (CBF) requirements.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<TXT>For this task order, the Government will supply the number of ESBF beds for the period of time as supported by 
the Contractor's personnel-loaded CPM schedule provided in Section <SRF>01 32 17.00 20</SRF> COST-LOADED NETWORK ANALYSIS 
SCHEDULE (NAS).  Except for allowed fair market rental units (Family/Management Quarters) Contractor employees 
(unaccompanied status) will be berthing with the Navy Exchange, Navy Gateway Inns and Suites Division (NGIS) 
in ESBF located on both sides of the bay; Windward (WW) and Leeward (LW).  ESBF primarily consists of multi-occupancy 
rooms with wither shared or gang head bathrooms.  Due to the configuration of most facilities, they are not suitable 
for mixing genders; therefore, female residents are not accepted by NGIS for occupancy in ESBF.  Provide alternate 
berthing for all female employees.</TXT><BRK/>
<BRK/>
<SPT><TTL>Pricing</TTL><BRK/>
<BRK/>
<TXT>Costs are based on occupied beds.  The current rate is $15.00 per person per bed, regardless of room configurations 
with the exception of suites located at Building AV640 which are $30.00.  Rates are reviewed each March for implementation 
each October.  Should prices increase, the Contractor will receive, at a minimum, 30 days notification.  Bed 
night costs are not negotiable.</TXT><BRK/>
<OLG><BRK/>
<OLI>Utility Rates:  In addition to the rates for berthing, the utility rate of $8.52 per day per person will 
apply, regardless of room configuration.  Rates may be adjusted each Fiscal Year.  This rate will be 
billed separately.  Any price increases [and][or] decreases to CBF and utility rates/costs will not be 
subject to economic price adjustment(s) and any increases [and][or] decreases to these areas of Contractor 
overhead will not be considered and reimbursed pursuant to the changes and disputes clauses to this contract.</OLI><BRK/>
<BRK/>
<OLI>At no additional cost to the Government, the Contractor must provide temporary housing for their unaccompanied 
employees who do not qualify for CBF or if CBF is full.  For transient lodging information or to make 
reservations contact the NGIS by e-mail at ngis.gtmo.reservation@navweb.org, by phone at 757-458-2044 
or by visiting their main office located at Building 1670.  Current transient rates as of June 2023 range 
from $60.00 to $90.00 depending on room configuration and location.</OLI><BRK/></OLG>
<BRK/></SPT>
<SPT><TTL>Billing</TTL><BRK/>
<BRK/>
<TXT>Contractors will be billed monthly for the number of beds assigned to their company.  Contractors are charged 
for beds assigned to employees on leave unless the employee removed all personal property and checks out of the 
facility.  Remit payment on or before due dates.  Administrative and late fees apply.  Failure to promptly pay 
can result in eviction from the premises regardless of impact to Contractor ability perform the contract specifications.  
NGIS makes no guarantee of bed availability or berthing locations.</TXT><BRK/>
<BRK/></SPT>
<SPT><TTL>Contractor Berthing Agreement</TTL><BRK/>
<BRK/>
<TXT>Prior to berthing any employees, complete a Contractor Berthing Agreement with the NGIS.  A copy of this agreement 
is available at the NGIS management offices located at Building 1670.  To determine availability, advance registration 
and notification of berthing requirements is highly recommended; send information via e-mail to NGIS mail box 
at <URL HREF="ngis.gtmo.reservation@navweb.org">ngis.gtmo.reservation@navweb.org</URL>.  Allow 5-10 days for responses.</TXT><BRK/>
<BRK/></SPT>
</SPT></SPT></SPT></TAI><TAI OPT="ARMY"><SPT><TTL>ARMY AND ARMY NATIONAL GUARD REQUIREMENTS AND RESTRICTIONS</TTL><BRK/>
<NTE><BRK/>
<AST/><BRK/>
<NPR>NOTE:  This paragraph is tailored for ARMY.  Use for projects on Army and Army 
National Guard installations.</NPR><BRK/>
<AST/><BRK/></NTE>
<BRK/>
<SPT><TTL><SUB>3Rs Explosive Safety Education Training Certificate</SUB></TTL><BRK/>
<BRK/>
<TXT>All Contractor and subcontractor employees requiring access to Army or Army National Guard installations, facilities, 
and areas for the performance of a contract or subcontract must complete the 3Rs (Recognize, Retreat, Report) 
Explosives Safety Education Program training.  Complete the training within 30 calendar days after the date of 
receipt of a written notice of award.  The Contractor is responsible for ensuring that all subcontractor employees 
complete the training before access to the installation is required for performance of the subcontract.  The 
Contractor is also responsible for ensuring that all contractor and subcontractor employees renew the training 
annually for the duration of the performance period of the contract or subcontract.  Submit certificates of completion 
for each Contractor and subcontractor employee subject to this requirement to the Contracting Officer’s Representative 
(COR) or to the Contracting Officer, if a COR is not assigned, within 5 calendar days after completion of training.  
3Rs Explosives Safety Education Program training is available at the following website: <URL HREF="https://www.denix.osd.mil/uxo/3rs-training">https://www.denix.osd.mil/uxo/3rs-training/</URL>
.</TXT><BRK/>
<BRK/></SPT>
</SPT></TAI></PRT><PRT><TTL>PART 2   PRODUCTS</TTL><NED/><BRK/>
<BRK/>
<TXT>Not used.</TXT><BRK/>
<BRK/></PRT>
<PRT><TTL>PART 3   EXECUTION</TTL><BRK/>
<BRK/>
<TXT>Not used.</TXT><BRK/>
<BRK/></PRT>
    <END/><BRK/></SEC>
